{"text_format":"5","workbook":"xls","n_sheets":9,"sheets":["Legend(RU)","Legend(EN)","Intellect","Intellect (ONVIF)","AxxonNext","AxxonNext (ONVIF)","Special Notes","AS IS","Out of Support"],"not_rendered":{"images":4,"external_links":1,"defined_names":6},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Legend(RU)","index":0,"n_rows":14,"n_cols":3,"rows_kept":14,"merged":[[0,0,1,2],[2,0,2,2],[3,0,3,2],[4,1,4,2],[13,1,18,2]],"flags":["formulas_cached_only"]}
["Список IP-устройств, поддерживаемых компанией ITV | AxxonSoft\nв Drivers Pack 3.2.24"]
[]
["Версия документа V2 от 19.05.2014"]
["Актуально для релиза ПО «Интеллект» 4.9.0, ПО  «Интеллект Лайт»  и Axxon Next 3.5.1 c установленным обновлением IPDriverPack build 3.2.24.1446"]
[null,"Закладки"]
[null,"Intellect","Список устройств, поддерживаемых в \"Интеллект\", \"Интеллект Лайт\""]
[null,"Intellect (ONVIF)","Список устройств, протестированных производителем оборудования и работающих в \"Интеллект\", \"Интеллект Лайт\" в соответствии со стандартом ONVIF"]
[null,"Axxon Next","Список устройств, поддерживаемых в Axxon Next"]
[null,"Axxon Next (ONVIF)","Список устройств, протестированных поизводителем оборудования и работающих в Axxon Next в соответствии со стандартом ONVIF"]
[null,"AS IS","Список интеграций, реализованных в ПО ITV | Axxonsoft, техническая поддержка по которым не оказывается. Вы можете использовать их по вашему усмотрению"]
[null,"Out of Support","Список интеграций, реализованных в ПО ITV | Axxonsoft, техническая поддержка по которым не оказывается, т.к. устройства сняты с поддержки самим производителем. Вы можете использовать их по вашему усмотрению"]
[null,null,"используйте стандартные функции Excel для поиска необходимой информации в списках"]
[]
[null,"Уважаемые партнеры! Будьте внимательны! \nКомпания несет ответственность за стабильную работу  с  ПО только IP-устройств, указанных в этом документе.  Обращайте внимание на версию прошивки и точное наименование модели для корректной совместной работы ПО и IP-устройства."]

{"sheet":"Legend(EN)","index":1,"n_rows":19,"n_cols":3,"rows_kept":19,"merged":[[0,0,1,2],[2,0,2,2],[3,0,3,2],[4,1,4,2],[10,1,10,2],[18,1,23,2]],"flags":["formulas_cached_only"]}
["List of  IP-devices, supported with DriversPack 3.2.24 by AxxonSoft"]
[]
["Document version V2 of May 19, 2014"]
["Is relevant for Axxon Intellect Enterprise v4.9.0, Axxon Intellect Lite and Axxon Next 3.5.1 with IPDriverPack build 3.2.24.1446"]
[null,"Sheets"]
[null,"Axxon Intellect Enterprise","List of devices, integrated to Axxon Intellect Enterprise and Axxon Intellect Lite "]
[null,"Axxon Intellect Enterprise (ONVIF)","List of devices, tested by vendor and working with Axxon Intellect Enterprise and Axxon Intellect Lite through ONVIF"]
[null,"Axxon Next","List of devices, integrated to Axxon Next"]
[null,"Axxon Next (ONVIF)","List of devices, tested by vendor and working with Axxon Next through ONVIF"]
[null,"AS IS","List of unsupported integrations which can be used at your own discretion "]
[null,"Color designations in the table  \"Full list\""]
[null,null,"New integrations in the version are underlined orange"]
[null,null,"Improved integrations  in the version are undelined pink"]
[null,null,"Integrations, borrowed from the earlier versions are underlined blue"]
[null,"Out of Support","List of unsupported devices since they are no longer supported by manufacturers. You are free to try them as you wish."]
[null,null,"use the  Excel standard functions for searching the necessary information in the lists"]
[]
[]
[null,"Dear partners! Pay attention!\nThe company is only  responsible for sustained performance of the software with IP-devices, stated in this document. Draw your attention to the firmware version and exact model name for correct joint cooperation of the software and IP-device."]

{"sheet":"Intellect","index":2,"n_rows":1205,"n_cols":28,"rows_kept":1205,"flags":["formulas_cached_only"]}
["Vendor","Model","Type","Firmware","Channel","Multistream","Streams","MJPEG","MPEG","H.264","Wavelet","MxPEG","Max resolution","Mid resolution","Min resolution","Settings","Multicast","Audio IN","Audio Out","PTZ","Alarm IN","Alarm OUT","Built-in Storage","Analytics","x64 modules support","Notes","Notes in English"]
["!ONVIF","1-channel device",null,"Onvif Spec v.1.02","1",null,null,"+","+","+",null,null,"depending on the device","depending on the device","depending on the device","+",null,"+","+","+.","+","+","+.","+.","+","1. Список устройств, поддерживающих ONVIF, перечислен на официальном сайте форума:\nhttp://www.onvif.org/ConformantProducts/ProductList.aspx \nОбращайте внимание на наименование модели и прошивку. 2. Работа устройства Onvif за NAT не поддерживается. Устройство должно быть с отдельным внешним IP адресом.","1. A list of ONVIF-conformant devices may be found at ONVIF's official website:\nhttp://www.onvif.org/ConformantProducts/ProductList.aspx\nPay attention to the model names and firmware. 2. It's not supported if device is connected via NAT. It must have separate external IP address."]
["!PSIA","1-channel device",null,"PSIA spec. 1.1","1","-",null,"+","-","+",null,null,"depending on the device","depending on the device","depending on the device","+",null,"+","-","-","-","-",null,"-","+",null,null,"improved"]
["360Vision","360Vision Predator Pred-XX-IP","Camera ","1.3/20090127","1",{"$nulls":3},"+",{"$nulls":3},"720x576","720х288","352x288","+",{"$nulls":3},"+",{"$nulls":4},"+"]
["3S Vision","3S Vision S4071","Camera ","V1.03_STD-1","4",null,null,"+",null,"+",null,null,"704x480","704x480","MJPEG: 352x288 | H.264: 352x240","+",null,null,"-","+","-","-",null,"-","+"]
["3S Vision","3S Vision N4012 / N5012","Camera","V1.04_STD-1.20131127","1","+","3","+",null,"+",null,null,"1920x1080","1280x720","720x400",null,null,"+","-","+","-","-","-","-","+",null,null,"new"]
["3S Vision","3S Vision N1011","Camera"," V1.04_STD-1","1","+","3","+",null,"+",null,null,"QSXGA Mode: 2560x1920(h.264)/1280x960(mjpeg). FullHD Mode: from web(h.264)/1920x1080(mjpeg)","QSXGA Mode: 1280x960. FullHD Mode: from web","QSXGA Mode: 640x480. FullHD Mode: from web","+",null,"+","-","-","-","-","-","-","+","Значения битрейта зависят от значения разрешенияНа третьем потоке потоке нельзя выставить значение разрешения 1600x1200 если на первом потоке стоит значение разрешения выше 1600x1200","Bit rate values depend on the selected resolution. It is impossible to set 1600x1200 resolution on the third stream, if the resolution is higher than 1600x1200 on the first stream.","new"]
["3S Vision","3S Vision N1031","Camera","V1.04_STD-1","1","+","3","+",null,"+",null,null,"QXGA Mode: 2048x1536(h.264)/1280x960(mjpeg). FullHD Mode: from web(h.264)/1920x1080(mjpeg)","QXGA Mode: 1280x960. FullHD Mode: from web","QXGA Mode: 640x480. FullHD Mode: from web","+",null,"+","-","-","-","-","-","-","+","Значения битрейта зависят от значения разрешенияНа третьем потоке потоке нельзя выставить значение разрешения 1600x1200 если на первом потоке стоит значение разрешения выше 1600x1200","Bit rate values depend on the selected resolution. It is impossible to set 1600x1200 resolution on the third stream, if the resolution is higher than 1600x1200 on the first stream.","new"]
["3S Vision","3S Vision N1072","Camera","V1.09.1_STD-1","1","+","3","+",null,"+",null,null,"UXGA Mode : 1600x1200 / WXGA Mode: from web","UXGA Mode : 640x480 / WXGA Mode: from web","UXGA Mode : 320x240 / WXGA Mode: from web","+",null,"+","-","-","-","-","-","-","+","Значения битрейта зависят от значения разрешения","Bit rate values depend on the selected resolution.","new"]
["3S Vision","3S Vision N6071","Camera ","V1.10_STD-1","1",null,null,"+",null,"+",null,null,"1600x1200","640x480","320x240","+",{"$nulls":8},"+","1. Диапазон доступных значений битрейта меняется в зависимости от значения выбранного разрешения.\n2. Диапазон доступных разрешений меняется в зависимости от значения настройки sensor-mode.","1. The range of available bit rate values ​​vary depends on the selected resolution.\n2. The range of available permits varies depends on the sensor-mode setting value."]
["3S Vision","3S Vision N8071","Camera","V1.08.1_STD-1","1","+","3","+",null,"+",null,null,"UXGA Mode : 1600x1200 / WXGA Mode: from web","UXGA Mode : 640x480 / WXGA Mode: from web","UXGA Mode : 320x240 / WXGA Mode: from web","+",null,"+","-",{"$nulls":3},"-","-","+","Значения битрейта зависят от значения разрешенияВ ПО ITV смену режима Sensor mode следует производить в веб-интерфейсе камеры","Bit rate values depend on the selected resolution. In Axxon software the Sensor mode is to be changed in the camera web interface.","new"]
["3S Vision","3S Vision N9018","Fisheye Camera","V1.00.1_STD-1","1","+","3","+",null,"+",null,null,"1920x1080","1280x720","720x400","+",null,"-","-","-","-","-","-","-","+","Настройка битрейта имеет динамический диапазон, который зависит от текущих значений настроек разрешений, частоты кадров, частоты включения опорных кадров, ТВ-стандарта.","Bit rate has a dynamic value range that depends on current resolution, fps, key frame rate and TV standard.","new"]
["Abron","Abron ABC-i422VR","Camera","C1.0.20.2_Y",1,null,null,"+","-","+","-","-","1920x1080","640x480","320x240","+","-","+","+","-","+","+","-","motion detection","+","Диапазон значений битрейта зависит от значения FPSВ ПО ITV настройку опорных кадров следует производить в веб-интерфейсе камеры.","Bitrate range depends on FPSB value. Key frames are to be set in the camera web interface."]
["ACTi","ACTi ACD-2000Q encoder","Encoder","V3.04.08","4",null,null,"+","+","-","-","-","720x480","720x480","352x240","+",null,"-","-","-","+","+","-","-","-"]
["ACTi","ACTi ACD-2100 encoder","Encoder","A1D-220-V3.14.19-AC","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","352x288","+",null,"+","-","+","+","+",null,"motion detection","-","1. при MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","1. With MPEG-4, in Intellect, you may use the Quality slider to adjust the video stream bit rate. "]
["ACTi","ACTi ACD-2400 encoder","Encoder","firmware system AGD-R2N-V2.06.00-AC; firmware channel A1D-220-V3.12.13-AC","16",null,null,"+","+",{"$nulls":3},"720x576","640x480","352x288","+",null,"+","-","+","+.","+.",null,"-","-","1. При задействовании сразу большого количества каналов устройству неоходимо около 2-х минут на старт после запуска Intellect.\n2. телеметрия будет пока что работать только с камерами с протоколом Pelco-D, 9600. В Intellect следует выбирать телеметрию \"IPCamera\"","1. When using multiple channels simultaneously, the device needs about 2 minutes to start up, after Intellect is started up. \n2. So far, telemetry only works with cameras that support the Pelco-D protocol, 9600 bps. In Intellect, select IPCamera telemetry."]
["ACTi","ACTi ACM-1101P","Camera ","A1D-220-V3.09.14-AC","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","352x288","+",null,"+","-",{"$nulls":4},"-","-","при MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","in MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate."]
["ACTi","ACTi ACM-1231","Camera ","A1D-V3.11.13","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",null,"+","-",{"$nulls":4},"-","-","1. У самой камеры есть ограничение на fps:\n-при разрешении 1280x1024 максимально 8 fps\n2. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\"  в Intellect регулирует bit rate MPEG-4 видеопотока","1. The camera itself has frame rate limits: \n1280x1024 resolution, max. 8 fps.\n2. The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream."]
["ACTi","ACTi ACM-1311","Camera ","A1D-V3.11.13","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","352x288","+",null,"+","-",{"$nulls":4},"-","-","1. при MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","1. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate."]
["ACTi","ACTi ACM-1431","Camera ","A1D-V3.11.13","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","352x288","+",null,"+","-",{"$nulls":4},"-","-","для MPEG-4 за неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","For MPEG-4, the device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream."]
["ACTi","ACTi ACM-1511","Camera ","A1D-V3.11.13","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",null,"+","-",{"$nulls":4},"-","-","1. У самой камеры есть ограничение на fps:\n-при разрешении 1280x1024 максимально 8 fps\n2. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate MPEG-4 видеопотока.","1) The camera itself has frame rate limits:\n- 1280x1024 resolution, max. 8 fps. The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream."]
["ACTi","ACTi ACM-3001","Camera ","V3.11.13-AV","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":4},"-","-",null,"-","-"]
["ACTi","ACTi ACM-3011","Camera ","V3.11.13-AV","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":4},"-","-",null,"-","-"]
["ACTi","ACTi ACM-3211","Camera ","A1D-V3.11.13","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","352x288","+",null,"+","-",{"$nulls":4},"-","-","для MPEG-4 за неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока ","For MPEG-4, the device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream. "]
["ACTi","ACTi ACM-3401","Camera ","A1D-220-V3.12.13-AC","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",null,"+","-",{"$nulls":4},"-","-","1. после переподключения питания камере видеопоток всегда восстанавливается в разрешении 1280x1024\n2. У самой камеры есть ограничение на fps:\n-при разрешении 1280х720 максимально 10 fps\n-при разрешении 1280x1024 максимально 8 fps\n3. для MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","1) After you reconnect the power adapter, the video stream always restarts with 1280x1024 resolution. The camera itself has frame rate limits:\nat 1280x720 resolution, max. 10 fps\nat 1280x1024 resolution, max. 8 fps\n3. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate."]
["ACTi","ACTi ACM-3411","Camera ","A1D-V3.11.13","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",null,"+","-",{"$nulls":4},"-","-"]
["ACTi","ACTi ACM-3511","Camera ","A1D-220-V3.12.15-AC","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",{"$nulls":7},"-","-"]
["ACTi","ACTi ACM-3601","Camera ","V3.11.13-AV","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":7},"-","-"]
["ACTi","ACTi ACM-3701 / ACM-3703","Camera ","V3.12.13-AC","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",{"$nulls":7},"-","-"]
["ACTi","ACTi ACM-4000","Camera ","A1D-220-V3.12.13-AC","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+","-",{"$nulls":4},"-","-"]
["ACTi","ACTi ACM-4001","Camera ","A1D-V3.11.13","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+","-",{"$nulls":4},"-","-"]
["ACTi","ACTi ACM-4200","Camera ","A1D-220--V3.12.13-AC","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",null,"+","-",{"$nulls":4},"-","-","1. У самой камеры есть ограничение на fps:\n-при разрешении 1280х720 максимально 10 fps\n-при разрешении 1280x1024 максимально 8 fps\n2. для MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n","1) The camera itself has frame rate limits:\nat 1280x720 resolution, max. 10 fps\nat 1280x1024 resolution, max. 8 fps\n2. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate.\n"]
["ACTi","ACTi ACM-4201","Camera ","A1D-220--V3.12.13-AC","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",null,"+","-",{"$nulls":4},"-","-","1. У самой камеры есть ограничение на fps:\n-при разрешении 1280х720 максимально 10 fps\n-при разрешении 1280x1024 максимально 8 fps\n2. для MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n\n","1. The camera itself has frame rate limits:\nat 1280x720 resolution, max. 10 fps\nat 1280x1024 resolution, max. 8 fps\n2. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate.\n\n"]
["ACTi","ACTi ACM-5001","Camera ","V3.12.13-AC","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":7},"-","-"]
["ACTi","ACTi ACM-5601","Camera ","A1D-220--V3.12.13-AC","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",null,"+","-",null,"+","+",null,"-","-","1. У самой камеры есть ограничение на fps:\n-при разрешении 1280х720 максимально 10 fps\n-при разрешении 1280x1024 максимально 8 fps\n2. для MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n3. при включении настройки Flickless Mode=50Hz в веб-интерфейсе возможно \"проседание\" fps до 7-8, но это особенность самой камеры.","1. The camera itself has frame rate limits:\nat 1280x720 resolution, max. 10 fps\nat 1280x1024 resolution, max. 8 fps\n2. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate.\n3. When the Flickerless Mode=50Hz setting is on in the web interface, the frame rate may drop to 7–8 fps, but this is a limitation of the camera itself. "]
["ACTi","ACTi ACM-5611","Camera ","A1D-220-V3.13.06-AC","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",null,"+","-",null,"+","+",null,"-","-","1. У самой камеры есть ограничение на fps:\n-при разрешении 1280х720 максимально 10 fps\n-при разрешении 1280x1024 максимально 8 fps\n2. для MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n","1. The camera itself has frame rate limits:\nat 1280x720 resolution, max. 10 fps\nat 1280x1024 resolution, max. 8 fps\n2. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate.\n"]
["ACTi","ACTi ACM-5711","Camera ","A1D-220-V3.12.13-AC","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","352x288","+",null,"+","-",null,"+","+",null,"-","-","1. при MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n \nкамера с прошивкой A1D-V3.11.13 не работает в Intellect 4.7.8","1. in MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate.\n \nIn Intellect 4.7.8, the camera does not work with the A1D-V3.11.13 firmware. "]
["ACTi","ACTi ACM-7411","Camera ","A1D-220-V3.12.15-AC","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",{"$nulls":7},"-","-"]
["ACTi","ACTi ACM-7511","Camera ","A1D-220-V3.12.13-AC","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","352x240","+",{"$nulls":7},"-","-"]
["ACTi","ACTi ACM-8211","Camera ","V3.11.13-AV","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",null,"+","-","+","+","+",null,"-","-","1. У самой камеры есть ограничение на fps:\n-при разрешении 1280х720 максимально 10 fps\n-при разрешении 1280x1024 максимально 8 fps\n2. для MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n","1. The camera itself has frame rate limits:\nat 1280x720 resolution, max. 10 fps\nat 1280x1024 resolution, max. 8 fps\n2. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate.\n"]
["ACTi","ACTi ACM-8511","Camera ","v3.12.15-AC ","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","352x288","+",{"$nulls":3},"+",{"$nulls":4},"-","1. при подключении к камере следует следить, чтобы значение настройки \"ТВ-стандарт\" в ПО ITV соответствовало типу камеры (PAL или NTSC).","1. When connecting to the camera, be sure to set the TV standard in the AxxonSoft software to the right camera type (PAL or NTSC). "]
["ACTi","ACTi CAM-5321HP","Camera ","A1C-2.09.11-AC (Full D1)","1",{"$nulls":3},"+",{"$nulls":3},"720x576(PAL)/720x480(NTSC)","720x576(PAL)/720x480(NTSC)","352x288(PAL)/352x240(NTSC)","+",{"$nulls":4},"+","+",null,"-","-","За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream."]
["ACTi","ACTi CAM-6600","Camera ","A1D-M2N-V2.09.11-AC","1",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352х288(PAL)/352x240(NTSC)","+",{"$nulls":3},"+",{"$nulls":3},"-","-","1. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","1. The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream."]
["ACTi","ACTi CAM-6610","Camera ","A1D-M2N-V2.09.11-AC","1",{"$nulls":3},"+",{"$nulls":3},"720x576(PAL)/720x480(NTSC)","720x576(PAL)/720x480(NTSC)","352x288(PAL)/352x240(NTSC)","+",{"$nulls":3},"+.",{"$nulls":4},"-","Для корректной работы самого устройства с прошивкой A1D-M2N-V2.09.11-AC рекомендуется выставлять только PAL","If the device has the A1D-M2N-V2.09.11-AC firmware, to ensure that the device works smoothly, set PAL."]
["ACTi","ACTi CAM-6630","Camera ","A1D-M2N-V2.09.11-AC","1",{"$nulls":3},"+",{"$nulls":3},"720x576(PAL)/720x480(NTSC)","720x576(PAL)/720x480(NTSC)","352x288(PAL)/352x240(NTSC)","+",{"$nulls":3},"+",{"$nulls":4},"-","Для корректной работы самого устройства с прошивкой A1D-M2N-V2.09.11-AC рекомендуется выставлять только NTSC","If the device has the A1D-M2N-V2.09.11-AC firmware, to ensure that the device works smoothly, set NTSC."]
["ACTi","ACTi CAM-7221","Camera ","A1D-V2.09.11-AC (Full D1)","1",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352х288(PAL)/352x240(NTSC)","+",null,"+","-",null,"+","+",null,"-","-","За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream."]
["ACTi","ACTi CAM-7321","Camera ","A1D-V2.09.11-AC (Full D1)","1",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720x576(PAL)/720x480(NTSC)","352x288(PAL)/352x240(NTSC)","+",null,"+","-",null,"+","+",null,"-","-","За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream."]
["ACTi","ACTi D11 / D21 / D31 / D41 / D51 / D54 / D61 / D64 / D71 / D81  / E21 / E31 / E41 / E45 / E51 / E52 / E61 / E64 / E66 / E71 / E81 / E85 / E91 / E94","Camera","A1D-500-V6.06.16-AC","1","+","2","+",null,"+",null,null,"1280x720","1280x720","640x360 (PAL) / 640x480 (NTSC)","+",{"$nulls":7},"motion detection","-","Прошивка 6.01.06: Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность прошивки.Частота опорных кадров задается в секундах и может принимать значения от 1 до 5.","6.01.06 firmware: for proper operation of MJPEG, please select low resolution, quality and FPS. This is a firmware feature. The keyframe rate is set in seconds and can range from 1 to 5.","improved"]
["ACTi","ACTi D12 / D32 / D42 / D52 / D55 / D65 / D72 / D82 / E24 / E32 / E34 / E42 / E46 / E53 / E62 / E65 / E72 / E74 / E82 / E86 / E92","Camera ","V6.03.17","1",null,null,"+",null,"+",null,null,"2048x1536 ","1920x1080","640x360","+",{"$nulls":7},"motion detection","-","1. Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность текущей прошивки.\n2. Частота опорных кадров задается в секундах и может принимать значения от 1 до 5. ","1. To work with MJPEG correctly, please select low resolution, quality and FPS. This is a limitation of the current firmware. 2. The keyframe rate is set in seconds and can range from 1 to 5."]
["ACTi","ACTi D22 / E22 / E33 / E43 / E43A / E54 / E63 / E73 / E83","Camera ","V6.04.15","1",null,null,"+",null,"+",null,null,"2592x1944 ","2048x1536 ","640x480 (NTSC) / 640x360 (PAL) ","+",{"$nulls":7},"motion detection","-","1. Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность прошивки V6.03.17.\n2. Частота опорных кадров задается в секундах и может принимать значения от 1 до 5. ","1. To work with MJPEG correctly, please select low resolution, quality and FPS. This is a limitation of firmware V6.03.17. 2. The keyframe rate is set in seconds and can range from 1 to 5."]
["ACTi","ACTi E11 ","Camera ","V6.02.03","1",null,null,"+",null,"+",null,null,"1280x720 ","1280x720 ","640x360","+",null,"-","-","-","-","-","-","-","-","1. Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность текущей прошивки. 2. В ПО Axxon аудио-кодек и для микрофона и для динамика устройства устанавливается в настройках объекта Микрофон.","1. To work with MJPEG correctly, please select low resolution, quality and FPS. This is a limitation of the current firmware. 2. In AxxonSoft software, you can set the codecs for mics and speakers in the Microphone object settings."]
["ACTi","ACTi E12 ","Camera ","V6.03.17 ","1",null,null,"+",null,"+",null,null,"2048x1536","1920x1080","640x360 (Auto) / 640x480 (4:3)","+",null,"+",{"$nulls":5},"motion detection","-","1. Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность текущей прошивки. 2. На камере есть два режима отображения Auto / 4:3, которые переключаются в веб-интерфейсе. ","1. To work with MJPEG correctly, please select low resolution, quality and FPS. This is a limitation of the current firmware. 2. The camera has two display modes, Auto/4:3, which can be toggled in the web interface. "]
["ACTi","ACTi E13","Camera ","V6.03.17 ","1",null,null,"+",null,"+",null,null,"2592x1944 ","2048x1536 ","640x360","+",null,"+",{"$nulls":5},"motion detection","-","Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность текущей прошивки. ","1. To work with MJPEG correctly, please select low resolution, quality and FPS. This is a limitation of the current firmware."]
["ACTi","ACTi E23 / E44 / D62 / E67 / E84 / E95 ","Camera ","V6.03.17 ","1",null,null,"+",null,"+",null,null,"1920x1080 ","1280x720","640x360","+",{"$nulls":7},"motion detection","-","Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность текущей прошивки. ","1. To work with MJPEG correctly, please select low resolution, quality and FPS. This is a limitation of the current firmware."]
["ACTi","ACTi KCM-3911 / KCM-7911","Camera ","5.07.05","1",null,null,"+","+","+",null,null,"1920x1072","from WEB: 1280x720","from WEB: 1280x720","+",null,"+","-",null,"+","+",null,"motion detection","-","1. Разрешение в Интеллект нужно настраивать через вэб-интерфейс","1. You can configure resolution in Intellect via web interface."]
["ACTi","ACTi KCM-5111","Camera ","5.07.05","1",null,null,"+","+","+",null,null,"2032x1920","1920x1072","640x480","+",null,"+.","-",null,"+","+",null,"motion detection","-","1. Устройство поддерживает 3 режима видео (в Axxon Next выбирается соответствующей настройкой в группе \"Другое\"): \n 1)Однопоточный. Используется поток 0. Максимально доступная частота кадров зависит от выбранного кодека и разрешения.\n2) Двухпоточный. Используются потоки 1 и 2. Доступность разрешений и значений частоты кадров в одном потоке зависит от текущей конфигурации другого потока. В режиме \"Двойной поток\" доступны комбинации кодеков:\nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) Четырёхпоточный. Используются потоки 3,4,5 и 6. Каждый поток показывает выбранную часть картинки от всего изображения, получаемого камерой. Координаты каждого фрагмента в Axxon Next задаются в группе настроек \"Другое\".","1. The device supports 3 video modes (in AN, you select a video mode in the Other group of settings): \n 1) 1 stream. Stream 0 is used. The maximum available frame rate depends on which codec and resolution are selected.\n2) 2 streams. Streams 1 and 2 are used. Which resolutions and frame rates are available for one stream depends on the current settings of the other. In *2 streams* mode, the following codec combinations are available: \nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) 4 streams. Streams 3, 4, 5, and 6 are used. Each stream shows a part of the image received from the camera. In AN, the coordinates of each part are set in the Other group of settings."]
["ACTi","ACTi KCM-5211(E)","Camera ","5.03.02","1",null,null,"+","+","+",null,null,"2032х1920","1920х1080","640х480","+",null,"+","-","+.","+","+",null,null,"-","1. Устройство поддерживает 3 режима видео (в Axxon Next выбирается соответствующей настройкой в группе \"Другое\"): \n 1)Однопоточный. Используется поток 0. Максимально доступная частота кадров зависит от выбранного кодека и разрешения.\n2) Двухпоточный. Используются потоки 1 и 2. \nДоступность разрешений и значений частоты кадров в одном потоке зависит от текущей конфигурации другого потока. \nВ режиме \"Двойной поток\" доступны комбинации кодеков:\nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) Четырёхпоточный. Используются потоки 3,4,5 и 6. Каждый поток показывает выбранную часть картинки от всего изображения, получаемого камерой. Координаты каждого фрагмента в Axxon Next задаются в группе настроек \"Другое\".","1. The device supports 3 video modes (in AN, you select a video mode in the Other group of settings): \n 1) 1 stream. Stream 0 is used. The maximum available frame rate depends on which codec and resolution are selected.\n2) 2 streams. Streams 1 and 2 are used. Which resolutions and frame rates are available for one stream depends on the current settings of the other. In *2 streams* mode, the following codec combinations are available: \nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) 4 streams. Streams 3, 4, 5, and 6 are used. Each stream shows a part of the image received from the camera. In AN, the coordinates of each part are set in the Other group of settings."]
["ACTi","ACTi KCM-5311 / KCM-5311E","Camera ","5.03.02","1",null,null,"+","+","+",null,null,"1920x1080","1280x720","640x480","+",null,"+","-","+.","+","+",null,"-","-","1. Устройство поддерживает 2 режима видео (в AxxonNext/Next выбирается соответствующей настройкой в группе \"Другое\"): \n 1)Однопоточный. Используется поток 0. Максимально доступная частота кадров зависит от выбранного кодека и разрешения.\n2) Двухпоточный. Используются потоки 1 и 2. Доступность разрешений и значений частоты кадров в одном потоке зависит от текущей конфигурации другого потока. В режиме \"Двойной поток\" доступны комбинации кодеков:\nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n2. Камера не поворотная, но есть встроенный трансфокатор.","1. The device supports 2 video modes (in AN, select the right video mode in the Other group of settings): \n1) Single Stream. Stream 0 is used. The maximum available frame rate depends on which codec and resolution are selected. \n2) Double Stream. Streams 1 and 2 are used. The availability of resolutions and frame rates for one stream depends on the current settings of the other. In Dual Stream mode, the following codec combinations are available: mjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n\n2. This is not a PTZ camera, but it has a built-in zoom lens. "]
["ACTi","ACTi KCM-5511","Camera","V5.11.17","1",null,null,"+","+","+","-","-","1920х1072","1280x720","640x480","+",null,"-","-","-","-","-","-","motion detection","-"]
["ACTi","ACTi KCM-7111","Camera ","5.03.02","1",null,null,"+","+","+",null,null,"2032х1920","1920х1072","640x480","+",null,"+","-",null,"+","+.",null,"-","-","1. Устройство поддерживает 3 режима видео (в AxxonNext/Next выбирается соответствующей настройкой в группе \"Другое\"): \n 1)Однопоточный. Используется поток 0. Максимально доступная частота кадров зависит от выбранного кодека и разрешения.\n2) Двухпоточный. Используются потоки 1 и 2. Доступность разрешений и значений частоты кадров в одном потоке зависит от текущей конфигурации другого потока. В режиме \"Двойной поток\" доступны комбинации кодеков:\nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) Четырёхпоточный. Используются потоки 3,4,5 и 6. Каждый поток показывает выбранную часть картинки от всего изображения, получаемого камерой. Координаты каждого фрагмента в AxxonNext/Next задаются в группе настроек \"Другое\".","1. The device supports 3 video modes (in AN, select the right video mode in the Other group of settings): \n1) Single Stream. Stream 0 is used. The maximum available frame rate depends on which codec and resolution are selected. \n2) Double Stream. Streams 1 and 2 are used. The availability of resolutions and frame rates for one stream depends on the current settings of the other. In Dual Stream mode, the following codec combinations are available: mjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) 4-stream. Streams 3, 4, 5, and 6 are used. Each stream shows a part of the image received from the camera. In AN, the coordinates of each part are set in the Other group of settings. "]
["ACTi","ACTi KCM-7211","Camera ","5.03.02","1",null,null,"+","+","+",null,null,"2032x1920","1920x1080","640x480","+",null,"+","-","+.","+","+.",null,"-","-","1. Устройство поддерживает 3 режима видео (в AxxonNext/Next выбирается соответствующей настройкой в группе \"Другое\"): \n 1)Однопоточный. Используется поток 0. Максимально доступная частота кадров зависит от выбранного кодека и разрешения.\n2) Двухпоточный. Используются потоки 1 и 2. Доступность разрешений и значений частоты кадров в одном потоке зависит от текущей конфигурации другого потока. В режиме \"Двойной поток\" доступны комбинации кодеков:\nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) Четырёхпоточный. Используются потоки 3,4,5 и 6. Каждый поток показывает выбранную часть картинки от всего изображения, получаемого камерой. Координаты каждого фрагмента в AxxonNext/Next задаются в группе настроек \"Другое\".\n2. Камера не поворотная, но есть встроенный трансфокатор.","1. The device supports 3 video modes (in AN, select the right video mode in the Other group of settings): \n1) Single Stream. Stream 0 is used. The maximum available frame rate depends on which codec and resolution are selected. \n2) Double Stream. Streams 1 and 2 are used. The availability of resolutions and frame rates for one stream depends on the current settings of the other. In Dual Stream mode, the following codec combinations are available: mjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) 4-stream. Streams 3, 4, 5, and 6 are used. Each stream shows a part of the image received from the camera. In AN, the coordinates of each part are set in the Other group of settings. \n2. This is not a PTZ camera, but it has a built-in zoom lens. "]
["ACTi","ACTi KCM-7311","Camera ","5.08.06","1",null,null,"+","+","+",null,null,"2032x1920 ","1920x1072","640x480","+",{"$nulls":3},"+",{"$nulls":3},"motion detection","-"]
["ACTi","ACTi KCM-8211","Camera ","V5.09.12","1",null,null,"+","+","+",null,null,"1280x720","1280x720","640x480","+",{"$nulls":3},"+",{"$nulls":3},"motion detection","-","Между потоками камеры есть следующая зависимость:\nесли на одном потоке выставить MPEG4, то на другом будут доступны только кодеки MJPEG и MPEG4\nесли на одном потоке выставить MJPEG, то на другом будут доступны все кодеки\nесли на одном потоке выставить H.264, то на другом будут доступны только кодеки H.264 и MJPEG\nПри выборе в по Axxon Next двухпоточного режима рекомендуется для настройки \"режим передачи видеоизображения\" выставить значение \"2 видеопотока\". Также необходимо для настройки \"режим передачи видеоизображения\" выставить значение \"2 видеопотока\", если в режиме однопоточности необходимо получать видео со второго потока\nДля того чтобы настройка фокуса работала в продукте, необходимо в веб-интерфейсе камеры режим управления фокусом выставить в ручной режим.\nДетектор движения работает только с кодеками H.264 и MPEG4","There is a following relationship between camera's streams:\nif one stream MPEG4, then on the other stream will be available codecs MJPEG and MPEG4;\nif one stream MJPEG, then on the other one will be available all codecs;\nif one stream H.264, then on the other one will be accessed only codecs H.264 and MJPEG;\nWhen selecting dualstream mode in Axxon Next is recommended for setting \"video transmission mode\" set to \"2 video stream\". Also need to adjust the \"transmission mode video\" set to \"2 video\" if you need to receive multistreaming mode with second video stream.\nTo adjust the focus setting in AxxonSoft products, it is necessary using camera's web interface, the camera focus control mode set to manual mode.\nMotion detector works only with codecs H.264 and MPEG4."]
["ACTi","ACTi TCD-2100 encoder","Encoder","V4.07.15-AC","1",null,null,"+","+","+",null,null,"720x480","720x480","352x240","+",{"$nulls":8},"-"]
["ACTi","ACTi TCD-2500 encoder","Encoder","A1D-310-V4.06.08-AC","1",null,null,"+","+","+",null,null,"720x576","720x576","352x288","+",null,"+","-","+","+","+",null,"-","-"]
["ACTi","ACTi TCM-1231","Camera ","V4.12.09-AC","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",null,"+","+",null,"+","+",null,"motion detection","-","Между потоками камеры есть следующая зависимость:\nесли на одном потоке выставить MPEG4, то на другом будут доступны только кодеки MJPEG и MPEG4\nесли на одном потоке выставить MJPEG, то на другом будут доступны все кодеки\nесли на одном потоке выставить H.264, то на другом будут доступны только кодеки H.264 и MJPEG.\nДля получения видео по Axxon Next с двух потоков или со второго потока необходимо для настройки \"режим передачи видеоизображения\" выставить значение \"2 видеопотока\".\nДетектор движения на камере доступен только если на первом потоке стоят кодеки H.264 и MPEG4.\nЕсли режим экспозиции выставить в ручной режим, то для настройки баланс белого становится недоступным значение \"авто\"\nДиапазон значений fps зависит от значения разрешения.","Streams of the camera depend on below behavior:\nif at one stream select MPEG4, at other one will be available MJPEG and MPEG4\nif at one stream select MJPEG, then, at second one will ba available all codecs\nif at one stream select H.264, at other one will be available only H.264 and MJPEG.\nTo get video from two or second stream(s) in Axxon Next Для need to select \"video transmit mode\" in value \"2 streams\".\nMotion detection is available only if at first stream schoosen codecs H.264 or MPEG4.\nIf you select exposition mode in manual mode, for white balance setting will be not available value \"auto\".\nFPS range depends on from resolution."]
["ACTi","ACTi TCM-1511","Camera ","V4.07.15-AC","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",{"$nulls":8},"-","Для H.264 и MPEG-4 качество регулируется через Bit Rate. Для корректной работы качества необходимо, что бы значение поля Video Bit Rate Mode было Constant Bit Rate.\n","For H.264 and MPEG-4, the quality is adjusted with Bit Rate. For the quality to work smoothly, be sure to set the Video Bit Rate Mode field to Constant Bit Rate.\n"]
["ACTi","ACTi TCM-3001","Camera ","V4.07.15-AC","1",null,null,"+","+","+",null,null,"640x480","640x480","320x240","+",{"$nulls":7},"-","-","Для H.264 и MPEG-4 качество регулируется через Bit Rate. Для корректной работы качества необходимо, что бы значение поля Video Bit Rate Mode было Constant Bit Rate.","For H.264 and MPEG-4, the quality is adjusted with Bit Rate. For the quality to work smoothly, be sure to set the Video Bit Rate Mode field to Constant Bit Rate."]
["ACTi","ACTi TCM-3011","Camera ","4.08.05","1",null,null,"+","+","+",null,null,"640x480","640x480","320x240","+",{"$nulls":8},"-"]
["ACTi","ACTi TCM-3401 / TCM-3411","Camera ","A1D-310-V4.07.15-AC","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",{"$nulls":7},"-","-"]
["ACTi","ACTi TCM-3511","Camera ","4.07.15-AC","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",{"$nulls":8},"-"]
["ACTi","ACTi TCM-4001","Camera ","V4.07.15-AC","1",null,null,"+","+","+",null,null,"640x480","640x480","320x240","+",{"$nulls":8},"-"]
["ACTi","ACTi TCM-4201","Camera ","V4.07.15-AC","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",null,"+",{"$nulls":5},"-","-"]
["ACTi","ACTi TCM-4301","Camera ","A1D-310-V4.06.09-AC","1",null,null,"+","+","+",null,null,"1024x768","640x480","320x240","+",null,"+","+",{"$nulls":4},"-","-"]
["ACTi","ACTi TCM-4511","Camera ","v4.12.09","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",{"$nulls":7},"motion detection","-","1. Детектор движения работает только при H.264 или MPEG4 на 1-ом потоке","1. VMD works only if H.264 or MPEG4 is enabled for stream 1."]
["ACTi","ACTi TCM-5001","Camera ","V4.07.15-AC","1",null,null,"+","+","+",null,null,"640x480","640x480","320x240","+",{"$nulls":8},"-"]
["ACTi","ACTi TCM-5111","Camera ","v4.12.09","2",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",{"$nulls":7},"motion detection","-","1. Детектор движения работает только при H.264 или MPEG4 на 1-ом потоке","1. VMD works only if H.264 or MPEG4 is enabled for stream 1."]
["ACTi","ACTi TCM-5311","Camera ","A1D-310-V4.06.09-AC","1",null,null,"+","+","+",null,null,"1280x960","640x480","320x240","+",null,"+","-",null,"+","+",null,"-","-","1. Поддержка двух стримингов (т.е. двух независимых видеоканалов в Intellect пока отсутствует)\n2. в разрешении 1280х960  сама камера выдает максимально 15 fps\n ","1. Dual streaming (i.e., two independent video channels ) is not yet supported by Intellect.\n2. At 1280x960 resolution, the camera itself is capable of running at 15 fps max. \n "]
["ACTi","ACTi TCM-5601","Camera ","V4.07.15-AC","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",{"$nulls":8},"-"]
["ACTi","ACTi TCM-5611","Camera ","V4.07.15-AC","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",{"$nulls":8},"-"]
["ACTi","ACTi TCM-7011","Camera ","V4.07.15-AC","1",null,null,"+","+","+",null,null,"640x480","640x480","320x240","+",{"$nulls":7},"-","-"]
["ACTi","ACTi TCM-7411","Camera ","V4.07.15-AC","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",{"$nulls":8},"-"]
["ACTi","ACTi TCM-7811","Camera ","V4.08.05-AC","1",null,null,"+","+","+",null,null,"1280x960","640x480","320x240","+",{"$nulls":8},"-"]
["Acumen","Acumen AiP-B34N 05Y2B","Camera ","1.0.506k(Ai)","1",null,null,"+",null,"+",null,null,"from WEB","from WEB","from WEB","+",null,"+",{"$nulls":6},"-","На камере есть настройка Profile, от которой зависят не только разрешение и кодеки на стримингах, но и количество этих самых стримингов. В настройках камеры в ПО ITV/AxxonSoft необходимо выбирать тот же кодек, который установлен в веб-интерфейсе камеры для соответствующего потока.\nНастраивать потоки необходимо исходя из зависимостей в веб-интерфейсе.\nПри смене профиля камера перезагружается в течение полутора минут.\nНастройка RTSP-порта не изменяет текущее значение порта на камере, её необходимо выставлять согласно вебу.","The camera has Profile setting, this setting influences to resolution, codecs available on streams, and to number of streams. In SW AxxonSoft you need to select the same codec as in camera's web-interface for corresponding stream. \nYou need to tune streams in accordance with dependences in web-interface.\nAfter profile changing camera will be rebooted during 90 seconds.\nRTSP port setting doesn't change current value at camera's port. You need to tune it in accordance with web-interface."]
["Acumen","Acumen AiP-L24N-66Y2B","Camera","1.0.504(Ai)","1","+","4","+",null,"+",null,null,"from WEB","from WEB","from WEB","+",null,"-","-","-","-","-","-","-","-","Значение настройки RTSP порт должно соответствовать значению аналогичной настройки, выставленному в веб-интерфейсе на странице Network → HTTP/RTSP Service. Особенность прошивки камеры не позволяет провести полноценную интеграцию настроек видео без необходимости совершения дополнительных действий в веб-интерфейсе камеры. Для корректной работы настроек в ПО ITV/Axxon необходимо, настройки \"Видеокодек\" и \"Разрешение\" в ПО ITV/Axxon соответствовали аналогичным настройкам в веб-интерфейсе камеры, где они зависят от значения параметра Profile (Settings → Video / Audio).","The value of RTSP port setting is to correspond to the value of the similar setting set in the web interface on the Network → HTTP/RTSP Service page. Camera firmware does not allow integrating video settings without other actions in the camera web interface. For proper operation of settings in Axxon software, the Video codec and Resolution settings in Axxon software are to correspond to the similar settings in the camera web interface where they depend on the Profile (Settings → Video / Audio) parameter. ","new"]
["Acumen","Acumen AIP-M53K(ONVIF)","Camera ","1.1.006(Ai)","1",null,null,"+",{"$nulls":4},"720x480","720x480","720x480","+",{"$nulls":8},"+"]
["Acumen","Acumen AiP-P53N-45Y2B","Camera","1.1.006.2(Ai) ","1","+","3","+",null,"+",null,null,"from WEB","from WEB","from WEB","+",null,"-","-",null,"-","-","-","-","-","Значение настройки RTSP порт должно соответствовать значению аналогичной настройки, выставленному в веб-интерфейсе на странице Network → HTTP/RTSP Service.Особенность прошивки камеры не позволяет провести полноценную интеграцию настроек видео без необходимости совершения дополнительных действий в веб-интерфейсе камеры. Для корректной работы настроек в ПО ITV/Axxon необходимо, настройки \"Видеокодек\" и \"Разрешение\" в ПО ITV/Axxon соответствовали аналогичным настройкам в веб-интерфейсе камеры, где они зависят от значения параметра Profile (Settings → Video / Audio). ","The value of RTSP port setting is to correspond to the value of the similar setting set in the web interface on the Network → HTTP/RTSP Service page. Camera firmware does not allow integrating video settings without other actions in the camera web interface. For proper operation of settings in Axxon software, the Video codec and Resolution settings in Axxon software are to correspond to the similar settings in the camera web interface where they depend on the Profile (Settings → Video / Audio) parameter. ","new"]
["Acumen","Acumen AiP-R53K-05Y1B","Camera","1.1.010(Ai)","1","+","3","+",null,"+",null,null,"from WEB","from WEB","from WEB","+",null,"-","-",{"$nulls":3},"-","-","-","Значение настройки RTSP порт должно соответствовать значению аналогичной настройки, выставленному в веб-интерфейсе на странице Network → HTTP/RTSP Service. Особенность прошивки камеры не позволяет провести полноценную интеграцию настроек видео без необходимости совершения дополнительных действий в веб-интерфейсе камеры. Для корректной работы настроек в ПО ITV/Axxon необходимо, настройки \"Видеокодек\" и \"Разрешение\" в ПО ITV/Axxon соответствовали аналогичным настройкам в веб-интерфейсе камеры, где они зависят от значения параметра Profile (Settings → Video / Audio).","The value of RTSP port setting is to correspond to the value of the similar setting set in the web interface on the Network → HTTP/RTSP Service page. Camera firmware does not allow integrating video settings without other actions in the camera web interface. For proper operation of settings in Axxon software, the Video codec and Resolution settings in Axxon software are to correspond to the similar settings in the camera web interface where they depend on the Profile (Settings → Video / Audio) parameter. ","new"]
["Adino","Adino TC-NC6453S2-2MP","Camera","NVSSv3.0.1_20120619","1",null,null,"+","-","+","-","-","1600x1200","1280x960","640x480","+","-","-","-","-","-","-","-","-","-","Диапазон значений битрейта на камере динамичен и зависит от текущего значения разрешения.","Camera bitrate range is dynamic and depends on the current resolution."]
["Alinking","Alinking ALC-9122P","Camera ","V1.32 STD-1","1",null,null,"+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4)","640x480(MJPEG) / 352x288(MPEG-4)","320x240","+",null,"-","-","-","-","-",null,"-","+","1. Настройка PAL / NTSC в ПО Intellect переключается режимы Partial / Full Scan\n2. Разрешение 1280х960 доступно только в MJPEG и только в режиме Full Scan (максимальный fps в данном режиме = 12)\n3. При смене разрешения на одном стримминге разрешение автоматически изменится и на втором. Особенность интеграции.","1. In Intellect, the PAL / NTSC setting switches between Partial mode and Full Scan mode.\n2. 1280х960 is available only in MJPEG and only in Full Scan mode (in this mode, max. frame rate is 12 fps).\n3. When you change the resolution of one stream, the resolution of the other one changes automatically. This is for integration. "]
["Alinking","Alinking ALC-9171P","Camera ","V1.04 STD-1","1",null,null,"+",null,"+",null,null,"1280x720/1600x1200","1280x720 / 640x480","640x352 / 320x240","+",null,"-","-","-","-","-",null,"-","+","1. Фактический fps видеопотока очень сильно зависит от разрешения, качества и фокусировки картинки.\n2. Настройка яркости не работает на самом устройстве\n3. Настройка PAL/NTSC в ПО ITV/Axxon переключает режимы UXGA / WXGA (различаются набором разрешений).","1. The actual frame rate very much depends on the image resolution, quality, and focus. \n2. The brightness setting does not work on the device itself. In the AxxonSoft software, the PAL/NTSC setting switches between the UXGA and WXGA modes (the modes offer different sets of resolutions). "]
["AMG","AMG-Panogenics PanoCam360","Camera ","01.04.03","1",null,null,"+","+","+",null,null,"2144x1944","640x480","320x240","+.",{"$nulls":3},"-","+.","+",null,"-","+","1. Видео кодек устанавливается на все потоки\n2. Настройка \"bitrateControl\" также устанавливается на все потоки","1. Video codec is applied to all streams.\n2. BitrateControl is applied to all streams either."]
["A-MTK ","A-MTK AM2030D / AM2290D / AM2530D / AM2560D / AM2570D / AM2630D / AM2730D ","Camera ","6.D.2.9659","1",null,null,"+","+","+",null,null,"1920x1080 ","640x360","640x360","+",{"$nulls":8},"+"]
["Arecont Vision","Arecont Vision AV10005/-DN","Camera ","65201","1","+.",null,"+",null,"+",null,null,"3648x2752","3648x2752","1824x1376","+",{"$nulls":4},"+","+",null,"+","-","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Камера имеет ограничение по FPS:\n - 6fps @ 3648x2752\n - 25fps @ 1824x1376Датчик должен быть под напряжением","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. The camera has frame rate limits:\n - 6 fps at 3648x2752\n - 25 fps at 1824x1376. Close the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV10115/-DN/-AI","Camera ",65218,"1",null,null,"+",null,"+",null,null,"3648x2752","3648x2752","1824x1376","+",{"$nulls":4},"+","+",null,"motion detection","-","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Камера имеет ограничение по FPS:\n - 7fps @ 3648x2752\n - 27fps @ 1824x1376Датчик должен быть под напряжением","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. The camera has frame rate limits:\n - 7 fps at 3648x2752\n - 27 fps at 1824x1376. Close the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV1115/-DN/-AI","Camera ","65200","1","+.",null,"+",null,"+",null,null,"1280x1024","1280x1024","640x512","+",{"$nulls":4},"+","+",null,"+","-","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Производитель заявляет о частоте кадров в 40 fps (2 x 20 fps в двухпотоковом режиме). Камера достигает заявленных fps только при работе через протокол TFTP. При работе через протокол HTTP максимальная частота кадров - 25 fps (2 x 12 fps в двухпотоковом режиме).Прошивка 65200: при использовании встроенного детектора частота кадров падает до 5 fps.Луч должен быть под напряжением.","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. The vendor states that the frame rate is 40 fps (2 x 20 fps in dual-stream mode). The camera reaches this frame rate only when using the TFTP protocol. When using the HTTP protocol, the max. frame rate is 25 fps (2 x 12 fps in dual-stream mode). 65200 firmware: when the embedded detection tool is used, the frame rate drops to 5 fps. Close the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV1125/-DN/-IR","Camera ","65201 / 65202","1","+.",null,"+",null,"+",null,null,"1280x1024","1280x1024","640x512","+",{"$nulls":4},"+",null,null,"+","-","AV1125 - прошивка 65201\nAV1125-DN/-IR - прошивка 65202\nПараметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет. \nЛуч должен быть под напряжением.","\"AV1125 - firmware v.65201 \nAV1125-DN/-IR - firmware v .65202\nThe Auto Iris and Shutter Speed parameters are integrated as telemetry settings - but the camera does not have the telemetry functionality. \nThe sensor must be energized.\n"]
["Arecont Vision","Arecont Vision AV12186DN","Camera ","65184","4","+.",null,"+",null,"+",null,null,"2048x1536","2048x1536","1024x768","+",{"$nulls":5},"+",null,"motion detection","-","Работа данной камеры по протоколу TFTP не поддерживается.","Work through RFTP protocol with this device is not supported."]
["Arecont Vision","Arecont Vision AV1300/-DN/-AI","Camera ","64116","1",null,null,"+",{"$nulls":4},"1280x1024","1280x1024","640x512","+",{"$nulls":4},"-","+",null,"+","-","1. при мегапиксельном разрешении макимально доступны fps ~20\n2. Лучи не могут быть интегрированы. ","1. With megapixel resolutions, the max. resolution is 20 fps.\n2. The sensor cannot be integrated. "]
["Arecont Vision","Arecont Vision AV1305/-DN/-AI","Camera ","65143 / 65144","1","+.",null,"+",null,"+",null,null,"1280x1024","1280x1024","640x512","+",{"$nulls":5},"+",null,"+","-","1. AV1305/-Ai - прошивка 65143\n AV1305DN - прошивка 65144\n 2. Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.\n\n","1. AV1305/-Ai - firmware 65143\n AV1305DN - firmware 65144\n2. The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. Close the sensor when it is energized"]
["Arecont Vision","Arecont Vision AV1310/-DN","Camera ","65143 / 65144","1",null,null,"+",{"$nulls":4},"1280x1024","1280x1024","640x512","+",{"$nulls":4},"+","+",null,null,"-","1) аналог камеры Arecont AV1300\nотличие - AV1310 имеет более компактный корпус , улучшена работы настройки насыщенности цвета \n2) AV1310 - прошивка 65143\n AV1310DN - прошивка 65144 \n3) Лучи замыкаются под напряжением. ","1. This camera is very similar to the Arecont AV1300.\nDifferences: the AV1310 is smaller, the saturation setting works better. 2) AV1310 - fw 65143\n AV1310DN - fw 65144 \n3) Close the sensor when it is energized. "]
["Arecont Vision","Arecont Vision AV1315/-DN / AV1325/-DN/-IR","Camera ","65201","1","+.",null,"+",null,"+",null,null,"1280x1024","1280x1024","640x512","+",{"$nulls":4},"+","+",null,"+","-","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.При просмотре видео через HTTP наблюдается падение FPS в AxxonNext/Next (MJPEG, H264) и Интеллект (H264) примерно до 6-10 кадров в секунду. По TFTP частота кадров нормальная.Датчик должен быть под напряжением","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. When the video is viewed via HTTP, the frame rate drops to 6–10 fps in AN (MJPEG and H.264) and in Intellect (H.264). When TFTP is used, the frame rate is normal. Close the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV1355/-DN/-HK/-DN-HK","Camera ","65139","1",null,null,"+",null,"+.",null,null,"1280x1024","1280x1024","640x512","+",{"$nulls":3},"+","-","+",null,"+","-","1. На прошивке 65139 H264-поток с камеры идет с искажениями. Искажения видны и в ПО ITV, и в ПО производителя камеры.\n","1. With the 65139 firmware, the H.264 stream becomes distorted. You can see the distortions both in the AxxonSoft software and in the vendor software. \n"]
["Arecont Vision","Arecont Vision AV20185DN / AV20365DN","Camera ","65170","4","+.",null,"+",null,"+",null,null,"2560x1920","2560x1600","1280x960","+",{"$nulls":4},"+","+",null,"+","-","Устройство представляет собой панорамную 4-объективную камеру.Модели 20185 и 20365 отличаются суммарным углом обзора: 180 и 360 градусов соответственно.Конструкция камеры имеет особенность: сенсор 2 и 4 перевернуты относительно сенсора 1 и 3 на 180 градусов. Поэтому изображение с них идет в нашем ПО перевернутым. Для коррекции в AxxonNext/Next нужно использовать специальный параметр, в Интеллекте - через веб-интерфейс.В ПО ITV интегрировано как видеосервер с 4-мя независимыми каналами видео, которые можно включать/отключать.Изменение некоторых настроек применяется ко всем каналам одновременно.Разрешения (см. выше) указаны для отдельного канала.Чем больше каналов одновременно используется, тем ниже частота кадров для каждого канала.Наивысшей частоты кадров камера достигает при работе по протоколу TFTP.Луч должен быть под напряжением.","This is a 4-lens panoramic camera. The 20185 and 20365 models have different total angles of view: 180 and 360 degrees, respectively. The camera's design has one peculiarity: sensors 2 and 4 are rotated by 180 degrees with respect to sensors 1 and 3. For this reason, for those rotated sensors, our software shows an upside-down image. To correct this, you must use a special parameter (in AN) or use the web interface (in Intellect). In the AxxonSoft software, the camera is integrated as a video encoder with 4 independent video channels, which can be switched on and off. Changes to some settings are applied to all the channels at once. The above resolutions are for a single channel. The more channels are used at the same time, the lower the frame rate is for each channel. The camera reaches the maximum frame rate when using the TFTP protocol. Close the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV2100/-DN/-AI","Camera ","64327 / 64328","1",null,null,"+",{"$nulls":4},"1600x1200","1600x1200","800x600","+",{"$nulls":4},"-","+",null,"+","-","1)AV2100/-Ai - прошивка 64327\n AV2100DN - прошивка 64328\n2_ Ограничение по fps: 800x600 - 15 fps, 1600x1200 -14 fps \n\n","1. AV2100/-Ai - firmware 64327\n AV2100DN - firmware 64328\n2. Frame rate limits:\n- 800x600: 15 fps\n- 1600x1200: 14 fps\nyou may find the right balance between quality and speed (by manually setting a value between 1 and 10 ms)"]
["Arecont Vision","Arecont Vision AV2105/-DN/-AI","Camera ","65009","1","+.",null,"+",null,"+.",null,null,"1600x1184","1600x1184","800x592","+",{"$nulls":4},"-","+",null,"+","-","1) проблемы с H.264 - с CUDA искажается живое видео, в архиве искажение ещё сильнее\n2) если отключить CUDA , то искажений почти нет, но при это в компоненте \"web-сервер\" - видео нет, изредка мигает - скорее всего проблема с h.264\n3)в Slave и УРМА искажение видео усиливаются\n ","1) Problems related to H.264: With CUDA on, live video is distorted and video in the archive is distorted even more.\n2) If you switch CUDA off, there is almost no distortion, but at the same time, there is almost no video in the web server component (occasional flickering) then most likely this is an H.264 problem,\n3) In Slave and URMA, the video is even more distorted.\n "]
["Arecont Vision","Arecont Vision AV2110/-DN","Camera ","65143 / 65144","1",null,null,"+",{"$nulls":4},"1600x1200","1600x1200","800x600","+",{"$nulls":4},"+","+",null,"+","-","1. AV2110 - прошивка 65143\nAV2110DN - прошивка 65144 \n2. Реальный fps сильно зависит от настроек камеры и может быть от 9 fps (при полном разрешении и макс. качестве) до 25 fps (при средних настройках)","1. AV2110 - firmware 65143\nAV2110DN - firmware 65144 \n2. The actual frame rate very much depends on the camera's settings: it ranges from 9 fps (at full resolution and maximum quality) to 25 fps (with medium settings). "]
["Arecont Vision","Arecont Vision AV2115/-DN/-AI","Camera ","65201","1","+.",null,"+",null,"+",null,null,"MJPEG: 1920x1072 H264: 1920x1056","MJPEG: 1920x1072 H264: 1920x1056","H264: 960x536 MJPEG: 960x528","+",{"$nulls":4},"+","+",null,"+","-","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Датчик должен быть под напряжением","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. Close the sensor when it is energized"]
["Arecont Vision","Arecont Vision AV2115v1 / AV2115DNAIv1 / AV2115DNv1 / AV2145-3310-D(-LG) / AV2145-3310-W / AV2145-04-D(-LG) / AV2145-04-W / AV2145DN-3310-D(-LG) / AV2145DN-3310-W / AV2145DN-04-D(-LG) / AV2145DN-04-W ","Camera ","65218 ","1","+.",null,"+",null,"+",null,null,"1920x1056 ","1920x1056 ","960x528","+",{"$nulls":4},"+","+",null,"motion detection","-","Камеры AV2145-3310-D(-LG) / AV2145-3310-W / AV2145-04-D(-LG) / AV2145-04-W / AV2145DN-3310-D(-LG) / AV2145DN-3310-W / AV2145DN-04-D(-LG) / AV2145DN-04-W определяются как AV2145. ","AV2145-3310-D(-LG) / AV2145-3310-W / AV2145-04-D(-LG) / AV2145-04-W / AV2145DN-3310-D(-LG) / AV2145DN-3310-W / AV2145DN-04-D(-LG) / AV2145DN-04-W cameras are identified as AV2145."]
["Arecont Vision","Arecont Vision AV2116DNv1 / AV2146DN-3310-D(-LG) / AV2146DN-3310-W / AV2146DN-04-D(-LG) / AV2146DN-04-W ","Camera ","65219 ","1","+.",null,"+",null,"+",null,null,"1920x1072","1920x1072","960x536","+",{"$nulls":4},"+","+",null,"motion detection","-","Модели AV2146DN-3310-D(-LG), AV2146DN-3310-W, AV2146DN-04-D(-LG), AV2146DN-04-W определяются, как AV2146\n","AV2146DN-3310-D(-LG), AV2146DN-3310-W, AV2146DN-04-D(-LG), AV2146DN-04-W cameras are identified as AV2146.\n"]
["Arecont Vision","Arecont Vision AV2125/-DN/-IR","Camera ","65201 / 65202","1","+.",null,"+",null,"+",null,null,"MJPEG: 1920x1072 | H264: 1920x1056","MJPEG: 1920x1072 | H264: 1920x1056","MJPEG: 960x536 | H264: 960x528","+",{"$nulls":4},"+",null,null,"+","-","1. AV2125 - прошивка 65201\nAV2125-DN/-IR - прошивка 65202\n2. Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.\n3. Луч должен быть под напряжением.\n4. Устройство выдает 64 fps при половинчатом разрешении","1. AV2125 - firmware v.65201\nAV2125-DN/-IR - firmware v .65202\n2. The Auto Iris and Shutter Speed parameters are integrated as telemetry settings - but the camera does not have the telemetry functionality.\n3. The sensor must be energized.\n4. The device allows 64 fps at half the resolution.\"\n"]
["Arecont Vision","Arecont Vision AV2155/-DN/-HK/-DN-HK","Camera ","65143 / 65144 ","1","+.",null,"+",null,"+.",null,null,"1600x1184","1600 x 1184","800 x 592","+",{"$nulls":4},"+","+",null,"+","-","1.AV2155/-HK - прошивка 65143\nAV2155DN/-DN-HK - прошивка 65144 \n2. При выборе протокола TFTP камера фактически не работает. \n3. Прошивка 65139, 65143: H264-поток с камеры идет с искажениями (картинка рассыпается, смазывается). Искажения видны и в ПО ITV, и в ПО производителя.","1.AV2155/-HK - firmware 65143\nAV2155DN/-DN-HK - firmware 65144 \n2. If you select the TFTP protocol, the camera practically stops working. \n3. 65139 and 65143 firmware: The H.264 stream becomes distorted (the image is pixelated and/or blurred). You can see the distortions both in the AxxonSoft software and in the vendor software."]
["Arecont Vision","Arecont Vision AV2255AM(IR)/-A/-H/-AH","Camera","65221","1","+.",2,"+","-","+","-","-","1920x1080","1920x1080","960x540","+","-","-","-","+","-","+","-","motion detection","-"]
["Arecont Vision","Arecont Vision AV2256PM-IR","Camera ","65221","1","+.",null,"+",null,"+",null,null,"1920x1080","1920x1080","960x540","+",{"$nulls":3},"+","+","+",null,"motion detection.","-"]
["Arecont Vision","Arecont Vision AV2456DN-F","Camera","65221","1","+",2,"+","-","+","-","-","1920x1080","1920x1080","960x540","+","-","-","-","-","+","-","-","motion detection","-"]
["Arecont Vision","Arecont Vision AV2805/-DN","Camera ","65197","1","+.",null,"+",null,"+",null,null,"1920x1080(MJPEG)/1920x1056(H.264)","1920x1080 (MJPEG) / 1920x1056(H264)","960x540 (MJPEG) / 960x528(H264)","+",{"$nulls":3},"-","+","+",null,"+","-","Луч должен быть под напряжениемСтабильный видеопоток с 30 fps с камеры возможно получить только по протоколу TFTP","Close the sensor when it is energized. The camera produces a stable video stream at 30 fps only when the TFTP protocol is used."]
["Arecont Vision","Arecont Vision AV2815/-DN / AV2825/-DN/-IR","Camera ","65201","1","+.",null,"+",null,"+",null,null,"1920x1080","1920x1080","960x540","+",{"$nulls":4},"+","+",null,"+","-","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Максимальная частота кадров значительно ниже заявленной и зависит от множества дополнительных условий (~15 fps).Прошивка 65197: при использовании встроенного детектора частота кадров падает до 5 fps.Луч должен быть под напряжением.","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have the telemetry functionality. The maximum frame rate is much lower than stated in the documentation; it also depends on many additional factors (around 15 fps). 65200 firmware: when the embedded detection tool is used, the frame rate drops to 5 fps. Close the sensor when it is energized"]
["Arecont Vision","Arecont Vision AV3100/-DN/-AI","Camera ","64327 / 64328","1",null,null,"+",{"$nulls":4},"2048x1536","2048x1536","1024x768","+",{"$nulls":5},"+",null,"+","-","1. AV3100/-Ai - прошивка 64327\nAV3100DN - прошивка 64328 \n2. При мегапиксельном разрешении ограничение по fps равны 6,5 -10 fps (в зависимости от качества)\n\n \n\n ","1. AV3100/-Ai - firmware 64327\nAV3100DN - firmware 64328 \n2. With megapixel resolutions, the frame rate is limited to 6.5 –10 fps (depending on the quality)\n\n \n\n "]
["Arecont Vision","Arecont Vision AV3105/-DN/-AI","Camera ","65151 / 65152","1","+.",null,"+",null,"+",null,null,"2048x1536","2048x1536","1024x768","+",{"$nulls":4},"+","+",null,"motion detection","-","1. AV3105/-Ai - прошивка 65151\nAV3105DN - прошивка 65152 \n2. max значение fps у камеры 14\n2. лучи не интегрировались\n3. fps можно регулировать в настройке Low Light Mode\n4. при включении режима поддержки CUDA в ПО ITV видео в формате H.264 не будет. Это ограничение самой технологии CUDA. Поддержка CUDA отключается через утилиту tweaki.exe (tweaki.exe - вкладка Video Subsystem) ","1. AV3105/-Ai - firmware 65151\nAV3105DN - firmware 65152 \n2. The max. frame rate is 14 fps.\n3. Sensors are not integrated.\n4. You can adjust the frame rate by using the Low Light Mode setting.\n5. When CUDA support mode is on, the AxxonSoft software does not show video in H.264 format. This has to do with the limitations of the CUDA technology itself. You may switch CUDA off by using the tweaki.exe tool (tweaki.exe, Video Subsystem tab)."]
["Arecont Vision","Arecont Vision AV3110/-DN","Camera ","65143 / 65144","1",null,null,"+",{"$nulls":4},"1920x1072","1920x1072","960x536","+",{"$nulls":4},"+","+",null,"+","-","1. AV3110 - прошивка 65143\n AV3110DN - прошивка 65144 ","1. AV3110 - firmware 65143\n AV3110DN - firmware 65144 "]
["Arecont Vision","Arecont Vision AV3115/-DN/-AI","Camera ","65201","1","+.",null,"+",null,"+",null,null,"2048x1536","2048x1536","1024x768","+",{"$nulls":4},"+","+",null,"+","-","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Датчик должен быть под напряжением","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. Close the sensor when it is energized"]
["Arecont Vision","Arecont Vision AV3115v1 / AV3115DNAIv1 / AV3115DNv1 / AV3145-3310-D(-LG) / AV3145-3310-W / AV3145-04-D(-LG) / AV3145-04-W / AV3145DN-3310-D(-LG) / AV3145DN-3310-W / AV3145DN-04-D(-LG) / AV3145DN-04-W","Camera ","65218 ","1","+.",null,"+",null,"+",null,null,"2048x1536 ","2048x1536 ","1024x768 ","+",{"$nulls":4},"+","+",null,"motion detection","-","1. Модели AV3145-3310-D(-LG), AV3145-3310-W, AV3145-04-D(-LG), AV3145-04-W, AV3145DN-3310-D(-LG), AV3145DN-3310-W, AV3145DN-04-D(-LG), AV3145DN-04-W определяются, как AV3145\n2. C кодеком MJPEG при включенном детекторе движение Частота кадров падает до 5-7 fps\n\n","1. AV3145-3310-D(-LG), AV3145-3310-W, AV3145-04-D(-LG), AV3145-04-W, AV3145DN-3310-D(-LG), AV3145DN-3310-W, AV3145DN-04-D(-LG), AV3145DN-04-W cameras are identified as AV3145\n2. With the motion detection tool enabled, the frame rate for MJPEG falls to 5–7 fps.\n\n"]
["Arecont Vision","Arecont Vision AV3116DNv1 / AV3146DN-3310-D(-LG) / AV3146DN-3310-W / AV3146DN-04-D(-LG) / AV3146DN-04-W","Camera ","65219 ","1","+.",null,"+",null,"+",null,null,"2048x1536","2048x1536","1024х768","+",{"$nulls":4},"+","+",null,"motion detection; ","-","Камеры AAV3146DN-3310-D(-LG) / AV3146DN-3310-W / AV3146DN-04-D(-LG) / AV3146DN-04-W определяются в ПО ITV/Axxon как AV3146. ","AV3146DN-3310-D(-LG) / AV3146DN-3310-W / AV3146DN-04-D(-LG) / AV3146DN-04-W cameras are identified as AV3146. "]
["Arecont Vision","Arecont Vision AV3125/-DN/-IR ","Camera ","65201 ","1","+.",null,"+",null,"+",null,null,"2048x1536","2048x1536","1024x768","+",{"$nulls":4},"+","+",null,"+","-","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Луч должен быть под напряжением.","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. Close the sensor when it is energized"]
["Arecont Vision","Arecont Vision AV3130/-DN","Camera ","64329","1",null,null,"+",{"$nulls":4},"2048х1536(day)/1280х1024(night)","2048х1536(day)/1280х1024(night)","1024x768(day)/640х512(night)","+",{"$nulls":4},"-","-",null,null,"-","Сама камера выдает не более 14 fps.Прошивка 64329: камера не поддерживает работу лучей и реле.","The camera itself allows max. 14 fps. 64329 firmware: the camera does not support sensors or relays. "]
["Arecont Vision","Arecont Vision AV3135","Camera ","65153","1","+.",null,"+",null,"+",null,null,"2048x1536 (Day)/1280x1024(Night)","2048x1536 (Day) / 1280x1024 (Night)","1024x768 (Day) / 640x512 (Night)","+",{"$nulls":4},"+","+",null,"+","-","Луч должен быть под напряжением","Close the sensor when it is energized. "]
["Arecont Vision","Arecont Vision AV3155/-DN/-HK/-DN-HK","Camera ","65143 / 65144","1","+.",null,"+",null,"+",null,null,"2048x1536","2048x1536","1024x768","+",{"$nulls":4},"+","+",null,"+","-","1. AV3155/-HK - прошивка 65143\nAV3155DN/-DN-HK - прошивка 65144 \n2. Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.","1. AV3155/-HK - firmware 65143\nAV3155DN/-DN-HK - firmware 65144 \n2. The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality."]
["Arecont Vision","Arecont Vision AV3255AM/-HK / AV3255AMIR","Camera ","65218 ","1","+.",null,"+",null,"+",null,null,"2048x1536","2048x1536","1024x768","+",{"$nulls":3},"+","+","+",null,"motion detection; ","-"]
["Arecont Vision","Arecont Vision AV3256PMIR","Camera ","65221","1","+.",null,"+",null,"+",null,null,"2048x1536","2048x1536","1024x768","+",{"$nulls":3},"+","+","+",null,"motion detection.","-"]
["Arecont Vision","Arecont Vision AV5100/-DN/-AI","Camera ","64327 / 64328","1",null,null,"+",{"$nulls":4},"2560x1600","2560x1600","1280x800","+",{"$nulls":5},"+",null,"+","-","1. AV5100/-AI - прошивка 64327\nAV5100DN - прошивка 64328 \n2. Ограничение по fps:\n2560x1600(SDK) 8-10 fps \n2560x1600(WEB) 10 fps\n1280x800(SDK)  10 fps \n1280x800(WEB)  10 fps\n\n\n\n ","1. AV5100/-AI - firmware 64327\nAV5100DN - firmware 64328 \n2. Frame rate limits: \n2560x1600(SDK) 8–10 fps \n2560x1600(WEB) 10 fps\n1280x800(SDK)  10 fps \n1280x800(WEB)  10 fps\n\n\n\n "]
["Arecont Vision","Arecont Vision AV5105/-DN/-AI","Camera ","65151 / 65152 ","1","+.",null,"+",null,"+",null,null,"2560x1600","2560x1600","1280x800","+.",{"$nulls":4},"+","+",null,"motion detection; ","-"," AV5105/-AI - прошивка 65151\n AV5105DN - прошивка 65152 "," AV5105/-AI - fw 65151\n AV5105DN - fw 65152 "]
["Arecont Vision","Arecont Vision AV5110/-DN","Camera ","65143 / 65144","1",null,null,"+",{"$nulls":4},"2592x1936","2592x1936","1296x968","+",{"$nulls":4},"+","+",null,"-","-","AV5110 - прошивка 65143\nAV5110-DN - прошивка 65144\nКамера имеет ограничение по fps:\n - 9fps @ 2592x1936\n - 12fps @ 1296x9686\nДатчик должен быть под напряжением","AV5110 - firmware v.65142\nAV5110 - firmware v.65144\nThe camera has frame rate limits:\n - 9fps @ 2592x1936 \n - 12fps @ 1296x9686\nThe sensor must be energized.\n"]
["Arecont Vision","Arecont Vision AV5115/-DN/-AI","Camera ","65201","1","+.",null,"+",null,"+",null,null,"2592x1936 (MJPEG)/2560x1920(H.264)","2592x1936 (MJPEG) / 2560x1920 (H264)","1296x968 (MJPEG) / 1280x960 (H264)","+",{"$nulls":4},"+","+",null,"+","-","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Луч должен быть под напряжением.","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. Close the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV5115v1 / AV5115DNAIv1 / AV5115DNv1 / AV5145-3310-D(-LG) / AV5145-3310-W / AV5145-04-D(-LG) / AV5145-04-W / AV5145DN-3310-D(-LG) / AV5145DN-3310-W / AV5145DN-04-D(-LG) / AV5145DN-04-W ","Camera ","65218 ","1","+.",null,"+",null,"+",null,null,"2560x1920(H.264)/2592x1936(MJPEG) ","2560x1920(H.264) / 2592x1936(MJPEG) ","1980x960(H.264) / 1296x968(MJPEG)","+",{"$nulls":4},"+","+",null,"motion detection","-","Модели AV5145-3310-D(-LG), AV5145-3310-W, AV5145-04-D(-LG), AV5145-04-W, AV5145DN-3310-D(-LG), AV5145DN-3310-W, AV5145DN-04-D(-LG), AV5145DN-04-W будут определяться как AV5145 ","AV5145-3310-D(-LG), AV5145-3310-W, AV5145-04-D(-LG), AV5145-04-W, AV5145DN-3310-D(-LG), AV5145DN-3310-W, AV5145DN-04-D(-LG), AV5145DN-04-W cameras are identified as AV5145 "]
["Arecont Vision","Arecont Vision AV5125/-DN/-IR","Camera ","65201","1","+.",null,"+",null,"+",null,null,"2592x1936 (MJPEG)/2560x1920(H.264)","2592x1936 (MJPEG) / 2560x1920 (H264)","1296x968 (MJPEG) / 1280x960 (H264)","+",{"$nulls":4},"+",null,null,"+","-","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Луч должен быть под напряжением.","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. Close the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV5155/-DN/-HK","Camera ","65151 / 65152","1","+.",null,"+",null,"+",null,null,"2560x1920","2560x1920","1280x960","+",{"$nulls":4},"+","+",null,"+","-","1. AV5155/-HK - прошивка 65151\nAV5155DN - прошивка 65152\n2. Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.\n3. Камера имеет ограничение по FPS:\n - 9fps @ 2592x1944\n - 12fps @ 2560x1600\n - 15fps @ 2048x1536\n - 24fpsfps @ 1600x1200\n - 30fps @ 1280x1024\n4. Датчик должен быть под напряжением ","1. AV5155/-HK - firmware 65151\nAV5155DN - firmware 65152\n2. The Auto Iris and Shutter Speed parameters are integrated as telemetry settings - but the camera itself does not have the telemetry functionality.\n3. The camera has the following frame rate / resolution limits:\n - 9fps @ 2592x1944\n - 12fps @ 2560x1600\n - 15fps @ 2048x1536\n - 24fpsfps @ 1600x1200\n - 30fps @ 1280x1024\n4. The sensor must be energized. "]
["Arecont Vision","Arecont Vision AV5255AM/-HK","Camera ","65218 ","1",null,null,"+",null,"+",null,null,"2592x1944 ","2592x1944 ","1296x972 ","+",{"$nulls":3},"+","+","+",null,"motion detection; ","-"]
["Arecont Vision","Arecont Vision AV8180/AV8360","Camera ","65010","4",null,null,"+",{"$nulls":4},"1600x1200","1600x1200","800x600","+",{"$nulls":7},"+","-","1. Сама камера имеет ограничение по fps:\n800x600 10-13fps в зависимости от качества\n1600x1200 7-8fps в зависимости от качества","1. The camera itself has frame rate limits:\n800x600 10–13 fps (depending on quality)\n1600x1200 7–13 fps (depending on quality)"]
["Arecont Vision","Arecont Vision AV8185DN","Camera ","65166","4","+.",null,"+",null,"+",null,null,"1600x1200","1600x1200","800x600","+",{"$nulls":4},"-","-",null,"+","-","Панорамные AV8185 и AV8365 отличаются только углом обзора: 180 и 360 градусов соответственно.Максимальная частота кадров: ~10 fps в разрешении \"800х600\" и ~5 fps в разрешении \"1600х1200\" в зависимости от качества.На всех 4х каналах устройства должен стоять один и тот же видеокодек. Луч должен быть под напряжениемПри выборе протокола TFTP камера фактически не работает.C текущей прошивкой 65166 интегрировать лучи и реле нет возможности.","The only difference between the panoramic AV8185 and AV8365 models is the total angle of view: 180 and 360 degrees, respectively. Max. frame rate: around 10 fps at 800х600 resolution and around 5 fps at 1600х1200 resolution, depending on the quality. All of the camera's 4 channels must have the same video codec. Close the sensor when it is energized. If you select the TFTP protocol, the camera practically stops working. With the current firmware (65166), sensors and relays cannot be integrated."]
["Arecont Vision","Arecont Vision AV8365DN","Camera ","65166","4","+.",null,"+",null,"+",null,null,"1600x1200","1600x1200","800x600","+",{"$nulls":4},"-","-",null,"+","-","Панорамные AV8185 и AV8365 отличаются только углом обзора: 180 и 360 градусов соответственно.Максимальная частота кадров: ~10 fps в разрешении \"800х600\" и ~5 fps в разрешении \"1600х1200\" в зависимости от качества.На всех 4х каналах устройства должен стоять один и тот же видеокодек. Луч должен быть под напряжениемПри выборе протокола TFTP камера фактически не работаетС текущей прошивкой 65166 интегрировать лучи и реле нет возможности.","The only difference between the panoramic AV8185 and AV8365 models is the total angle of view: 180 and 360 degrees, respectively. Around 10 fps at 800х600 resolution and around 5 fps at 1600х1200 resolution, depending on the quality. All of the camera's 4 channels must have the same video codec. Close the sensor when it is energized. If you select the TFTP protocol, the camera practically stops working. With the current firmware (65166), sensors and relays cannot be integrated."]
["ARH","ARH ParkIT","Camera ","1.11.1.0","1",null,null,"+",{"$nulls":4},"752x480","752x480","752x480","-",{"$nulls":3},"+.","-","-",null,"-","+","Камера не поворотная, но есть встроенный трансфокатор.","This is not a PTZ camera, but it has a built-in zoom lens."]
["Arlotto","Arlotto AR1500(H/T)","Camera ","2.60.27","1",null,null,"+","+","+",null,null,"1280x720","720x480","320x190","+",null,"+","-",null,"+","+",null,"motion detection","+","1. С камеры можно получать от одного до трех видеопотоков, на камере есть три режима работы: Single, Dual и Tri-Stream. Существует зависимость между параметрами поток-кодек-разрешение, т.к. набор разрешений для потока зависит от того, сколько потоков сейчас включено. При настройке камеры в ПО Axxon необходимо об этом помнить и выставлять на камере только совместимые настройки.\n2. Лучи необходимо замыкать под напряжением\n3. В ПО Intellect максимальное разрешение 1280х720\n4. В кодеке H264 в разрешении 5MP частота кадров недоступна для изменения.\n5. Прошивка 2.60.17: Встроенный детектор в Axxon Next начинает работать только после изменения любых параметров видео. 6. Поиск находит камеру как неподдерживаемое устройство.","1. From the camera, you can receive from one to three video streams. The camera has three operation modes: Single, Dual, and Tri-Stream. The Stream, Codec, and Resolution parameters are interrelated, because the set of available resolutions for a stream depends on how many streams are currently on. When you configure the camera in the AxxonSoft software, remember this and use compatible values for the camera's settings. \n2. Close the sensors when they are energized.\n3. In Intellect, the max. resolution is 1280x720.\n4. At 5MP resolution, the H.264 codec does not allow you to change the frame rate. \n5. 2.60.17 firmware: In Axxon Next, the embedded detection tool starts working only after a video setting is changed. \n6. Search detects the camera as an unsupported device. "]
["Arlotto","Arlotto AR2200(H/T)","Camera ","2.60.18","1",null,null,"+","+","+",null,null,"1920x1080","H.264, MJPEG: 1600x1200, MPEG4: 1280x960","H.264, MPEG4: 720x480, MJPEG: 640х352","+",null,null,"-",{"$nulls":4},"+","+","Камера поддерживает до трех потоков, при этом параметры \"Кодек\" и \"Разрешение\" на разных потоках взаимосвязаны.","The camera supports up to three streams; the Codec and Resolution parameters for different streams are interdependent. "]
["Arlotto","Arlotto AR2500(H/T)","Camera ","2.60.18","1",null,null,"+","+","+",null,null,"H.264/MJPEG:2592x1920,MPEG4:1920x1080","H.264, MJPEG: 1600x1200, MPEG4: 1280x960","H.264, MPEG4: 720x480, MJPEG: 640х352","+",null,null,"-",{"$nulls":4},"+","+","Камера поддерживает до трех потоков, при этом параметры \"Кодек\" и \"Разрешение\" на разных потоках взаимосвязаны. ","The camera supports up to three streams; the Codec and Resolution parameters for different streams are interdependent. "]
["Arlotto","Arlotto AR2510/AR2520","Camera ","2.60.18","1",null,null,"+","+","+",null,null,"2592x1920 (h264, mjpeg) / 1920x1080 (mpeg4)","1600x1200 (h264, mjpeg) / 1280x960 (mpeg4)","720x480 (h264, mpeg4) / 640x352 (mjpeg)","+",null,null,"-",{"$nulls":4},"+.","+","С камеры можно получать от одного до трех видеопотоков, на камере есть три режима работы: Single, Dual и Tri-Stream. Параметры \"кодек\" и \"разрешение\" разных потоков зависят друг от друга. При настройке камеры в ПО Axxon необходимо об этом помнить и выставлять на камере только совместимые настройки.В первом потоке в кодеке mpeg4 не доступны разрешения выше 1920х1080, а в кодеке mjpeg не доступны разрешения ниже 1600x1200.Прошивка 2.60.18: поиск обнаруживает устройство как AR1500.Максимальная частота кадров в разрешении 5MP - 10fps.Прошивка 2.60.18: камера в целом ведет себя достаточно нестабильно - иногда зависает, перестает передавать видео.Максимальное значение битрейта для первого потока - 7000, а для второго - 800. В стандартном разрешении Интеллект подключается ко второму потоку для всех кодеков, поэтому качество картинки на стандартном разрешении значительно уступает качеству на высоком и полном разрешениях.","From the camera, you can receive from one to three video streams. The camera has three operation modes: Single, Dual, and Tri-Stream. The Codec and Resolution parameters for different streams are interdependent. When you configure the camera in the AxxonSoft software, remember this and use compatible values for the camera's settings. In the first stream, the mpeg4 codec does not allow resolutions higher than 1920x1080 and the mjpeg codec does not allow resolutions lower than 1600x1200. 2.60.18 firmware: Search detects the device as AR1500.With 5PM resolution, the maximum frame rate is 10 fps. 2.60.18 firmware: in general, the camera is pretty unstable – sometimes it freezes and stops sending video. The max. bit rate is 7,000 for the first stream and 800 for the second stream. At standard resolution, Intellect connects to the second stream for all codecs; for this reason, at standard resolution, the image quality is much lower than the quality at high and full resolutions. "]
["Arlotto","Arlotto AR3210","Camera ","2.60.18.r1","1",null,null,"+","+","+",null,null,"1920x1080","H.264, MJPEG: 1600x1200, MPEG4: 1280x960","H.264, MPEG4: 720x480, MJPEG: 640x352","+",null,null,"-",{"$nulls":4},"+","+","Камера поддерживает до трех потоков, при этом параметры \"Кодек\" и \"Разрешение\" на разных потоках взаимосвязаны.","The camera supports up to three streams; the Codec and Resolution parameters for different streams are interdependent."]
["Arlotto","Arlotto AR3510","Camera ","2.60.18.r1","1",null,null,"+","+","+",null,null,"H.264, MJPEG: 2595x1920, MPEG4: 1920x1080","H.264, MJPEG: 1600x1200, MPEG4: 1280x960","H.264, MPEG4: 720x480, MJPEG:640x352","+",null,null,"-",{"$nulls":4},"+","+","Камера поддерживает до трех потоков, при этом параметры \"Кодек\" и \"Разрешение\" на разных потоках взаимосвязаны.","The camera supports up to three streams; the Codec and Resolution parameters for different streams are interdependent."]
["Arlotto","Arlotto AR4200(H/T)","Camera ","2.60.18","1",null,null,"+","+","+",null,null,"1920x1080","1600x1200 (h264, mjpeg) / 1280x960 (mpeg4)","720x480 (h264, mpeg4) / 640x352 (mjpeg)","+",null,null,"-",{"$nulls":4},"+","+","С камеры можно получать от одного до трех видеопотоков, на камере есть три режима работы: Single, Dual и Tri-Stream. Параметры \"кодек\" и \"разрешение\" разных потоков зависят друг от друга. При настройке камеры в ПО Axxon необходимо об этом помнить и выставлять на камере только совместимые настройки.","From the camera, you can receive from one to three video streams. The camera has three operation modes: Single, Dual, and Tri-Stream. The Codec and Resolution parameters for different streams are interdependent. When you configure the camera in the AxxonSoft software, remember this and use compatible values for the camera's settings."]
["Arlotto","Arlotto AR4500(H/T)","Camera ","2.60.18","1",null,null,"+","+","+",null,null,"2592x1960 (h264, mjpeg) / 1920x1080 (mpeg4)","1600x1200 (h264, mjpeg) / 1280x960 (mpeg4)","720x480 (h264, mpeg4) / 640x352 (mjpeg)","+",null,null,"-",{"$nulls":4},"+","+","С камеры можно получать от одного до трех видеопотоков, на камере есть три режима работы: Single, Dual и Tri-Stream. Параметры \"кодек\" и \"разрешение\" разных потоков зависят друг от друга. При настройке камеры в ПО Axxon необходимо об этом помнить и выставлять на камере только совместимые настройки.","From the camera, you can receive from one to three video streams. The camera has three operation modes: Single, Dual, and Tri-Stream. The Codec and Resolution parameters for different streams are interdependent. When you configure the camera in the AxxonSoft software, remember this and use compatible values for the camera's settings."]
["Asoni","Asoni CAM439P","Camera ","V3.2.66_As.1","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",null,"-","-",{"$nulls":4},"+","+","В максимальном разрешении (1280x1024) максимальная частота кадров - 10 fpsПри одновременном использовании нескольких видеопотоков суммарная частота кадров должна быть 25 fps. Причем после изменения частоты кадров на значение A на одном из потоков частота кадров на другом потоке автоматически становится равной 25 - A.","At the maximum resolution (1280x1024), the max. frame rate is 10 fps. When multiple video streams are used simultaneously, the total frame rate must be 25 fps. After the frame rate for a stream is changed by A fps, the frame rate for the other stream automatically becomes (25-A) fps. "]
["Asoni","Asoni CAM636MVP / CAM613","Camera ","V1.0.14_As.1","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+","+",null,"+","+",null,"+","+","На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AxxonNext/Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.Тревога по замыканию луча срабатывает при условии соблюдения заданного временного интервала (мин. 10 сек) между замыканиями. Интервал настраивается в веб-интерфейсе. Особенность камеры.В Интеллект поиск находит камеру как FineCCTV IP-Cam.","The camera has the Video Parameters option (the max. resolution and max. frame rate). In AN, you must make sure that there is no conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value. Closing the sensor makes the alarm go off, but only if the time between two consecutive closures is a minimum of 10 seconds. You must set the interval using the web interface. This is a limitation of the camera itself. In Intellect, search detects the camera as FineCCTV IP-Cam."]
["Asoni","Asoni SVR610-PoE","Camera ","V1.0.8_As.1","1",null,null,"+",null,"+",null,null,"720x576","704x576","352x288","+",null,"+","-","+","+","+",null,"+","+","Тревога по замыканию луча срабатывает при условии соблюдения заданного временного интервала (мин. 10 сек) между замыканиями. Интервал настраивается в веб-интерфейсе. Особенность камеры.Правильный ТВ-стандарт (PAL/NTSC) нужно выставить в зависимости от подключенной аналоговой камеры.В Интеллект поиск находит камеру как FineCCTV IP-Cam.","Closing the sensor makes the alarm go off, but only if the time between two consecutive closures is a minimum of 10 seconds. You must set the interval using the web interface. This is a peculiarity of the camera itself. You must set the right TV standard (PAL/NTSC), depending on what analog camera is connected. In Intellect, search detects the camera as FineCCTV IP-Cam."]
["Aver","Aver FD2000","Camera ","0.1.28 ","1",null,null,"+","-","+",null,null,"1920x1080","640x480","320x240","+",null,"+",null,"-","-",null,null,"-","+","Значение настройки ТВ-стандарт в ПО ITV/Axxon следует выставлять в соответствии со значением ТВ-стандарта в веб-интерфейсе.","TV-standard value in ITV | AxxonSoft should be put in line with the value of TV-standard in the web-interface."]
["Aver","Aver SF2121H-BHR","Camera ","1.1.1.38","1",null,null,"+","+","+",null,null,"1920x1080","800x600","640x480","+",null,"+","-","+","-","-","-","-","+","Камера передает видео только в Full HD (1920x1080). При выборе меньших разрешений изображение обрезается до нужного размера. Область отображения настраивается через веб-интерфейс.","The camera transmits video only in Full HD (1920x1080). When you select the image resolution less that Full HD, image will be cut to the desired size. The display area chould be configured via web-interface."]
["Aver","Aver SF1311H-C","Camera ","5.a.2.7766 ","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",null,null,"-",{"$nulls":4},"-","+"]
["Avigilon","Avigilon 2.0W-H3PTZ-DP20 (ONVIF)","Camera","2.4.4.38","1",null,null,"+","-","+",null,null,"1920x1080","1280x720","762х432","-",null,"-","-","+",{"$nulls":4},"+"]
["Avigilon","Avigilon 3.0W-H3-D2 (ONVIF)","Camera","2.4.2.8","1",null,null,"+",null,"+",null,null,"2048x1536","1280x960","768x576","+",null,"+",null,"+.",{"$nulls":4},"+"]
["AVTech","AVTech AVM504","Camera","1038-1021-1024-1012-A3","1",null,null,"+","-","+","-","-","from WEB","from WEB","from WEB","+","-","-","-","+","-","-","-","-","+","При смене значения настройки антимерцания камера перезагружается.","When the anti blink setting is changed, the camera reboots."]
["Axis","Axis 206","Camera ","4.40","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":8},"+"]
["Axis","Axis 206M","Camera ","4.40.1","1",null,null,"+",{"$nulls":4},"1280x1024","640x480","320x240","+",{"$nulls":8},"+"]
["Axis","Axis 207","Camera ","4.40.1","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",null,"+",null,null,"+","+",null,"-","+"]
["Axis","Axis 207MW","Camera ","4.44","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x360","320x240","+",null,"+",null,null,"+","+",null,"-","+"]
["Axis","Axis 207W","Camera ","4.44","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",null,"+",null,null,"+","+",null,"-","+"]
["Axis","Axis 209FD/-R","Camera ","4.47","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",{"$nulls":7},"-","+"]
["Axis","Axis 209MFD/-R","Camera ","4.47","1",null,null,"+","+",{"$nulls":3},"1280x1024","1024x768","640x480","+",{"$nulls":3},"-",{"$nulls":3},"-","+","1. У самой камеры есть ограничение fps при мегапиксельном разрешении (1280х1024):\nMJPEG -  12 fps\nMPEG-4 - 8 fps\n2. Камера не поворотная, но есть цифровая телеметрия (Digital PTZ)","1. With the megapixel resolution (1280x1024), the camera itself has frame rate limits: \nMJPEG –  12 fps\nMPEG-4 – 8 fps\n2. This is not a PTZ camera, but it has digital telemetry (Digital PTZ)."]
["Axis","Axis 210","Camera ","4.40","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",{"$nulls":4},"+","+",null,"-","+"]
["Axis","Axis 210A","Camera ","4.47","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",null,"+","+",null,"+","+",null,"-","+"]
["Axis","Axis 211","Camera ","4.40","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",{"$nulls":4},"+","+",null,"-","+"]
["Axis","Axis 211A","Camera ","4.47","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+","+","+","+",null,"+","+",null,"-","+","1. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","1. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 211M","Camera ","4.41","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x360","320x240","+",null,"+","+",null,"+","+",null,"-","+"]
["Axis","Axis 211W","Camera ","4.40.1","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",null,"+","+",null,"+","+",null,"-","+"]
["Axis","Axis 2120","Camera ","2.40","1",null,null,"+",{"$nulls":4},"720x576","720х288","352x288","+",null,"-","-",null,"+","+",null,"-","-","1.В Полном (720х576) разрешении камера способна выдавать максимум 8-10 fps. Ограничение самой камеры. \n   В Высоком (720х288) разрешении камера способна выдавать максимум 12-15 fps. Ограничение самой камеры \n2. Лучи следует замыкать под напряжением\n3. Звук скамеру можно получить только с помощью спец. устройства \"дополнительный модуль Axis 2191 audio module\" (у нас его нет)","1. At full resolution (720х576), the camera allows 8–10 fps max. This is a limitation of the camera itself. \nAt high resolution (720х288), the camera allows 12–15 fps max. This is a limitation of the camera itself. \n2. Close the sensors when they are energized.\n3. You can get audio from the camera only by using an additional device (Axis 2191 Audio Module); we do not have one. "]
["Axis","Axis 212PTZ","Camera ","4.40","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",null,"+","+","+","+","+",null,"-","+"]
["Axis","Axis 2130 PTZ","Camera ","2.43","1",null,null,"+.",{"$nulls":4},"704x480","704x480","704x480","-",{"$nulls":3},"+.","+","-",null,"-","-"]
["Axis","Axis 213PTZ","Camera ","4.35","1",null,null,"+","+",{"$nulls":3},"704x576","704x288","352x288","+",{"$nulls":3},"+",{"$nulls":3},"-","+"]
["Axis","Axis 214PTZ","Camera ","4.40","1",null,null,"+","+",{"$nulls":3},"704x576","704x288","352x288","+",null,"+","+","+","+","+",null,"-","+"]
["Axis","Axis 215PTZ","Camera ","4.40","1",null,null,"+","+",{"$nulls":3},"704x576","704x288","352x288","+",null,"+","+","+","+","+",null,"-","+"]
["Axis","Axis 216FD","Camera ","4.47","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+","+","+","-",null,"+","+",null,"-","+","1. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","1. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 216MFD","Camera ","4.47.1","1",null,null,"+","+",{"$nulls":3},"1280x1024","1024x768","640x480","+",null,"+","+",null,"+","+",null,"-","+","1. Ограничения fps самой камеры:\n- 1280х1024 - max. 12 fps для MJPEG и 8 fps для MPEG-4\n- 1024x768 - max. 20 fps для MJPEG и 13 fps для MPEG-4\n ","1. The camera itself has frame rate limits: \n- 1280х1024 – max. 12 fps for MJPEG and 8 fps for MPEG-4\n- 1024x768 – max. 20 fps for MPEG and 13 fps for MPEG-4\n "]
["Axis","Axis 221","Camera ","4.45.1","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+","+",{"$nulls":3},"+","+",null,"-","+","максимальное значение fps = 49 1. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","The max. frame rate is 49 fps. 1. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 223М","Camera ","4.47","1",null,null,"+","+",{"$nulls":3},"1600x1200(MJPEG) / 640x480(MPEG-4)","1024x768(MJPEG) / 480x360(MPEG-4)","640x480(MJPEG) / 320x240(MPEG-4)","+",null,"+","+",null,"+","+",null,"-","+","У камеры два режима. «Normal resolutions (NR)» и «Widescreen resolutions (WR)». Соответственно набор разрешений для этих режимов разный, fps также разный. Для NR max fps=9, для WR max fps=12. Это ограничение самой камеры.","The camera has two modes: Normal Resolutions (NR) and Widescreen Resolutions (WR). The two modes differ in the set of resolutions and in frame rate. For NR, the max. frame rate is 9 fps; for WR, the max. frame rate is 12 fps. This is a limitation of the camera itself. "]
["Axis","Axis 225FD","Camera ","4.45.1","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+","+",{"$nulls":3},"+","+",null,"-","+","1. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","1. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 231D+","Camera ","4.41","1",null,null,"+","+",{"$nulls":3},"704x576","704x576","352x288","+",{"$nulls":3},"+.","-","+",null,"-","+"]
["Axis","Axis 232D+","Camera ","4.47","1",null,null,"+","+",{"$nulls":3},"704x576","704x576","352x288","+","+",null,null,"+.","-","+",null,"-","+","1. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","1. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 233D","Camera ","4.48","1",null,null,"+","+",{"$nulls":3},"704x576","704x288","352x288","+",null,"+","-","+.","+","+",null,"-","+"]
["Axis","Axis 2400 encoder","Encoder ","2.34","4",null,null,"+",{"$nulls":4},"720x576","720x576","352x288","+",null,"-","-","+.","+","+",null,null,"-","1. В \"Полном\" разрешении сервер способен выдавать максимум 8-10 fps. \n2. В родном веб-интерфейсе работает так: Доступны или каждый из четырех каналов, но одновременно работает только один канал и он выдает 25 fps. Или же квадро-режим, тогда работают сразу все четыре канала и они выдают по 5 fps каждый. В Intellect сделано лучше. Можно сделать чтобы работал только один канал (25 fps), сразу два канал (по 12 fps), три канала (по 8 fps), или же четыре (по 5-6 fps) \n3. Лучи следует замыкать под напряжением\n4. Звук скамеру можно получить только с помощью спец. устройства \"дополнительный модуль Axis 2191 audio module\" (у нас его нет)","1. At full resolution, the encoder allows 8–10 fps max. \n2. The device's own web interface works like this: Either each of the 4 channels is available, but at a given moment in time only 1 channel is working, at 25 fps. Or you have quad mode, in which all the 4 channels are working at the same time, at 5 fps each. Intellect offers more flexibility: you can select only 1 channel (at 25 fps), 2 channels at the same time (at 12 fps each), 3 channels at the same time (at 8 fps each), or 4 channels at the same time (at 5–6 fps each). \n3. Close the sensors when they are energized.\n4. You can get audio from the camera only by using an additional device (Axis 2191 Audio Module); we do not have it."]
["Axis","Axis 2400+ encoder","Encoder ","3.13","4",null,null,"+",{"$nulls":4},"720x576","720х288","352x288","+",null,"-","-","+.","+","+",null,null,"-","1. В Полном (720х576) разрешении сервер способен выдавать максимум 8-10 fps. Ограничение самого сервера. 2. В Высоком (720х288) разрешении сервер способен выдавать максимум 12-15 fps. Ограничение самого сервера 3. В родном веб-интерфейсе работает так: Доступны или каждый из четырех каналов, но одновременно работает только один канал и он выдает 25 fps. Или же квадро-режим, тогда работают сразу все четыре канала и они выдают по 5 fps каждый. В Intellect сделано лучше. Можно сделать чтобы работал только один канал (25 fps), сразу два канал (по 12 fps), три канала (по 8 fps), или же четыре (по 5-6 fps) \n4. Звук работает только с доп. устройством «AXIS 2191 Audio Module» (у нас его нет)","1. At full resolution (720х576), the encoder allows 8–10 fps max. This is a limitation of the encoder itself. 2. At high resolution (720х288), the encoder allows 12–15 fps max. This is a limitation of the encoder itself. 3. The device's own web interface works like this: Either each of the 4 channels is available, but at a given moment in time only 1 channel is working, at 25 fps. Or you have quad mode, in which all the 4 channels are working at the same time, at 5 fps each. Intellect offers more flexibility: you can select only 1 channel (at 25 fps), 2 channels at the same time (at 12 fps each), 4 channels at the same time (at 8 fps each), or 4 channels at the same time (at 5–6 fps each). You can get audio only by using an additional device (Axis 2191 Audio Module); we do not have it."]
["Axis","Axis 240Q encoder","Encoder ","4.40","4",null,null,"+",{"$nulls":4},"704x576","704x576","352x288","+",{"$nulls":3},"+","+","+",null,"-","+"]
["Axis","Axis 2411 encoder","Encoder ","3.13","1",null,null,"+",{"$nulls":4},"704x576","704x576","352x288","+.",{"$nulls":8},"-","В \"Полном\" разрешении сервер способен выдавать максимум 8-10 fps. ","At full resolution, the encoder allows 8–10 fps max. "]
["Axis","Axis 241Q encoder","Encoder ","4.47","4",null,null,"+","+",{"$nulls":3},"704x576","704x576","352x288","+","+",null,null,"+","+","+",null,"-","+","1. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","1. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 241QA encoder","Encoder ","4.47","4",null,null,"+","+",{"$nulls":3},"704x576","704x576","352x288","+",null,"+","+","+","+","+",null,"-","+"]
["Axis","Axis 241S encoder","Encoder ","4.47","1",null,null,"+","+",{"$nulls":3},"704x576","704x576","352x288","+",{"$nulls":3},"+","+","+",null,"-","+"]
["Axis","Axis 2420 encoder","Encoder ","2.43","1",null,null,"+",{"$nulls":4},"720x576","720х288","352x288","+",null,"-","-",null,"+","+",null,"-","-","1. В Полном (720х576) разрешении камера способна выдавать максимум 8-10 fps. Ограничение самой камеры. 2. В Высоком (720х288) разрешении камера способна выдавать максимум 12-15 fps. Ограничение самой камеры \n3. Лучи следует замыкать под напряжением\n4. Звук будет раотать только с доп. устройством «AXIS 2191 Audio Module» ","1. At full resolution (720х576), the camera allows 8–10 fps max. This is a limitation of the camera itself. \n2. At high resolution (720х288), the camera allows 12–15 fps max. This is a limitation of the camera itself. \n3. Close the sensors when they are energized.\n4. You can get audio only by using an additional device (Axis 2191 Audio Module); we do not have it. "]
["Axis","Axis 243Q blade encoder","Encoder ","4.41","4",null,null,"+","+",{"$nulls":3},"704x576","704x576","352x288","+","+",null,null,"+","+","+",null,"-","+","ВАЖНО!\n1. данный сервер - устройство для подключения 4 аналоговых камер, но при этом каждый канал сервера имеет свой собственный ip-адрес. Поэтому в ПО ITV чтобы задействовать все 4 канала необходимо создавать 4 Граббера (на каждый канал свой граббер). Поэтому и ключ нужно иметь соответствующий.\n2.лучи/реле - по одному на каждый вход т.е. нельзя для одной камеры создать несколько лучей/реле на разные каналы 3. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","THIS IS IMPORTANT!\n1. This encoder is a single device that allows you to connect 4 analog cameras; however, each channel of the encoder has its own IP address. For this reason, in AxxonSoft software, if you want to use all the 4 channels, you must create 4 Grabber objects (one grabber per channel). \n2. Sensors/relays, one for each port (i.e., only one sensor/relay per camera). 3. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 243SA encoder","Encoder ","4.45","1",null,null,"+","+",{"$nulls":3},"704x576","704x288","352x288","+","+","+","+","+","+","+",null,"-","+","1. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","1. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 247S encoder","Encoder ","4.42","1",null,null,"+","+",{"$nulls":3},"704x576","704x288","352x288","+",null,"+",null,null,"+","+",null,"-","+"]
["Axis","Axis M1011","Camera ","5.00","1","+",null,"+","+","+.",null,null,"640x480","480x360","320x240","+",{"$nulls":7},"-","+","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n\n ","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution). \n\n "]
["Axis","Axis M1011-W","Camera ","5.00","1","+",null,"+","+","+.",null,null,"640x480","480x360","320x240","+",{"$nulls":7},"-","+","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n\n","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution).\n\n"]
["Axis","Axis M1013","Camera ","5.40.5.2","1","+",null,"+",null,"+",null,null,"800x600","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"motion detection","+","1. Через AxxonNext настраивается только первый поток, остальные - через web-интерфейс;\n2. При включенной настройке \"цифровая ptz телеметрия\" не применяются некоторые настройки, в частности - видеопотока.\n3. Для подключения камеры как ONVIF device необходимо произвести дополнительные настройки через web-интерфейс: синхронизировать время с локальным сервером, добавить пользователя ONVIF; снять галку Enable replay attack protection по пути: System Options -> Advanced -> Plain Config -> Select Group -> Web-service","1. In AxxonNext, you can configure only stream 1, while other stream are set up in the camera's web interface;\n2. With Digital PTZ enabled, the video stream settings, among others, become unavailable.\n3. To connect the camera via ONVIF, use following settings in the camera's web interface: Sync time with the local Server, Add ONVIF User, deselect the checkbox for Enable replay attack protection. You can do this here: System Options -> Advanced -> Plain Config -> Select Group -> Web-service"]
["Axis","Axis M1014 ","Camera ","5.40.5.1","1","+",null,"+",null,"+",null,null,"1280x800","800x600","320x240","+",{"$nulls":3},"+",{"$nulls":3},"motion detection, tampering detection","+","1. Чтобы работала цифровая телеметрия, необходимо включить соответствующую настройку на камере. \n2. Для работы в ПО ITV/Axxon RTSP порт должен быть стандартным - 554 ","1. To use digital PTZ, it must be on in camera web interface. \n2. To work in Axxonsoft SW RTSP port should be staddard - 554."]
["Axis","Axis M1031-W","Camera ","5.20.3","1","+",null,"+","+.","+.",null,null,"640x480","480x360","320x240","+",null,"+","+",{"$nulls":4},"+","+"]
["Axis","Axis M1034-W","Camera","5.40.5.4","1",null,null,"+","-","+",null,null,"1280x800","800x600","320x240","+",null,"+","+","+","-","-","-","motion detection; audio detection; tampering detection","+"]
["Axis","Axis M1054","Camera ","5.15.1","1","+",null,"+",null,"+.",null,null,"1280x800","1024x768","640x480","+",null,"+",null,"+",{"$nulls":3},"-","+","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном веб-интерфейсе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect. \n3. Preset 1 is reserved for Home Position."]
["Axis","Axis M1103","Camera ","5.08.1","1","+",null,"+",null,"+.",null,null,"800x600","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","+","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position\n","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Preset 1 is reserved for Home Position.\n"]
["Axis","Axis M1104","Camera ","5.09","1","+",null,"+",null,"+.",null,null,"1280x800","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":3},"-","+","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position\n","1. This is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Preset 1 is reserved for Home Position.\n"]
["Axis","Axis M1113","Camera ","5.09","1","+",null,"+",null,"+",null,null,"800x600","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","+","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position\n","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Preset 1 is reserved for Home Position.\n"]
["Axis","Axis M1114","Camera ","5.08","1","+",null,"+",null,"+.",null,null,"1280x800","1024x768","640x480","+",{"$nulls":7},"-","+","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position\n","1. This is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Preset 1 is reserved for Home Position.\n"]
["Axis","Axis M1144-L","Camera ","5.40.10.6","1","+",null,"+",null,"+",null,null,"1280x800","800x600","640x480","+",{"$nulls":3},"+","+","+","+.","motion detection, tampering detection","+","На устройстве для кодека MJPEG недоступны следующие разрешения:\n\n 480x300\n 480x270\n 800x500\n 800x450 ","Unavailable resolution for MJPEG is the folowing:\n\n 480x300\n 480x270\n 800x500\n 800x450 "]
["Axis","Axis M3004-V","Camera ","5.40.5","1","+",null,"+",null,"+",null,null,"1280x800","800x600","320x240","+",{"$nulls":3},"+",{"$nulls":4},"+"]
["Axis","Axis M3005-V ","Camera ","5.40.5.5","1","+",null,"+",null,"+",null,null,"1920x1080 ","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":3},"motion detection, tampering detection","+"]
["Axis","Axis M3006-V","Camera ","5.40.13.2","1","+",null,"+",null,"+",null,null,"2048x1536","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":3},"motion detection, tampering detection","+","Чтобы работала цифровая телеметрия, необходимо включить соответствующую настройку. ","To use digital PTZ, it must be on in camera web interface."]
["Axis","Axis M3007-P/-PV","Fisheye Camera","5.40.13.1","1","+",4,"+","-","+","-","-","2592x1944","1024x768","640x480","+","-","-","-","-","-","-","-","motion detection","+","\nКамера имеет две степени свободы поворотного крепления. Если открыть кожух, то камеру можно наклонять вверх-вниз, а так же вращать вокруг оси линзы. Для корректной работы настройки \"Поворот видеоизображения\" необходимо в устанавливать поворотное крепление в правильное положение.","Camera rotary fastening has 2 degrees of freedom. If you open the camera casing, then you can tilt the camera up and down and rotate it around the lens axis. For proper operation of the Video rotation setting, you are to place the rotary fastening into the correct position."]
["Axis","Axis M3011","Camera ","5.01","1","+",null,"+","+","+.",null,null,"640x480","480x360","320x240","+",{"$nulls":7},"-","+","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n\n","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution).\n\n"]
["Axis","Axis M3014","Camera ","5.05","1","+",null,"+",null,"+.",null,null,"1280x800","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","+","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\", результаты работы телеметрии будут видны при достаточном зумировании картинки.\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Для корректной работы H.264-видеопотока следует настройку \"Качество\" выставить в среднее положение","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box. You will see the result of PTZ after you zoom enough. \n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. To make the H.264 video stream work correctly, set the Quality setting at a medium position. "]
["Axis","Axis M3024-LVE","Camera","5.40.5","1","+","2","+",null,"+",null,null,"1280x800","800x600","320x240","+",{"$nulls":3},"-","-","-","-","motion detection","+",null,null,"new"]
["Axis","Axis M3113-R","Camera ","5.12","1","+",null,"+",null,"+",null,null,"800x600","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","+","у камеры Digital PTZ (цифровая телеметрия)","The camera has Digital PTZ (digital telemetry). "]
["Axis","Axis M3114-R","Camera ","5.12","1","+",null,"+",null,"+.",null,null,"1280x800","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":4},"+","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellecte необходимо поставить галочку в родном вебе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellecte будет игнорироваться.\n","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n"]
["Axis","Axis M3203","Camera ","5.11","1","+",null,"+",null,"+.",null,null,"800x600","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","+","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Preset 1 is reserved for Home Position."]
["Axis","Axis M5013","Camera ","5.25.2 ","1","+",null,"+",null,"+",null,null,"800x600","640x480","320x240","+",null,"+",null,"+",{"$nulls":3},"+","+","На камере предусмотрены 5 видеопотоков:0. Получение видео H264/MJPEG и применение настроек.1. Соответствует профилю \"Quality\" в веб-интерфейсе камеры. Получение видео без настроек.2. Соответствует профилю \"Balanced\" в веб-интерфейсе камеры. Получение видео без настроек.3. Соответствует профилю \"Bandwith\" в веб-интерфейсе камеры. Получение видео без настроек.4. Соответствует профилю \"Mobile\" в веб-интерфейсе камеры. Получение видео без настроек.При использовании потоков 1-4 после изменения настроек (через веб-интерфейсе) необходимо перезапускать поток или объект \"камера\".Встроенная аналитика работает:В 0-м потоке в любом кодеке.В любом другом потоке, но только в H264.Камера поворотная, но зум у нее только цифровой.Через Onvif не работают настройки изображения - проблема устройства.Работа камеры проверялась только по протоколу TCP - из-за особенностей удаленного доступа.","2. At the included digital telemetry resolution of a video stream will be limited to the resolution exposed in settings of telemetry in web. In this case the switch of resolution in Intellecte will be ignored "]
["Axis","Axis M5014/-V","Camera ","5.40.11.2","1","+",null,"+",null,"+",null,null,"1280x720","800x600","320x240","+",null,"+",null,"+",{"$nulls":3},"motion detection; audio detection","+"]
["Axis","Axis M7001 encoder","Encoder ","5.02","1",null,null,"+",null,"+.",null,null,"720x576","704x576","352x288","+",{"$nulls":3},"+",{"$nulls":3},"+","+","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.","3. Preset No. 1 is reserved for Home position"]
["Axis","Axis M7014 encoder","Encoder ","5.40.7.1","4","+",null,"+",null,"+",null,null,"720x576","704x576","352x288","+",{"$nulls":3},"+",{"$nulls":3},"motion detection, tampering detection","+"]
["Axis","Axis P1311","Camera ","5.01.1","1","+",null,"+","+","+.",null,null,"640x480","480x360","320x240","+",null,"+","+",null,"+","+",null,"-","+","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.","4. In Axxon Next streams with 2 on 5 (Auto) answer Stream Profiles of the web interface and are set only from there."]
["Axis","Axis P1343","Camera ","5.06","1","+",null,"+",null,"+",null,null,"800x600","640x480","320x240","+",null,"+","+","+","+","+",null,"-","+","1) данная камера является аналогом камеры Axis P1344, от которой отличается другим набором разрешений видеопотока.\n2) камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n3) при включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии. В этом случае переключатель разрешений в Intellect будет игнорироваться.","1. This camera is very similar to the Axis P1344 camera; the cameras differ in the set of available resolutions.\n2. This is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own web interface and select the Enable PTZ check box.\n3. When digital PTZ telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the telemetry settings. In this case, Intellect's resolution switch has no effect."]
["Axis","Axis P1344","Camera ","5.06","1","+",null,"+",null,"+.",null,null,"1280x800","640x480","320x240","+",null,"+","+","+","+","+",null,"-","+","1) данная камера является аналогом камеры Axis P1346, от которой отличается отстутствием режимов Capture mode, View Areas, а также набором разрешений видеопотока.\n2) камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n3) при включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n4) начиная с DP 3.2.5.678 камера (как и другие Axis с прошивкой 5.хх) поддерживает работу со стриммингами в ПО AxxonSoft","1. This camera is very similar to the Axis P1346 camera. Differences: This camera has a different set of resolutions, and it does not have Capture Mode or View Areas. \n2. This is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own web interface and select the Enable PTZ check box.\n3. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n4. Starting with DP 3.2.5.687, the camera (just like other Axis cameras with the 5.xx firmware) supports streams in the AxxonSoft software. "]
["Axis","Axis P1346","Camera","5.40.9.5","1","+","4","+",null,"+",null,null,"2048x1536 / 1920x1080 / 1600x1200","1024x768","640x480","+",null,"+","+","+","+","+","-","motion detection;audio detection;tampering detection","+","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellecte необходимо поставить галочку в родном вебе \"enable PTZ\", в режиме View Areas\n \n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии. В этом случае переключатель разрешений в Intellecte будет игнорироваться.\n \n3. Пресет №1 зарезервирован за Home position\n \n4. максимальное разрешение зависит от режима Capture mode, включенного на камере\n \n5. при Capture mode HDTV или 2MP видео в Полном разрешении в Intellecte не отображается. Чтобы видео появилось, необходимо в веб-интерфейсе сменить разрешение на 1920х1080 или 1600х1200 соответсвенно. Разрешения Высокое и Стандартное доступны при любых режимах Capture mode ","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box in View Areas mode. 2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect. 3. Preset 1 is for Home position 4.The highest resolution depends on the Capture mode enabled on the camera. 5. HDTV or 2MP video is not displayed with High resolution in Intellect when Capture mode is enabled. In web interface change the resolution for 1920х1080 or 1600х1200 correspondingly to display video. Full and Standard resolutions are available in any state of Capture mode.","improved"]
["Axis","Axis P1347","Camera ","5.11","1","+",null,"+",null,"+.",null,null,"2560x1920 / 2048x1536 / 1920x1080 / 1600x1200","1024x768","640x480","+",null,"+","+","+","+","+",null,"-","+","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\", в режиме View Areas\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position\n4. максимальное разрешение зависит от режима Capture mode, включенного на камере\n5. при Capture mode HDTV, 2MP или 3MP видео в Полном разрешении в Intellect не отображается. Чтобы видео появилось, необходимо в веб-интерфейсе сменить разрешение на 1920х1080 или 1600х1200 bили 2048х1536 соответсвенно. Разрешения Высокое и Стандартное доступны при любых режимах Capture mode \n","1. This is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box, in View Areas mode\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Preset 1 is reserved for Home Position.\n4. The max. resolution depends on which Capture mode, is on for the camera.\n5. When Capture mode is HDTV, 2MP, or 3MP and with full resolution, Intellect does not show video. To fix this, go to the web interface and change the resolution to 1920x1080 (for HDTV), 1600x1200 (for 2MP), or 2048x1536 (for 3MP). High and Standard resolutions are available in any Capture mode. \n"]
["Axis","Axis P1353/-Е ","Camera ","5.40.19","1","+",null,"+",null,"+",null,null,"800x600","640x480","320x240","+",null,"+","+","+","+","+",null,"motion detection, tampering detection, audio detection","+"]
["Axis","Axis P1354/-E","Camera","5.40.18 ","1","+",4,"+","-","+","-","-","1280x960","1024x768","800x600","+","-","+","+","+","+","-","-","motion detection; audio detection; tampering detection","+","Встроенные детекторы работают только с кодеком MJPEGКамера имеет две степени свободы поворотного крепления. Если открыть кожух, то камеру можно наклонять вверх-вниз, а так же вращать вокруг оси линзы. Для корректной работы настройки \"Поворот видеоизображения\" необходимо в устанавливать поворотное крепление в правильное положение.","On-board detection tools work only with MJPEG codec.  Camera rotary fastening has 2 degrees of freedom. If you open the camera casing, then you can tilt the camera up and down and rotate it around the lens axis. For proper operation of the Video rotation setting, you are to place the rotary fastening into the correct position."]
["Axis","Axis P1355/-E","Camera","5.40.19","1","+",4,"+","-","+","-","-","1920x1080","1024x768","640x480","+","-","-","-","+","-","-","-","motion detection","+","Для того, чтобы на камере заработала цифровая телеметрия, нужно включить соответствующую настройку.Камера имеет две степени свободы поворотного крепления. Если открыть кожух, то камеру можно наклонять вверх-вниз, а так же вращать вокруг оси линзы. Для корректной работы настройки \"Поворот видеоизображения\" необходимо в устанавливать поворотное крепление в правильное положение.","To use digital PTZ, enable the appropriate setting. Camera rotary fastening has 2 degrees of freedom. If you open the camera casing, then you can tilt the camera up and down and rotate it around the lens axis. For proper operation of the Video rotation setting, you are to place the rotary fastening into the correct position."]
["Axis","Axis P1357/-Е","Camera ","5.40.19.1","1","+",null,"+",null,"+",null,null,"2592x1944 / 1920x1080","1024x768","640x480","+",null,"+","+","+","+","+",null,"motion detection, tampering detection, audio detection","+","Максимальное разрешение в Интеллекте зависит от настройки \"Capture mode\" в веб-интерфейсе камеры","Max resolution depends on \"Capture mode\" setting in camera web interface."]
["Axis","Axis P3301/-V","Camera ","5.11","1","+",null,"+",null,"+.",null,null,"640x480","480x360","320x240","+",null,"+","+",null,"+","+",null,"-","+","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n\n","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution).\n\n"]
["Axis","Axis P3304/-V","Camera","5.40.9.2","1","+","4","+",null,"+",null,null,"1280x800","1024x768","640x480","+",null,"+","+","+","+","+","-","audio detection","+","При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.Диапазон значений настроек Максимальное время экспозиции и минимальное время экспозиции зависят от значения настройки режим экспозиции\n\n","In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution). Range of values of the Max.exposure and min.exposure parameters depends on the values of the exposure mode setting.\n","improved"]
["Axis","Axis P3343","Camera ","5.20.1","1","+",null,"+",null,"+.",null,null,"800x600","640x480","320x240","+",null,"+","+","+","+","+",null,"-","+","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\", выставить разрешение не больше чем ограниение на странице телеметрии и сделать увеличение.\n2. помимо \"цифровой\" телеметрии у камеры есть оптические зум и фокус, но они не интегрированы. Настраиваются из родного веба.\n3. пресет №1 = home position\n4. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n5. В настройках микрофона при выборе кодека AAC и частоты дискретизации 8 КГц необходимо выбирать битрейт <= 32 Кбит/с","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box. Then set the resolution to the limit on the telemetry web page, or lower, and zoom in. \n2. Apart from digital telemetry, the camera has optical zoom and focus, but they are not integrated. Must be configured from the device's own web interface. \n3. Preset 1 = home position.\n4. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution).\n5. In the microphone settings, when selecting the AAC codec and the 8 kHz sampling rate, set the bit rate to equal to or less than 32 kbps. "]
["Axis","Axis P3344","Camera ","5.06","1","+",null,"+",null,"+.",null,null,"1280x800","640x480","320x240","+",null,"+","+","+","+","+",null,"-","+","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\", результаты работы телеметрии будут видны при достаточном зумировании картинки.\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. помимо \"цифровой\" телеметрии у камеры есть оптические зум и фокус, но они не интегрированы. Настраиваются из родного веба. \n4. Preset №1 зарезервирован за Home Position\n \n","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box. You will see the result of PTZ after you zoom enough.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Apart from digital telemetry, the camera has optical zoom and focus, but they are not integrated. Must be configured from the device's own web interface. \n4. Preset 1 is reserved for Home Position.\n \n"]
["Axis","Axis P3346/P3346-V/P3346-VE","Camera ","5.40.9.3","1","+",null,"+",null,"+",null,null,"2048x1536","1024x768","640x480","+",null,"+","+","+","+","+",null,"motion detection, tampering detection, audio detection","+","На камере предусмотрены 5 видеопотоков:0. Получение видео H264/MJPEG и применение настроек.1. Соответствует профилю \"Quality\" в веб-интерфейсе камеры. Получение видео без настроек.2. Соответствует профилю \"Balanced\" в веб-интерфейсе камеры. Получение видео без настроек.3. Соответствует профилю \"Bandwith\" в веб-интерфейсе камеры. Получение видео без настроек.4. Соответствует профилю \"Mobile\" в веб-интерфейсе камеры. Получение видео без настроек.При использовании потоков 1-4 после изменения настроек (через веб-интерфейс) необходимо перезапускать поток или объект \"камера\".Встроенная аналитика работает:В 0-м потоке в любом кодеке.В любом другом потоке, но только в H264.В максимальном разрешении при максимальном качестве во время съемки быстро движущихся объектов возможны замедления и искажения видео.","The camera allows 5 video streams: 0. Receiving video in H.264/MJPEG with settings applied. 1. Corresponds to the Quality profile in the camera's web interface. Receiving video without settings applied. 2. Corresponds to the Balanced profile in the camera's web interface. Receiving video without settings applied. 3. Corresponds to the Bandwidth profile in the camera's web interface. Receiving video without settings applied. 4. Corresponds to the Mobile profile in the camera's web interface. Receiving video without settings applied. When you use a stream 1 to 4, you must restart the stream or the Camera object after you change settings in the web interface .The embedded video analytics work in stream 0 with any codec. In any other stream, they work only with H.264. At max. resolution and max. quality, fast-moving objects may cause the video to slow down or become distorted. "]
["Axis","Axis P3353","Camera ","5.40.10.2","1","+",null,"+",null,"+",null,null,"800x600","640x480","320x240","+",{"$nulls":3},"+.",{"$nulls":3},"motion detection","+","1. Для того, чтобы заработала телеметрия, необходимо включить настройку \"Цифровая PTZ телеметрия\". \n2. При включенной опции не работают настройки видеопотока.","1. To enable PTZ, select the Digital PTZ checkbox. \n2. With this option enabled, the video stream settings become unavailable."]
["Axis","Axis P3354","Camera","5.40.17","1","+","4","+","-","+",null,null,"1280x960","1024x768","640x480","+",null,"-","-","+","-","-","-","motion detection; tampering detection","+","Для того чтобы работала телеметрия, необходимо включить соответствующую настройку в свойствах камеры. При включенной опции \"Цифровая PTZ телеметрия\" не работают настройки видеопотока.","To make PTZ works, you need to turn on appropriate setting in device's properties. If you select \"Digital PTZ telemetry\", videostream settings will not be active."]
["Axis","Axis P3363-V/VE","Camera ","5.40.10.2","1","+",null,"+",null,"+",null,null,"800x600","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":4},"+","1. В AxxonNext/Next потоки со 2 по 5 (Авто) отвечают Stream Profiles веб-интерфейса и задаются только от туда\n2. Чтобы заработала телеметрия, нужно включить в веб-интерфейсе Enable View Areas ","1. In AxxonNext/AxxonNext, streams 2 to 5 correspond to the relevant Stream profiles in the camera's web interface and can be configured from there\n2. To enable PTZ, select Enable View Areas in the camera's web interface. "]
["Axis","Axis P3364-V/VE","Camera ","5.40.10.2","1","+",null,"+",null,"+",null,null,"1280x960","1024x768","640x480","+",null,"+","+","+.","+","+",null,"motion detection, tampering detection, audio detection","+","1. На камере предусмотрены 5 видеопотоков:\n0 Получение видео H264/MJPEG и применение настроек\n1-4 Соответствует профилям \"Quality\", \"Balanced\", \"Bandwith\" и \"Mobile\" в веб-интерфейсе камеры. Получение видео без настроек.\n2. При включенной опции \"Цифровая PTZ телеметрия\" не работают настройки видеопотока.","1. The camera allows 5 video streams:\n0 Receiving H264/MJPEG video and applying the settings Corresponds to the Quality, Balanced, Bandwidth and Mobile profiles in the camera's web interface.\n1-4 Corresponds to the Quality, Balanced, Bandwidth and Mobile profiles in the camera's web interface. Receiving video without settings.\n2. With Digital PTZ enabled, the video stream settings become unavailable."]
["Axis","Axis P3367-V/VE","Camera ","5.40.3.2","1","+",null,"+",null,"+",null,null,"2592x1944","1024x768","640x480","+",null,"+","+.","+","+","+",null,"+","+","1. В AxxonNext/Next потоки со 2 по 5 (Авто) отвечают Stream Profiles веб-интерфейса и задаются только от туда\n2. Чтобы заработала телеметрия, нужно включить в веб-интерфейсе Enable View Areas ","1. In AxxonNext flows with 2 on 5 (Auto) respond Stream Profiles of the web interface and are set only from there\n2. That the telemetry earned, it is necessary to include in web interface the Enable View Areas "]
["Axis","Axis P5512","Camera ","5.25","1","+",null,"+",null,"+",null,null,"704x576","704x288","352x288","+",{"$nulls":3},"+",{"$nulls":3},"+.","+","На камере предусмотрены 5 видеопотоков:0. Получение видео H264/MJPEG и применение настроек.1. Соответствует профилю \"Quality\" в веб-интерфейсе камеры. Получение видео без настроек.2. Соответствует профилю \"Balanced\" в веб-интерфейсе камеры. Получение видео без настроек.3. Соответствует профилю \"Bandwith\" в веб-интерфейсе камеры. Получение видео без настроек.4. Соответствует профилю \"Mobile\" в веб-интерфейсе камеры. Получение видео без настроек.При использовании потоков 1-4 после изменения настроек (через веб-интерфейсе) необходимо перезапускать поток или объект \"камера\".Встроенная аналитика работает:В 0-м потоке в любом кодеке.В любом другом потоке, но только в H264.Через Onvif не работают настройки изображения - проблема устройства.Работа камеры проверялась только по протоколу TCP - из-за особенностей удаленного доступа.","The camera allows 5 video streams: 0. Receiving video in H264/MJPEG and applying settings. 1. Corresponds to the Quality profile in the camera's web interface. Receiving video without settings. 2. Corresponds to the Balanced profile in the camera's web interface. Receiving video without settings. 3. Corresponds to the Bandwidth profile in the camera's web interface. Receiving video without settings. 4. Corresponds to the Mobile profile in the camera's web interface. Receiving video without settings. When you use a stream 1 to 4, you must restart the stream or the Camera object after you change settings in the web interface. The embedded video analytics work in stream 0 with any codec; in any other stream, they work only with H264. The image settings do not work via the ONVIF protocol. This is a problem of the device itself. When checking how the camera works, we checked only the TCP protocol; this is a limitation of remote access."]
["Axis","Axis P5522 ","Camera ","5.50.2 ","1","+",null,"+",null,"+",null,null,"720x576","704x576","352x288 ","+",null,"+","+.","+.","+","+",null,"motion detection; audio detection","+","На камере есть 4 программируемых луча/реле, настройка происходит в меню камеры System Options > Port & Devices > Port Status","There's 4 alarm In/Out on camera. To set up it, please use System Options > Port & Devices > Port Status in camera menu."]
["Axis","Axis P5522-E ","Camera ","5.50.2 ","1","+",null,"+",null,"+",null,null,"720x576","704x576","352x288 ","+",{"$nulls":3},"+.",{"$nulls":3},"motion detection","+"]
["Axis","Axis P5532","Camera ","5.41.2 ","1","+",null,"+",null,"+",null,null,"720x576","704x576","352x288","+",{"$nulls":3},"+",{"$nulls":3},"motion detection","+","1. Звук, лучи и реле остались непроверенными по причине отстуствия необходимого оборудования","1. Audio, sensors, and relays were not tested, because we did not have the necessary equipment. "]
["Axis","Axis P5534","Camera ","5.40.9.3","1","+",null,"+",null,"+",null,null,"1280x720","800x450","480x270","+",null,"+","-","+",{"$nulls":3},"motion detection","+","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution)."]
["Axis","Axis P7210 / P7214","Encoder ","5.40.7.1","16 / 4",null,null,"+",null,"+",null,null,"720x576","704x576","352x288","+",null,"+.","+.","+","+","+",null,"motion detection, tampering detection, audio detection","+","P7210 представляет из себя 4 4-х канальных одинаковых модуля в одном корпусе, каждый из которых имеет собственный сетевой интерфейс и интегрирован в ПО ITV как отдельное устройство. Назначение контактов лучей/реле нужно настраивать в веб-интерфейсе устройства, в ПО ITV они будут работать соответственно.\nДля того, чтобы в Интеллекте корректно работала привязка микрофонов к видео-каналам, рекомендуется либо использовать транспортный протокол HTTP (используется по умолчанию), либо осуществлять аналогичную настройку в веб-интерфейсе.","P7210 is 4 of the 4th channel identical the module in one casing, each of which has own network interface and is integrated into ITV software as the separate device. Pin assignment of Alarm I/O needs to be set up in the device web interface, in ITV | AxxonSoft software they will work respectively.\nIn order that in Intellect the binding of microphones to video channels correctly worked, the transport protocol HTTP (it is used by default) is recommended or to use, or to realize similar setup in the web interface."]
["Axis","Axis P8221","I/O Module","5.10","8",{"$nulls":7},"-","-","-",null,null,"+.","+.","-","+","+",null,null,"+","1. Устройство не имеет видео-канала; только лучи, реле, аудио и телеметрию.","1. No video channel on the device. Only sensors, relays, audio channels and PTZ. "]
["Axis","Axis Q1602/-E","Camera","5.40.3.3","1","+",4,"+","-","+","-","-","768x576","640x480","320x240","+","-","+","+","-","+","+","-","+","+","В ASIP потоки со 2 по 5 (Авто) отвечают Stream Profiles веб-интерфейса и задаются только от тудаКамера имеет две степени свободы поворотного крепления. Если открыть кожух, то камеру можно наклонять вверх-вниз, а так же вращать вокруг оси линзы. Для корректной работы настройки \"Поворот видеоизображения\" необходимо в устанавливать поворотное крепление в правильное положение.","In ASIP, streams 2 to 5 (Auto) are configured via web interface in Stream Profiles. Camera rotary fastening has 2 degrees of freedom. If you open the camera casing, then you can tilt the camera up and down and rotate it around the lens axis. For proper operation of the Video rotation setting, you are to place the rotary fastening into the correct position."]
["Axis","Axis Q1604/-E","Camera ","5.40.3.2","1","+",null,"+",null,"+",null,null,"1280x960","1024x768","640x480","+",null,"+","+.",null,"+","+",null,"+","+","В AxxonNext/Next потоки со 2 по 5 (Авто) отвечают Stream Profiles веб-интерфейса и задаются только от туда","In AxxonNext streams from 2 to 5 (Auto) respond Stream Profiles of the web interface and are set only from there"]
["Axis","Axis Q1755/-E","Camera","5.02","1","+","4","+",null,"+",null,null,"1920x1080","1280x720","480x270","+",null,"+","+","+","+","+","-","-","+","1. в режиме Capture mode=1080i при выставленном разрешении 1920х1080 реально видео будет идти в разрешении 1440х1080. Это особенность самой камеры.\n \n2. у камеры 2 порта I\\O, каждый из которых можно настроить и как Луч и как Реле. Если в Intellecte создать и Луч и Реле проассоциированные с одним и тем же портом, то может наблюдаться картина, когда при замыкании Реле автоматически будет срабатывать и Луч. Особенность интеграции.\n 3. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n ","1. When Capture mode=1080i and you select the 1920x1080 resolution, the actual video resolution is only 1440x1080. This is a limitation of the camera itself.\n2. The camera has 2 I/O ports; each port may be configured as a Sensor and as a Relay at the same time. In Intellect, if you associate a Sensor and a Relay with the same port, then sometimes when the Relay is closed, the Sensor goes off as well. This is how integration has been done.\n3. In H.264 mode and with max. settings, the video may shutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution).","improved"]
["Axis","Axis Q1910","Thermal Imaging Camera ","5.08","1","+",null,"+",null,"+",null,null,"720x576","640x480","320x240","+",null,"+","+","-","+.","+",null,"-","+","1. Камера не обычная, а термальная. Воспринимает тепловое излучение и конвертирует его в цветную картинку.\n2. Максимально доступны 8 fps, это ограничение самой камеры.\n3. Сама камера не PTZ, но позволяет подключать сторонее поворотное устроййство и управлять им.","1. This is a thermal camera, not an ordinary one. It \"sees\" thermal radiation and converts it to a color image. \n2. The max. frame rate is 8 fps; this is a limitation of the camera itself.\n3. The camera itself is not a PTZ camera, but you may attach a third-party pan/tilt drive and control it. "]
["Axis","Axis Q1921/-E","Thermal Imaging Camera","5.50.2","1","+",4,"+","-","+","-","-","768x576","480x360","320x240","+","-","+","+","+","+","+","-","motion detection; audio detection; tampering detection","+","\n1. Камера не обычная, а термальная. Воспринимает тепловое излучение и конвертирует его в цветную картинку.\n3. Сама камера не PTZ, но позволяет подключать стороннее поворотное устройство и управлять им.\n","1. This is a thermal imaging camera. It \"sees\" thermal radiation and converts it to a color image. 3. The camera itself is not a PTZ one, but you may attach a third-party pan/tilt drive and control it."]
["Axis","Axis Q6032/Q6032-E","Camera ","5.41.1.2 ","1","+",null,"+",null,"+",null,null,"704x576","704x288","352x288","+",{"$nulls":3},"+",{"$nulls":3},"motion detection","+","При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.Для управление функцией автоматического слежения необходимо:AxxonNext/Next:Создать предустановки с номерами 20 и 21Переход на предустановку #20 включает автоматическое слежениеПереход на предустановку #21 выключает автоматическое слежениеИнтеллект:Переход на предустановку #21 включает автоматическое слежениеПереход на предустановку #22 выключает автоматическое слежение","In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution). To manage the auto-tracking functionality: In AN: Create presets numbered 20 and 21. By switching to preset 20, you switch auto-tracking on. By switching to preset 21, you switch auto-tracking off. In Intellect: By switching to preset 21, you switch auto-tracking on. By switching to preset 22, you switch auto-tracking off."]
["Axis","Axis Q6034","Camera ","5.15","1","+",null,"+",null,"+",null,null,"1280x720","800x450","480x270","+",null,"+",null,"+",{"$nulls":3},"-","+"]
["Axis","Axis Q6034-E","Camera ","5.20.2","1","+",null,"+",null,"+",null,null,"1280x720","800x450","480x270","+",{"$nulls":3},"+",{"$nulls":3},"-","+"]
["Axis","Axis Q6035 / Q6035-E","Camera ","5.25","1","+",null,"+",null,"+",null,null,"1920x1080","1280x720","480x270","+",{"$nulls":3},"+",{"$nulls":3},"+","+"]
["Axis","Axis Q7401 encoder","Encoder ","5.01","1","+",null,"+",null,"+.",null,null,"768x576 / 720x576","768x576 / 704x576","384x288 / 352x288","+",null,"+","+.","+","+","+",null,"-","+","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times, the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution)."]
["Axis","Axis Q7404 encoder","Encoder ","5.02","4","+",null,"+",null,"+.",null,null,"720x576 (PAL) / 720x480 (NTSC) or768x576 (PAL) / 640x480 (NTSC)","704x576 (PAL) / 704x480 (NTSC)","352x288 (PAL) / 352x240 (NTSC)","+",null,"+","+.","+","+.","+",null,"-","+","1. Максимальное разрешение зависит от настройки \"Aspect ratio correction\"\n2. Каждый канал как отдельное устройство, имеет свой веб-интерфейс. Поэтому в нашем ПО надо создавать 4 граббера (и ключ иметь соответствующий)\n3. Звук есть только на первом \"канале\". IP-wizard будет создавать \"Звуковые платы\" на всех 4-х \"каналах\", но работать будет только звук с 1-го \"канала\"\n4. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.","1. The max. resolution depends on how Aspect Ratio Correction is configured. \n2. Each channel is like a separate device and has its own web interface. For this reason, in our software, you must create 4 grabbers\n3. You have audio only on the first channel. The IP Wizard creates an Audio Card for each channel, but only the first channel has audio.\n4. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution)."]
["Axis","Axis Q7406 encoder","Encoder ","5.01","6","+",null,"+",null,"+.",null,null,"720x576 (PAL) / 720x480 (NTSC) or 768x576 (PAL) / 640x480 (NTSC)","704x576 (PAL) / 704x480 (NTSC)","352x288 (PAL) / 352x240 (NTSC)","+",{"$nulls":3},"+","+","+",null,"-","+","аналог Axis 7404\nисполнено в виде платы\nособенности - 6 каналов, каждый из которых имеет свой IP, т.е. в нашем ПО нужно создавать 6 плат видеоввода\n1. Каждый канал как отдельное устройство, имеет свой веб-интерфейс. Поэтому в нашем ПО надо создавать 6 грабберов \n2. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n3. Максимальное разрешение зависит от настройки \"Aspect ratio correction\" ","Very similar to Axis 7404\nCard form factor.\nUnique features: 6 channels and each channel has its own IP address, so in our software you must create 6 grabbers.\n1. Each channel is like a separate device and has its own web interface. For this reason, in our software, you must create 6 grabbers. \n2. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution).\n3. The max. resolution depends on how Aspect Ratio Correction is configured. "]
["Axis","Axis Q7414","Encoder ","5.25.1","4","+",null,"+",null,"+",null,null,"720x576","704x576","352x288","+",{"$nulls":8},"+","Устройство 4-канальное, но каждый канал имеет собственный IP-адрес и интегрирован в ПО ITV/Axxon как отдельное устройство. ","It's 4-channel device, however every channel has its own ip address and integrated in Axxonsoft SW as separate device. "]
["Basler","Basler BIP-1000c/c-dn","Camera ","1.5-0","1",null,null,"+","+","+",null,null,"1024x768","640x480","320x240","+",{"$nulls":4},"+","+",null,"-","+","1. Ограничение по fps:\n-MJPEG:\n1024x768 - 20 fps\n720x576 - 30 fps\n-MPEG-4:\n1024x768 - 12 fps\n720x576 - 30 fps\n-H.264:\n1024x768 - 7 fps\n720x576 - 18 fps\n2. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.","1. Frame rate limits:\n-MJPEG:\n1024x768 – 20 fps\n720x576 – 30 fps\n-MPEG-4:\n1024x768 – 12 fps\n720x576 – 30 fps\n-H.264:\n1024x768 – 7 fps\n720x576 – 18 fps\n2. Intellect supports for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry."]
["Basler","Basler BIP-1300c/c-dn","Camera ","1.6-1","1",null,null,"+","+","+",null,null,"1280x960","1024x768","640x480","+",{"$nulls":4},"+","+",null,"-","+","1. Ограничение fps на самой камере при разрешении 1280х960:\n-MJPEG   11 fps\n-MPEG-4  9 fps\n-H.264     7 fps\n2. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.","1. At 1280x960 resolution, the camera has the following frame rate limits: \n-MJPEG – 11 fps\n-MPEG-4 – 9 fps\n-H.264 – 7 fps\n2. Intellect supports for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry."]
["Basler","Basler BIP-1600c/c-dn","Camera ","1.6-1","1",null,null,"+","+","+",null,null,"1600x1200","1024x768","640x480","+",{"$nulls":4},"+","+",null,"-","+","1. Ограничение fps на самой камере при разрешении 1600х1200:\n-MJPEG   8 fps\n-MPEG-4  5 fps\n-H.264     4 fps\n2. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.","1. At 1600x1200 resolution, the camera has the following frame rate limits:\n-MJPEG – 8 fps\n-MPEG-4 – 5 fps\n-H.264 – 4 fps\n2. Intellect supports for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry."]
["Basler","Basler BIP2-1000c-dn","Camera ","BIP2-3.0.1","1",null,null,"+","+","+",null,null,"1024x768","640x480","320x240","+",{"$nulls":7},"-","+","1. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.\n\n","1. Intellect implements support for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry.\n\n"]
["Basler","Basler BIP2-1300c/с-dn","Camera ","3.5.1","1",null,null,"+","+","+",null,null,"1280x960","1024x768","640x480","+",{"$nulls":4},"+","+",null,"+","+","Разрешения 800х600 и 480х360 недоступны в кодеке H264\nВ Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.Встроенная аналитика будет работать только при активных кодеках MJPEG/H264.","With the H.264 codec, you cannot get the 800x600 and 480x360 resolutions. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 in the Windows Registry. The embedded video analytics woks only when the MJPEG/H264 codecs are active."]
["Basler","Basler BIP2-1600c-dn ","Camera ","BIP2-3.0.1","1",null,null,"+","+","+",null,null,"1600x1200","1024x768","640x480","+",{"$nulls":7},"-","+","1. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.","1. Intellect supports for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry."]
["Basler","Basler BIP2-1600-25c-dn","Camera ","3.11.1","1",null,null,"+","+","+",null,null,"1600x1200","1024x768","640x480","+",null,"-","-","-","-","-",null,"-","+","В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Примечание: fps по каждому стриммингу необходимо настраивать через веб-интерфейс с выбранной галочкой \"Использовать настройки устройства\" в продукте. ","In ITV | AxxonSoft it is supported streaming mode. To turn it need to adjust in configuration 3 Grabbers (available with different codecs) for the same camera. Note: fps on each stream must be configured through web-interface with the selected check \"Use same settings as the device\" in the ITV | AxxonSoft software."]
["Basler","Basler BIP2-1920c-dn","Camera ","3.4.0","1",null,null,"+","+","+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":4},"+","+",null,"-","+","Для поддержки многопоточности в Интеллекте камера интегрирована как двухканальный ip-сервер, где каждому каналу соответствует отдельный поток.Для получения видео с потоков в разных кодеках в Интеллекте нужно создать дополнительную плату видеоввода и переместить на нее одну из камер с соответствующим потоку номером канала. После этого кодек выбирается в свойствах платы видеоввода.В Интеллекте частота кадров и настройки изображения применяются для обоих потоков сразу при изменении их на любом из каналов.Для получения потоков с различной частотой кадров нужно:Создать дополнительную плату видеоввода и переместить на нее одну из камер с соответствующим потоку номером канала.Включить в реестре UseConfigureByWeb = 1.Перезапустить Интеллект и настраивать частоту кадров через веб-интерфейс.","To support multistreaming, Intellect integrates the cameras as a dual-channel IP server, where each channel corresponds to a stream. To receive video from streams with different codecs in Intellect, create an additional grabber and associate it with one of the cameras, so that the channel number corresponds to the required stream. After that, go to the grabber's properties and select a codec. In Intellect, when you change the frame rate and image settings for one of the channels, the changes are applied to both streams. To get streams with different frame rates: Create an additional grabber and associate it with one of the cameras, so that the channel number corresponds to the required stream. Set UseConfigureByWeb = 1 in the Windows Registry. Restart Intellect and set the frame rate in the web interface."]
["Basler","Basler BIP2-2500c-dn ","Camera ","3.11.1","1",null,null,"+",null,"+",null,null,"from WEB","1024x768","640x480","+",null,"-","-","-","-","-","-","-","+","В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 2 Граббера (можно с разными кодеками) на одну и ту же камеру. Примечание: fps по каждому стриммингу необходимо настраивать через веб-интерфейс с выбранной галочкой \"Использовать настройки устройства\" в продукте. ","In ITV | AxxonSoft it is supported streaming mode. To turn it need to adjust in configuration 3 Grabbers (available with different codecs) for the same camera. Note: fps on each stream must be configured through web-interface with the selected check \"Use same settings as the device\" in the ITV | AxxonSoft software."]
["Basler","Basler BIP2-640c-dn ","Camera ","BIP2-3.0.1","1",null,null,"+","+","+",null,null,"640x480","480x360","320x240","+",{"$nulls":7},"-","+","1. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.\n\n","1. Intellect supports for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry.\n\n"]
["Basler","Basler BIP2-D1920c-dn","Camera ","3.4.0 ","1",null,null,"+","+","+",null,null,"1920x1080","1024x768","640x480","+",null,"-","-",null,"+","+",null,"-","+","Для поддержки многопоточности в Интеллекте камера интегрирована как двухканальный ip-сервер, где каждому каналу соответствует отдельный поток.Для получения видео с потоков в разных кодеках в Интеллекте нужно создать дополнительную плату видеоввода и переместить на нее одну из камер с соответствующим потоку номером канала. После этого кодек выбирается в свойствах платы видеоввода.В Интеллекте частота кадров и настройки изображения применяются для обоих потоков сразу при изменении их на любом из каналов.Для получения потоков с различной частотой кадров нужно:Создать дополнительную плату видеоввода и переместить на нее одну из камер с соответствующим потоку номером канала.Включить в реестре UseConfigureByWeb = 1.Перезапустить Интеллект и настраивать частоту кадров через веб-интерфейс.","To support multistreaming, Intellect integrates the cameras as a dual-channel IP server, where each channel corresponds to a stream. To receive video from streams with different codecs in Intellect, create an additional grabber and associate it with one of the cameras, so that the channel number corresponds to the required stream. After that, go to the grabber's properties and select a codec. In Intellect, when you change the frame rate and image settings for one of the channels, the changes are applied to both streams. To get streams with different frame rates: Create an additional grabber and associate it with one of the cameras, so that the channel number corresponds to the required stream. Set UseConfigureByWeb = 1 in the Windows Registry. Restart Intellect and set the frame rate in the web interface."]
["Basler","Basler BIP-640c/c-dn","Camera ","1.6-1","1",null,null,"+","+","+",null,null,"640x480","640x480","320x240","+",{"$nulls":4},"+","+",null,"-","+","1. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.","1. Intellect supports streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry."]
["Basler","Basler BIP-D1300c-dn","Camera ","1.6-1","1",null,null,"+","+","+",null,null,"1280x960","1024x768","640x480","+",{"$nulls":3},"-","+","+",null,"-","+","1. Ограничение fps на самой камере при разрешении 1280х960:\n-MJPEG   11 fps\n-MPEG-4  9 fps\n-H.264     7 fps\n \n2. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.","1. At 1280x960 resolution, the camera has the following frame rate limits:\n-MJPEG: 11 fps\n-MPEG-4: 9 fps\n-H.264: 7 fps\n \n2. Intellect supports for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry."]
["Beward","Beward B-1014","Camera ","2.2.1.5()","4",null,null,"+",null,"+",null,null,"704x576","704x288","352x288","+",null,"+","-","+","-","+",null,"-","-","1. При подключении к камере следует указвать порт 5000 ","1. To connect to the camera, enter port 5000. \n\n "]
["Beward","Beward B-1070","Camera ","2.2.1.5(reove-iris)","1",null,null,"+",null,"+",null,null,"704x576","704x288","352x288","+",null,"+",null,null,"-","+",null,"-","-","1. При подключении к камере следует указвать порт 5000 \n2. лучи не работают даже в веб-интерфейсе камеры","1. To connect to the camera, enter port 5000. \n2. Sensors do not work in the camera's web interface. \n"]
["Beward","Beward B-2.920","Camera ","2.0.2.2(1000103)","1",null,null,"-",null,"+",null,null,"1600x1200","1280x960","1280x960","+",null,"+","-",null,"-","+",null,"-","-","1. Порт по-умолчанию на камере 5000, а в Intellect 80. \n2. Ограничение fps:\n1280x720 - 25 fps при H.264 и 15 fps при MJPEG\n1280x960 - 21 fps при H.264 и 7 fps при MJPEG\n1600х1200 - 15 fps при H.264 и 5 fps при MJPEG\n3. чтобы в Intellect Луч работал правильно, нужно чтобы в вебе в разделе Sensor стояло NO, если будет стоять NC, то луч в Intellece,  будет работать наоборот.\n4. При изменении одновременно нескольких настроек, некоторые настройки могут не применяться. Т.е. при изменении допустим разрешения, сама камера перезагружается и в течении 20-30 секунд она недоступна, если в это время (пока камера недоступна) изменить еще и fps, например, то эта настройка (fps) может не примениться. Особенность самой камеры.\n\n\n\n ","1. The default port is 5000; in Intellect, we have 80 as the default port. \n2. Frame rate limits:\n1280x720: 25 fps with H.264 and 15 fps with MJPEG\n1280x960: 21 fps with H.264 and 7 fps with MJPEG\n1600х1200: 15 fps with H.264 and 5 fps with MJPEG\n3. In Intellect, to make Sensor work correctly, set NO in the Sensor section; if you set NC, Sensor works in the opposite way in Intellect. \n4. If you change multiple settings at the same time, some of the settings may not be applied. For example, after you change the resolution, the camera reboots and remains unavailable for 20–30 seconds; if during that time (when the camera is unavailable) you change the frame rate as well, then the changed frame rate may not be applied. This is a limitation of the camera itself.\n\n\n\n "]
["Beward","Beward B85-5-IP","Camera ","6.0.5.7","1",{"$nulls":4},"+",null,null,"704x576","704x288","352x288","+",null,"+","-","+","+","+",null,"-","-","1. При подключении к камере следует указвать порт 5000 \n2. чтобы в Intellect Луч работал правильно, нужно чтобы в вебе в разделе Sensor стояло NO, если будет стоять NC, то луч в Intellece,  будет работать наоборот \n3. Звук, лучи, реле подключаются внутри ящика к ip-камере без объектива.\n 4. При изменении одновременно нескольких настроек, некоторые настройки могут не применяться. Т.е. при изменении допустим разрешения, сама камера перезагружается и в течении 20-30 секунд она недоступна, если в это время (пока камера недоступна) изменить еще и fps, например, то эта настройка (fps) может не примениться. Особенность самой камеры.","1. To connect to the camera, enter port 5000. \n2. In Intellect, to make Sensor work correctly, set NO in the Sensor section; if you set NC, Sensor works in the opposite way in Intellect. \n3. To connect audio, sensors, or relays to the IP camera, you have to remove its lens and get inside the case. \n4. If you change multiple settings at the same time, some of the settings may not be applied. For example, after you change the resolution, the camera reboots and remains unavailable for 20–30 seconds; if during that time (when the camera is unavailable) you change the frame rate as well, then the changed frame rate may not be applied. This is a limitation of the camera itself."]
["Beward","Beward B-915","Camera ","6.0.5.7","1",{"$nulls":4},"+",null,null,"704x576","704x288","352x288","+",null,"+","-",null,"+","+",null,"-","-","1. При подключении к камере следует указвать порт 5000 \n2. чтобы в Intellect Луч работал правильно, нужно чтобы в вебе в разделе Sensor стояло NO, если будет стоять NC, то луч в Intellece,  будет работать наоборот \n3. При изменении одновременно нескольких настроек, некоторые настройки могут не применяться. Т.е. при изменении допустим разрешения, сама камера перезагружается и в течении 20-30 секунд она недоступна, если в это время (пока камера недоступна) изменить еще и fps, например, то эта настройка (fps) может не примениться. Особенность самой камеры.\n ","1. To connect to the camera, enter port 5000. \n2. In Intellect, to make Sensor work correctly, set NO in the Sensor section; if you set NC, Sensor works in the opposite way in Intellect. \n3. If you change multiple settings at the same time, some of the settings may not be applied. For example, after you change the resolution, the camera reboots and remains unavailable for 20–30 seconds; if during that time (when the camera is unavailable) you change the frame rate as well, then the changed frame rate may not be applied. This is a limitation of the camera itself.\n "]
["Beward","Beward B-920WF","Camera ","2.2.1.5","1",null,null,"+",null,"+",null,null,"1600x1200","1280x960","800x592","+",null,"+","-",null,"-","+",null,"-","-","1. при подключении к камере необходимо указывать порт 5000 (по-умолчанию он стоит 80)\n2. лучи неработоспособны - заявлено производителем ","1. To connect the camera, enter port 5000 (it is 80 by default).\n2. The sensors do not work (as stated by the manufacturer). "]
["Beward","Beward B-970","Camera ","6.0.5.7","1",{"$nulls":4},"+",null,null,"704x576","704x288","352x288","+",null,"+","-",null,"+","+",null,"-","-","1. При подключении к камере следует указвать порт 5000 \n2. Чтобы в Intellect Луч работал правильно, нужно чтобы в вебе в разделе Sensor стояло NO, если будет стоять NC, то луч в Intellece,  будет работать наоборот \n3. При изменении одновременно нескольких настроек, некоторые настройки могут не применяться. Т.е. при изменении допустим разрешения, сама камера перезагружается и в течении 20-30 секунд она недоступна, если в это время (пока камера недоступна) изменить еще и fps, например, то эта настройка (fps) может не примениться. Особенность самой камеры.","1. To connect to the camera, enter port 5000. \n2. In Intellect, to make Sensor work correctly, set NO in the Sensor section; if you set NC, Sensor works in the opposite way in Intellect. \n3. If you change multiple settings at the same time, some of the settings may not be applied. For example, after you change the resolution, the camera reboots and remains unavailable for 20–30 seconds; if during that time (when the camera is unavailable) you change the frame rate as well, then the changed frame rate may not be applied. This is a limitation of the camera itself."]
["Beward","Beward B-975","Camera ","6.0.5.7","1",{"$nulls":4},"+",null,null,"704x576","704x288","352x288","+",null,"+","-",null,"+","+",null,"-","-","1. При подключении к камере следует указвать порт 5000 \n2. чтобы в Intellect Луч работал правильно, нужно чтобы в вебе в разделе Sensor стояло NO, если будет стоять NC, то луч в Intellece,  будет работать наоборот \n3. При изменении одновременно нескольких настроек, некоторые настройки могут не применяться. Т.е. при изменении допустим разрешения, сама камера перезагружается и в течении 20-30 секунд она недоступна, если в это время (пока камера недоступна) изменить еще и fps, например, то эта настройка (fps) может не примениться. Особенность самой камеры.","1. To connect to the camera, enter port 5000. \n2. In Intellect, to make Sensor work correctly, set NO in the Sensor section; if you set NC, Sensor works in the opposite way in Intellect. \n3. If you change multiple settings at the same time, some of the settings may not be applied. For example, after you change the resolution, the camera reboots and remains unavailable for 20–30 seconds; if during that time (when the camera is unavailable) you change the frame rate as well, then the changed frame rate may not be applied. This is a limitation of the camera itself."]
["Beward","Beward N-1000","Camera ","LM.1.6.16.03","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+","-",{"$nulls":4},"-","-","1) звук есть только с видео в формате MPEG-4\n2)ограничения fps:\nMJPEG - 320*240 - 14 fps\nMPEG-4 - 320*240 - 29 fps","1) Audio works only with video in MPEG-4 format.\n2) Frame rate limits: \nMJPEG - 320*240 – 14 fps\nMPEG-4 - 320*240 – 29 fps"]
["Bosch","Bosch NBC-255-P","Camera ","4.53 (09500453)","1","+",null,"+",null,"+",null,null,"640x480","640x480","320x240(H.264) / 640x480(MJPEG)","+",null,"+","+",null,"+","+",null,"+.","-","1. Лучи/Реле работают только если подключаться к камере с логином «service»\n ","1. To use Sensors/Relays, connect to the camera with the user name \"service\" . \n "]
["Bosch","Bosch NBC-455-12P","Camera ","4.53","1","+",null,"+",null,"+",null,null,"704x576","704x576","704x576 (MJPEG) / 352x288 (H264)","+",null,"+","-",null,"+.","+.",null,"+.","-","Разрешение в MJPEG совпадает с выбранным разрешением в H264 и отдельно не настраивается.Поиск в AxxonNext/Next возвращает модель камеры \"NBC-455-P-IVA series\"Перед работой с лучами/реле необходимо настроить их на режим \"N.O.\" в веб-интерфейсеДля работы с лучами/реле к устройству следует подключаться с логином service","The resolution with MPEG is the same as with H.264 (cannot be set separately). In AN, the camera is detected as the NBC-455-P-IVA series. Before using sensors/relays, go to the web interface and switch them to NO mode. To use Sensors/Relays, connect to the camera with the user name \"service\". "]
["Bosch","Bosch NBN-498-12P","Camera ","4.10 (46500410)","1","+",null,"+",null,"+",null,null,"704x576","704x576","352x288(H.264) / 704x576(MJPEG)","+",null,"+",null,"+","-","+",null,"+.","-","1. Телеметрия реализована только в ПО Intellect\n2. Лучи/Реле работают только если подключаться к камере с логином «service»","1. Telemetry is implemented only in Intellect\n2. To use Sensors/Relays, connect to the camera with the user name \"service\"."]
["Bosch","Bosch NBN-733V-IP","Camera ","73500580 ","1","+",null,"+",null,"+",null,null,"from WEB(H.264) / 1280x720(mjpeg)","from WEB(H.264) / 1280x720(mjpeg)","from WEB(H.264) / 512x288(mjpeg)","+",null,"-",{"$nulls":5},"-","-","Разрешение настраивается в веб-интерфейсе камеры. В продукте настройка разрешения доступна только для потока в MJPEG.\nВcтроенный детектор IVA4 (intelligent video analytics).\n","You need to set resolution in web-interface of the camera. Only for MLPEG codec accessible to set resolution via ITV | AxxonSoft products. Analytics on-board: intelligent video analytics."]
["Bosch","Bosch NBN-932V-IP","Camera ","73500580 ","1","+",null,"+",null,"+",null,null,"from WEB(H.264) / 1920x1080(mjpeg)","from WEB(H.264) / 1280x720(mjpeg)","from WEB(H.264) / 512x288(mjpeg)","+",{"$nulls":8},"-","Разрешение настраивается в веб-интерфейсе камеры. В продукте настройка разрешения доступна только для потока в MJPEG.\nВcтроенный детектор IVA4 (intelligent video analytics).\n","You need to set resolution in web-interface of the camera. Only for MLPEG codec accessible to set resolution via ITV | AxxonSoft products. Analytics on-board: intelligent video analytics."]
["Bosch","Bosch NDC-265-P","Camera ","5.51","1","+",null,"+",null,"+",null,null,"1280x720","704x480","352x240","+",null,"+","+",null,"+","+",null,"+","-","1. На устройстве две группы разрешений выставляемые в вебе (\"свойство\") - HD и стандартные. На первом канале работает только HD, второй канал можно дублировать с первого, тогда доступно одно разрешение HD или выставить \"h264 BP+\", тогда можно переключаться между двумя малыми разрешениями. Если выбрать свойство \"h264 BP+ с ограничением скорости\", то из продукта можно регулировать ещё и FPS.","1. In web interface, you can select resolutions from 2 types in Properties - HD and standard. Stream 1 work with HD only, stream 2 can be set up to inherit settings from stream 1 and work with HD only or, if you select h264 BP+, then you can switch between two resolutions. If you select \"h264 BP+ with max.fps limit\", then you can also adjust fps on the device.\n"]
["Bosch","Bosch NDC-274-PT (ONVIF)","Camera ","5.80.0032","1",null,null,"+",null,"+",null,null,"1920x1080 ","1280x720","H.264: 1280x720; MJPEG: 768x432","+",{"$nulls":6},"+",null,"-"]
["Bosch","Bosch NDC-455V09-12PS","Camera ","5.51","1","+",null,"+",null,"+",null,null,"704x576","704x576","352x288","+",null,"+","+",null,"+","+",null,"+.","-","1. На устройстве две группы разрешений выставляемые в вебе (\"свойство\") - HD и стандартные. На первом канале работает только HD, второй канал можно дублировать с первого, тогда доступно одно разрешение HD или выставить \"h264 BP+\", тогда можно переключаться между двумя разрешениями. если выбрать свойство \"h264 BP+ с ограничением скорости\", то из продукта можно регулировать ещё и FPS.","1. In web interface, you can select resolutions from 2 types in Properties - HD and standard. Stream 1 work with HD only, stream 2 can be set up to inherit settings from stream 1 and work with HD only or, if you select h264 BP+, then you can switch between two resolutions. If you select \"h264 BP+ with max.fps limit\", then you can also adjust fps on the device.\n"]
["Bosch","Bosch NDN-832V03-P","Camera ","5.01","1","+",null,"+",null,"+",null,null,"H.264: 1280x720; MJPEG: 704x480","704x480","H.264: 352x240; MJPEG: 704x480","+",{"$nulls":7},"+.","-"]
["Bosch","Bosch NIN-832-V03P","Camera","5.85 build 16","1","+","3","+","-","-",null,null,"1920x1080","768x432","512x288","+",null,"-","-","-","-","-","-","-","-","Разрешение настраивается в веб-интерфейсе камеры. В продукте настройка разрешения доступна только для потока в MJPEGВcтроенный детектор IVA4 (intelligent video analytics).","You need to adjust resolution in web-interface. In AxxonSoft products resolution is setting available only for MJPEG stream IVA4 (intelligent video analytics)."]
["Bosch","Bosch NWC-0455-10P","Camera ","4.10","1","+",null,"-","+.",{"$nulls":3},"look at notes","look at notes","look at notes","-",{"$nulls":4},"+","+",null,"other detectors; inbuilt tracker","-","1. SDK производителя не позволяет провести полноценную интеграцию камеры.  Все настройки (разрешение, битрейт и проч.) необходимо выставлять в веб-интерфейсе камеры, и в Intellect видео будет менятся.\n2. Лучи/Реле работают только если подключаться к камере с логином «service»\n3. Камера поддерживает встроенную аналитику IVA.","1. The vendor's SDK does not allow us to fully integrate the camera.   In Intellect, you cannot change any setting (resolution, bit rate, color, etc.). To make the video change in Intellect, you must go to the camera's web interface and configure all the settings there. \n2. To use Sensors/Relays, connect to the camera with the user name \"service\" .\n3. Onboard analytics IVA"]
["Bosch","Bosch NWC-0495-10P","Camera ","4.10(19500410)","1","+",null,"-","+.",{"$nulls":3},"from WEB","from WEB","from WEB","-",{"$nulls":4},"+.","+",null,"other detectors; inbuilt tracker","-","1. SDK производителя не позволяет провести полноценную интеграцию камеры.  Все настройки (разрешение, битрейт и проч.) необходимо выставлять в вебе, и в Intellect видео будет менятся.\n2. Лучи/Реле работают только если подключаться к камере с логином «service».3. Камера поддерживает встроенную аналитику IVA.","1. The vendor's SDK does not allow us to fully integrate the camera.  You cannot change any settings in Intellect (resolution, bit rate, color, etc.). To make the video change in Intellect, you must go to the camera's web interface and configure all the settings there.\n2. To use Sensors/Relays, connect to the camera with the user name \"service\".\n3. Onboard analytics IVA"]
["Bosch","Bosch NWD-495V03-10P","Camera ","4.00","1","+",null,"-","+.",{"$nulls":3},"704x576","704x576","704x576","-",{"$nulls":7},"-","-","1. SDK производителя не позволяет провести полноценную интеграцию камеры.  Все настройки (разрешение, битрейт, цветность и проч.) необходимо делать в веб-интерфейсе камеры, и в Intellect видео будет менятся.\n2. Камера работает через ONVIF, но только в режиме совместимости","1. The vendor's SDK does not allow us to fully integrate the camera.  To make the video change in Intellect, you must go to the camera's web interface and set all the settings (resolution, bit rate, color, etc.) there.\n2. The camera works via the ONVIF protocol, but only in compatibility mode."]
["Bosch","Bosch VG4-3xx series","Camera","Hardware version F0000E41 / Firmware version 01500415 / Major version number 4.15 / Build number 01","1","+","3","+","+","-",null,null,"look at notes","look at notes","look at notes","-",null,"-","-","+","+.","+.","-","other detectors; inbuilt tracker","-","SDK производителя не позволяет провести полноценную интеграцию камеры.  Все настройки (разрешение, битрейт и проч.) необходимо выставлять в вебе, и в Intellect видео будет изменяться.Для полноценной работы телеметрии в ПО ITV рекомендуется  выбирать \"протокол\" телеметрии \"Bosch-Autodome\". Назначение пресетов осуществляется с подтверждением (нажатие кнопки \"Фокус +\" на панели телеметрии).Прошивка 30500410: для того, чтобы получить в ПО ITV видео в формате h263, в веб-интерфейсе устройства необходимо выбрать кодек mpeg4 HS++. Камера поддерживает встроенную аналитику IVA.","Manufacture's SDK doesn't allow to do full integration. You need to adjust all device settings (resolution, bitrate, ect.) in web-interface, then settings will be shanged in Axxon Intellect. In AxxonSoft products for complete works of PTZ is recommended to select Bosch-Autodome PTZ-protocol. To adjust presets you need to approve it by pressure \"Focus +\" in telemetry panel. Firmware 30500410: to get video in h263 codec in AxxonSoft products you need to select MPEG4 HS++ codec in web-interface. Camera supports inbuilt analitics IVA."]
["Bosch","Bosch VG5 AutoDome 700 Series","Camera ","5.52","1","+",null,"+",null,"+",null,null,"704x576","704x576","352x288","+",{"$nulls":3},"+",{"$nulls":3},"+","-","1. Перечень встроенных детекторов: \nIVA 5.5 \nОбъект в поле\nПересечение линии\nПраздношатание\nИзменение условий\nСледование по маршруту\nНесанкционированный доступ\nУдаленный объект\nБездействующий объект\nВход в поле\nВыход из поля\nПоиск сходства\nСчетчик\nСчетчик BEVIVA 5.5 Flow\nНесанкционированный доступ\nОбнаружение скоплений\nПоток в поле\nПротивопоток в поле\n2. Для корректного отображения и записи видео в формате H264 для настройки частоты опорных кадров не следует выбирать значение 0.\n3. Для работы функций Zoom и Focus в ПО Интеллект нужно в реестре Wondows в папке HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\TELEMETRY\\ создать строковый параметр UseBoschOSRD40 со значением 1.","1. Embedded IVA 5.5 detection allows you to: \nDetect objects entering, leaving, or just being within an area (detection field)Detect multiple line crossing from single line up to three lines combined in a logical row Detect loitering in an area related to radius and time Detect condition change properties such as size, speed, direction, and aspect ratio change within a specified time span (for example something falling down)Detect trajectories/routes of objects, passing in the scene, displayed with tracking lines Detect Camera Tampering (alarms on camera hooding/masking, blinding, defocusing, and repositioning).Detect removed objects within a configurable time span Detect idle objects within a configurable time span Count objects crossing a virtual line or entering a certain area (Counter)Detect a certain crowd level in a predefined field Detect flow of constantly moving objects Detect object that moves against a flow of objects\n2. H264 video is displayed correctly only if you set the key frame frequency value other than 0.\n3. In Intellect, to enable Zoom and Focus, you should create a string parameter UseBoschOSRD40 in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\TELEMETRY\\ folder and assign it the value of 1."]
["Bosch","Bosch VG5 AutoDome 800 Series  ","Camera","5.52","1","+","3","+",null,"+",null,null,"H.264: 1920x1084; MJPEG: 1920x1072","H.264: 704x480; MJPEG: 768x432","352x240","-",null,"-","-","+","-","-","-","-","-","Что бы настройки изменялись на втором потоке нужно выставить определенные настройки в веб-интерфейсе:Max. frame rate - \"25/30 ips (up to 1920x1080)\"Property на Stream 1 - \"H.264 MP 7200p25/30 fixed\"Property на Stream 2 - \"H.264 BP+bit-rate-limited\" или \"H.264 MP SD\" В ПО Интеллект версии 4.8 и ниже для работы функций Zoom и Focus в ПО Интеллект нужно в реестре Wondows в папке HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\TELEMETRY\\ создать строковый параметр UseBoschOSRD40 со значением 1","To change the settings of the second stream, the settings in the web interface are to be: Max. frame rate - \"25/30 fps (up to 1920x1080)\"Property for Stream 1 - \"H.264 MP 7200p25/30 fixed\"Property for Stream 2 - \"H.264 BP+bit-rate-limited\" or \"H.264 MP SD\". In Intellect software (version 4.8 or older) to enable Zoom and Focus features, create 'UseBoschOSRD40' string parameter with '1' value in HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\TELEMETRY\\ folder of Windows registry.","improved"]
["Bosch","Bosch VIP X1 encoder","Encoder ","2.53(05500253)","1","+",null,"-","+.",{"$nulls":3},"from WEB","from WEB","from WEB",{"$nulls":4},"+","+","+",null,"other detectors; inbuilt tracker","-","1. SDK производителя не позволяет провести полноценную интеграцию камеры.  Все настройки (разрешение, битрейт и проч.) необходимо выставлять в вебе, и в Intellect видео будет изменяться.\n2. Лучи/Реле работают только если подключаться к камере с логином «service»\n3. Телеметрия работает только в ПО Intellect и только через \"явный\" протокол (напр. Pelco-D)\n4. Камера поддерживает встроенную аналитику IVA.","1. The vendor's SDK does not allow us to fully integrate the camera.  You cannot change any settings in Intellect (resolution, bit rate, color, etc.). To make the video change in Intellect, you must go to the camera's web interface and configure all the settings there.\n2. To use Sensors/Relays, connect to the camera with the user name \"service\". \n3. Telemetry works only in Intellect and only via an \"explicit\" protocol (for example, Pelco-D). .\n4. Onboard analytics IVA"]
["Bosch","Bosch VIP X1 XF encoder","Encoder ","4.53 (09500453)","1","+",null,"+",null,"+.",null,null,"704x576","704x576","704x576 (MJPEG) / 352x288 (H264)","+",null,"+","+","+","+","+",null,"+.","-","1. Телеметрия реализована только в ПО Intellect\n2. Лучи/Реле работают только если подключаться к камере с логином «service»\n","1. Telemetry is implemented only in Intellect.\n2. To use Sensors/Relays, connect to the camera with the user name \"service\" .\n"]
["Bosch","Bosch VIP X16 XF E","Encoder","28500570","16","+","3","+",null,"+",null,null,"704x576","704x576","704x576","+",null,"+","-","+","+","+","-","motion detection","-","Настройки контроллера телеметрии в Интеллекте должны совпадать с настройками на вкладке COM1 в веб-интерфейсе камеры.","In Intellect setting of PTZ controller are to be the same as the setting in COM1 tab in the camera web interface.","new"]
["Bosch","Bosch VIP X1600 encoder","Encoder ","3.53","16","+",null,"-","+.",{"$nulls":3},"704x576 (from web)","704x288 (выставляется в вебе)","352x288 (выставляется в вебе)","-",{"$nulls":3},"-","+","+",null,"-","-","1. Интеграция выполнена через SDK, поэтому не важно какой порт, логин и пароль указывать при подключении.\n2. Сам сервер – это 4 отдельных сетевых устройства (модуля)  в одном корпусе. Каждый модуль настраивается в Intellect как отдельный 4-х канальный граббер. На это нужно обратить внимание при покупке/создании ключа для ПО\n3. MJPEG видео - вспомогательный видеопоток. В Intellect его не интегрируем.\n4. Все настройки (разрешение/цветность/яркость и проч.) через Intellect менять нельзя, необходимо настраивать через веб-интерфейс камеры, а в Intellect настройки будут применяться и видео изменяться.","1. The camera is integrated using the SDK; therefore, it does not matter which port, user name, or password is used to connect. \n2. The encoder itself consists of 4 separate network devices (units) in the same case. In Intellect, configure each unit as a separate 4-channel grabber. Have this in mind when buying/creating a key for the software.\n3. MJPEG is an auxiliary video stream. We cannot integrate it with Intellect. \n4. You cannot change any settings in Intellect (resolution, bit rate, color, etc.). To make the video change in Intellect, you must go to the camera's web interface and configure all the settings there."]
["Bosch","Bosch VIP X1600 M4SA","Encoder ","4.10","4","+",null,"+","+",{"$nulls":3},"from WEB","from WEB","from WEB","-",null,"+",null,"+","+","+.",null,"+.","-","Сам сервер – это 4 отдельных сетевых устройства (модуля) в одном корпусе. Каждый модуль настраивается в Intellect как отдельный 4-х канальный граббер. На это нужно обратить внимание при покупке\\создании ключа для ПО","The server consists of 4 separate network devices (units) in the same case. In Intellect, configure each unit as a separate 4-channel grabber. Have this in mind when buying/creating a license key for the software."]
["Bosch","Bosch VIP-X1600 XFM4","Encoder ","4.21","4","+",null,"+",null,"+",null,null,"480x576","352x576","352x288","-",null,"+","+","+","+","+",null,"+.","-","Сам сервер – это 4 отдельных сетевых устройства (модуля) в одном корпусе. Каждый модуль настраивается в Intellect как отдельный 4-х канальный граббер. На это нужно обратить внимание при покупке\\создании ключа для ПО","The server consists of 4 separate network devices (units) in the same case. In Intellect, configure each unit as a separate 4-channel grabber. Have this in mind when buying/creating a license key for the software."]
["Bosch","Bosch VJR-F801-IxxV","Camera ","4.53","1","+",null,"+",null,"+",null,null,"1280x720","H.264: 704x480; MJPEG: 1280x720","H.264: 352x240; MJPEG: 1280x720","+",{"$nulls":3},"-",{"$nulls":4},"-","В драйвере прописан только один набор для значений Частоты кадров для 50Hz. Если активирован режим 60 Гц, то устройство само ставит ближайшее подходящее значение","Only one set of values of fps for 50Hz is registered in the driver. If the mode of 60 Hz is activated, the device itself puts the next suitable value."]
["Bosch","Bosch VOT-320V060L","Thermal Imaging Camera ","4.51(05500451)","1","+",null,"+",null,"+",null,null,"320x240","320x240","320x240","+",{"$nulls":3},"+","+","+",null,"+.","-","1. Камера не обычная, а термальная. Воспринимает тепловое излучение и конвертирует его в цветную картинку.\n2. Cамо устройство выдает только 8 fps максимум\n3. Cамо устройство выдает видео в разрешении 320х240 максимум \n4. Управление телеметрией возможно реализовать только в ПО Intellect\n5. Само устройство с прошивкой 4.51 при подключении по ONVIF не может выдавать MJPEG-видео, только H.264","1. This is a thermal camera, not an ordinary one. It \"sees\" thermal radiation and converts it to a color image.\n2. Frame rate: the device itself allows max. 8 fps.\n3. Resolution: the device itself allows max. 320x240. \n4. Telemetry is implemented only in Intellect.\n5. With the 4.51 firmware and when you connect via the ONVIF protocol, the device itself allows only H.264 video; no MJPEG support. "]
["Brickcom","Brickcom (W)CB-100Ae-08","Camera ","3.0.6.12","1","+.",null,"+.","+",{"$nulls":3},"1280x800","640x400","640x400","+",null,"+",{"$nulls":5},"-","+","1. В ПО ITV/Axxon камеры определяются как CB-100Ae и WCB-100Ae. 2. С прошивкой 3.0.6.12 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу не будет. \n3. AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","1. In ITV/Axxon software cameras are identified as CB-100Ae and WCB-100Ae. 2. With the 3.0.6.12 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. \n3. ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W)CB-100Ae-08(VGA)","Camera ","v3.0.6.12","1","+.",null,"+","+","+",null,null,"640x480","640x480","320x240","+",null,"+",{"$nulls":5},"-","+","В ПО ITV/Axxon камеры определяются как CB-100Ae-VGA и WCB-100Ae-VGA. Прошивка v3.0.6.12: камера обнаруживается поиском как Onvif, но работать по этому протоколу не будет.AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество","In ITV/Axxon software cameras are identified as CB-100Ae-VGA and WCB-100Ae-VGA. 3.0.6.12 firmware: Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W)CB-100Ap","Camera ","3.0.6.12","1","+.",null,"+","+","+",null,null,"1280x800","1280x800","640х400","+",null,"+","+",{"$nulls":4},"-","+","С прошивкой 3.0.6.12 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет.В кодеке MPEG4 в сочетании с максимальным разрешением 1280x800 видео поступает с максимальной частотой кадров, равной 15 fps. (Ограничение самого устройства)AxxonNext/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the 3.0.6.12 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. With the MPEG4 codec and the max. frame rate (1280x800), video comes at 15 fps max (this is a limitation of the device itself). AN: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W)CB-100Ap-0c ","Camera ","3.0.6.12","1",null,null,"+","+","+",null,null,"1280x800","1280x800","640x400","+",null,"+","+",{"$nulls":4},"-","+","С прошивкой 3.0.6.12 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет.В кодеке MPEG4 в сочетании с максимальным разрешением 1280x800 видео поступает с максимальной частотой кадров, равной 15 fps. (Ограничение самого устройства)AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the 3.0.6.12 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. With the MPEG4 codec and the max. frame rate (1280x800), video comes at 15 fps max (this is a limitation of the device itself). ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W)FB-100Ap-31","Camera ","3.0.6.12","1","+.",null,"+","+","+",null,null,"1280x800","1280x800","640x400","+",null,"+","+",null,"+","+",null,"-","+","С прошивкой 3.0.6.12 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет.В кодеке MPEG4 в сочетании с максимальным разрешением 1280x800 видео поступает с максимальной частотой кадров, равной 15 fps. (Ограничение самого устройства)AxxonNext/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the 3.0.6.12 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. With the MPEG4 codec and the max. frame rate (1280x800), video comes at 15 fps max (this is a limitation of the device itself). AN: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W)FB-130Np","Camera ","3.0.6.25 ","1","+.",null,"+","+","+",null,null,"1280x1024(PAL) / 640x480(NTSC)","640x512 (PAL) / 640x480(NTSC)","320x256(PAL) / 320x240(NTSC)","+",null,"+","+",null,"+","+",null,"-","+","1. Под ТВ-стандартами PAL / NTSC в ПО Intellect подразумеваются форматы отображения 4:3 и 16:9 соответственно\n\n","1. In Intellect, TV standard means aspect ratio (PAL for 4:3 and NTSC for 16:9). \n\n"]
["Brickcom","Brickcom (W)OB-100Ae","Camera ","3.1.0.6C15","1","+.",null,"+","+","+",null,null,"1280x800","1280x800","640x400","+",null,"+","+",null,"+","+",null,"+","+","Максимальный FPS для H264 составляет 15 кадров в секунду.Аудио на камере не работает, если выбран кодек MJPEG.Детектор движения не работает, если выбран кодек MJPEG.","With H.264, the max. frame rate is 15 fps. If you select the MJPEG codec, audio does not work on the camera and the motion detection tool does not work."]
["Brickcom","Brickcom (W)OB-100Ap-73","Camera ","3.0.6.27","1",null,null,"+","+","+",null,null,"1280x800","640x400","640x400","+",null,"+","+","-","+","+",null,"-","+","В кодеке MPEG4 при максимальном разрешении 1280x800 есть ограничение на максимальную частоту кадров - 15 fpsВ кодеке MJPEG при увеличении качества падает частота кадров.Прошивка 3.0.6.27: Камера обнаруживается поиском как устройство, поддерживающее Onvif, но не работает.Прошивка 3.0.6.27: Управление фокусом не всегда работает. Такое же поведение и в веб-интерфейсе - проблема самой камеры.AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the MPEG4 codec and the max. frame rate (1280x800), the max. frame rate is 15 fps. With the MJPEG codec, the frame rate drops when you increase the quality. 3.0.6.27 firmware: Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol.3.0.6.27 firmware: Sometimes focus control does not work. The same is true in the web interface; this is a problem of the device itself. Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W)VS-01Ap","Camera ","3.1.0.3","1","+.",null,"+","+","+",null,null,"720x576","720x576","352x288","+",null,"+","+","+","+","+",null,"-","+","1. С прошивкой 3.0.6.18 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет. \n2. AxxonNext/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","1. With the 3.0.6.18 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. \n2. AN: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality. "]
["Brickcom","Brickcom (W/G)OB/FD/VD-300Np ","Camera ","3.2.1.3","1","+.",null,"+","+","+",null,null,"2032x1536","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":3},"motion detection;","+","Чтобы было видео на 2-ом потоке, нужно чтобы TV-out был выключен и разрешение на 1-ом потоке было ниже, чем 2032х1536.","To receive video with stream 2, you should make sure that TV-out is disabled and the resolution for stream 1 is lower than 2032х1536."]
["Brickcom","Brickcom (W/G)OB/FD/VD-302Np / FB-300Np","Camera ","3.2.1.3","1","+.",null,"+","+","+",null,null,"2032x1536","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":4},"+"]
["Brickcom","Brickcom (W/G)OB-100Ap-73","Camera ","3.0.6.14","1","+.",null,"+","+","+",null,null,"1280x800","1280x800","640х400","+",null,"+","+","-","+","+",null,"-","+","В ПО ITV/Axxon камеры определяются как OB-100Ap, GOB-100Ap и WOB-100Ap. В кодеке MPEG4 при максимальном разрешении 1280x800 есть ограничение на максимальную частоту кадров - 15 fpsВ кодеке MJPEG при увеличении качества падает частота кадров.Прошивка 3.0.6.14: Через Onvif работает только получение видео (без настроек) и поискПрошивка 3.0.6.14: Управление фокусом не всегда работает. Такое же поведение и в веб-интерфейсе - проблема самой камеры.AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","In ITV/Axxon software cameras are identified as OB-100Ap, GOB-100Ap and WOB-100Ap. With the MPEG4 codec and the max. frame rate (1280x800), the max. frame rate is 15 fps. With the MJPEG codec, the frame rate drops when you increase the quality. 3.0.6.14 firmware: Via the ONVIF protocol, you can only search and receive video (the settings do not work). 3.0.6.14 firmware: Sometimes focus control does not work. The same is true in the web interface; this is a problem of the device itself. ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W/G)OB-130Np / (F/V)D-130Np ","Camera ","3.1.0.9","1","+.",null,"+","+","+",null,null,"1280x1024 (PAL) / 640x480 (NTSC)","640x512 (PAL) / 640x480 (NTSC)","320x256 (PAL) / 320x240 (NTSC)","+",{"$nulls":3},"+",{"$nulls":3},"-","+","Камера не поворотная, но имеет встроенный трансфокатор.Максимальная частота кадров в кодеке mjpeg в максимальном разрешении - 15 fps.Переключение соотношения сторон реализовано через параметр \"ТВ-стандарт\" по следующей схеме: PAL = 5:4, NTSC = 4:3, 16:9 = 16:9. Данный параметр меняется для обоих потоках сразу.","This is not a PTZ camera, but it has a built-in zoom lens. With the MJPEG codec, the maximum frame rate is 15 fps. The aspect ratio is changed by changing the value of the TV standard parameter: PAL = 5:4, NTSC = 4:3, 16:9 = 16:9. A change to this parameter applies to both streams at the same time. "]
["Brickcom","Brickcom CB-100Ae-08","Camera ","2.3.7.8","1",null,null,"+","+","-",null,null,"1280x800","640x400","640x400","+",null,"+",{"$nulls":5},"-","+","Пока не интегрированы h.264 и аналитикаПрошивка 2.3.7.8: при поиске устройство возвращает неверную прошивку \"100\" - проблема самой камеры.AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","H.264 and the embedded video analytics are not yet integrated. 2.3.7.8 firmware: the search returns the wrong firmware, 100, for the device; this is the problem of the device itself. ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom CB-100Ae-08(VGA)","Camera ","v3.0.4.0","1",null,null,"+","+","+",null,null,"640x480","640x480","320x240","+",null,"+",{"$nulls":5},"-","+","AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество","ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality. "]
["Brickcom","Brickcom FB-100Ae-21","Camera ","2.3.7.8","1","+.",null,"+","+",{"$nulls":3},"1280x800","1280x800","640x400","+",null,"+.","+",null,"+","+",null,"-","+","1. С прошивкой 2.3.7.8 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет. \n2. AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","1. With the 2.3.7.8 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. \n2. ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom FB-100Ap","Camera ","v3.0.6.12","1","+.",null,"+","+","+",null,null,"1280x800","640x400","640x400","+",null,"+.","+",null,"+","+",null,"-","+","В кодеке MPEG4 при максимальном разрешении 1280x800 есть ограничение на максимальную частоту кадров - 15 fpsВ кодеке MJPEG при увеличении качества падает частота кадров. При максимальном качестве видео может не поступать вообще - особенность камеры.Прошивка 3.0.6.12: Камера обнаруживается поиском как устройство, поддерживающее ONVIF, но через ONVIF не работает.AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the MPEG4 codec and the max. frame rate (1280x800), the max. frame rate is 15 fps. With the MJPEG codec, when you increase the quality, the frame rate drops. At max. quality, video does not come from the camera at all. This is a problem of the camera. The 3.0.6.12 firmware: Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom FB-200Np","Camera","3.2.2.7.1","1","+","3","+","+","+",null,null,"1920x1080","1024x768","640x480","+",null,"-","-",null,"-","-","-","-","+",null,null,"new"]
["Brickcom","Brickcom FD-100Ae-73","Camera ","2.3.7.8","1","+.",null,"+","+",{"$nulls":3},"1280x800","1280x800","640x400","+",null,"+","+",null,"+","+",null,"-","+","Прошивка 2.3.7.8: при поиске устройство возвращает неверную прошивку \"100\" - проблема самой камеры.Прошивка 2.3.7.8: Реле камеры по умолчанию находится в состоянии замкнуто (хотя в настройках камеры стоит \"нормально разомкнуто\"). Следует сделать пробное замыкание-размыкание его через ПО Axxon/ITV, тогда дальнейшая работа с реле проходит корректно.Прошивка 2.3.7.8: Возможно, что при первичном подключении камера не заработает. Нужно перезапустить камеру.В кодеке MPEG4 видео поступает с максимальной частотой кадров, равной 15 fps. (Ограничение самого устройства)AxxonNext/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","2.3.7.8 firmware: Search returns the wrong firmware, 100, for the device; this is a problem of the device itself. 2.3.7.8 firmware: By default, the camera's relay is closed (though the camera's settings are set to \"normally open\"). To make the relay work correctly, test it: open/close the relay in the AxxonSoft software. 2.3.7.8 firmware: Sometimes, the camera does not work at the first connection. Restart the camera. With the MPEG4 codec, video comes at 15 fps max (this is a limitation of the device itself). AN: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom FD-100Ap-73","Camera ","3.0.6.13","1","+.",null,"+","+","+",null,null,"1280x800","640x400","640x400","+",null,"+.","+",null,"+","+",null,"-","+","1. Камера определяется поиском как onvif, но с данной прошивкой 3.0.6.13 через ONVIF не работает. \n2. AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"\n","1. With the 3.0.6.13 firmware, Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. \n2. ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality.\n"]
["Brickcom","Brickcom FD-130Ap-73","Camera ","3.0.6.13","1","+.",null,"+","+","+",null,null,"1280x1024","640x512","320x256","+",null,"+","+",null,"+","+",null,"-","+","С прошивкой 3.0.6.13 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет.AxxonNext/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the 3.0.6.13 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. AN: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom FD-300Ap","Camera ","3.1.0.8","1","+.",null,"+","+","+",null,null,"2032x1536","1024x768","640x480","+",null,"+","+",null,"+","+",null,"+","+"," 1. Для мегапиксельных разрешений максимальный FPS = 8.\n 2. Разрешение на втором потоке всегда такое же, как на первом. ","1. With megapixel resolution, max. FPS is 8. \n2. Resolution for the 2nd video stream is the same as for the 1st video stream."]
["Brickcom","Brickcom MB-130Ap / WMB-130Ap","Camera","v3.2.2.8","1","+",3,"+","+","+","-","-","1280x1024","1024x768","640x480","+","-","-","-","-","-","-","-","-","+"]
["Brickcom","Brickcom MB-300A_series","Camera ","v3.2.1.3","1","+.",null,"+","+","+",null,null,"H.264/MPEG4: 2032x1536; MJPEG: 2048x1536","1024x768","640x480","+",{"$nulls":8},"+"]
["Brickcom","Brickcom MD-100Ae","Camera ","3.0.6.12","1","+.",null,"+","+",{"$nulls":3},"1280x800","640x400","320x192","+",{"$nulls":7},"-","+","1. С прошивкой 3.0.6.12 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет. \n2. AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","1. With the 3.0.6.12 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. \n2. ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom MD-100Ap","Camera ","v3.1.0.8","1","+.",null,"+","+","+",null,null,"PAL: 640x480; NTSC: 1280x720","PAL: 640x480; NTSC: 1280x720","PAL: 320x240; NTSC: 640x352","+",{"$nulls":8},"+"]
["Brickcom","BrickCom MD-130Ap","Camera","v3.2.2.8","1","+",3,"+","+","+","-","-","1280x1024","1024x768","640x480","+","-","-","-","-","-","-","-","-","+"]
["Brickcom","Brickcom MD-300Ap-360 / MD-300Np-360 / VD-300Af-360 ","Fisheye Camera","3.2.2.6","1","+.",null,"+","+","+",null,null,"2032x1536","1024x768","640x480","+",{"$nulls":8},"+"]
["Brickcom","Brickcom MD-300Np","Camera ","3.2.1.3","1","+.",null,"+","+","+",null,null,"2032x1536","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":3},"motion detection;","+","1. Чтобы было видео на 2-ом потоке, нужно чтобы TV-out был выключен и разрешение на 1-ом потоке было ниже, чем 2032х1536.","1. To receive video with stream 2, you should make sure that TV-out is disabled and the resolution for stream 1 is lower than 2032х1536."]
["Brickcom","Brickcom MD-300Np-360P","Fisheye Camera","v3.2.2.8","1","+.",null,"+","+","+",null,null,"2032x1536(H264) / 2048x1536","1024x768","640x480","+",null,"-","-","-","-","-","-","-","+"]
["Brickcom","Brickcom MD-500Ap-360","Fisheye Camera","v3.2.2.7","1","+.",null,"+","+","+",null,null,"2032x1936(H264/MPEG4) / 2592x1944(MJPEG)","1024x768","640x480","+",null,"-","-","-","-","-","-","-","+"]
["Brickcom","Brickcom OSD-040-D/-E","Camera","v3.1.1.3","1","+.",null,"+","+","+",null,null,"720x480","720x480","352x240","+",null,"-","-","+","-","-","-","motion detection","+"]
["Brickcom","Brickcom OSD-200A","Camera","gk20121228NSA","1",null,null,"+","-","+",null,null,"1920x1080","1024x768","640x480","-",null,"-","-","+","-","-","-","-","+"]
["Brickcom","Brickcom OB-100Ap-73","Camera ","v3.0.6.27","1",null,null,"+","+","+",null,null,"1280x800","640x400","640x400","+",null,"+","+","-","+","+",null,"-","+","В кодеке MPEG4 при максимальном разрешении 1280x800 есть ограничение на максимальную частоту кадров - 15 fpsВ кодеке MJPEG при увеличении качества падает частота кадров.Прошивка 3.0.6.27: Камера обнаруживается поиском как устройство, поддерживающее Onvif, но не работает.Прошивка 3.0.6.27: Управление фокусом не всегда работает. Такое же поведение и в веб-интерфейсе - проблема самой камеры.AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the MPEG4 codec and the max. frame rate (1280x800), the max. frame rate is 15 fps. With the MJPEG codec, the frame rate drops when you increase the quality. 3.0.6.27 firmware: Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. 3.0.6.27 firmware: Sometimes focus control does not work. The same is true in the web interface; this is a problem of the device itself. Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom 50xA_series","Camera ","v3.2.2.3 ","1","+.",null,"+","+","+",null,null,"H.264/MPEG4: 2032x1936; MJPEG: 2592х1944","1024x768","640x480","+",null,"+","-",null,"+","+",null,"+","+","В высоких разрешениях частота кадров ограничена до 15-20 fps\nПри выборе высоких разрешений в первом потоке второй и третий потоки становятся ограниченно доступны:2592x1944 в 1-м потоке: 2-й и 3-й недоступны2032x1936, 2032x1536 в 1-м потоке: 2-й недоступен, в 3-м доступно только разрешение 336х240\nВстроенный детектор движения не работает с кодеком mjpeg.Встроенный детектор движения присылает уведомление об окончании тревоги спустя 3-5 секунд после окончания движения.\nfw 3.2.0.2, 3.2.0.6: Аудио-выход не работает на самом устройстве. Возможно, проблема в конкретном экземпляре, т.к. производители уверяют, что на этих же прошивках у них аудио-выход работает.","At high resolutions, the max. frame rate is 15–20 fps. When you select a high resolution for the first stream, the second and third streams are not always available. 2592x1944 for the 1st stream: the 2nd and 3rd streams are not available; 2092x1936 or 2032x1536 for the 1st stream: the 2nd stream is not available; for the third stream, only 336x240 resolution is available. With the MJPEG codec, the embedded motion detection tool does not work. The embedded motion detection tool notifies about the end of an alarm only 3–5 seconds after the motion stops."]
["Brickcom","Brickcom PZ-040D/E","Camera ","3.1.0.8","1",null,null,"+","+","+",null,null,"720x480 / 720x576","720x480 / 720x576","352x240 / 352x288","+",{"$nulls":3},"+",{"$nulls":3},"-","+"]
["Brickcom","Brickcom VD-100Ap-73","Camera ","3.0.6.12","1","+.",null,"+","+","+",null,null,"1280x800","1280x800","640x400","+",null,"+","+",null,"+","+",null,"-","+","1. Камера обнаруживается поиском как устройство, поддерживающее Onvif, но не работает. \n2. AxxonNext/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","1. Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. \n2. AN: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom VD-130Ap-73","Camera ","3.0.6.13","1","+.",null,"+","+","+",null,null,"1280x1024","640x512","320x256","+",null,"+","+",null,"+","+",null,"-","+","В кодеке MJPEG при увеличении качества падает частота кадров.Прошивка 3.0.6.13: Устройство обнаруживается поиском как поддерживающее Onvif, но не работает.AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the MJPEG codec, when you increase the quality, the frame rate drops. 3.0.6.13 firmware: Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom VD-200Np ","Camera","v3.2.2.7","1","+.",null,"+","+","+",null,null,"1920x1080","1024x768","640x480","+",null,"-","-","-","-","-","-",null,"+"]
["Canon","Canon VB-H610 / VB-H610D / VB-H610VE","Camera","Ver. 1.2.0","1",null,null,"+","-","+",null,null,"1920x1080","960x540","320x240 (MJPEG) / 960x540 (H.264)","-",null,"-","-","-","+","+","-","-","+"]
["Canon","Canon VB-H710F","Camera","Ver. 1.2.0 3015","1",null,null,"+","-","+","-","-","1920x1080","960x540","320x240 (MJPEG) / from WEB (H.264)","-","-","-","-","-","+","+","-","-","+"]
["Canon","Canon VB-M40","Camera","Ver. 1.1.0","1",null,null,"+","-","+",null,null,"1280x960","640x480","320x240","-",null,"-","-","+.","+.","+","-","-","+"]
["Canon","Canon VB-S900F","Camera","Ver. 1.1.0","1","+","2","+",null,"+",null,null,"1920x1080","960x540","480x270","+",null,"-",null,null,"+","+","-",null,"+",null,null,"improved"]
["Certis","Certis NBV-3800RFH","Camera ","ce20130424NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":8},"+","При смене режима ТВ-стандарта камера перезагружается.","After changing TV-standart, the camera will be rebooted."]
["Certis","Certis NDF-3100FH","Camera ","ce20120202ANS","1",null,null,"+",null,"+",null,null,"1920x1080","1280x1024 (MJPEG)","640x480","+",null,null,"-",{"$nulls":5},"+","1. Разрешения 1280х1024 и 1920х1080 во втором потоке доступны только для кодека MJPEG.\n2. Использование максимальных разрешений (1280х1024 и 1920х1080) доступно только в однопоточном режиме","1. 1280х1024 and 1920х1080 resolution for the 2nd video stream is available just for MJPEG. \n2. 1280х1024 and 1920х1080 using is available just for a single stream mode."]
["Certis","Certis NDF-3100FH-E","Camera ","ce20120615NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":8},"+","1. Разрешения 1280х1024 и 1920х1080 во втором потоке доступны только для кодека MJPEG\n2. Использование максимальных разрешений (1280х1024 и 1920х1080) доступно только в однопоточном режиме","1. 1280х1024 and 1920х1080 resolution for the 2nd video stream is available just for MJPEG. \n2. 1280х1024 and 1920х1080 using is available just for a single stream mode."]
["Certis","Certis NDV-3300RFH","Camera ","ce20120202ANS","1",null,null,"+",null,"+",null,null,"1920x1080","1280x1024 (MJPEG)","640x480","+",null,null,"-",{"$nulls":5},"+"," Частота кадров меняется для обоих потоков одновременно\n Максимальные разрешения 1280х1024 и 1920х1080 доступны только в однопоточном режиме\n Во втором потоке разрешения 1280х720, 1280х1024 и 1920х1080 доступны только для кодека MJPEG","The frame rate is changed for both streams simultaneously. \n1280х1024 and 1920х1080 resolutions are available only for a single stream mode. \n1280х720, 1280х1024 and 1920х1080 resolutions for the 2nd video stream are available only for MJPEG."]
["Certis","Certis NDV-3300RFH-E","Camera ","ce20120615NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":8},"+","1. Разрешения 1280х1024 и 1920х1080 во втором потоке доступны только для кодека MJPEG\n2. Использование максимальных разрешений (1280х1024 и 1920х1080) доступно только в однопоточном режиме\n3. Настройки аудио-кодека и битрейта для динамика и микрофона переключаются одновременно (одна настройка в веб-интерфейсе) ","1. 1280х1024 and 1920х1080 resolution for the 2nd video stream is available just for MJPEG. \n2. 1280х1024 and 1920х1080 using is available just for a single stream mode."]
["Certis","Certis NDV-4100HD","Camera ","ce20120202NS","1",null,null,"+","+","+",null,null,"1280x960","640x480","320x240","+",null,null,"-",{"$nulls":5},"+"," Максимальная частота кадров в разрешении 1280х960 - 12.5 fps.\n Во втором потоке разрешение 1280х960 доступно только для кодека MJPEG.\n При использовании комбинации кодеков h264+h264 разрешение 1280х720 во втором потоке доступно только при выборе 1280х720 на первом потоке. При этом максимальная частота кадров составляет 12.5 fps.","The max. frame rate for 1280х960 resolution is 12.5 fps. \n1280х960 resolution for the 2nd video stream is available only for MJPEG. \nFor combination of h264+h264 codecs, 1280х720 resolution for the 2nd stream is available, when 1280х720 resolution is for the 1st stream, and its max. frame rate is 12.5 fps.\n"]
["Certis","Certis NSD-6036H / NSD-6030H / NSD-6018H / NSD-6018PI-X","Camera ","ce20121228NSA ","1",null,null,"+",null,"+",null,null,"720x576 ","640x480","352x288 ","+",{"$nulls":3},"+",{"$nulls":4},"+"]
["Certis","Certis NSD-7018FH / NSD-7020FH","Camera ","ce20120413NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":3},"+","+","Поворот изображения на 90 градусов по/против часовой стрелки работают только при разрешениях начиная с 640x480.","Image turn on / counter-clockwise on 90 degrees is possible only in case of resolution since 640x480."]
["Cisco","Cisco 2500","Camera ","2.1.0","1",null,null,"-","+",{"$nulls":3},"720x576(PAL)/720x480(NTSC)","704x576(PAL)/704x480(NTSC)","352x288(PAL)/352x240(NTSC)","+",null,"+","-",null,"-","+",null,"-","+","для корректной работы реле следует в настройках камеры выставить Curren Status в положение \"Low\"в вебе камеры есть настройка \"Enable Multicast for MPEG-4 Stream1\" - активируется через чек-бокс. При включенной настройке, если камера в сети, где работают не только IP-камеры могут быть проблемы. Например у нас, в этом случае зависла IP-телефония во всем филиале.проблемы с прошивкой - яркость в вебе не работает, контраст так же, вместо цветности регулируется резкость","To make the relay work correctly, set the camera's Current Status setting to Low. The camera's web interface has the Enable Multicast for MPEG-4 Stream1 check box. When you select this check box and the camera is connected to a network that contains other devices in addition to IP cameras, you may encounter a problem. For example, at our place, IP telephony froze throughout the entire office. Firmware problems: brightness does not work in the web interface, contrast the same, when you try to adjust color, sharpness gets adjusted. "]
["Cisco","Cisco 4500","Camera ","1.0.1","1",null,null,"+.",null,"+.",null,null,"1280x720(H.264)/720x576(MJPEG)","704x576","352x288","+.",null,"+","-",null,"+","+",null,"-","+","1) камере Cisco 4500 имеет 2 потока.\nпервый (1) - формат видео H.264\nвторой (2) - формат видео MJPEG\nв вебе камеры количество доступных разрешений в разных форматах различно\nпри этом первый канал (1) имеет приоритет над вторым (2), т.е. нельзя выставить разрешение для MJPEG большее чем установлено в данный момент на канале с H.264\nесли переключиться в стандартном разрешении из формата H.264 в формат MJPEG, то изменить разрешение в формате H.264 невозможно\nтак же, если из потока MJPEG с разрешением полное (704*576) переключиться в поток H.264 (выставится полное разрешение 1280*720), а затем обратно в MJPEG то полное разрешение уже станет не 704*576, а 720*576\n2) звук должен быть только с потоком H.264","1) The Cisco 4500 camera has two streams:\nFirst (1) – the H.264 Video Parameters\nSecond (2) – the MJPEG Video Parameters\nIn the camera's web interface, the number of available resolutions is different for different formats; \nthe first channel (1) has priority over the second channel (2), so for MJPEG you cannot set a resolution higher than is now set for the H.264 channel.\nAt standard resolution, if you switch from H.264 to MJPEG, then you cannot\nchange the resolution for H.264. Additionally, if you first select full (704x576) resolution for the MJPEG stream and then switch to the H.264 channel (which will set the new full resolution at 1280x720) and back to MJPEG, then the full resolution becomes 720*576 instead of 704x576.\n2) Audio works only with the H.264 stream"]
["CNB","CNB IDC 4050F","Camera ","XNET.M1-1.01.10.1021","1","+.",null,"+",null,"+",null,null,"640x480 (MJPEG) / 1920x1080 (H264)","640x480 (MJPEG) / 1280x960 (H264)","320x240 (MJPEG) / 640x480 (H264)","+",null,"+","-",null,"-",null,null,"+","+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.Набор доступных разрешений во втором потоке зависит от выбранного кодека во втором потоке и текущего разрешения в первом потоке: Разр-е в 1м потоке Кодек в 2-м потоке Доступные разр-я в 2-м потоке 352x288 h264 352x288 mjpeg 352x288 640x480 h264 320x240 mjpeg 320x240,640x480 720x576 h264 352x288 mjpeg 352x288, 720x576 1280x720 h264 352x288 mjpeg 352x288, 720x576 1280x1960 --- --- 1920x1080 --- --- Перед сменой потока на \"1.MJPEG/H264\" (в AxxonNext/Next) или кодека на \"MJPEG\" (в Интеллекте) необходимо выбрать в потоке \"0.H264\" (в AxxonNext/Next) или в кодеке \"H264\" (в Интеллекте) приемлемое разрешение (см. таблицу выше)В Интеллекте в кодеке MJPEG \"полное\" разрешение недоступно","According to the vendor, currently it is not possible to integrate sensors. Which resolutions are available for the second stream depends on the codec selected for the second stream and the current resolution for the first stream: Resolution (1st stream) Codec (2nd stream) Resolutions available (2nd stream) 352x288 h264 352x288 mjpeg 352x288 640x480 h264 320x240 mjpeg 320x240,640x480 720x576 h264 352x288 mjpeg 352x288, 720x576 1280x720 h264 352x288 mjpeg 352x288, 720x576 1280x1960 --- --- 1920x1080 --- --- Before changing the stream to 1.MJPEG/H264 (in AN) or the codec to MJPEG (in Intellect), select the acceptable resolution for the 0.H264 stream (in AN) or H264 codec (in Intellect) (see the table above). In Intellect, \"full\" resolution is not available for the MJPEG codec."]
["CNB","CNB IDC 4050IR","Camera ","XNET.A2-1.01.10.0827","1","+.",null,"+",null,"+",null,null,"640x480 (MJPEG) / 1920x1080 (H264)","640x480 (MJPEG) / 1280x960 (H264)","320x240 (MJPEG) / 640x480 (H264)","+",null,"+","-",null,"-",null,null,"+","+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.Набор доступных разрешений во втором потоке зависит от выбранного кодека во втором потоке и текущего разрешения в первом потоке: Разр-е в 1м потоке Кодек в 2-м потоке Доступные разр-я в 2-м потоке 352x288 h264 352x288 mjpeg 352x288 640x480 h264 320x240 mjpeg 320x240,640x480 720x576 h264 352x288 mjpeg 352x288, 720x576 1280x720 h264 352x288 mjpeg 352x288, 720x576 1280x1960 --- --- 1920x1080 --- --- Перед сменой потока на \"1.MJPEG/H264\" (в AxxonNext/Next) или кодека на \"MJPEG\" (в Интеллекте) необходимо выбрать в потоке \"0.H264\" (в AxxonNext/Next) или в кодеке \"H264\" (в Интеллекте) приемлемое разрешение (см. таблицу выше)В Интеллекте в кодеке MJPEG \"полное\" разрешение недоступноПрошивка XNET.A2-1.01.10.0827: значение \"25 fps\" параметра \"частота кадров\" не работает на самой камере.","According to the vendor, currently it is not possible to integrate sensors. Which resolutions are available for the second stream depends on the codec selected for the second stream and the current resolution for the first stream: Resolution (1st stream) Codec (2nd stream) Resolutions available (2nd stream) 352x288 h264 352x288 mjpeg 352x288 640x480 h264 320x240 mjpeg 320x240,640x480 720x576 h264 352x288 mjpeg 352x288, 720x576 1280x720 h264 352x288 mjpeg 352x288, 720x576 1280x1960 --- --- 1920x1080 --- --- Before changing the stream to 1.MJPEG/H264 (in AN) or the codec to MJPEG (in Intellect), select the acceptable resolution for the 0.H264 stream (in AN) or H264 codec (in Intellect) (see the table above). In Intellect, the \"full\" resolution is not available for the MJPEG codec. XNET.A2-1.01.10.0827 firmware: the value of 25 fps for the Frame Rate parameter does not work on the camera itself. "]
["CNB","CNB IDC 4050VR","Camera ","XNET.M1-3.00.13.0204","1","+.",null,"+",null,"+",null,null,"1920x1080 (H264) / 720x576 (MJPEG)","1280x960 (H264) / 640x480 (MJPEG)","640x480 (H264) / 320x240 (MJPEG)","+",{"$nulls":8},"+","1. Настройка битрейта / качества на камере имеет динамический диапазон значений (зависит от выбранного разрешения). В ПО ITV/Axxon такую зависимость реализовать невозможно, поэтому интегрирован весь диапазон возможных значений.\n2. Набор разрешений на потоках взаимозависим:\n(1-ый поток) 1920x1080, 1280x1024, 1280x960 <=> (2-й поток) недоступен вообще\n(1-ый поток) 1280x720, 720x576 <=> (2-й поток) 720x576, 352x288\n(1-ый поток) 640x480 <=> (2-й поток) 640x480, 320x240\n(1-ый поток) 352x288 <=> (2-й поток) 352x288","1. Bitrate / quality on camera has dynamic value range (it depends on selected resolution). It can't be implemented in Axxosoft SW, that's why the whole range of possible value has been integrated. \n2. The list of resolution for the streams is interdependent:\n(1st stream) 1920x1080, 1280x1024, 1280x960 <=> (2nd stream) not available;\n(1st stream) 1280x720, 720x576 <=> (2nd stream) 720x576, 352x288;\n(1st stream) 640x480 <=> (2nd stream) 640x480, 320x240;\n(1st stream) 352x288 <=> (2nd stream) 352x288"]
["CNB","CNB IDP 4000VD","Camera ","XNET.A1-1.1.10.0630","1","+.",null,"+","+","+",null,null,"640x480","640x480","320x240","+",null,"+","-",null,"-","+",null,"+","+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной. ","According to the vendor, currently it is not possible to integrate sensors. "]
["CNB","CNB IDP 4000VR","Camera ","XPDN.A1-1.1.10.126","1","+.",null,"+","+","+",null,null,"640x480","640x480","320x240","+",null,null,"-",null,"-",null,null,"+","+"]
["CNB","CNB IDP 4030VR","Camera ","XNET.A1-1.1.11.0325","1","+.",null,"+","+","+",null,null,"H264/MPEG4: 640x480; MJPEG: 1280x960","H264/MPEG4: 640x480; MJPEG: 1024x678","320x240","+",null,"+","-",null,"-","+",null,"+","+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.Прошивка XNET.A1-1.01.10.0630: Камера присылает неправильные метки времени - время идет ускоренно, поэтому архив не будет работать правильно.Прямое переключение потоков \"2.MJPEG\" -> \"1.MJPEG\" не работает. Нужно выполнять переключение по схеме \"2.MJPEG\" -> \"0.MPEG4/H264\" -> \"1.MJPEG\".","According to the vendor, currently it is not possible to integrate sensors. XNET.A1-1.01.10.0630 firmware: The camera sends wrong timestamps: the archive does not work correctly, because time \"moves\" faster than it should. You cannot switch from the 2.MJPEG stream to the 1.MJPEG stream directly. You must switch from 2.MJPEG first to 0.MPEG4/H264 and then to 1.MJPEG. "]
["CNB","CNB IGP 1030","Camera ","XNET.A1-1.01.10.634","1","+.",null,"+","+","+",null,null,"1280x960(MJPEG) / 640x480(MPEG-4) / 640x480(H.264)","640x480","320x240","+",null,"+","-","+","-","+",null,"+","+","1. По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной. \n2. Из цифровой телеметрии доступно только перемещение изображения. Реализация увеличения и предустановок невозможна по утверждению производителя. ","1. According to the vendor, currently it is not possible to integrate sensors. \n2. Of the digital telemetry functions, only image movement is available. According to the vendor, zoom and presets cannot be implemented. "]
["CNB","CNB INS 2000 encoder","Encoder ","XNET.x1-1.1.10.304","1","+.",null,"+","+","+",null,null,"704x576(PAL) / 704x480 (NTSC)","704x576(PAL) / 704x480 (NTSC)","352x288(PAL) / 352x240 (NTSC)","+",null,"+","-","+","-","+",null,"+","+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.","According to the vendor, currently it is not possible to integrate sensors. "]
["CNB","CNB IPM 3063 N(P)","Camera ","XPDN.A1-1.1.10.126","1","+.",null,"+","+","+",null,null,"704x576","704x576","352x288","+",null,"+","-","+","-","+",null,"-","+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.","According to the vendor, currently it is not possible to integrate sensors. "]
["CNB","CNB ISMC 1063N","Camera ","XPDN.A1-1.1.10.126","1","+.",null,"+","+","+",null,null,"704x480","704x480","352x240","+",null,null,"-","+","-",null,null,"+","+"]
["CNB","CNB IVC 4000T","Camera ","XNET.T1-1.0.10.1222","1","+.",null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"-","-",null,"-","+",null,"-","+","1. Разрешение меняется сразу для обоих стриммингов одновременно. Это особенность самой камеры.\n2. По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной. ","1. The resolution is adjusted for both streams at the same time. This is a limitation of the camera itself. \n2. According to the vendor, currently it is not possible to integrate sensors. "]
["CNB","CNB IVP 4030VR","Camera ","XNET.A1-1.1.11.0325","1","+.",null,"+","+","+",null,null,"1280x960(MJPEG) 640x480(MPEG-4) 640x480(H.264)","640x480","320x240","+",null,"+","-",null,"-","+",null,"+","+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.Прошивка XNET.A1-1.01.10.0630: Камера присылает неправильные метки времени - время идет ускоренно, поэтому архив не будет работать правильно.","According to the vendor, currently it is not possible to integrate sensors. XNET.A1-1.01.10.0630 firmware: The camera sends wrong timestamps and the archive does not work correctly, because time \"moves\" faster than it should. "]
["ComOnyx","ComOnyx CO-i03MY1","Camera ","V1.0.32_Y ","1",null,null,"+","-","+",null,null,"640x480","640x480","320x240","+",null,"+","+",{"$nulls":4},"+","+","Камера определяется как Yudor CO-i03MY1 (YUC-HS94)","In the AxxonSoft products, the camera is identified as Yudor CO-i03MY1 (YUC-HS94)"]
["ComOnyx","ComOnyx CO-i04DY2","Camera ","V1.0.32_Y","1",null,null,"+","-","+",null,null,"720x576","704x576","352x288","+",null,"+","+",null,"+","+",null,"+","+","Камера определяется как Yudor CO-i03MY1 (YUC-HS94)","In the AxxonSoft products, the camera is identified as Yudor CO-i03MY1 (YUC-HS94)"]
["ComOnyx","ComOnyx CO-i13MY1","Camera ","V1.0.32_Y","1",null,null,"+","-","+",null,null,"1280x1024","1280x960","640x480","+",null,"+","+",{"$nulls":4},"+","+","1. Между переходами луча в состояние \"замкнуто\" должен соблюдаться временной интервал, настраиваемый через веб-интерфейс. Минимальное значение - 10 секунд.\n2. Через Onvif камера работает только в режиме совместимости. Видео и звук идут, но никакие настройки не применяются.\n3. В Интеллект поиск находит камеру как FineCCTV.\n4. Камера определяется как Yudor CO-i04DY2(3.7-12) (YUC-HM93-312)","1. You can configure the delay before a sensor closes in the camera's web interface. Min 10 seconds.\n2. Via the ONVIF protocol, the camera works only in the compatibility mode. Video and audio streams are there but changes can't be applied.\n3. In AxxonSoft Intellect, the camera is identified as FineCCTV IP-Cam.\n4. In the AxxonSoft products, the camera is identified as CO-i04DY2(3.7-12) (YUC-HM93-312)"]
["ComOnyx","ComOnyx CO-i20DY2(P)","Camera ","V1.0.32_Y","1",null,null,"+","-","+",null,null,"1600x1200","1280x960","640x480","+",null,"+","+",null,"+","+",null,"+","+","1. На камере есть ограничение FPS в зависимости от разрешения:\n Для разрешений не больше 640x480 ограничение составляет 30 fps, для больших разрешений - 15. Ограничение включается для всех потоков, если разрешение >640x480 установлено хотя бы на одном из двух потоков. \n2. Камера определяется как Yudor CO-i13MY1 (CO-YUC-HS95)","1. The camera has frame rate limits (depending on the resolution):\n For resolutions lower than 640x480 the max fps is 30, fro greater resolutions it is 15. This limitation applies to all streams if a resolution greater than 640x480 is set for any of the 2 streams. \n2. In the AxxonSoft products, the camera is identified as Yudor CO-i13MY1 (CO-YUC-HS95)."]
["ComOnyx","ComOnyx CO-i20DY2IRPV","Camera ","V1.0.32_Y","1",null,null,"+","-","+",null,null,"1600x1200","1280x960","640x480","+",null,"+","+",null,"+","+",null,"+","+","1. Поиск в AN не определяет прошивку: ее нужно выбрать самостоятельно.\n2. Между переходами луча в состояние \"замкнуто\" должен соблюдаться временной интервал, настраиваемый через веб-интерфейс. Минимальное значение - 10 секунд.\n3. Прошивка V1.0.32_Y: через Onvif камера работает только в режиме совместимости. Видео и звук идут, но никакие настройки не применяются. \n4. В Интеллекте поиск находит камеру как FineCCTV.\n5. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.\n6. Камера определяется как Yudor CO-i20DY2(2,7-9) (CO-YUC-HM96-279)","1. In the AxxonSoft products, the device's firmware version cannot be identified. You must select the firmware version yourself.\n2. You can configure the delay before a sensor closes in the camera's web interface. Min 10 seconds.\n3. The V1.0.32_Y firmware: via the ONVIF protocol, the camera works only in the compatibility mode. Video and audio streams are there but changes can't be applied. \n4. In AxxonSoft Intellect, the camera is identified as FineCCTV.\n5. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, before using the camera, go to the web interface and select the required value.\n6. In the AxxonSoft products, the camera is identified as Yudor CO-i20DY2(2,7-9) (CO-YUC-HM96-279)."]
["ComOnyx","ComOnyx CO-i20HY0","Camera ","V1.0.26_Y","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+","-","+","+","+",null,"+","+","1. Настройка \"Параметры видео\" определяет ограничение FPS в зависимости от разрешения. Для получения максимального FPS необходимо следить за тем, чтобы разрешение настройки \"Параметры видео\" было не больше, чем выбренное разрешение получаемого видео.\n2. После размыкания датчика реакция на следующее замыкание может произойти не раньше, чем через 10 секунд.\n3. Камера определяется как Yudor CO-i20DY2IRPV (CO-YUC-Hi96RP)","1. The Video Parameters setting is used to limit fps depending on the resolution. To get the maximum frame rate, make sure that the Video Parameters setting has the the same or lower resolution than you selected on the VMS.\n2. After opening, the sensor can close in not earlier than 10 seconds.\n3. In the AxxonSoft products, the camera is identified as Yudor CO-i20DY2IRPV (CO-YUC-Hi96RP)."]
["ComOnyx","ComOnyx CO-i20HY0DNP","Camera ","V1.0.26_Y","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+","-","+","+","+",null,"+","+","1. Поиск в AN не определяет прошивку: ее нужно выбрать самостоятельно.\n2. Прошивка V1.0.26_Y: камера работает по Onvif только в режиме совместимости, поиском как Onvif не находится.\n3. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.\n4. Камера определяется как Yudor CO-YUC-H696","1. In the AxxonSoft products, the device's firmware version cannot be identified. You must select the firmware version yourself.\n2. The V1.0.26_Y firmware: Via the ONVIF protocol, the camera works only in compatibility mode; the search does not find the camera as a device that supports ONVIF.\n3. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, before using the camera, go to the web interface and select the required value.\n4. In the AxxonSoft products, the camera is identified as Yudor CO-YUC-H696."]
["ComOnyx","ComOnyx CO-i20HY0DNW","Camera ","V1.0.20_Y","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+","-","+","+","+",null,"+","+","1. Поиск в AN не определяет прошивку: ее нужно выбрать самостоятельно.\n2. Прошивка V1.0.26_Y: камера работает по Onvif только в режиме совместимости, поиском как Onvif не находится.\n3. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.\n4. Камера определяется как Yudor CO-YUC-H696RP","1. In the AxxonSoft products, the device's firmware version cannot be identified. You must select the firmware version yourself.\n2. The V1.0.26_Y firmware: Via the ONVIF protocol, the camera works only in compatibility mode; the search does not find the camera as a device that supports ONVIF.\n3. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, before using the camera, go to the web interface and select the required value.\n4. n the AxxonSoft products, the camera is identified as Yudor CO-YUC-H696RP."]
["ComOnyx","ComOnyx CO-i20HY0P","Camera ","V1.0.26._Y","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+","-","+","+","+",null,"+","+","1. Поиск в AN не определяет прошивку: ее нужно выбрать самостоятельно.\n2. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.\n3. Камера определяется как Yudor CO-YUC-H696RW","1. In the AxxonSoft products, the device's firmware version cannot be identified. You must select the firmware version yourself.\n2. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, before using the camera, go to the web interface and select the required value.\n3. In the AxxonSoft products, the camera is identified as Yudor CO-YUC-H696RW."]
["ComOnyx","ComOnyx CO-i20SY2IR(P/W)","Camera ","1.0.38_Y","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"-","-",null,"+","+",null,"motion detection; ","+","1. Поиск в AN не определяет прошивку: ее нужно выбрать самостоятельно.\n2. Прошивка V1.0.26_Y: камера работает по Onvif только в режиме совместимости, поиском как Onvif не находится.\n3. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.\n4. Камера определяется как Yudor CO-YUC-H696P","1. In the AxxonSoft products, the device's firmware version cannot be identified. You must select the firmware version yourself.\n2. The V1.0.26_Y firmware: Via the ONVIF protocol, the camera works only in compatibility mode; the search does not find the camera as a device that supports ONVIF.\n3. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, before using the camera, go to the web interface and select the required value.\n4. In the AxxonSoft products, the camera is identified as Yudor CO-YUC-H696P."]
["Compotrol","Compotrol IP-5130","Camera ","V3.0 110921","1",null,null,"+","+","+",null,null,"2560x1920","1600x1200","320x240","+",null,"+","+","+","+","-",null,"motion detection","+","1. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект после добавления камеры необходимо выбрать нужное значение в веб-интерфейсе.\n2. Протокол ONVIF: при переключение кодека с MJPEG на H.264 - нет видео. Проблема устройства. Чтобы получить видео необходимо выставить кодек в веб-интерфейсе и перезапустить продукт\n3. Камера определяется как Yudor YUC-H796R\n","1. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, after adding the camera, go to the web interface and select the required value.\n2. ONVIF: when you switch from MJPEG to H.264, video stream is lost. This is a problem of the camera itself. To make it work, go to the camera's web interface, select a codec and restart the VMS. In the AxxonSoft products, the camera is identified as Yudor YUC-H796R.\n"]
["Compotrol","Compotrol-VA500","Camera ","1.06.02","1",null,null,"+","+","+",null,null,"720x576(PAL) / 720x480(NTSC)","640x576(PAL) / 640x480(NTSC)","320x288(PAL) / 320x240(NTSC)","+",null,"-","-",{"$nulls":4},"motion detection","+","1. В MJPEG при максимальном качестве само устройство выдает ~15 fps максимум","1. With MJPEG and the max quality, the device itself allows 15 fps max. "]
["CP Plus","CP Plus CP-UNC-BP50C","Camera","3.000.AT00.0.R","1",null,null,"+","-","+",null,null,"2560x1920","2048x1536","1280x960","+",null,"-","-","-","-","-","-","-","+","Диапазон значений битрейта зависит от значений разрешения и fps.Максимально возможное разрешение определяется текущим значением частоты кадров. При максимальных значениях частоты кадров недоступны большие разрешения. Более подробно зависимость описана в документации производителей.","Range of value ​​depends on the bit rate of the resolution and fps. The highest resolution is determines by current value of frame rate. At maximum frame rate not available high resolution. This dependence described detaily in manufacturer's documentation."]
["CP Plus ","CP Plus CP-UNC-BY20C","Camera ","3.000.AT00.0.R, build : 2013-05-13","1",null,null,"+",null,"+",null,null,"1920x1080","1280x960","352x288","+",{"$nulls":8},"+","Диапазон допустимых значений битрейта зависит от текущего значения разрешения и fps.\nНастройку качества для ПО ITV рекомендуется производить в веб-интерфейсе камеры.","Range of available bit rate values ​​depends on current resolution and fps.\nQuality setting for AxxonSOft software recommended to select in camera's web interface."]
["CP Plus ","CP Plus CP-UNC-DP10","Camera ","3.000.AT00.0.R, build : 2013-05-13","1",null,null,"+",null,"+",null,null,"1280x960","1280x720","352x288(PAL) / 352x240 (NTSC)","+",{"$nulls":8},"+","Диапазон значений битрейта зависит от значений разрешения и FPS. Если вводимое значение не входит в доступный диапазон, то значение не применяется.\nПри работе с камерой в ПО ITV настройку качества для кодека MJPEG рекомендуется производить в веб-интерфейсе.","Range of bit rate values ​​depends on the resolution and FPS. If entered value is not included in available range, the value will not be applied.\nWhen using the camera in AxxonSoft software quality setting for MJPEG codec is recommended to select in camera's web interface."]
["CP Plus","CP Plus CP-UNC-TP10L2C","Camera","3.000.AT00.0.T, build : 2014-01-16","1","+","2","+",null,"+",null,null,"1280x960","1280x720","352x288 (PAL) / 352x240 (NTSC)","+",{"$nulls":8},"+","Диапазон значений битрейта зависит от значений разрешения и FPS. Если вводимое значение не входит в доступный диапазон, то значение не применяется.Диапазон значений fps на втором потоке зависит от значения разрешения на первом.","Bit rate value depends on the resolution and fps. If the specified value is not included in available range, the value will not be applied. Range of fps values for the second stream depends on the value of resolution for the first stream.","new"]
["CP Plus","CP Plus CP-UNC-TP13FL2CD","Camera","3.000.AT00.0.R, build : 2013-05-13","1","+","2","+",null,"+",null,null,"1280x960","1280x720","352x288","+",null,"-","-",null,"-","-","-","-","+","Диапазон значений битрейта зависит от значений разрешения и FPS. Если вводимое значение не входит в доступный диапазон, то значение не применяется.","Bit rate value depends on the resolution and fps. If the specified value is not included in available range, the value will not be applied. ","new"]
["CP Plus ","CP Plus CP-UNC-TY10FL5C","Camera ","3.000.AT00.0.R","1",null,null,"+",null,"+",null,null,"1280x960","1280x720","352x288","+",{"$nulls":8},"+"]
["CP Plus ","CP Plus CP-UNC-TY20ZL2C","Camera ","3.000.AT00.0.R","1",null,null,"+",null,"+",null,null,"1920x1080","1280x960","352x288","+",{"$nulls":8},"+"]
["CP Plus","CP Plus CP-UNC-VP13FCD / CP-UNC-VP13FL2CD","Camera","3.000.AT00.0.R, build : 2013-05-13","1","+","2","+",null,"+",null,null,"1280x960","1280x720","352x288","+",null,"-","-",null,"-","-","-","-","+","Диапазон значений битрейта зависит от значений разрешения и FPS. Если вводимое значение не входит в доступный диапазон, то значение не применяется.","Bit rate value depends on the resolution and fps. If the specified value is not included in available range, the value will not be applied. ","new"]
["CP Plus","CP Plus CP-UNP-2020L10","Camera","3.000.AT00.0.R","1",null,null,"+","-","+",null,null,"1920x1080","1280x720","352x288","+",null,"-","-","+","-","-","-","-","+"]
["CP Plus","CP Plus CP-UNP-37","Camera","3.000.AT00.0.R, build 2013-04-18","1",null,null,"+","-","+","-","-","704x576","704x576","640x480","+","-","-","-","+","-","-","-",null,"+"]
["Dahua","Dahua IPC-HDB3200C","Camera","2.211.0000.0.R","1",null,null,"+","-","+",null,null,"1920x1080","1280x960","352x288","+",null,"-","-","-","-","-","-","-","+","Максимальное разрешение на первом потоке ограничивает выбор частоты кадров до 18 на двух потоках. Диапазон значений битрейта зависит от значений разрешения и FPS. Если вводимое значение не входит в доступный диапазон, то значение не применяется. При работе с камерой в ПО ITV настройку качества для кодека MJPEG рекомендуется производить в веб-интерфейсе. При разрешении выше 720p не поддерживается настройки зеркального отображения и поворота изображения. Настройка ТВ-стандарт не меняет формат видео. Ее значение следует выбирать в соответствии с версией модели (существуют PAL и NTSC версии).","The max. resolution settings for stream 1 limit fps settings to 18 fps for both streams. The Bit Rate range depends on the stream settings. The lower fps, resolution, key frame rate you have for the stream, the shorter is the bit rate range. In the AxxonSoft products, the bit rate span is set to max. values. With resolutions exceeding 720p, the image rotation and mirroring settings do not work. TV standart setting does not change video format. To need to change the setting in accordance with model version (there are PAL and NTSC versions)."]
["Dahua","Dahua IPC-HDBW3300 / IPC-HF3300 / IPC-HDB3300 / IPC-HFW3300(C)","Camera ","2.210.0000.0.R, build: 2013-01-25","1",null,null,"+",null,"+",null,null,"2048x1536","1280x960","352x288","+.",{"$nulls":4},"-","-",null,"-","+","1. Максимальное разрешение на первом потоке ограничивает выбор частоты кадров до 18 на двух потоках.\n2. Диапазон значений битрейта зависит от настроек потока. Чем меньше значения таких настроек как частота кадров, разрешение, частота опорных кадров, тем меньше диапазон битрейта. В продукте для битрейта задан диапазон от самого маленького значения до самого большого.\n3. При разрешении выше 720p не поддерживается настройки зеркального отображения и поворота изображения.\n4. Для того, чтобы у нас в продукте заработали настройки изображения, нужно в веб-интерфейсе устройства выбрать Профиль \"Day\" (Setup -> Camera -> Conditions -> Config File)\n5. Настройка качества для MJPEG производится в веб-интерфейсе","1. The max. resolution settings for stream 1 limit fps settings to 18 fps for both streams.\n2. The Bit Rate range depends on the stream settings. The lower fps, resolution, key frame rate you have for the stream, the shorter is the bit rate range. In the AxxonSoft products, the bit rate span is set to max. values.\n3. With resolutions exceeding 720p, the image rotation and mirroring settings do not work.\n4. To make video settings work, go to the camera's web interface and select the Day profile in Setup -> Camera -> Conditions -> Config File\n5. You can configure quality settings for MJPEG stream in the camera's web interface."]
["Dahua","Dahua IPC-HFW3101C","Camera ","2.103.0001.0.R","1",null,null,"+",null,"+",null,null,"1280x960","1280x720","704x576","+",{"$nulls":8},"+"]
["Dahua","Dahua IPC-HFW3200C / IPC-HDBW3200","Camera ","2.210.0000.0.R, build : 2013-03-13","1",null,null,"+",null,"+",null,null,"1920x1080","704x576","352x288","+",{"$nulls":8},"+","1. Для работы настроек изображения в ПО ITV | AxxonSoft необходимо в настройках камеры Camera > Conditions > Config file выбрать значение Day\n2. Значения \"поворота на 90 градусов\" настройки Поворот видеоизображения применяются только при разрешении не выше 720р. ","1. To work with image settings in Axxonsoft SW, please select Day in the camera settings (Camera > Conditions > Config file).\n2. The value of \"90 degree rotation\" is applied only if resolution is not higher than 720p. "]
["Dahua","Dahua IPC-HFW3200S","Camera ","2.103.0000.2.R, build : 2013-03-21","1",null,null,"+",null,"+",null,null,"1920x1080","1280x960","352x288","+",{"$nulls":8},"+","1. Диапазон допустимых значений битрейта зависит от текущих значений настроек потока (частота кадров, разрешение, частота опорных кадров). В ПО ITV/Axxon интегрирован максимально возможный диапазон значений.\n2. Настройка качества для MJPEG производится в веб-интерфейсе ","1. Valid range of the bit rate depends on the current stream settings (FPS, resolution, keyframe rate). Axxonsoft software supports the maximum possible range of values. 2. To configure quality for MJPEG, please use camera web-interface."]
["Dahua","Dahua SD6582A-HN ","Camera ","2.103.0003.0.R, build : 2012-10-16","1",null,null,"+",null,"+",null,null,"1920x1080","1280x720","704x480","+",{"$nulls":3},"+",{"$nulls":4},"+","1. Диапазон допустимых значений битрейта зависит от текущих значений настроек потока (частота кадров, разрешение, частота опорных кадров). В ПО ITV/Axxon интегрирован максимально возможный диапазон значений.\n2. Настройка качества для MJPEG производится в веб-интерфейсе ","1. Valid range of the bit rate depends on the current stream settings (FPS, resolution, keyframe rate). Axxonsoft software supports the maximum possible range of values. 2. To configure quality for MJPEG, please use camera web-interface."]
["Dahua","Dahua SD6982A-HN","Camera","2.212.0000.0.R, build : 2013-09-12","1",null,null,"-","-","+",null,null,"1920x1080","704x576","640x480","+",null,"-","-","+.","-","-","-","-","+","Диапазон допустимых значений битрейта зависит от текущего значения разрешения и fps. Значение разрешения 704x576, для второго потока, недоступно если на первом потоке стоит значение разрешения в 640x480Камера интегрирована под названием SD6XXX-HN.","Bitrate value ​​depends on current resolution and fps. Resolution 704x576 for second stream is not available, at first stream adjusted resolution 640x480. Camera is integrated as SD6XXX-HN."]
["Dahua","Dahua SDZ2020B-N","Camera","2.103.0002.0.R, build : 2012-10-31","1",null,null,"+","-","+","-","-","1920x1080","1280x720","352x288","-","-","-","-","+","-","-","-","-","+","Диапазон значений битрейта зависит от значений разрешения и частоты кадров в секунду.Минимально допустимое значение частоты опорных кадров соответствует текущему значению FPS, это ограничение камеры.Настройку качества для MJPEG рекомендуется производить в веб-интерфейсе камеры.","Bitrate range depends on resolution and fps. Minimal key frame rate is equal to the current fps- it’s a camera restriction. To set the MJPEG quality, use the camera web interface."]
["Dallmeier","Dallmeier DDF3000IPV (ONVIF)","Camera ","V2.4.4","1",null,null,"+","+",{"$nulls":3},"720x576","704x576","352x288","+",{"$nulls":7},"-","+","\nработает только через ONVIF\n \n1) в веб-интерфейсе есть вкладки с настройками реле - физически же подключить их некуда\n \n2) настройка звука недоступна на самой камере \n \n3) чтобы камера работала через ONVIF его (т.е. ONVIF) надо активировать\n \n4) поиск через IP-Wizard не реализован - проблемы связаны с самой камерой, а не с ПО ITV\n \n\n5) mpeg2 через ONVIF не реализован","\nWorks only via the ONVIF protocol. \n \n1. The web interface has tabs with relay settings; however, you cannot connect relays physically.\n \n2. The device itself does not allow you to configure audio. \n \n3. To make the camera work via the ONVIF protocol, enable ONVIF.\n \n4. Search through IP Wizard is not implemented, because of a problem with the camera, not with the AxxonSoft software.\n \n\n5. MPEG2 via the ONVIF protocol is not implemented."]
["Dallmeier","Dallmeier MicroStreamer (ONVIF)","Encoder ","V2.4.4","1",null,null,"+","+",{"$nulls":3},"720x576","704x576","352x288","+",{"$nulls":8},"+","\n\n\nработает только через ONVIF\n \n1) в веб-интерфейсе есть вкладки с настройками реле - физически же подключить их некуда\n \n2) настройка звука недоступна в самом устройстве \n \n3) чтобы устройство работало через ONVIF его (т.е. ONVIF) надо активировать\n \n4) поиск через IP-Wizard не реализован- проблемы связаны с самим устройством, а не с ПО ITV\n \n5) mpeg2 через ONVIF не реализован","\n\n\nWorks only via the ONVIF\n protocol.  \n1. The web interface has tabs with relay settings; however, you cannot connect relays physically.\n \n2. The device itself does not allow you to configure audio. \n \n3. To make the device work via the ONVIF protocol, enable ONVIF.\n \n4. Search through IP Wizard is not implemented, because of a problem with the device, not with the AxxonSoft software.\n \n5. MPEG2 via the ONVIF protocol is not implemented."]
["D-Link ","D-Link DCS-932L","Camera ","1.06","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":8},"-"," В ПО ITV устройство обнаруживается поиском как Trendnet DCS-932L ","In Axxonsoft SW camera is detected as Trendnet DCS-932L."]
["D-Link ","D-Link DCS-930L","Camera ","1.08","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":8},"-"]
["Dynacolor","Dynacolor nZH061 -V6A (NV062)","Camera ","d20100630NS ","1",null,null,"+",null,"+",null,null,"1920x1080","1280x720","352x288","+",null,null,"-",{"$nulls":4},"-","+","1. Камера подключается в продуктах ITV/Axxon под \"именем\" NV062","1. In AxxonSoft products, the camera is connected as NV062"]
["Dynacolor","DynaHawk 801","Camera ","0228-0031-0263","1",null,null,"+","+",{"$nulls":3},"720x576","720x576","352x288","+",null,"-","-","+",{"$nulls":3},"-","-","1. При смене потока, разрешения, качества, fps (а значит и при старте Intellect, когда все эти настройки применяются) камера на 60 сек. уходит в ребут. И в Intellect и в родном вебе.\n2. При максимальных настройках в MJPEG сама камера способна выдавать только 12 fps\n ","1. After you change the stream, resolution, quality, or frame rate (and on Intellect's startup, when all these settings are applied), the camera restarts for 60 seconds. Both in Intellect and the device's own web interface. \n2. With MJPEG and the max. settings, the camera allows 12 fps max.\n "]
["Dynacolor","DynaHawk 811","Camera ","0167-0010-0232","1",null,null,"+","+",{"$nulls":3},"720x576","720x576","352x288","+",{"$nulls":3},"+",{"$nulls":3},"-","-","1. Видео по камере стартует не сразу, а в течении 7-10 секунд. Это связано с тем, что на камере в это время применяются \"интеллектовские\" настройки. ","1. Video does not start immediately, only after 7–10 seconds. This is because it takes time to apply Intellect's settings to the camera. "]
["Dynacolor","DynaHawk NH061","Camera ","d20100310NS","1",null,null,"+","+","+",null,null,"1280x960","1280x720","640x480","+",null,"+.","-",null,"+","+",null,"-","+"," Реле камеры по умолчанию работает в режиме \"Нормально замкнуто\". Перед работой можно изменить это через веб-интерфейс камеры.","By default, the camera relay works in Normally Closed mode. Before using the relay, change this in the camera's web interface. "]
["Dynacolor","DynaHawk nZH060","Camera ","d20081226NS","1",null,null,"+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4)","1280x960(MJPEG)/352x288(MPEG-4)","640x480(MJPEG)/320х240(MPEG-4)","+",null,"+","-",null,"+","+",null,"-","+","В MJPEG в максимальном разрешении 1280x960 максимальная частота кадров - 15 fps.При одновременном использовании нескольких видеопотоков доступные разрешения в них взаимозависимы. Необходимо вручную контролировать эту зависимость в нашем ПО. Подробнее о взаимосвязи потоков можно узнать в инструкции к камере.","With MJPEG and the max. resolution (1280x960), the max. frame rate is 15 fps. When multiple video streams are used simultaneously, their available resolutions are interrelated. In our software, you must manage this interrelation manually. For more details on how the streams are interrelated, refer to the camera's guide. "]
["EasyN","EasyN F-series","Camera ","4.37.2.38","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+.",null,"+.","-","+","+.","+",null,"+","-","1. Камеры EasyN FM166I, FS-613A-M136 интегрированы как линейка EasyN F-series, весь линейный ряд не тестировался.\n2. Тревога от встроенного детектора длится ровно минуту независимо от фактической продолжительности события - особенность камеры.\n3. Макс fsp: 640x480 - 15 fps | 320x240 - 20 fps | 160x120 - 30 fps ","1. Camera EasyN FM166I has been integrated as , EasyN F-series, although the other models from the range have not been tested yet.\n2. The alarms from embedded detection go off and remain active for 60 seconds sharp, regardless of the actual duration of an alarm event. This is a limitation of the camera.\n3. Max fps: 640x480 - 15 fps | 320x240 - 20 fps | 160x120 - 30 fps "]
["EasyN","EasyN HV10DI","Camera ","V3.4.6.1.1-20111227","1",{"$nulls":4},"+",null,null,"1280x720 ","1280x720","640x352","+",null,"+",null,"+","+",null,null,"motion detection;","-","Поиском камера обнаруживается как \"EasyN ZNY10.22\" ","The device is identified as EasyN ZNY10.22. "]
["Eneo","Eneo GXB-1710M-IR","Camera ","2.07","1",null,null,"+","+","+",null,null,"1920x1080","800x450","480x270","+",null,null,"-",{"$nulls":5},"+","Есть проблема с применением разрешений (при переходе к более высокому разрешению видео может не измениться), проблема производителя","There is an issue with higher resolutions. When you set one, video may stay the same. This is a problem of the camera itself."]
["Eneo","Eneo GXB-1720MIR / Eneo GXD-1720MIR","Camera","1.22","1","+","3","+","+","+",null,null,"from WEB","from WEB","from WEB","+",null,"-","-","-","-","-","-","-","+",null,null,"new"]
["Eneo","Eneo NLD-1422","Camera ","2.9.5-T1_release","1",null,null,"+","+","+",null,null,"704x576","640x480","320x240","+",null,null,"-","+",{"$nulls":4},"+"]
["Eneo","Eneo NXC-1403F03 ","Camera ","1.7.0-T5_release","1",null,null,"+","+","+",null,null,"1600x1200","800x600 ","640x480","+",null,"-","-","-","-","-","-","-","+"]
["Eneo","Eneo NXC-1602M","Camera ","2.2.107","1",null,null,"+",null,"+",null,null,"1920x1080(H264) / 640x480(MJPEG)","1152x864(H264) / 352x288(MJPEG)","640x480(H264) / 320x240(MJPEG)","+",null,null,"-",{"$nulls":5},"+"]
["Eneo","Eneo PXB-2020M-IR","Camera ","4.17-72-fs","1",null,null,"+",null,"+",null,null,"1280x720","640x352","640x352","+",{"$nulls":7},"-","+"]
["Eneo","Eneo PXD-1010F02 / PXD-1020F02 ","Camera ","vr20130122NSA ","1",null,null,"+",null,"+",null,null,"1920x1080 ","1024x768","640x480","+",null,"-","-","-","-","-","-","motion detection;","+","1) Разрешение на втором потоке не может быть больше, чем на первом.","The resolution for stream 2 should be lower than or equal to the resolution setting for stream 1."]
["Eneo","Eneo PXD-2018PTZ1080","Camera ","vr20121016NSA ","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":3},"motion detection;","+"]
["Eneo","Eneo PXD-5360F01IR / PXD-5362F01IR ","Fisheye Camera","vr20130515NSA ","1",null,null,"+",null,"+",null,null,"H.264: 2592x1944; MJPEG: 1920x1080","1024x768","640x480","+",{"$nulls":8},"+","1. Значения \"Поворот на 90° по часовой стрелки\" и \"Поворот на 90° против часовой стрелки\" настройки Тип отображения не работают при разрешении CIF (352x288)\n2. Значения настроек \"Алгоритм компрессии\", \"Аудиокодек\" и \"Битрейт\" для объектов \"Микрофон\" и \"Динамик\" должны совпадать для корректной работы обоих объектов в ПО Axxon.\n","1. \"90 ° clockwise rotation\"and \"90 ° counter-clockwise rotation\" (Type of mapping) doesn't work for 352x288 resolution. 2. The setting values of \"Compression algorithm \", \" Audio Codec \" and \" Bitrate \" for Microphone and Speaker must be the same for the correct operation of both objects in Axxon software ."]
["Etrovision","Etrovision EV3151A","Camera ","1.9.9","1",null,null,"+","+.","+",null,null,"720x576","720x576","352x288","+",null,"+","-","+","+","+",null,"-","+","1. Само устройство с прошивкой 1.9.9 в разрешении 720x576 выдает MPEG-4 видео с \"плавающим\" fps.\n2. Телеметрию можно настроить только в ПО Intellect (протокол телеметрии IPCamera)","1. 1.9.9 firmware: At 720x576 resolution and MPEG-4, the device sends video with a variable frame rate. \n2. Telemetry can be configured only in Intellect (the IPCamera protocol)."]
["Etrovision","Etrovision EV8150A","Camera ","2.0.3 Build 20110513","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",null,"+","-","+","+","+",null,"-","+","1. Само устройство с прошивкой 1.9.9 в мегапиксельном разрешении ввыдает искаженное H.264 видео\n\n ","1. 1.9.9 firmware: With megapixel resolutions and H.264, the device sends distorted video.\n\n "]
["Etrovision","Etrovision EV8x8xA","Camera ","1.1.2","1",null,null,"+","+","+",null,null,"1280x1024","1024x768","640x480","+",null,"+.","-","+","+","+",null,"+","+"]
["Etrovision","Etrovision EV8x8xF","Camera ","1.1.2","1",null,null,"+","+","+",null,null,"2592x1920(MJPEG, H.264); 1920x1080(MPEG-4)","1024x768","640x480","+",null,"+.","-","+","+","+",null,"+","+","1. В ПО Axxon под разрешениями 5МР, 3МР и 1080р в кодеке MPEG-4 подразумевается одно и то же фактическое разрешение 1920х1080.\n2. Максимальный fps зависит от значения настройки \"Max. Resolution\" в веб-интерфейсе ","1. In the AxxonSoft software, with the MPEG-4 codec, the 5MP, 3MP, and 1080p resolutions all mean the same actual resolution of 1920x1080. \n2. The max. resolution depends on Max. Resolution settings in web interface.\n"]
["Etrovision","Etrovision EV8x8xQ","Camera ","1.1.2","1",null,null,"+","+","+",null,null,"2048x1536 (H264 / MJPEG) / 1920x1080 (MPEG4)","1024x768","640x480","+",null,"+.","-","+","+","+",null,"+","+"]
["Etrovision","Etrovision EV8x8xU","Camera ","1.1.2","1",null,null,"+","+","+",null,null,"1920x1080","1024x768","640x480","+",null,"+.","-","+","+","+",null,"+","+"]
["ETZ","ETZ DVR 9116 (I/O PTZ module)","I/O PTZ Module","auto","16",{"$nulls":7},"-","-","-",{"$nulls":4},"+","+","+",null,null,"-","1. Спец. интеграция. Видео- и аудиоканалы не реализованы. Работают только Лучи, Реле и Телеметрия.","2. The maximum fps depends on value of control \"Max. Resolution\" in the web interface"]
["Euresys","Euresys Picolo .net HD4 IP Video Encoder (ONVIF)","Encoder ","4.0","4",null,null,"+",null,"+",null,null,"1920x1080","960x540","640x360",{"$nulls":9},"+"]
["EverFocus","EverFocus EAN3120 (Onvif)","Camera ","1.0.17","1",null,null,"+",null,"+",null,null,"1280x1024 (MJPEG) / 720x576 (H264)","1024x768 (MJPEG) / 640x480 (H264)","640x480 (MJPEG) / 320x240 (H264)","+",null,"+","-",null,"-","+",null,"+.","+","Камера интегрирована только по протоколу Onvif.\nЧтобы получать видео в формате H264 с такими же разрешениями, как и MJPEG, нужно в веб-интерфейсе для первого потока выбрать кодек H264.","The camera is integrated only according to the Onvif protocol. \nTo receive video in the H264 format with the same permissions, as well as MJPEG, it is necessary in the web interface for the first flow to select the H264 codec"]
["EverFocus","EverFocus EAN3220 (Onvif)","Camera ","1.0.17","1",null,null,"+",null,"+",null,null,"1920x1080 (MJPEG) / 720x576 (H264)","1024x768 (MJPEG) / 640x480 (H264)","640x480 (MJPEG) / 320x240 (H264)","+",null,"+","-",null,"-","+",null,"+.","+","Камера интегрирована только по протоколу Onvif.\nЧтобы получать видео в формате H264 с такими же разрешениями, как и MJPEG, нужно в веб-интерфейсе для первого потока выбрать кодек H264.","The camera is integrated only according to the Onvif protocol. \nTo receive video in the H264 format with the same permissions, as well as MJPEG, it is necessary in the web interface for the first flow to select the H264 codec"]
["EverFocus","EverFocus EAN750","Camera ","1.1.0.5","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","352x288","+",null,"+","-",null,"+.","+",null,"-","-","1. Любое изменение настроек (разрешение, качество, fps) вызывает ребут самой камеры.\n2. Луч работает только на замыкание","1. Any change in the settings (resolution, quality, or frame rate) causes the camera itself to restart. \n2. The sensor goes off when you close it. "]
["EverFocus","EverFocus EAN850A","Camera ","1.2.5","1",null,null,"+","+","+",null,null,"704x560","640x480","320x240","+",null,"-","-",null,"+","+",null,"-","+","1. При активации одновременно 3-4 стриммингов видео с камеры может пропадать. Особенность интеграции. Исправляется отключением \"лишних\" стриммингов в веб-интерфейсе камеры","1. If 3–4 streams are enabled at the same time, video may disappear. This is how integration was done. To correct this, go to the camera's web interface and disable \"extra\" streams."]
["EverFocus","EverFocus EDN800","Camera ","1.1.0","1",null,null,"+","+","+",null,null,"704x576","640x480","320x240","+",{"$nulls":7},"-","+"]
["EverFocus","EverFocus EPN3600","Camera ","1.0.0","1",null,null,"+","+","+",null,null,"720x560","640x480","320x240","+",null,"-","-","+","+","+",null,"-","+"]
["EverFocus","Everfocus EPN4122 / EPN4220 / EPN4220i (PSIA) ","Camera ","1.0.3","1",null,null,"+",null,"+",null,null,"from WEB ","from WEB ","from WEB ","+",null,"+",{"$nulls":6},"+"]
["EverFocus","EverFocus EVS100 encoder","Encoder ","1.1.0.5","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","352x288","+",null,"+",null,"+","+","+",null,null,"-","1. луч работает только на замыкание","1. The sensor goes off when you close it."]
["EverFocus","EverFocus EVS200 encoder","Encoder ","1.0.6","2",null,null,"+","+","+",null,null,"704x576(H.264) / 352x288 (MJPEG) / 352x288 (MPEG-4)","640x480(H.264) / 352x288 (MJPEG) / 352x288 (MPEG-4)","320x240","+",null,"+","+",null,"+","+",null,"-","+","1. 2 канала, на каждом по 2 стримминга\n2. телеметрия может быть реализована только в ПО Intellect, и не может быть реализована в ПО AxxonNext/Next. Чтобы она заработала, необходимо в веб-интерфейсе выставить нужный протокол+скорость, затем то же самое установить в Intellect.","1. 2 channels, each has 2 streams.\n2. Telemetry may be used only in Intellect, not in AN. To make it work, go to the web interface and set the required protocol and baud rate; then go to Intellect and set the same there. "]
["EverFocus","EverFocus EZN3260 (Onvif)","Camera ","1.0.17","1",null,null,"+",null,"+",null,null,"1920x1080 (MJPEG) / 720x576 (H264)","1024x768 (MJPEG) / 640x480 (H264)","640x480 (MJPEG) / 320x240 (H264)","+",null,"+","-","-","-","+",null,"-","+","Камера интегрирована только по протоколу Onvif. \nЧтобы получать видео в формате H264 с такими же разрешениями, как и MJPEG, нужно в веб-интерфейсе для первого потока выбрать кодек H264.","The camera is integrated only according to the Onvif protocol. \nTo receive video in the H264 format with the same permissions, as well as MJPEG, it is necessary in the web interface for the first flow to select the H264 codec"]
["EverFocus","Everfocus EZN3260 / EDN3260 / EHN3260 (PSIA)","Camera ","1.0.17","1",null,null,"+",null,"+",null,null,"from WEB ","from WEB ","from WEB ","+",null,"+",{"$nulls":6},"+"]
["EverFocus","EverFocus EZN850","Camera ","1.1.35","1",null,null,"+","+","+",null,null,"704x560","640x480","320x240","+",{"$nulls":3},"+","+","+",null,"-","+"]
["eVidence","eVidence Apix - 10ZBox / M1","Camera ","p20101125NS","1",null,null,"+","+","+",null,null,"1280x960","640x480","320x240","+",null,"+","-","+","+","+",null,"+","+","В максимальном разрешении (1280x960) максимальная частота кадров - 12.5 fps.Черезх Onvif работает получение видео с настройками качества и разрешения и звук.Телеметрия: камера не поворотная, но с трансфокальным фокусным объективом. Зум и фокус в нашем ПО поддержаны.Доступны следующие комбинации кодеков и разрешений в потоках:0.MJPEG + 1.MPEG4/H264MJPEG + MPEG4MJPEG + H264При выборе максимального разрешения 1280х960 необходимо выбирать его в обоих потоках.1.MPEG4/H264 + 2.H264-2H264 + H264-2Разрешение 1280х720 в кодеке H264-2 доступно только в том случае, если в кодеке H264 также выбрано разрешение 1280х720.","At maximum resolution (1280x960), the max. frame rate is 12.5 fps. Via the ONVIF protocol, the following work: receiving video, setting the quality and resolution, and receiving audio Telemetry: this is not a PTZ camera, but it has a zoom lens. Our software supports zoom and focus. The available combinations of codecs and resolutions are: 0. MJPEG + 1. MPEG4/H264MJPEG + MPEG4MJPEG + H264. To select the max. resolution (1280x960), you must select it in both streams. 1. MPEG4/H264 + 2. H264-2H264 + H264-2. For the H.264-2 codec, 1280х720 resolution is available only if the same resolution is selected for the H.264 codec."]
["eVidence","eVidence Apix - 12ZDome / D1","Camera ","p20110825NS","1",null,null,"+",null,"+",null,null,"720x576","720x576","352x288","+",null,"+","-","+","+","+",null,null,"+","На камере есть 4 луча и 1 реле. Однако в комплекте с тестовым устройством был кабель, не имеющий тревожных входов/выходов. В инструкции к камере сказано, что кабель с тревожными разъемами идет только в комплекте с \"Outdoor Dome Camera\" - видимо, имеется ввиду модель с индексом \"EXT\". Хотя лучи и реле есть у обеих моделей. Проверка работы тревожных входов и выходов производилась с помощью ручного подключения обычных проводов к нужным разъемам.В Интеллекте не работает изменение частоты кадров в минимальном разрешении 352х288 в кодеке H264 - особенность камеры.В Интеллекте минимальное и среднее значение частоты кадров совпадают - особенность интеграции.","The camera has 4 sensors and 1 relay. However, the trial device came with a cable that had no alarm input/output ports. The camera's guide says that the cable with alarm connectors comes only with the Outdoor Dome Camera: they most likely mean the model whose name contains the string \"EXT\", although both models have sensors and relays. The alarm inputs/outputs were tested by manually connecting ordinary cables to the right connectors. In Intellect, with the min. resolution (352x288) and H.264 codec, frame rate control does not work. This is a limitation of the camera itself. In Intellect, the min. and medium frame rates are the same: this is how the integration was done. "]
["eVidence","eVidence Apix - 18ZBox / M2","Camera ","d20110729NSA","1",null,null,"+",null,"+",null,null,"1920x1080","800x600","640x480","+",null,"-","-","+","-","-",null,"-","+"]
["eVidence","eVidence Apix - 18ZDome / M2","Camera ","st20120217NSA","1",null,null,"+",null,"+",null,null,"1920x1080","800x600","640x480","+",null,"-","-","+","-","-",null,"+","+"]
["eVidence","eVidence Apix - 20ZDome / M2-ext","Camera","st20130610NSA","1","+","2","+",null,"+",null,null,"1920x1080","1024x768","640x480",null,null,"+","-","+","+","+","-","motion detection","+",null,null,"new"]
["eVidence","eVidence Apix - 18ZDome / M2-ext","Camera ","st20130924NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480",null,null,"+","+.","+","+","+",null,"motion detection","+"]
["eVidence","eVidence Apix - 36ZDome / D1 ","Camera ","p20110825NS","1",null,null,"+",null,"+",null,null,"720x576","720x576","352x288","+",null,"+","-","+","+","+",null,null,"+","На камере есть 4 луча и 1 реле. Однако в комплекте с тестовым устройством был кабель, не имеющий тревожных входов/выходов. В инструкции к камере сказано, что кабель с тревожными разъемами идет только в комплекте с \"Outdoor Dome Camera\" - видимо, имеется ввиду модель с индексом \"EXT\". Хотя лучи и реле есть у обеих моделей. Проверка работы тревожных входов и выходов производилась с помощью ручного подключения обычных проводов к нужным разъемам.В Интеллекте не работает изменение частоты кадров в минимальном разрешении 352х288 в кодеке H264 - особенность камеры.В Интеллекте минимальное и среднее значение частоты кадров совпадают - особенность интеграции. ","The camera has 4 sensors and 1 relay. However, the trial device came with a cable that had no alarm input/output ports. The camera's guide says that the cable with alarm connectors comes only with the Outdoor Dome Camera: they most likely mean the model whose name contains the string \"EXT\", although both models have sensors and relays. The alarm inputs/outputs were tested by manually connecting ordinary cables to the right connectors. In Intellect, with the min. resolution (352x288) and H.264 codec, frame rate control does not work. This is a limitation of the camera itself. In Intellect, the min. and medium frame rates are the same: this is how the integration was done. "]
["eVidence","eVidence Apix - Box / M1","Camera ","p20100310NS ","1",null,null,"+","+","+",null,null,"1280x960","640x480","320x240","+",null,"+","-",null,"+","+",null,"-","+","1. Поиск находит камеру как Dynacolor NH061\n2. Во время получения видео с обоих видеопотоков доступны следующие комбинации кодеков:\nMJPEG + H264\nMJPEG + MPEG4\nH264 + H264-2\n3. Для получения видео с обоих видеопотоков действуют следующие ограничения:\n- Различные разрешения в потоках поддерживаются только при комбинации H264 + H264-2. \n- В остальных комбинациях разрешение будет одинаковым для обоих потоков и задает оно из второго потока.\n- Для кодека H264-2 постоянно недоступно максимальное разрешение 1280х960, а разрешение 1280х720 доступно только в том случае, когда для кодека H264 в этот момент выставлено это же разрешение 1280х720.\n4. Реле камеры по-умолчанию работает в режиме \"нормально-замкнуто\". Особенность устройства, при необходимости можно изменить через web-интерфейс.","1. Search detects the camera as Dynacolor NH061. \n2. When you use both streams, the following codec combinations are available: \nMJPEG + H264\nMJPEG + MPEG4\nH264 + H264-2. \n3. When you use both streams, the following limitations apply: \n- Different resolutions for the streams are supported only for the H264 + H264-2 combination. \n- For all the other combinations, the resolutions will be the same for both streams; to set this common resolution, set the resolution for the second stream. \n- For the H264-2 codec, the max. resolution (1280x960) is never available, and the 1280x720 resolution is available for this codec only when the same resolution (1280x720) is set for the H264 codec. \n4. By default, the camera's relay works in Normally Closed mode. This is a feature of the device; if necessary, you can change it in the web interface. "]
["eVidence","eVidence Apix - Box / M2","Camera ","p20110824BNS","1",null,null,"+",null,"+",null,null,"1920x1080","1280x720(MJPEG) / 1920x1080(H264)","352x288(MJPEG) / 1280x720(H264)","+",null,"+","-","-","+","+",null,"+","+","В максимальном разрешении 1920х1080 максимальная частота кадров 12.5 fps.При одновременном использовании 2х потоков доступны следующие комбинации:H264 (1280x720) + MJPEG (352x288, 720x576)H264 (1280x720) + H264-2 (352x288, 720x576)","At maximum resolution (1280x1080), the max. frame rate is 12.5 fps. When you use two streams at the same time, the following combinations are available: H264 (1280x720) + MJPEG (352x288, 720x576) H264 (1280x720) + H264-2 (352x288, 720x576)"]
["eVidence","eVidence Apix - Box / M2 WDR","Camera","st20131230NSX","1",null,null,"+","-","+","-","-","1920x1080 (H.264) / 1280x1024 (MJPEG)","1024x768","640x480","+","-","+","+","-","+","+","-","motion detection","+","Доступность настроек экспозиции зависит от текущего значения настройки TV System (интегрирована в ПО Axxon как \"ТВ-стандарт\").При изменении TV System настройки видео на камере сбрасываются на дефолтные (особенность камеры). Поэтому для корректной работы камеры после смены ТВ-стандарта требуется через веб-интерфейс привести настройки видео (кодек, разрешение) в соответствие с текущими настройками в ПО Axxon.","Availability of exposure settings depends on the current value of the TV System setting (integrated in Axxon as TV standard). When the TV System setting is changed, settings of camera video become default (camera’s feature). For proper camera operation after changing the TV standard setting, video settings (codec, resolution) are to be in accordance with current settings in Axxon."]
["eVidence","eVidence Apix - Box / M2 Lite","Camera ","st20130924NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",null,"+","+.",null,"+","+",null,"motion detection","+"]
["eVidence","eVidence Apix - Box / M3","Camera ","st20130129NSA","1",null,null,"+",null,"+",null,null,"1920x1080 (MJPEG) / 2048x1536 (H.264)","1024x768","1024x768","+",null,"+.","+",null,"+.","+",null,"motion detection","+","Функционал: лучи, реле, аудиовход, аудиовыход в ПО Интеллект необходимо добавлять вручную.","Features rays, relays, audio Input and audio Output required to add manually."]
["eVidence","eVidence Apix - Box / M5","Camera ","st20120217NSA","1",null,null,"+",null,"+",null,null,"1920x1080","MJPEG: 800x600 | H.264: 1920x1080","MJPEG: 640x480 | H.264: 1920x1080","+",null,"-","-",null,"-","-",null,"-","+"]
["eVidence","eVidence Apix - Bullet / M2","Camera ","p20120308BNS","1",null,null,"+",null,"+",null,null,"1920x1080","1280x1024","640x480","+",null,"-","-",null,"-","-",null,"-","+","1. В Интеллекте при смене грабера с H.264 на MJPEG (стандартное разрешение, настройка цвет выключено, первое подключение к устройству - черно-белое изображение) - цвет меняться не будет","1. In Intellect, if you change the grabber from H.264 to MJPEG (standard resolution, color off, first connection to device is black and white) - the color will not change."]
["eVidence","eVidence Apix - Bullet / M2 Lite","Camera "," st20130129NSA ","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",null,"+","+.","-","+","+",null,"motion detection;","+"]
["eVidence","eVidence Apix - Bullet / M2 Lite 279","Camera ","st20120713NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1280x1024","640x480","+",null,"+","+",null,"+","+",null,"motion detection;","+"]
["eVidence","eVidence Apix - Compact / M1","Camera ","VB1.0.26_ST","1",null,null,"+","+","+",null,null,"1280x800","640x480","320x240","+",null,"+.","+.",null,"+","+",null,"motion detection; ","+","1. Картинка на камере периодически замирает на несколько секунд при физическом воздействии (тряска). В веб интерфейсе наблюдается тот же эффект.\n2. В ПО Axxon камера обнаруживается поиском как Apix-Dome/M2 Lite.\n3. В ПО ITV камера обнаруживается поиском как FineCCTV.","1. When you subject the camera to physical impact, i.e. you shake it, video may freeze for a few seconds. The same happens in the web interface.\n2. In the AxxonSoft products, the camera is identified as Apix-Dome/M2 Lite.\n3. In the AxxonSoft products, the camera is identified as FineCCTV."]
["eVidence","eVidence Apix - Dome/ E2 LED 309","Camera","VC1.0.14_ST","1",null,null,"+","-","+","-","-","1920x1080","640x480","320x240","+","-","+","+","-","+","+","-","motion detection","+","Диапазон значений битрейта зависит от значения FPS","Bitrate range depends on FPS."]
["eVidence","eVidence Apix - Dome/ E2 309","Camera","VC1.0.14_ST","1",null,null,"+","-","+","-","-","1920x1080","640x480","320x240","+","-","+","+","-","+","+","-","motion detection","+","Диапазон значений битрейта зависит от значения FPS","Bitrate range depends on FPS."]
["eVidence","eVidence Apix - Dome / M2 LED","Camera ","V1.0.16_ST","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+","-",null,"+","+",null,"-","+","В Интеллекте поиск находит камеру как FineCCTV IPCam.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров) - в веб-интерфейсе называется \"Input resolution\". В AxxonNext/Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе. ","In Intellect, search detects the camera as FineCCTV IPCam. The camera has the Video Parameters option (max. resolution and max. frame rate); in the web interface, this is called Input Resolution. In AN, you must make sure that there is no conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value. "]
["eVidence","eVidence Apix - Dome / M2 Lite","Camera ","V1.0.26_ST","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+","-",null,"+","+",null,"+","+","В Интеллекте поиск находит камеру как FineCCTV IPCam.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров) - в веб-интерфейсе называется \"Input resolution\". В AxxonNext/Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе","In Intellect, search detects the camera as FineCCTV IPCam. The camera has the Video Parameters option (max. resolution and max. frame rate); in the web interface, this is called Input Resolution. In AN, you must make sure that there is no conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value."]
["eVidence","eVidence Apix - MiniDome / M143","Camera ","p20110816ANS","1",null,null,"+",null,"+",null,null,"1280x1024","1280x720 (MJPEG) / 1280x1024 (H264)","352x288 (MJPEG) / 1280x720 (H264)","+",null,"+",{"$nulls":5},"+","+","При одновременном использовании 2х потоков доступны следующие комбинации:H264 (1280x720) + MJPEG (352x288, 720x576)H264 (1280x720) + H264(352x288, 720x576)","When you use two streams at the same time, the following combinations are available: H264 (1280x720) + MJPEG (352x288, 720x576) H264 (1280x720) + H264-2 (352x288, 720x576)"]
["eVidence","eVidence Apix - MiniDome / M2 Lite 40","Camera ","st20120910NSA","1",null,null,"+",null,"+",null,null,"1920x1080","800x600","640x480","+",null,"+",{"$nulls":5},"motion detection, tampering detection","+","В максимальном разрешении (1920х1080) максимальная частота кадров 12 fpsДоступны следующие комбинации кодеков и разрешений в потоках:0.H264 (1280x720) + 1.MJPEG (320x240...1280x720)0.H264 (1280x720) + 2.H264-2","At maximum resolution (1920x1080), the max. frame rate is 12 fps. The available combinations of codecs and resolutions are: 0. H264 (1280x720) + 1. MJPEG (320x240...1280x720) 0.H264 (1280x720) + 2. H264-2."]
["eVidence","eVidence Apix - VDome / M1","Camera ","p20100310NS","1",null,null,"+","+","+",null,null,"1280x960","640x480","320x240","+",null,"+","-",null,"+","+",null,"-","+","Поиск находит камеру как InMotion HD-WDRВо время получения видео с обоих видеопотоков доступны следующие комбинации кодеков:MJPEG + H264MJPEG + MPEG4H264 + H264-2Для получения видео с обоих видеопотоков действуют следующие ограничения:Различные разрешения в потоках поддерживаются только при комбинации H264 + H264-2.В остальных комбинациях разрешение будет одинаковым для обоих потоков и задает оно из второго потока.Для кодека H264-2 постоянно недоступно максимальное разрешение 1280х960, а разрешение 1280х720 доступно только в том случае, когда для кодека H264 в этот момент выставлено это же разрешение 1280х720.Реле камеры по-умолчанию работает в режиме \"нормально-замкнуто\". Особенность устройства, при необходимости можно изменить через web-интерфейс.","Search detects the camera as InMotion HD-WDR. When you use both streams, the following codec combinations are available: MJPEG + H264MJPEG + MPEG4H264 + H264-2. When you use both streams, the following limitations apply: Different resolutions for the streams are supported only for the H264 + H264-2 combination. For all the other combinations, the resolutions will be the same for both streams; to set this common resolution, set the resolution for the second stream. For the H264-2 codec, the max. resolution (1280x960) is never available, and the 1280x720 resolution is available for this codec only when the same resolution (1280x720) is set for the H264 codec. By default, the camera's relay works in Normally Closed mode. This is a feature of the device; if necessary, you can change it in the web interface."]
["eVidence","eVidence Apix - VDome / M1 EXT 3312","Camera ","p20110824NS","1",null,null,"+","+","+",null,null,"1280x960","640x480","320x240","+",null,"+","-",null,"+","+",null,"+","+","Доступны следующие комбинации кодеков и разрешений в потоках:0.MJPEG + 1.MPEG4/H264MJPEG + MPEG4MJPEG + H264При выборе максимального разрешения 1280х960 необходимо выбирать его в обоих потоках.1.MPEG4/H264 + 2.H264-2H264 + H264-2Разрешение 1280х720 в кодеке H264-2 доступно только в том случае, если в кодеке H264 также выбрано разрешение 1280х720.Ограничение частоты кадров в 12.5 fps:Во всех кодеках в максимальном разрешении1280х960В потоке H264-2 в разрешении 1280х720В потоке H264 в разрешении 1280х720 при использовании одновременно H264+H264-2","The available combinations of codecs and resolutions are: 0. MJPEG + 1. MPEG4/H264MJPEG + MPEG4MJPEG + H264. To select the max. resolution (1280x960), you must select it in both streams. 1. MPEG4/H264 + 2. H264-2H264 + H264-2 For the H.264-2 codec, 1280х720 resolution is available only if the same resolution is selected for the H.264 codec. The frame rate is limited to 12.5 fps for all codecs, at max. resolution (1280х960) For the H.264-2 codec, at 1280x720 resolution For the H.264 codec, at 1280x720 resolution when you use H.264 and H.264-2 at the same time"]
["eVidence","eVidence Apix - VDome / M2 LED","Camera ","p20110121BNS","1",null,null,"+",null,"+",null,null,"1920x1080","1280x1024","1280x720","+",null,"+","-",null,"+","+",null,"+","+","В MJPEG в разрешении 1920х1080 максимальная частота кадров ~15 fpsЧерез Onvif работает поиск, видео с настройками и звук.Видеопотоки сильно зависят друг от друга. Правильную комбинацию потоков/кодеков/разрешений нужно выбирать самостоятельно.Таблица комбинаций потоков в AxxonNext/Next: \nКодек в 1-м потоке\nКодек во 2-м потоке\nДоступные разрешения в 1-м потоке\nДоступные разрешения во 2-м потоке\nMJPEG\n-\n320x240...1920x1080\n-\n\nMJPEG\nH.264\n320x240...1280x720\n1280x720\n\nMJPEG\nH.264-2\n-\n-\nH.264\n-\n\n320x240...1920x1080\n-\n\nH.264\nH.264\n-\n-\n\nH.264\nH.264-2\n1280x720\n320x240...720x576\n-\nH.264\n-\n1280x720 - H.264-2 -\n320x240...720x576","With MJPEG and the maximum resolution (1920x1080), the max. frame rate is around 15 fps. Via the ONVIF protocol the following work: search, video (+ settings), and audio. Video streams are very interdependent. You have to select the right combination of streams/codecs/resolutions yourself. The stream combination table for AN: \nCodec (1st stream)\nCodec (2nd stream)\nResolutions available (1st stream)\nResolutions available (2nd stream)\nMJPEG\n-\n320x240...1920x1080\n-\n\nMJPEG\nH.264\n320x240...1280x720\n1280x720\n\nMJPEG\nH.264-2\n-\n-\nH.264\n-\n\n320x240...1920x1080\n-\n\nH.264\nH.264\n-\n-\n\nH.264\nH.264-2\n1280x720\n320x240...720x576\n-\nH.264\n-\n1280x720 - H.264-2 -\n320x240...720x576"]
["eVidence","eVidence Apix - ViCoder","Encoder ","p20110704NS","1",null,null,"+",null,"+",null,null,"PAL: 720x576 | NTSC: 720x480","PAL: 720x576 | NTSC: 720x480","PAL: 352x288 | NTSC: 352x240","+",null,"-","-","-","-","-",null,"-","+","1. Разрешения и свето-передача зависят от ТВ-стандарта подключенной аналоговой камеры (нужно перезагрузить устройство, чтобы оно переменило ТВ-стандарт).","1. Resolutions and color rendering depend on the TV standard of the analog camera connected. Restart the device to switch the TV standard.\n"]
["EVS","EVS VEC-255-IP / VEN-255-IP","Camera","5.00.00.08.2.1","1",null,null,"+","+","+",null,null,"1600x1200(MJPEG/H264) / 1280x960(MPEG4)","1280x960","from WEB","+",null,"-","-","-","-","-","-","-","+","С комбинацией разрешений D1:D1 может не идти видео","With a combination of permissions D1: D1 may not be video"]
["EVS","EVS VEC-355-IP / VEN-355-IP","Camera","5.00.00.08.3.1","1",null,null,"+","+","+",null,null,"2048x1536(MJPEG/H264) / 1280x960(MPEG4)","1600x1200(MJPEG/H264) / 1280x960(MPEG4)","720x480(MPEG4/H264) / 640x352(MJPEG)","+",null,"-","-","-","-","-","-","-","+"]
["EVS","EVS VEC-555-IP / VEN-555-IP","Camera","5.00.00.08.5.1","1",null,null,"+","+","+",null,null,"From Web(MJPEG) / 2592x1920(H264) / 1280x960(MPEG4)","1600x1200(MJPEG/H264) / 1280x960(MPEG4)","720x480(MPEG4/H264) / 640x352(MJPEG)","+",null,"-","-","-","-","-","-","-","+","Прошивка 5.00.00.08.5.1: передача видео в MJPEG с разрешением 5 MP не поддерживается камерой. С комбинацией разрешений D1:D1 может не идти видео","Firmware 5.00.00.08.5.1: camera with MJPEG codec and resolution 5MP doesn't transmit video. With a combination permits D1: D1 may not be video."]
["FineCCTV","FineCCTV CDV-3V930HU","Camera ","3.2.62","1",null,null,"+","+",{"$nulls":3},"720x576","704x576","352x288","+",{"$nulls":4},"-",{"$nulls":3},"+"]
["FineCCTV","FineCCTV CDV-3VM501 ","Camera ","V1.0.40_F","1",null,null,"+",null,"+",null,null,"1600x1200 ","800x600","640x480","+.",{"$nulls":7},"motion detection; ","+"]
["FlexWatch","FlexWatch FW-1178-PE ","Camera ","4.10-06","1",null,null,"+",null,"+",null,null,"720x576","704x576","352x288","+",null,null,"-","+",{"$nulls":3},"-","+","1. C текущей прошивкой 4.10-06 Зум и Фокус очень чувствительные на самом устройстве и меняются очень значительно даже при однократном нажатии на кнопки/рычажки органов управления.","1. With the current (4.10-06) firmware, zoom and focus are very sensitive on the device itself: their values change very significantly even if you click the relevant button only once. "]
["FlexWatch","FlexWatch FW-117x-Dx","Camera ","4.18-B1-ds","1",null,null,"+",null,"+",null,null,"720x480","704x480","352x240","+",null,null,"-",{"$nulls":4},"-","+"]
["FlexWatch","FlexWatch FW-117x-Fx","Camera","4.18-B1-ds","1",null,null,"+","-","+","-","-","640х352","640х352","320х176","+","-","-","-","-","-","-","-","-","+"]
["FlexWatch","FlexWatch FW-117x-Mx","Camera ","4.18-B1-ds ","1",null,null,"+",null,"+",null,null,"1280x1024","704x480","320x240","+",null,null,"-",{"$nulls":4},"-","+"]
["FlexWatch","FlexWatch FW-3470 (NVR)","NVR","4.06-04","4",null,null,"+",null,"+",null,null,"704x576","704x288","352x288","+",{"$nulls":7},"-","+","Настройки кодека, разрешения, частоты кадров в AxxonNext/Next применяются для всех каналов сразу.","In AN, the codec, resolution, and frame rate settings are applied for all the channels at once. "]
["FlexWatch","FlexWatch FW-5071 (NVR)","NVR","4.10","16",null,null,"+","+","+",null,null,"auto","auto","auto",null,null,"-",null,"-","-","-",null,null,"+","Интегрировано только получение видеоПоиск находит устройство в сети, но правильную прошивку нужно выбрать самостоятельно.","Only video receipt is integrated. Search detects the device on the network, but you have to select the right firmware yourself."]
["FlexWatch","FlexWatch FW-5470C (NVR)","Encoder","4.06-04","4",null,null,"+.","-","+",null,null,"704x576","704x288","352x288","+",null,"+","-","+","+","+","-","-","+","1. В ПО ITV реализована только подержка аналоговых камер (4 канала), подключаемых к устройству.\n2. Телеметрия настраивается и работает в ПО ITV через \"протокол\" IPCamera","1. In AxxonSoft products, only digital cameras (4 channels), connected to the devices, could be supported.\n2. You should tune telemetry in AxxonSoft products through IPCamera protocol."]
["FlexWatch","FlexWatch FW-5870C (NVR)","NVR","4.07-17","8",null,null,"+",null,"+",null,null,"704x576","704x288","352x288","+",null,"-","-","+","+","+",null,"-","+","1. В ПО ITV реализована только подержка аналоговых камер (8 каналов), подключаемых к устройству.\n2. Телеметрия настраивается и работает в ПО ITV через \"протокол\" IPCamera\n3. *использование устройства в Intellect 4.7.8.release не предусмотрено* ","1. The AxxonSoft software implements only support for analog cameras (8 channels) connected to the device. \n2. The telemetry functionality can be configured and used only via the IPCamera \"protocol\".\n3. *in the Intellect 4.7.8 release, the device is not used* "]
["G4S","G4S GIU03-VIR","Camera ","1.0/1.0.0","1",null,null,"-",null,"+",null,null,"from WEB","from WEB","from WEB","-",null,"+.","-",{"$nulls":4},"-","-","Для получения видео в продукте нужно указать порт \"Watch\" из настроек в веб-интерфейсе","Select the Watch port in the camera's web interface."]
["Ganz","Ganz MP2DN","Camera ","65140","1",null,null,"+",null,"+",null,null,"1600x1200","1600x1200","800x600","+",{"$nulls":4},"-","+",null,"-","+","1. ограничение fps самой камеры:\n MJPEG:\n -при 1600х1200 fps=12-20 (в зависимости от качества)\n -при 800x600 fps =~22\n H.264\n - при любом разрешении fps=~23","1. The camera itself has frame rate limits:\n MJPEG:\n -at 1600х1200, fps=12–20 (depending on quality)\n -at 800x600, fps = around 22\n H.264\n - at any resolution, fps= around 23"]
["Ganz","Ganz ZN-B1MAP","Camera ","ZN2C0.2.1917.32","1",null,null,"+",null,"+",null,null,"1280x1024(H264) / 704x576 (MJPEG)","1024x768(H264) / 640x480 (MJPEG)","640x480(H264) / 320x240 (MJPEG)","+",null,"+","+","+","+",null,null,"motion detection; ","+"]
["Ganz","Ganz ZN-DT350VPE / ZN-DNT350VPE / ZN-DWNT350VPE / ZN-DNT350VPEL","Camera ","1.8.1","1",null,null,"+","+","+",null,null,"720x576","640x576","320x288","+",null,"+.","+","+","+","+",null,"motion detection and others;","+","1. Устройства в продукте определяется как ZN-D350 series\n2. Видеоаналитика VCA:\nДетектор взлома\nДетектор движущихся/неподвижных объектов\nДетектор низкой освещенности\nДетектор оставленных предметов","1. In the AxxonSoft products, the camera is identified as ZN-D350 series\n2. Video Analytics (VCA):\nCamera tampering detection\nVMD/Abandoned object detection\n"]
["Ganz","Ganz ZN-M2AF","Camera ","ZN2C0.2.2046.32","1",{"$nulls":4},"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":4},"+"]
["Ganz","Ganz ZN-MD221M / ZN-MD243M / ZN-MD260M ","Camera ","ZN2C0.2.2046.32","1",{"$nulls":4},"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":8},"+"]
["Ganz","GANZ ZN-PTZ220M-XT","Camera","51110.2.6056.100","1",null,null,"+","-","+","-","-","1920x1080","1024x768","640x480","+",null,"-","-","+","-","-","-",null,"+","Прошивка 51110.2.6056.100: после установки данной прошивки на камеру в ее веб-интерфейсе в разделе информации об устройстве отображается версия встроенного ПО ZN2C0.2.6056.32.Для работы с камерой в ПО ITV необходимо выбирать тип платы GanzZNC.","51110.2.6056.100 firmware: when the firmware is updated on the camera, ZN2C0.2.6056.32 version is displayed in the properties section in the camera web interface. To work with camera in AxxonSoft software, select the GanzZNC board type."]
["Ganz","Ganz ZN-VS801P encoder","Encoder ","V3.2.36_C","1",null,null,"+","+",{"$nulls":3},"720x576(PAL)/720x480(NTSC)","704x576(PAL)/704x480(NTSC)","352x288(PAL)/352x240(NTSC)","+",null,"+","-","+","-","-",null,"-","+","1. В ПО ITV следует выбирать граббера Ganz-s(jpeg) и Ganz-s(h264)\n2. у камеры нет монохромного режима, но в Intellect данный функционал реализуется за счтет сброса насыщенности на минимум. В Axxon Next настройки \"Цвет\" не будет.","1. In the AxxonSoft software, select the Ganz-s(jpeg) and Ganz-s(h264) grabbers.\n2. The camera does not have a black-and-white mode, but Intellect implements this functionality by setting the saturation to the minimum. In Axxon Next, the Color setting is not available."]
["Ganz","Ganz ZN-VS804P encoder","Encoder ","v. 1.1.14_i","4",null,null,"+","+",{"$nulls":3},"688x544(PAL) / 668x448(NTSC)","688x544(PAL) / 668x448(NTSC)","336x272(PAL) / 668x448(NTSC)","+",null,"+","-","+","-","-",null,"-","+","1) Аналог устройства Ganz ZN-VS804P-WL, от которого отличается только отсутствием возможности беспроводного подключения к сети\n2) для работы с устройством в ПО ITV следует выбирать граббера Ganz-s\n3) при Полном и Высоком разрешении максимальный fps =6 (ограничение самого устройства)\n4) при максимальном значении настройки \"насыщенность цвета\" видеоизображение становится черно-белым (ошибка самого устройства)\n5) \"диагональные\" кнопки управления телеметрией на Панели телеметрии не работают (ограничение самого устройства)","1) This device is very similar to the Ganz ZN-VS804P-WL. The only difference is that by contrast to the Ganz ZN-VS804P-WL, this device does not have any wireless network connectivity.\nTo use the device, in the AxxonSoft software, select the Ganz-s grabber.\n3. At full or high resolution, the max. frame rate is 6 fps (this is a limitation of the device itself).\n4. When you set the saturation setting to the maximum, video turns into black and white (this is a problem of the device itself).\n5) On the PTZ Control Panel, the diagonal telemetry control buttons do not work (this is a limitation of the device itself)."]
["Ganz","Ganz ZN-VS804P-WL encoder","Encoder ","v1.1.11_i","4",null,null,"+","+",{"$nulls":3},"688x544(PAL)/688x448(NTSC)","688x544(PAL)/688x448(NTSC)","336x272(PAL)/688x448(NTSC)","+",null,"+","-","+","-","-",null,"-","+","1. В ПО ITV следует выбирать граббера Ganz-s(jpeg) и Ganz-s(h264)\n2. При выставлении высокого и полного разрешений fps падают до ~4-5","1. In the AxxonSoft software, select the Ganz-s(jpeg) and Ganz-s(h264) grabbers. \n2. If you set high or full resolution, the frame rate drops to around 4–5 fps. "]
["Ganz","Ganz ZN-Y11VPE / ZN-NH11VPE / ZN-NHW11VPE / ZN-NH11VPEL","Camera ","1.8.1","1",null,null,"+","+","+",null,null,"720x576","640x576","320x288","+",null,"+.","+","+","+","+",null,"motion detection and others;","+","1. Устройства в продукте определяется как ZN-CS series\n2. Видеоаналитика VCA:\nДетектор взлома\nДетектор движущихся/неподвижных объектов\nДетектор низкой освещенности\nДетектор оставленных предметов","1. In the AxxonSoft products, the camera is identified as ZN-CS series\n2. Video Analytics (VCA):\nCamera tampering detection\nVMD/Abandoned object detection"]
["Ganz ZNC","Ganz ZN-C1","Camera ","ZN2C0.2.1517.32","1",null,null,"+",null,"+",null,null,"704x576","640x480","320x240","+",null,"+","-",null,"+","+",null,"+.","+","1. fps меняется сразу для двух стриммингов одновременно, разрешение второго стримминга зависит от разрешения первого - особенность интеграции в ПО ITV\n2. Луч(Датчик), Реле и Встроенный детектор срабатывает с задержкой в 2-3 секунды, особенность самой камеры","1. The frame rate is adjusted for both streams at once; the resolution of the second stream depends on the resolution of the first stream (this is for integration with AxxonSoft software). \n2. Sensor, Relay, and Embedded Sensor work with a delay (around 2–3 seconds), this is a limitation of the camera itself. "]
["Ganz ZNC","Ganz ZN-C1M","Camera ","ZN2C0.2.1517.32","1",null,null,"+",null,"+",null,null,"704x576 (MJPEG) / 1280x1024 (H.264)","640x480 (MJPEG) / 1024x768 (H.264)","320x240 (MJPEG) / 640x480 (H.264)","+",null,"+","-",null,"+","+",null,"+.","+"," 0. Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".\n 1. Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В AxxonNext/Next записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\") \n2. Смена настроек видео происходит с задержкой (от 30 сек. до 1 мин. в случае смены видеопотоков)- особенность камеры. \n3. В MJPEG параметр \"качество\" отсутствует на самой камере, в H264 привязан к параметру \"битрейт\"\n4. Луч, реле и встроенный детектор срабатывают с небольшой задержкой (3-4 секунды)"," 0. Before using the camera, go to the web interface and disable the Installation Mode: assign \"Off\" to this parameter. \n 1. The resolution and frame rate are adjusted for both streams at the same time; this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\" : \"resolution, stream 2\") \n2. Changes to the settings are applied with a delay (30–60 seconds for switching to a different video stream); this is a limitation of the camera itself. \n3. With MJPEG, the Quality parameter is missing on the camera itself; in H.264, this parameter depends on the Bit Rate parameter.\n4. Sensor, Relay, and Embedded Sensor work with a short delay (around 3–4 seconds). "]
["Ganz ZNC","Ganz ZN-C2M","Camera ","ZN2C0.2.1517.32","1",null,null,"+",null,"+",null,null,"704x576 (MJPEG) / 1920x1080 (H264)","640x480 (MJPEG) / 1024x768 (H264)","320x240 (MJPEG) / 640x480 (H264)","+",null,"+","-",null,"+","+",null,"+.","+"," Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В AxxonNext/Next записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")При максимальном битрейте в максимальном разрешении падает fps, видео идет с задержками - особенность устройства.Прошивка 51110.2.1499.100 : камера определяется поиском как NCX-2000Смена настроек видео, а также срабатывание лучей и реле происходит с задержкой (от 30 сек. до 1 мин. в случае смены видеопотоков)- особенность камеры.Луч должен быть под напряжением.В MJPEG параметр \"качество\" отсутствует на самой камере, в H264 привязан к параметру \"битрейт\"Луч(Датчик), Реле и Втроенный детектор могут срабатывать с небольшой задержкой (~3 сек)"," Before using the camera, go to the web interface and disable the Installation Mode: assign \"Off\" to this parameter. The resolution and frame rate are adjusted for both streams at the same time; this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\" : \"resolution, stream 2\"). With the max. bit rate, the frame rate drops when you switch to the max. resolution and video comes with delays. This is a limitation of the device itself. 51110.2.1499.100 firmware: Search detects the device as NCX-2000. Changes to the settings are applied with a delay (30–60 seconds for switching to a different video stream). This is a limitation of the camera itself; the same for how sensors and relays work. Close the sensor when it is energized. With MJPEG, the Quality parameter is missing on the camera itself; in H.264 this parameter depends on the Bit Rate parameter. Sensor, Relay, and Embedded Sensor work with a short delay (around 3 seconds)."]
["Grandstream","Grandstream GXV3500","Encoder/Decoder","1.0.1.75","1",null,null,"+",null,"+",null,null,"704x576 (PAL) / 704x480 (NTSC)","640x480 ","320x240 ","+",null,"-","-","+",{"$nulls":4},"+"]
["Grandstream","Grandstream GXV3501","Encoder ","v1.0.4.34","1",null,null,"+",null,"+",null,null,"PAL: 704x576, NTSC: 704x480","PAL: 704x288, NTSC: 704x240","PAL: 352x288, NTSC: 352x240","+",null,"+","+",null,"-","-",null,"-","+","1. Луч должен замыкаться под напряжением.\n2. Разрешения и максимальный fps зависят от ТВ-стандарта подключенной аналоговой камеры. ","1. Alarm in is to be closed being energized.\n2. Resolutions and the maximum fps depend on a TV-standard of the connected analog camera.\n"]
["Grandstream","Grandstream GXV3504","Encoder ","v1.0.4.34","4",null,null,"+",null,"+",null,null,"PAL: 704x576, NTSC: 704x480","PAL: 704x288, NTSC: 704x240","PAL: 352x288, NTSC: 352x240","+",null,"+","+",null,"-","-",null,"-","+","Луч должен замыкаться под напряжением.\nДля MJPEG 704x576 максимальный FPS - 15\nРазрешения и максимальный fps зависят от ТВ-стандарта подключенной аналоговой камеры. \nРазрешения и максимальный fps зависят от ТВ-стандарта подключенной аналоговой камеры. ","1. Alarm in is to be closed being energized.\n2. For 704x576 MJPEG maximum FPS is 15\n3. Resolutions and the maximum fps depend on a TV-standard of the connected analog camera.\n"]
["Grandstream","Grandstream GXV3601 / -LL","Camera ","1.0.4.27","1",null,null,"+",null,"+",null,null,"720x576 (PAL)","704x288 (PAL)","352x288 (PAL)","+",null,"+.","+.",null,"+","+",null,"-","+","Прошивка 1.0.4.27: видео совместно со звуком идет только по протоколу UDP.Луч должен замыкаться под напряжением.","1.0.4.27 firmware: Video comes together with audio only via the UDP protocol. Close the sensor when it is energized."]
["Grandstream","Grandstream GXV3611_HD","Camera ","1.0.4.42","1",null,null,"+",null,"+",null,null,"1600x1200","1024x768","640x480","+",null,"-","-",null,null,"-",null,"-","+","На втором потоке нельзя выставить разрешение большее чем на первом.","At second stream can not be set resolution higher than at first one."]
["Grandstream","Grandstream GXV3611_LL","Camera ","1.0.4.27","1",null,null,"+",null,"+",null,null,"PAL: 720x576 NTSC: 720x480","PAL: 720x576 NTSC: 640x480","PAL: 352x288 NTSC: 320x240","+.",null,"+.","+.",null,"+","+",null,"-","+","1. Луч должен быть под напряжением.\n2. Прошивка 1.0.4.27: видео совместно со звуком идет только по протоколу UDP.","Close the sensor when it is energized. 1.0.4.27 firmware: Video comes together with audio only via the UDP protocol."]
["Grandstream","Grandstream GXV3615/W","Camera ","1.0.4.34","1",null,null,"+",null,"+",null,null,"720x576 (PAL) / 720x480 (NTSC)","352x288 (PAL) / 640x480 (NTSC)","320x240","+",null,"+.","+",{"$nulls":4},"-","+","1. Луч должен замыкаться под напряжением.\n2.Прошивка 1.0.4.27: видео совместно со звуком идет только по протоколу UDP.","1. Close the sensor when it is energized.\n2. The 1.0.4.27 firmware: Video comes together with audio only via the UDP protocol.\n"]
["Grandstream","Grandstream GXV3615WP_HD","Camera ","1.0.1.69","1",null,null,"+",null,"+",null,null,"1600x1200","1024x768","640x480","+",null,"+","+",{"$nulls":4},"-","+"]
["Grandstream","Grandstream GXV3651_FHD","Camera ","1.0.1.57","1",null,null,"+",null,"+",null,null,"2048x1536","1024x768","640x480","+",null,"+","+",null,"+","+",null,"-","+","Прошивка 1.0.1.45: видео совместно со звуком идет только по протоколу UDP.\nМаксимальный FPS зависит от разрешения: 2560x1920 - 10 2048x1536 - 15\nЛуч должен замыкаться под напряжением.","1.0.1.45 firmware: Video comes together with audio only via the UDP protocol. The max. frame rate depends on the resolution: 2560x1920 – 10 fps, 2048x1536 – 15 fps. \nClose Alarm Input when it is energized."]
["Grandstream","Grandstream GXV3662_HD","Camera ","1.0.1.45","1",null,null,"+",null,"+",null,null,"1280x960","1024x768","640x480","+.",null,"+.","+.",null,"+","+",null,"-","+","1. Луч должен замыкаться под напряжением.\n2. Прошивка 1.0.1.45: видео совместно со звуком идет только по протоколу UDP.","Close the sensor when it is energized. 1.0.1.45 firmware: Video comes together with audio only via the UDP protocol."]
["Grundig","Grundig Encoder GEC-D2201AR","Encoder","720130527ANS","1",null,null,"+","-","+","-","-","720x576","720x576","352x288","-",null,"-","-","-","-","-","-","-","+","В ПО Axxon Next, в двухпоточном режиме, настройка fps применяется на оба потока.","In Axxon Next fps setting is applied to both streams in 2-stream mode. "]
["Grundig","Grundig GCI-C0745P","Camera ","720110412NS","1",null,null,"+",null,"+",null,null,"720x576","720x576","352x288","+",null,null,"-","+",{"$nulls":3},"-","+","На камере не работает параметр Частота опорных кадров. Значения в Интеллект и в AxxonNext/Next применяются в веб-интерфейсе, но реальная частота опорных кадров не совпадает с установленным значением.","On the camera, the Keyframes Interval parameter does not work. If set a value in Intellect or AN, the value is applied in the web interface, but the actual keyframes interval does not match the value that is set. "]
["Grundig","Grundig GCI-F0505B","Camera ","gr20121228NSA ","1",null,null,"+",null,"+",null,null,"2048x1536 ","1024x768 ","640x480","+",{"$nulls":8},"+"]
["Grundig","Grundig GCI-G0509B","Camera ","gr20120613NSA","1",null,null,"+",null,"+",null,null,"2592х1944 (H.264) / 1920x1080 (MJPEG)","1024x768","640x480","+",{"$nulls":7},"motion detection; ","+"]
["Grundig","Grundig GCI-H0503B","Camera ","720110422NS","1",null,null,"+","+","+",null,null,"1280x960 (H264 / MJPEG) / --- (MPEG4)","640x480","320x240","+",null,null,"-",{"$nulls":4},"-","+","Настройки видео (кодек, разрешение, частота кадров) в разных потоках взаимозависимы. Пользователь должен самостоятельно следить за совместимостью выбранной конфигурации.","The video settings (codec, resolution, frame rate) for different streams are interdependent. The user must independently ensure that the selected values are compatible. "]
["Grundig","Grundig GCI-H0522V","Camera ","720120117NS","1",null,null,"+",null,"+",null,null,"1920x1080","640x480","320x240","+",null,null,"-",{"$nulls":4},"-","+","В многопотоковом режиме для первого потока доступен только кодек h264 в разрешении 720p.Частота кадров меняется для обоих потоков одновременно.","In multi-stream mode, only the H.264 codec and 720p resolution are available for the first stream. The frame rate is adjusted for both streams at once."]
["Grundig","Grundig GCI-H2505B","Camera","gr20130417NSX","1",null,null,"+","-","+","-","-","1024x768","800x600","640x480","+","-","-","-","-","-","-","-","-","+"]
["Grundig","Grundig GCI-H0602B","Camera ","720110217NS","1",null,null,"+",null,"+",null,null,"1920x1080","640x480","320x240","+",null,null,"-",{"$nulls":4},"-","+","Частота кадров меняется для обоих потоков сразу.При совместном использовании 2х потоков в первом доступен только H264 в разрешении 1280х720.","The frame rate is adjusted for both streams at once. When you use two streams at the same time, only H.264 and the 1280x720 resolution are available for the first stream."]
["Grundig","Grundig GCI-K0322V","Camera ","720110413NS","1",null,null,"+",null,"+",null,null,"1920x1080","640x480","320x240","+",null,null,"-",{"$nulls":4},"-","+"]
["Grundig","Grundig GCI-K0503B","Camera ","720110413NS","1",null,null,"+",null,"+",null,null,"1920x1080","640x480","320x240","+",null,null,"-",{"$nulls":4},"-","+"]
["Grundig","Grundig GCI-K0512W","Camera ","720101228NS","1",null,null,"+",null,"+",null,null,"1920x1080","640x480","320x240","+",{"$nulls":7},"-","+"]
["Grundig","Grundig GCI-K0523T","Camera ","720110413NS","1",null,null,"+",null,"+",null,null,"1920x1080","640x480","320x240","+",null,null,"-",{"$nulls":4},"-","+"]
["Grundig","Grundig GCI-K0779P / GCI-K1779P ","Camera ","gr20120522NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","-",{"$nulls":3},"+",{"$nulls":3},"motion detection; ","+"]
["Grundig","Grundig GCI-K1503B(S) / GCI-K1523V(S) / GCI-K1526V(S)","Camera ","gr20130314NSX ","1",null,null,"+",null,"+",null,null,"1920x1080 ","1024x768","640x480","+",{"$nulls":8},"+"]
["Grundig","Grundig GCI-K1526T / GCI-K1526V / GCI-K1586V / GCI-K1503B / GCI-K1585V / GCI-K1812W / GCI-K0589T ","Camera ","gr20121228NSA ","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":7},"motion detection;","+"]
["Grundig","Grundig GCI-K1603B / GCI-K1523V ","Camera ","gr20121228NSA ","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":7},"motion detection; ","+"]
["Grundig","Grundig GCI-K1607B","Camera ","gr20130131NSA ","1",null,null,"+",null,"+",null,null,"1920x1080 ","1024x768","640x480","+",{"$nulls":8},"+"]
["Grundig","Grundig GCI-K2505B","Camera ","gr20131101NSX","1",null,null,"+",null,"+",null,null,"1280x1024 (MJPEG) / 1920x1080 (H.264)","1024x768","640x480","+",{"$nulls":8},"+"]
["Gunnebo","Gunnebo GFD7200-IP-SR","Camera ","A1D-M2N-V2.05.12-NB","1",{"$nulls":3},"+",{"$nulls":3},"720x576","720x576","352x288","+",{"$nulls":4},"-","-",null,"-","+"]
["HikVision","Hikvision DS-2CD2012-I / DS-2CD2112-I","Camera ","V5.0.0 130412","1",null,null,"+",null,"+",null,null,"1280x960","640x480","320x240","+",null,"-","-","-","-","-","-","motion detection","+","На втором потоке нельзя выставить значение разрешения большее, чем стоит на первом.\nДетектор движения работает только при заполненной таблице \"Arming Schedule\", в веб-интерфейсе камеры.\n","At second stream can not be set resolution higher than at first one. Motion detection works only with filled table \"Arming Schedule\" from web-interface."]
["HikVision","Hikvision DS-2CD2032-I / DS-2CD2132-I","Camera ","V5.0.0.130412","1",null,null,"+",null,"+",null,null,"2048x1536","1280x720","320x240","+",null,"-","-","-","-","-","-","motion detection;","+","Детектор движения работает только при заполненной таблице \"Arming Schedule\", в веб-интерфейсе камеры.","Motion detection works only with filled table \"Arming Schedule\" from web-interface."]
["HikVision","Hikvision DS-2CD2432F-I(W)","Camera","V5.1.0 build 131202","1",null,null,"+","-","+","-","-","2048x1536 (H.264) / 704x576 (MJPEG)","1280x720 (H.264) / 640x480 (MJPEG)","640x480 (H.264) / 352x288 (MJPEG)","+","-","+","-","-","-","-","-","motion detection","+"]
["HikVision","Hikvision DS-2CD2712F-IS / DS-2CD2612F-IS","Camera ","V5.0.2 130805","1",null,null,"+",null,"+",null,null,"704x576(MJPEG)/1280x960(H264)","352x288(MJPEG)/640x480(H264) ","320x240","+",{"$nulls":8},"+"]
["HikVision","Hikvision DS-2CD2632F-IS","Camera","V5.0.0 130412","1",null,null,"+","-","+",null,null,"2048x1536(H264)/704x576 (MJPEG)","1280x720(H264) / 353x288(MJPEG)","320x240","+",null,"+","+","-","+","-","-","motion detection","+"]
["HikVision","Hikvision DS-2CD7133-E","Camera ","V3.0 110516 ","1",null,null,"+","+","+",null,null,"352x288 (MJPEG) / 640x480 (H264) / 640x480 (MPEG4)","352x288 (MJPEG) / 352x288 (H264) / 640x480 (MPEG4)","320x240 (MJPEG) / 320x240 (H264) / 640x480 (MPEG4)","+",{"$nulls":7},"-","+","В AxxonNext/Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.В AxxonNext/Next Смена потоков / кодеков требует перезагрузки устройства (~ 1 мин.)В Интеллекте переключение между полным и средним (минимальным) разрешением требует перезагрузки устройства (~ 1 мин).","In AN, search does not detect the device's firmware. You must yourself select the right version of the camera's software. In AN, after you switch to a different stream or codec, you must restart the device (around 1 minute). In AN, after you switch to a different stream or codec, you must restart the device (around 1 minute)."]
["HikVision","Hikvision DS-2CD7153-E","Camera ","V3.0 build 111017","1",null,null,"+","+","+",null,null,"1600x1200","800x600","640x480","+",{"$nulls":3},"-",{"$nulls":3},"+","+","В разрешении 1600х1200 сама камера выдает только 12 fps максимум.Прошивка 2.0 100423: все настройки видеопотока (разрешение, fps и пр.) меняются только после reboot камеры.Прошивка 2.0 100423: камера не поддерживает ни ONVIF, ни PSIA.Прошивка 3.0 110516: камера работает и по ONVIF и по PSIAПрошивка 2.0 100423 :настройка \"Раскрытие диафрагмы\" работает неправильно на самой камереПрошивка 3.0 110516: настройка \"Раскрытие диафрагмы\"  НЕ работает на самой камере","At 1600x1200 resolution, the camera itself allows 12 fps max. 2.0 100423 firmware: changes to all the settings of a video stream (resolution, frame rate, etc.) are applied only after you restart the camera. 2.0 100423 firmware: the camera does not support ONVIF or PSIA. 3.0 110516 firmware: the camera works via both ONVIF and PSIA. 2.0 100423 firmware: the Iris Adjustment setting does not work correctly on the camera itself. 3.0 110516 firmware: the Iris Adjustment setting DOES NOT work on the camera itself"]
["HikVision","Hikvision DS-2CD7164-E","Camera ","V4.0.3 121010","1",null,null,"+","+","+",null,null,"1280x960(MPEG4/H.264)/704х576(MJPEG)","640x480(MPEG4/H.264)/352x288(MJPEG)","320x240(MPEG4/H.264)/320x240(MJPEG)","+",{"$nulls":8},"+"]
["HikVision","Hikvision DS-2CD732F-E","Camera ","V2.0 build 110829","1",{"$nulls":4},"+",null,null,"704x576","528х384","352x288","+",null,"+.","+","-","+","-",null,"+","+","Камера поддерживает разрешения видео стандарта NTSC, а передает видео в разрешениях стандарта PAL. Аналогичная ситуация и в веб-интерфейсе камеры. В результате после выбора в нашем ПО, например, разрешения 704х80, видео будет идти в разрешении 704х576. ","The camera seems to support the NTSC resolutions, but sends video with PAL resolutions instead. In the web interface, it is the same. As a result, if you select, for example, 704x80 resolution, video comes at 704x576 resolution. "]
["HikVision","Hikvision DS-2CD733F-E","Camera ","V3.0 110510","1",null,null,"+",null,"+",null,null,"352x288 (MJPEG) / 640x480 (H264)","352x288","320x240","+",null,"+.","-","-","+","-",null,"-","+","При высоких настройках (разрешение, битрейт и качество) видеопоток с камеры может поступать нестабильно. Может наблюдаться \"подтормаживание\" видео, \"проседание\" fps и т.д. - проблема самой камеры.Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельноПрошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства. ","With high settings (resolution, bit rate, and quality), the camera's video stream is unstable. Video may be slow and the frame rate may drop, etc. – this is a problem of the camera itself. Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. V3.0 110510 firmware: If you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device. "]
["HikVision","Hikvision DS-2CD752MF-E","Camera ","V2.0 110902","1",null,null,"+",null,"+",null,null,"352x288 (MJPEG) / 1600x1200 (H264)","352x288 (MJPEG) / 800x600 (H264)","352x288 (MJPEG) / 640x480 (H264)","+",null,"+.","+","-","+","-",null,"+","+","В AxxonNext/Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.Через Onvif не работает луч и кодек MJPEG.Камера поддерживает одни разрешения, а передает видео в других. Аналогичная ситуация и в веб-интерфейсе камеры.","In AN, search does not detect the device's firmware. You must select, yourself, the right version of the camera's software. The sensor and MJPEG codec do not work via the ONVIF protocol. The camera seems to support one set of resolutions, but sends video with other resolutions. In the web interface, it is the same."]
["HikVision","Hikvision DS-2CD752MF-FB","Camera ","V2.0 110902","1",null,null,"+",null,"+",null,null,"352x288 (MJPEG) / 1600x1200 (H264)","352x288 (MJPEG) / 800x600 (H264)","352x288 (MJPEG) / 640x480 (H264)","+",null,"+.","+","-","+","-",null,"+","+","В AxxonNext/Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.Поиск может находить камеру как Onvif-устройство, однако работать по этому протоколу она не будетКамера поддерживает одни разрешения, а передает видео в других. Аналогичная ситуация и в веб-интерфейсе камеры.","In AN, search does not detect the device's firmware. You must select, yourself, the right version of the camera's software. Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. The camera seems to support one set of resolutions, but sends video with other resolutions. In the web interface, it is the same."]
["HikVision","Hikvision DS-2CD753F-E","Camera ","V3.0 110510","1",null,null,"+",null,"+",null,null,"352x288 (MJPEG) / 1600x1200 (H264)","352x288 (MJPEG) / 800x600 (H264)","320x240 (MJPEG) / 640x480 (H264)","+",null,"+.","+","-","+","-",null,"-","+","Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельноПрошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.","Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. V3.0 110510 firmware: If you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device."]
["HikVision","Hikvision DS-2CD754F-E","Camera ","V3.2 120105","1",null,null,"+","+","+",null,null,"2048x1536 (h264, mpeg4) / 320x240 (mjpeg)","1600x1200 (h264, mpeg4) / 320x240 (mjpeg)","320x240 (h264, mjpeg) / 1280x720 (mpeg4)","+",null,"+.","+","-","+","-",null,"+","+","Смена кодека приводит к перезагрузке камеры (~1 минута)Во втором потоке звук с камеры идет с прерываниями. В Интеллекте это воспроизводится в кодеке H264 (в минимальном разрешении) и в кодеке MJPEG.Если на первом потоке выставлен кодек H264, то на втором может быть либо H264, либо MJPEG. Если на первом потоке выставлен кодек MPEG4, то на втором может быть либо MPEG4, либо MJPEG.","If you switch to a different codec, the camera must restart (1 minute). In the second stream, audio is intermittent. In Intellect, this happens with the H.264 codec (at the min. resolution) and with the MJPEG codec. If you set the H.264 codec for the first stream, you must set either H.264 or MJPEG for the second stream. If you set the MPEG4 codec for the first stream, you must set either MPEG4 or MJPEG for the second stream."]
["HikVision","Hikvision DS-2CD754FWD-E / DS-2CD754FWD-EI","Camera","V4.1.0 130111","1","-",null,"+","+","+",null,null,"H.264/MPEG4: 1920x1080; MJPEG: 704x576","H.264/MPEG4: 704x576; MJPEG: 352x288","320x240","+",null,"-","-",null,"-","-","-","-","+","Чтобы кодек H.264 (MPEG4) был доступен на втором потоке, нужно выставить такой же кодек на первом","To enable H.264 (MPEG4) for stream 2, select the same codec for  stream 1.","improved"]
["HikVision","Hikvision DS-2CD762MF-FB","Camera ","V2.0 build 110902","1",null,null,"+",null,"+",null,null,"320x240 (MJPEG) / 1280x960 (H264)","320x240 (MJPEG) / 1280x720 (H264)","320x240 (MJPEG) / 640x480 (H264)","+",null,"+.","+","-","+","-",null,"+","+","В AxxonNext/Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.Поиск может находить камеру как Onvif-устройство, однако работать по этому протоколу она не будетКамера поддерживает одни разрешения, а передает видео в других. Аналогичная ситуация и в веб-интерфейсе камеры. В результате после выбора в нашем ПО, например, разрешения 352х288, видео будет идти в разрешении 320х240.","In AN, search does not detect the device's firmware. You must select, yourself, the right version of the camera's software. Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol The camera seems to support one set of resolutions, but sends video with other resolutions. In the web interface, it is the same. As a result, if you select, for example, the 352x288 resolution in our software, video comes in 320x240 resolution."]
["HikVision","Hikvision DS-2CD762MF-FBH","Camera ","V2.0 build 110902","1",null,null,"+",null,"+",null,null,"320x240 (MJPEG) / 1280x960 (H264)","320x240 (MJPEG) / 1280x720 (H264)","320x240 (MJPEG) / 640x480 (H264)","+",null,"+.","+","-","+","-",null,"+","+","В AxxonNext/Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.Поиск может находить камеру как Onvif-устройство, однако работать по этому протоколу она не будетКамера поддерживает одни разрешения, а передает видео в других. Аналогичная ситуация и в веб-интерфейсе камеры. В результате после выбора в нашем ПО, например, разрешения 352х288, видео будет идти в разрешении 320х240.","In AN, search does not detect the device's firmware. You must select, yourself, the right version of the camera's software. Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol The camera seems to support one set of resolutions, but sends video with other resolutions. In the web interface, it is the same. As a result, if you select, for example, the 352x288 resolution in our software, video comes in 320x240 resolution."]
["HikVision","Hikvision DS-2CD763PF-E","Camera ","V3.0 build 110516 ","1",null,null,"+","+","+",null,null,"352x288 (MJPEG) / 1280x960 (MPEG4) / 1280x960 (H264)","352x288 (MJPEG) / 1280x720 (MPEG4) / 1280x960 (H264)","352x288 (MJPEG) / 640x480 (MPEG4) / 1280x960 (H264)","+",null,"+.","+","-","+","-",null,"-","+","В AxxonNext/Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.В AxxonNext/Next Смена потоков / кодеков требует перезагрузки устройства (~ 1 мин.)В Интеллекте переключение между полным и средним (минимальным) разрешением требует перезагрузки устройства (~ 1 мин).Через Onvif не работают лучи","In AN, search does not detect the device's firmware. You must yourself select the right version of the camera's software. In AN, after you switch to a different stream or codec, you must restart the device (around 1 minute). In Intellect, after you switch between the full and medium (average) resolutions, you must restart the device (around 1 min.) Via the ONVIF protocol, the sensors do not work."]
["HikVision","Hikvision DS-2CD764F-E / DS-2CD8264F-E ","Camera ","V4.1.0 130111","1",null,null,"+","+","+",null,null,"1280x960(H264; Mpeg4); НИ(MJPEG)","640x480(H264; Mpeg4); НИ(MJPEG)","320x240","+",null,"-","-","-","-","-","-",null,"+","Для изменения кодека в Интеллекте сначала необходимо выбрать на камере Полное или Высокое разрешение ","To change codecs in Intellect, you should select Full or High resolution in the camera. "]
["HikVision","Hikvision DS-2CD764FWD-E","Camera","V5.0.0 130412","1",null,null,"+","+","+","-","-","1280x960","640x480","320x240","+",null,"+","+","+","-","-","-","motion detection","+","Кодеки на основном и дополнительном потоках взаимозависимы.детектор движения работает только при заполненной таблице \"Arming Schedule\", в веб-интерфейсе камеры.","Codecs on primary and secondary streams are interdependent. From web-interface motion detection tool works only with \"Arming Schedule\" table filled."]
["HikVision","Hikvision DS-2CD783F-E","Camera ","V3.2 120105","1",null,null,"+","+","+",null,null,"H264, MPEG4: 2560x1920, MJPEG: 320x240","H264, MPEG4: 1600x1200, MJPEG: 320x240","320x240","+",null,"+.","+","-","+","-",null,"+","+","Камера имеет ограничение по FPS в зависимости от разрешения: 6.25 к/сек (2560 × 1920), 12.5 к/сек (2048 × 1536), 25 к/сек (1920 × 1080), 25 к/сек (1600 × 1200), 25 к/сек (1280 × 720)Если на первом потоке выставлен кодек H264, то на втором может быть либо H264, либо MJPEG. Если на первом потоке выставлен кодек MPEG4, то на втором может быть либо MPEG4, либо MJPEG. Нужно учитывать эту зависимость при работе в ПО ITV.","The camera has frame rate limits (depending on the resolution): 6.25 fps (2560 × 1920), 12.5 fps (2048 × 1536), 25 fps (1920 × 1080), 25 fps (1600 × 1200), 25 fps (1280 × 720). If you set the H.264 codec for the first stream, you must set either H.264 or MJPEG for the second stream. If you set the MPEG4 codec for the first stream, you must set either MPEG4 or MJPEG for the second stream. Have this in mind when you use the AxxonSoft software. "]
["HikVision","Hikvision DS-2CD792PF-E","Camera ","V2.0 build 110829","1",{"$nulls":4},"+",null,null,"704x576","528х384","352x288","+",null,"+.","+","-","+","-",null,"+","+","Камера поддерживает разрешения видео стандарта NTSC, а передает видео в разрешениях стандарта PAL. Аналогичная ситуация и в веб-интерфейсе камеры. В результате после выбора в нашем ПО, например, разрешения 704х480, видео будет идти в разрешении 704х576.Прошивка V2.0 build 110829: камера передает изображение с искажениями (черными полосами, идущими по картинке).","The camera seems to support the NTSC resolutions, but sends video with PAL resolutions instead. In the web interface, it is the same. As a result, if you select, for example, 704x480 resolution, video comes with the 704x576 resolution. The V2.0 build 110829 firmware: the camera sends distorted video (black lines over the image). "]
["HikVision","Hikvision DS-2CD793PF-E ","Camera ","V3.0 110510","1",null,null,"+",null,"+",null,null,"352x288 (MJPEG) / 704x576 (H264)","352x288 (MJPEG) / 704x576 (H264)","352x288","+",null,"+.","+",null,"+","-",null,"-","+","Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельноПрошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.Звук с устройства прерывается:Во втором потоке. В Интеллекте это проявляется при выборе кодека mjpeg.В обоих потоках при выборе транспортного протокола TCP.","Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. V3.0 110510 firmware: if you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remain the same; this is a problem of the device itself. Audio is intermittent. In the second stream. In Intellect, this happens if you select the MJPEG codec in both streams if you select the TCP protocol."]
["HikVision","Hikvision DS-2CD793PFWD-E ","Camera ","V3.0 110510","1",null,null,"+",null,"+",null,null,"352x288 (MJPEG) / 704x576 (H264)","352x288 (MJPEG) / 704x576 (H264)","352x288","+",null,"+.","+","-","+","-",null,"-","+","Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельно.Прошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.","Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. V3.0 110510 firmware: If you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device."]
["HikVision","Hikvision DS-2CD8133F-E","Camera ","V3.0 110516 ","1",null,null,"+","+","+",null,null,"H264, MPEG4: 640x480, MJPEG: 352x288","352x288","320x240","+",null,"+.","+",{"$nulls":4},"+","+","Если на первом потоке выставлен кодек H264, то на втором может быть либо H264, либо MJPEG. Если на первом потоке выставлен кодек MPEG4, то на втором может быть либо MPEG4, либо MJPEG.","If you set the H.264 codec for the first stream, you must set either H.264 or MJPEG for the second stream. If you set the MPEG4 codec for the first stream, you must set either MPEG4 or MJPEG for the second stream."]
["HikVision","Hikvision DS-2CD8153F-E / Hikvision DS-2CD8153F-EW","Camera ","V5.0.0 ","1",null,null,"+","+","+",null,null,"1600x1200","800x600","640x480","+",null,"+","+",{"$nulls":4},"+","+","1. Камера имеет ограничения по FPS: 12,5к/с (1600 × 1200), 12,5к/с (1600 × 912), 25к/с (1280 x 960), 25к/с (1280 х 720)\n2. Если на первом потоке выставлен кодек H264, то на втором может быть либо H264, либо MJPEG. \n3. Если на первом потоке выставлен кодек MPEG4, то на втором может быть либо MPEG4, либо MJPEG. ","1. The camera has frame rate limits: 12.5 fps (1600 × 1200), 12.5 fps (1600 × 912), 25 fps (1280 x 960), 25 fps (1280 х 720). 2. If you set the H.264 codec for the first stream, you must set either H.264 or MJPEG for the second stream. \n3. If you set the MPEG4 codec for the first stream, you must set either MPEG4 or MJPEG for the second stream. "]
["HikVision","Hikvision DS-2CD8254F-EI","Camera ","V4.1.0","1",null,null,"+","+","+",null,null,"H.264/MPEG4: 2048x1536; MJPEG: 704x576 ","H.264/MPEG4: 1600x1200; MJPEG: 352x288 ","320x240","+",{"$nulls":8},"+"]
["HikVision","Hikvision DS-2CD8254FWD-EIS","Camera","V4.1.0 130111","1","-",null,"+","+","+",null,null,"2048x1536 (H.264, MPEG4) / 704x576 (MJPEG)","1280x720 (H.264, MPEG4) / 352x288 (MJPEG)","320x240","+",null,"-","-",null,"-","-",null,"-","+",null,null,"improved"]
["HikVision","Hikvision DS-2CD8264FWD-EIS ","Camera ","V4.1.0 130111 ","1",null,null,"+","+","+",null,null,"1280x960(H264; Mpeg4); НИ(MJPEG)","640x480(H264; Mpeg4); НИ(MJPEG)","320x240","+",{"$nulls":8},"+","Кодеки H264 или MPEG4 на втором потоке камеры доступны в зависимости от выбранного кодека на первом потоке. ","H264 / MPEG4 codecs are available for stream 2 depending the codecs set for stream 1. "]
["HikVision","Hikvision DS-2CD832F-E","Camera ","V2.0 build 110829 ","1",{"$nulls":4},"+",null,null,"704x576","528х384","352x288","+",null,"+.","+","-","+","-",null,"+","+","Камера поддерживает разрешения видео стандарта NTSC, а передает видео в разрешениях стандарта PAL. Аналогичная ситуация и в веб-интерфейсе камеры. В результате после выбора в нашем ПО, например, разрешения 704х80, видео будет идти в разрешении 704х576.","The camera seems to support the NTSC resolutions, but sends video with PAL resolutions instead. In the web interface, it is the same. As a result, if you select, for example, 704x80 resolution, video comes at 704x576 resolution."]
["HikVision","Hikvision DS-2CD833F-E","Camera ","V3.0 110510","1",null,null,"+",null,"+",null,null,"352x288 (MJPEG) / 640x480 (H264)","352x288","320x240","+",null,"+.","+","-","+","-",null,"-","+","Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельноПрошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.","Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. V3.0 110510 firmware: If you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device."]
["HikVision","Hikvision DS-2CD852MF-E","Camera ","V2.0 110902","1",null,null,"-",null,"+",null,null,"1600x1200 (H264) / 320x240 (MJPEG)","800x600 (H264) / 320x240 (MJPEG)","640x480 (H264) / 320x240 (MJPEG)","+",null,"+.","+","-","+","-",null,"+","+","В спецификации камеры заявлен MPEG4, однако фактически камера не поддерживает этот кодек (прошивка V2.0 101426)Прошика V2.0 110117, V2.0 110902: Камера иногда передает видео в неправильном разрешении - проблема устройства.","According to the specification, the camera supports the MPEG4 codec; however, in reality the camera does not support this codec (firmware V2.0 101426). V2.0 110117 and V2.0 110902 firmware: Via the ONVIF protocol, the camera sometimes sends video with the wrong resolution; this is a problem of the device itself. "]
["HikVision","Hikvision DS-2CD853F-E","Camera ","V3.0 110510","1",null,null,"+",null,"+.",null,null,"352x288 (MJPEG) / 1600x1200 (H264)","352x288 (MJPEG) / 800x600 (H264)","320x240 (MJPEG) / 640x480 (H264)","+",null,"+.","-","-","+","-",null,"-","+","Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельноПрошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.","Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. V3.0 110510 firmware: If you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device."]
["HikVision","Hikvision DS-2CD854F-E","Camera ","V3.2 120105","1",null,null,"+","+","+",null,null,"2048x1536 (h264, mpeg4) / 320x240 (mjpeg)","1600x1200 (h264, mpeg4) / 320x240 (mjpeg)","320x240 (h264, mjpeg) / 1280x720 (mpeg4)","+",null,"+","+","-","+","-",null,"+","+","Смена кодека приводит к перезагрузке камеры (~1 минута)Во втором потоке звук с камеры идет с прерываниями. В Интеллекте это воспроизводится в кодеке H264 (в минимальном разрешении) и в кодеке MJPEG.При получении видео по протоколу tcp звук также прерывается. Для получения качественного звука нужно переключиться на udp.","If you switch to a different codec, the camera must restart (1 minute). In the second stream, audio is intermittent. In Intellect, this happens with the H.264 codec (at min. resolution) and with the MJPEG codec. When video comes via the TCP, audio is intermittent. To get quality audio, switch to UDP. "]
["HikVision","Hikvision DS-2CD854FWD-E","Camera ","V5.0.0 130412","1",null,null,"+","+","+",null,null,"2048x1536(H.264 / MPEG4) / 704x576(PAL MJPEG) / 704x480 (NTSC MJPEG)","1280x720(H.264 / MPEG4) / 352x288(PAL MJPEG) / 352x240 (NTSC MJPEG)","320x240","+",null,"+","+","+","+","-",null,"motion detection","+","Если на первом потоке стоит H.264, то на втором нельзя выставить MPEG4 и наоборот, если на первом потоке стоит MPEG4, то на втором нельзя выставить H.264\nДетектор движения в продукте срабатывает только если в веб-интерфейсе камеры для детектора движения заполнена таблица Arming Schedule\nЛучи в продукте срабатывает только если в веб-интерфейсе камеры для Alarm input заполнена таблица Arming Schedule\nЕсли выбрать максимальное значение разрешения, то уменьшается максимальное значение FPS.","If first stream is in H.264 codec, it is impossible to use at second one MPEG4, and conversely, if the first stream stands in MPEG4, it is impossible to set on second one H.264.\nMotion detector in AxxonSoft products works only if in camera's web interface filled Arming Schedule table.\nRays in AxxonSoft products works only if in camera's web interface filled Arming Schedule table for Alarm input.\nIf you select maximum resolution, maximum FPS will be decreased."]
["HikVision","Hikvision DS-2CD862MF-E","Camera ","V2.0 build 110902","1",null,null,"+",null,"+",null,null,"320x240(MJPEG) / 1280x960 (H264)","320x240(MJPEG) / 1280x720 (H264)","320x240(MJPEG) / 640x480 (H264)","+",null,"+.","+","-","+","-",null,"+","+","В AxxonNext/Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.Через Onvif камера работает только в режиме совместимости.Камера поддерживает одни разрешения, а передает видео в других. Аналогичная ситуация и в веб-интерфейсе камеры","In AN, search does not detect the device's firmware. You must yourself select the right version of the camera's software. Over ONVIF the camera works only in compatibility mode. The camera seems to support one set of resolutions, but sends video with other resolutions. In the web interface, it is the same."]
["HikVision","Hikvision DS-2CD863PF-E ","Camera ","V3.0 110510","1",null,null,"+",null,"+",null,null,"352x288 (MJPEG) / 1280x960 (H264)","352x288 (MJPEG) / 640x480 (H264)","320x240","+",null,"+.","+",null,"+","-",null,"-","+","Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельноПри подключении ко второму стриммингу камера вещает с частотой ~12 fps. И в Интеллекте, и в AxxonNext/Next. Особенность камеры.Прошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.","Search detects the camera's vendor and model correctly, but you have to select the right firmware yourself. When you connect to the second stream, the camera sends video at around 12 fps. Both in Intellect and AN. This is a limitation of the camera itself. V3.0 110510 firmware: If you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device."]
["HikVision","Hikvision DS-2CD864FWD-E","Camera ","V3.2 120105","1",null,null,"+","+","+",null,null,"MPEG4, H264: 1280x960; MJPEG: 320x240","MPEG4, H264: 640x480; MJPEG: 320x240","320x240","+",null,"+","+",null,"+",null,null,"+","+","Если установить FPS = 8, реально приходит примерно один кадр в секунду - проблема камеры. Другие значения работают корректно.","If you set the frame rate to 8 fps, you get only around 1 fps in reality. This is a problem of the camera itself. Other values work fine. "]
["HikVision","Hikvision DS-2CD883F-E","Camera ","V3.0 build 110516 ","1",null,null,"+","+","+",null,null,"320x240 (MJPEG) / 2560x1920 (H264) / 2560x1920 (MPEG4)","320x240 (MJPEG) / 1600x1200 (H264) / 2048x1536 (MPEG4)","320x240 (MJPEG) / 320x240 (H264) / 800x600 (MPEG4)","+",null,"+","+","-","+","-",null,"-","+","В AxxonNext/Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.В AxxonNext/Next Смена потоков / кодеков требует перезагрузки устройства (~ 1 мин.)В Интеллекте переключение между полным и средним (минимальным) разрешением требует перезагрузки устройства (~ 1 мин).","In AN, search does not detect the device's firmware. You must yourself select the right version of the camera's software. In AN. After you switch to a different stream or codec, you must restart the device (around 1 minute). In Intellect, after you switch between the full and medium (average) resolutions, you must restart the device (around 1 minute). "]
["HikVision","Hikvision DS-2CD893PFWD-E / DS-2CD893PF-E","Camera ","V3.0 110510","1",null,null,"+",null,"+",null,null,"352x288 (MJPEG) / 704x576 (H264)","352x288 (MJPEG) / 704x576 (H264)","352x288","+",null,"+.","+",null,"+","-",null,"-","+","1. Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельно\n2. Прошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.","1. Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. \n2. V3.0 110510 firmware: \nIf you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device."]
["HikVision","Hikvision DS-2DF1-401H","Camera ","V3.1.0 120107","1",null,null,"+",null,"+",null,null,"704x576","528x384","352x288","+",null,"+.","+","+","+","-",null,"+","+","Смена кодека приводит к перезагрузке камеры (~1 минута).Во втором потоке звук с камеры идет с прерываниями.","If you switch to a different codec, the camera must restart (1 minute). In the second stream, audio is intermittent. "]
["HikVision","Hikvision DS-2DF1-402H","Camera ","V3.1.0 110811","1",null,null,"+",null,"+",null,null,"704x576","528x384","352x288","+",null,"-","-","+","-","-","-","-","+"]
["HikVision","Hikvision DS-2DF1-512/514/516/518","Camera ","V3.1.0 120107","1",null,null,"+",null,"+",null,null,"704x576","528x384","352x288","+",null,"+","+","+","+","-",null,"+","+","1. Смена кодека приводит к перезагрузке камеры (~1 минута).\n2. Во втором потоке звук с камеры идет с прерываниями.","1. If you switch to a different codec, the camera must restart (1 minute). \n2. In the second stream, audio is intermittent. "]
["HikVision","Hikvision DS-2DF1-572","Camera ","4.0.0 111122","1",null,null,"+",null,"+",null,null,"1280x720","1280x720","704x576","+",null,"+","+","+","+","-",null,"+","+","Смена кодека приводит к перезагрузке камеры (~1 минута)Во втором потоке звук с камеры идет с прерываниями. В Интеллекте это воспроизводится при выборе минимальных разрешений.","If you switch to a different codec, the camera must restart (1 minute). In the second stream, audio is intermittent. In Intellect, this happens if you select the minimum resolution. "]
["HikVision","Hikvision DS-2DF1-607(H) / 617(H)","Camera ","V3.1.0 110811","1",null,null,"+",null,"+",null,null,"704x576","528x384","352x288","+",{"$nulls":3},"+",{"$nulls":4},"+"]
["HikVision","Hikvision DS-2DF1-614H","Camera ","V3.1.0 110811","1",null,null,"+",null,"+",null,null,"704x576","528x384","352x288","+",null,"+.","-","+","+","-",null,"+","+"]
["HikVision","Hikvision DS-2DF1-714/716/718","Camera ","V3.1.0 120107","1",null,null,"+",null,"+",null,null,"704x576","528x384","352x288","+",null,"+.","+","+","+","-",null,"+","+","На камерах физически есть 7 лучей, в нашем ПО они все также интегрированы, но по умолчанию работают только первые 2. Поддержка остальных опциональна. За подробной информацией нужно обращаться к производителю.Камера HikVision DS-2DF1-714 (прошивка V3.1.0 110811) отличается несколько нестабильным поведением: при изменении разрешения камера очень долго его применяет (3-5 минут). Сначала камера долго думает, затем перезагружается, и после перезагрузки видео начинает идти в установленном разрешении.","Physically, the camera has 7 sensors; in our software, they are all integrated, but only the first 2 work by default. The others are supported optionally. For detailed information, refer to the vendor. The HikVision DS-2DF1-714 camera (V3.1.0 110811 firmware) is somewhat unstable: when you change the resolution, the camera takes a very long time to apply the change (3–5 min.). The camera first \"thinks\" for a long time, then restarts, and after that video comes at the new resolution. "]
["HikVision","Hikvision DS-2DF5284-A","Camera ","V5.0.0 build 130518","1",null,null,"+","+","+",null,null,"1920x1080(H.264 / MPEG4) / 704x576(MJPEG PAL) / 704x480(MJPEG NTSC)","1280x960(H.264 / MPEG4) / 704x576(MJPEG PAL) / 704x480(MJPEG NTSC)","1280x720(H.264 / MPEG4) / 352x288(MJPEG PAL) / 352x240(MJPEG NTSC)","+",null,"+","+","+","+","-",null,"motion detection","+","Детектор движения в продукте срабатывает только если в веб-интерфейсе камеры для детектора движения заполнена таблица Arming Schedule\nЛучи в продукте срабатывает только если в веб-интерфейсе камеры для Alarm input заполнена таблица Arming Schedule","Motion detector in AxxonSoft products works only if in camera's web interface filled Arming Schedule table.\nRays in AxxonSoft products works only if in camera's web interface filled Arming Schedule table for Alarm input."]
["HikVision","Hikvision DS-2DZ216","Camera ","V3.0 build 111226","1",null,null,"+","-","+",null,null,"H264:1280x960 MJPEG:352x288","H264:640x480 MJPEG:352x288","320x240","+",null,"+.","+","-","+","-",null,"+","+","Параметр Image Flip (отражение) интегрирован, но на самой камере он не работает. Т.е. при изменении параметра через наш продукт в веб-интерфейсе значение применяется, но реально картинка не отражается.Прошивка V3.0 110408: Устройство обнаруживается поиском только как Onvif.","The Image Flip parameter is integrated, but it does not work on the camera itself. That is, when you change this parameter in our software, the change is applied in the web interface, but in reality the image does not flip. V3.0 110408 firmware: Search detects the device only as a device that supports ONVIF. "]
["HikVision","Hikvision DS6101HFI-IP","Encoder ","auto ","1",{"$nulls":4},"+",null,null,"704x576","704x288","352x288","+",{"$nulls":8},"-"]
["HikVision","Hikvision DS-6504HFI","DVR","V1.0.1 build 110104","4",null,null,"-","-","+","-","-","704x576","528x384","352x288","+","-","-","-","-","-","-","-","-","-","В настройках подключения необходимо указывать порт 8000.","Specify port 8000 in the connection settings."]
["HikVision","HikVision DS-6508HFI","Encoder ","V1.0.1 build 110104","8",{"$nulls":4},"+",null,null,"704x576","704x288","352x288","+",{"$nulls":3},"-",{"$nulls":3},"-","-","Порт должен быть 8000.","Set the port number to 8000."]
["HikVision","Hikvision DS-6516HFI","Encoder ","V1.0.1 build 110104 ","16",{"$nulls":4},"+",null,null,"704x576","704x288","352x288","+",null,"+",null,"+",null,"+",null,"-","-","Порт должен быть 8000.","Set the port number to 8000."]
["HikVision","Hikvision DS-6701HFI","Encoder/Decoder","V1.1.0 build 130709","1",null,null,"+","+","+","-","-","704x576","704x288","352x288","+","-","-","-","-","-","-","-","-","+"]
["HikVision","Hikvision DS-7204HFI-SH","DVR","V2.2.10 build 130924","4",{"$nulls":4},"+",null,null,"704x576","704x288","352x288","+",{"$nulls":8},"-"]
["HikVision","Hikvision DS-7204HVI-SH","NVR","V2.1.2 build 121024","4",{"$nulls":4},"+",null,null,"-","704x288","352x288","+",{"$nulls":3},"+","+","+","+",null,"-","Устройство поддерживает 4 резрешения:\n\n 176 x 144\n 352 x 288\n 704 x 288\n 704 x 576 \n\nЕсли на любом канале выбрать разрешение больше чем 352 x 288, то на других будут доступны только 352 x 288 и 176 x 144.","The camera supports four resolutions:\n\n 176 x 144\n 352 x 288\n 704 x 288\n 704 x 576 \n\nIf a resolution greater than 352 x 288 is chosen on any channel, then only 352 x 288 and 176 x 144 will be available on the others."]
["HikVision","Hikvision DS-7204HV-ST","DVR","Master verson: V1.3.2 build 121107 Encode Version: V5.0 build 120807","4",null,null,"-","-","+","-","-","704x576","704x288","352x288","+",null,"-","-","-","-","-","+","-","+"]
["HikVision","Hikvision DS-7216-HWI-SH/A","DVR","V2.2.8 build 130815","16","-","1",null,null,"+",null,null,"960x576","704x576","352x288",null,null,"-","-","-","-","-","+","-","-",null,null,"new"]
["HikVision","Hikvision DS-2CD8254FWD-EIS","Camera","V4.1.0 130111","1","-",null,"+","+","+",null,null,"2048x1536 (H.264, MPEG4) / 704x576 (MJPEG)","1280x720 (H.264, MPEG4) / 352x288 (MJPEG)","320x240","+",null,"-","-",null,"-","-",null,"-","+",null,null,"new"]
["HikVision","Hikvision DS-8104HMFI-ST","NVR","V2.1.0.120112","4",{"$nulls":4},"+",null,null,"704x576","704x576","704x288 ","+",{"$nulls":8},"-"]
["HikVision","Hikvision DVR DS-9632NI-ST","DVR","V2.1.0 build 111017","32",{"$nulls":4},"+",null,null,"2048x1536","1600x1200","320x240","-",null,"-","-",{"$nulls":3},"+",null,"-","Для подключения к устройству используется порт 8000.","To connect the device need to use 8000 port."]
["Honeywell","Honeywell H3D1F1X (ONVIF)","Camera","40.0.6","1",null,null,"+","-","+",null,null,"1280x720 (H264) / 640x368 (MJPEG)","800x448 (H264) / 640x368 (MJPEG)","640x368","+",null,"+","-","-","-","+","-","-","+"]
["Honeywell","Honeywell H4D2F1X (ONVIF)","Camera","V40.0.6","1",null,null,"+","-","+",null,null,"1920x1080(H264)/640x368(MJPEG)","800x448 (H264) / 640x368 (MJPEG)","640x368","+","-","+","-","-","-","+","-","-","+"]
["Honeywell","Honeywell HCD2FX (ONVIF)","Camera","40.0.6","1",null,null,"+","-","+",null,null,"1280x720 (H264) / 640x368 (MJPEG)","800x448 (H264) / 640x368 (MJPEG)","640x368","-",null,"+","-","-","-","+","-","-","+"]
["Honeywell","Honeywell HDZ20HDEX (ONVIF)","Camera","MW1D-9C2B ","1",null,null,"+","-","+",null,null,"1920x1080","800x600","640x480","-",null,"+","-","+","-","+.","-","-","+"]
["Hunt","Hunt HLV-1FM","Camera ","3.2.44","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","320x240","+",null,"-","-",null,null,"+",null,"-","-","1. При мегапиксельном разрешении видео идет с max. 10 fps\n2. У камеры 2 канала (хоть объектив и один). С одного объектива можно получить два видеопотока с разными настройками. В нашем ПО нужно создавать на одном граббере две камеры на 1-ый и 2-ой каналы","1. At megapixel resolutions, the max. resolution is 10 fps \n2. The camera has two channels (though only 1 lens). With the same lens, you can get two video streams with different settings. In our software, you must create two cameras for the same grabber. "]
["Hunt","Hunt HR-HLC-1NCD/P, HR-HLV-1WCD/P","Camera ","VC1.0.18.2","1",null,null,"+",null,"+",null,null,"1920x1080","640x480","320x240","+",null,"+","+","-","+","+","-","motion detection;","+"]
["Hunt","Hunt HR-HLC-79CD/W","Camera ","VC1.0.18.2","1",null,null,"+",null,"+",null,null,"1920x1080","640x480","320x240","+",null,"+","+","-","+","+","-","motion detection;","+"]
["Hunt","Hunt HR-HLC-84BM/W","Camera ","VB1.0.40","1",null,null,"+","+","+",null,null,"1280x800","640x480","320x240","+",null,"+","+","-","+","+",null,null,"+"]
["Hunt","Hunt HR-HLT-S30/22x/P","Camera ","VB1.0.40.dc","1",null,null,"+","+","+",null,null,"1280x1024","1280x960","640x480","-",null,"+","+","+.","+","+","-","motion detection;","+"]
["Infinity","Infinity IPB-TDN540SL","Camera ","4.1.2.-50","1",{"$nulls":3},"+",{"$nulls":3},"720x576","640x480","320x240","+",{"$nulls":4},"+","-",null,"-","+"]
["Infinity","Infinity IPB-TDN540SLHP","Camera ","1.6.0-release","1",null,null,"+","+","+",null,null,"704x576","640x480","320x240","+",null,"-","-",null,"-","-",null,"-","+"]
["Infinity","Infinity IPD-S10ZVP540SL","Camera ","4.1.2-50","1",{"$nulls":3},"+",{"$nulls":3},"720x576","640x480","320x240","+",null,"+","-","+","+","-",null,"-","+"]
["Infinity","Infinity IPS-18ZDN480SD","Camera ","4.1.2-50","1",{"$nulls":3},"+",{"$nulls":3},"704x576","640x480","320x240","+",null,"+.","-","+.","+","-",null,"-","+","1. С прошивкой 4.1.2-50 будет такая проблема - звук отстает от видео на 25 секунд - проблема в прошивке.","1. With the 4.1.2-50 firmware, we have the following problem: – audio lags behind video by 25 seconds. This is a firmware problem. "]
["Infinity","Infinity IPS-26ZDN480ED","Camera ","4.1.2-51","1",{"$nulls":3},"+",{"$nulls":3},"720x576","640x480","320x240","+",null,"+.","-","+.","+.","+",null,"-","+"]
["Infinity","Infinity IPZ-22WDN480SL","Camera ","4.1.2-50","1",{"$nulls":3},"+",{"$nulls":3},"720x576","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","+","1) Телеметрия у камеры состоит из зума и фокуса\n2) Видео с камеры в Intellect примерно каждые 10-15 секунд подвисает на секунду - это проблема самой камеры (если посмотреть на видео не через Интеллект, а например через VLC плеер, то в эти моменты видео искажается)","1) The camera's telemetry functionality consists of zoom and focus.\n2) In Intellect, video freezes for 1 sec. every 10–15 sec. This is a problem of the camera itself (if you view video with a different viewer, for example, the VLC player, then the video is distorted when it is frozen in Intellect)."]
["Infinova","Infinova V17xxN-M Series ","Camera ","1.05.01.20100730","1",null,null,"+","+",{"$nulls":3},"720x480","704x240","352x240","+",null,null,"-","+","-","-",null,"-","+","Прошивка 1.05.01.20100730: значение \"1 fps\" параметра \"Частота кадров\" в кодеке MJPEG не применяется - проблема устройства.","1.05.01.20100730 firmware: with the MJPEG codec, the value of 1 fps for the Frame Rate parameter cannot be applied. This is a problem of the device itself."]
["Infinova","Infinova V17xxN-N Series","Camera ","2.00.01.20111014","1",null,null,"+",null,"+",null,null,"704x480","704x480","352x240","+",null,null,"-","+","-","-",null,"-","+"]
["Infinova","Infinova V6201-N0320","Camera ","1.00.00.201108015_onvif ","1",null,null,"+",null,"+",null,null,"2048x1536 (MJPEG) / 1920x1080 (H264)","2048x1536 (MJPEG) / 1280x720 (H264)","2048x1536 (MJPEG) / 1280x720 (H264)","+",null,"-","-",null,"-","-",null,"-","+","Через Onvif работает получение видео.","Via the ONVIF protocol, you can receive video. "]
["InMotion","InMotion HD WDR","Camera ","d20100414NS","1",null,null,"+","+","+",null,null,"1280x960(MJPEG) / 1280x960(MPEG-4) / 640x480(H.264)","640x480","320x240","+",null,"+.","-","+.","+","+",null,"-","+","Кнопки упраления Zoom'ом и Focus'ом перепутаны, но это проблема самого устойства, в \"родном\" ПО точно такая же проблема.При разрешении 1280x960 максимальный доступный fps = 12,5Реле камеры по-умолчанию работает в режиме \"нормально-замкнуто\". Особенность устройства, при необходимости можно изменить через web-интерфейс.","The buttons for controlling zoom and focus are mixed up, but this is the problem of the device itself: the device's own software has the same problem. At 1280x960 resolution, the max. frame rate is 12.5 fps. By default, the camera's relay works in Normally Closed mode. This is a feature of the device; if necessary, you can change it in the web interface."]
["InMotion","InMotion L84II","Encoder ","0063-027y-0639-625z","4",{"$nulls":4},"+",null,null,"720x576","720x576","720x576","+.",null,null,"-",{"$nulls":4},"-","+"]
["InMotion","InMotion L86T","Encoder ","0027-010a-0608-587a","16",{"$nulls":4},"+",null,null,"720x576","720x576","720x576","-",null,null,"-",{"$nulls":4},"-","+"]
["InMotion","InMotion L88II","Encoder ","0049-023E-0615-609H","8",{"$nulls":4},"+",null,null,"720x576","720x576","720x576","+.",null,"+.","-","-","+","+",null,"-","+","Приемлемую частоту кадров можно настроить только через OSD-меню DVR'а.Длительность тревоги после срабатывания луча настраивается в веб-интерфейсе. По умолчанию стоит минимальное значение - 5 секунд.","An acceptable frame rate may be set only using the DVR's OSD menu. To set how long an alarm is \"sounded\" after the sensor goes off, go to the web interface. By default, the minimum value is set (5 seconds). "]
["Intellico ","Intellico IL-IZH72DX ","Camera ","2.3.0.5.56.2 ","1",null,null,"+",null,"+",null,null,"1280x960 ","1280x720 ","1280x720 ","+",null,"+.",null,"+",null,"+",null,null,"-","Для подключения к камере необходимо в ПО ITV/Axxon указывать порт, настроенный в веб-интерфейсе камеры (Network Settings -> Basic -> Data port). По умолчанию он равен 5000. ","To connect to the camera, please specify in Axxon SW a port that is configured in the web interface of the camera (Network Settings -> Basic -> Data port). The default is 5000."]
["IPS ","IPS IPS-9XX/IPS-Eye-XXX Series ","Camera ","1.8.1.1i_201302211839_DBU","1",{"$nulls":4},"+",null,null,"1600x1200 ","1280x720","640x360","+",{"$nulls":3},"+",{"$nulls":4},"+","Прошивка 1.8.1.1i_201302211839_DBU: Для получения видео со второго потока, необходимо чтобы на первом потоке было установлено разрешение 720р. ","Firmware 1.8.1.1i_201302211839_DBU: to get video from the 2nd stream, please specify 720p resolution for the 1st stream. "]
["iPUX","iPUX ICS1330","Camera ","1.1.0","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":3},"+.",{"$nulls":3},"motion detection","+","Применение настроек видео требует перезагрузки камеры, поэтому на изменение любой настройки уходит около минуты.","Changes are applied after reboot. This is why to change any setting, it takes about 1 minute."]
["iPUX","iPUX ICS203A","Camera ","1.0.0","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":7},"motion detection","+","Применение настроек видео требует перезагрузки камеры, поэтому на изменение любой настройки уходит около минуты.","Changes are applied after reboot. This is why to change any setting, it takes about 1 minute."]
["iPUX","iPUX ICS2330","Camera ","1.1.0","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",{"$nulls":3},"+.",{"$nulls":3},"motion detection","+"]
["iPUX","iPUX ICS7232","Camera ","1.0.0","1",null,null,"+","+","+",null,null,"1280x1024 (H264, MJPEG) / 640x480 (MPEG4)","640x480","320x240","+",{"$nulls":7},"motion detection","+","Применение настроек видео требует перезагрузки камеры, поэтому на изменение любой настройки уходит около минуты.","Changes are applied after reboot. This is why to change any setting, it takes about 1 minute."]
["iPUX","iPUX ICS8200 / ICS8220","Camera ","1.0.0","1",null,null,"+","+","+",null,null,"2048x1536 (H264, MJPEG) / 1920x1080 (MPEG4)","1280x960","640x480","+",{"$nulls":7},"motion detection","+","1. На камере есть зависимость разрешений от кодеков и fps от разрешений.\n2. При разрешениях больше 1280x720 недоступен двухпоточный режим.\n3. Применение настроек видео требует перезагрузки камеры, поэтому на изменение любой настройки уходит около минуты.","1. The camera's resolutions depend on codecs, and fps depend on resolutions. \n2. Dual stream mode is not available with resolutions over 1280x720. \n3. Changes are applied after reboot. This is why to change any setting, it takes about 1 minute."]
["iPUX","iPUX IVS7100","Camera ","1.0.0 build: 122","1",null,null,"+","+","+",null,null,"from WEB","from WEB","from WEB","+",{"$nulls":7},"motion detection","+","1. На камере не применяются разрешения (ошибка прошивки) f.w. 1.0.0 build: 122","1. You can't change resolutions for that camera, due to a bug in firmware. 1.0.0 build: 122"]
["IQinVision","IQeye IQ040S","Camera ","V3.1/8(101026)","1",null,null,"+",{"$nulls":4},"704x480","from WEB","from WEB","+",{"$nulls":7},"-","+","Можно выставить любое разрешение из диапазона [704x480; 320x240]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [704x480; 320x240] range. To use it in Intellect, set the resolution in the camera's web interface. "]
["IQinVision","IQeye IQ041S","Camera ","V3.1/8(101026)","1",null,null,"+",{"$nulls":4},"1280x1024","from WEB","from WEB","+",{"$nulls":7},"-","+","Можно выставить любое разрешение из диапазона [1280x1024; 320x240]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1280x1024; 320x240] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ042S","Camera ","V3.1/8(101026)","1",null,null,"+",{"$nulls":4},"1600x1200","from WEB","from WEB","+",{"$nulls":7},"-","+","в AxxonNext/Next можно задать любое разрешение из диапазона [320*240 ; 1600*1200] - при этом обрезается картинка и отображается только её часть (чем меньше часть, тем больше fps)\nв Intellect разрешение изменить нельзя (можно только через web камеры)","In AN, you can select any resolution in the [320*240 ; 1600*1200] range; when you do so, the image is cropped and only a part of the image is shown (the smaller the part, the higher the frame rate).\nIn Intellect, you cannot change the resolution (only in the web interface)."]
["IQinVision","IQeye IQ510","Camera ","V2.8/7(090818)","1",null,null,"+",{"$nulls":4},"752x480","from WEB","from WEB","+",{"$nulls":7},"-","+","Можно выставить любое разрешение из диапазона [752x480; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [752x480; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ511","Camera ","V2.8/7(090818)","1",null,null,"+",{"$nulls":4},"1280x1024","from WEB","from WEB","+",{"$nulls":7},"-","+","Можно выставить любое разрешение из диапазона [1280x1024; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры. прошивки V2.8/7(090818) в аттаче нет, есть предыдущая V2.8/6(080313)","You can select any resolution from the [1280x1024; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface. The attachment does not contain the V2.8/7(090818) firmware, it contains only the previous version, V2.8/6(080313)."]
["IQinVision","IQeye IQ541S","Camera ","V3.1/7(100810)","1",null,null,"+",{"$nulls":4},"1280x1024","from WEB","from WEB","+",{"$nulls":7},"-","+","Можно выставить любое разрешение из диапазона [1280x1024; 320x240]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1280x1024; 320x240] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ702","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"1600x1200","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [1600x1200; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1600x1200; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ703","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"2048x1536","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [2048x1536; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [2048x1536; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ705","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"2560x1920","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [2560x1920; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры","You can select any resolution from the [2560x1920; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ711","Camera ","IQeye711 Version V3.0/8","1",null,null,"+",{"$nulls":4},"1280x1024","from WEB","from WEB","+",{"$nulls":4},"-","+",null,"-","+","1. Для Intellect разрешение выставляется в web-интерфейсе камеры из диапазона [1280x1024; 512x256]","1. You can select any resolution from the [1280x1024; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ732N","Camera ","V3.2/2(101109)","1",null,null,"+",{"$nulls":4},"from WEB","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+"]
["IQinVision","IQeye IQ751","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"1280x1024","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [1280x1024; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры","You can select any resolution from the [1280x1024; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ752","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"1600x1200","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [1600x1200; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1600x1200; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ753","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"2048x1536","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [2048x1536; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [2048x1536; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ755","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"2560x1920","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [2560x1920; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры","You can select any resolution from the [2560x1920; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ851","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"1280x1024","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [1280x1024; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1280x1024; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ852","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"1600x1200","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [1600x1200; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1600x1200; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ853","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"2048x1536","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [2048x1536; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [2048x1536; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ855","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"2560x1920","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [2560x1920; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры","You can select any resolution from the [2560x1920; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ861N","Camera ","V3.4/2(120925)","1",null,null,"+",null,"+",null,null,"1280x720","720x480","352x240","+",{"$nulls":3},"-",{"$nulls":4},"+"]
["IQinVision","IQeye IQA20S","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"640x480","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [640x480; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [640x480; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQA22S","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"1600x1200","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [1600x1200; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1600x1200; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQA23S","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"2048x1536","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [2048x1536; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [2048x1536; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQA25S","Camera ","V3.0/8(100702)","1",null,null,"+",{"$nulls":4},"2560x1920","from WEB","from WEB","+",{"$nulls":4},"-",null,null,"-","+","Можно выставить любое разрешение из диапазона [2560x1920; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры","You can select any resolution from the [2560x1920; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQD30S","Camera ","B3.1/609(100329)","1",null,null,"+",null,"+.",null,null,"720x480","720x480","720x480 (H.264) / 352x240 (MJPEG)","+",null,"+","-",{"$nulls":4},"-","+"]
["IQinVision","IQeye IQD31S","Camera ","B3.1/602(100217","1",null,null,"+",null,"+",null,null,"1280x720","1280x720","1280x720(H.264) / 720x480(MJPEG)","+",null,"+.","-",{"$nulls":4},"-","+"]
["IQinVision","IQeye IQD32S","Camera ","V3.3/4(120130)","1",null,null,"+",null,"+",null,null,"1920x1080","1280x720","704x480","+",null,"+","-",{"$nulls":4},"-","+","Продукт может получать видео одновременно только с 1. и 2. ; с 5. и 6. потока","The VMS receives video from streams 1 and 2 or 5 and 6 at the same time. ; с 5. и 6. потока"]
["IQinVision","IQeye IQD40S","Camera ","V3.1/8(101026)","1",null,null,"+",{"$nulls":4},"720x480","from WEB","from WEB","+",{"$nulls":7},"-","+","Можно выставить любое разрешение из диапазона [720x480; 320x240]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [720x480; 320x240] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQD41S","Camera ","V3.1/8(101026)","1",null,null,"+",{"$nulls":4},"1280x1024","from WEB","from WEB","+",{"$nulls":7},"-","+","Можно выставить любое разрешение из диапазона [1280x1024; 320x240]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1280x1024; 320x240] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQD42S","Camera ","V3.1/8(101026)","1",null,null,"+",{"$nulls":4},"1600x1200","from WEB","from WEB","+",{"$nulls":7},"-","+","Можно выставить любое разрешение из диапазона [1600x1200; 320x240]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1600x1200; 320x240] range. To use it in Intellect, set the resolution in the camera's web interface."]
["iZett","iZett HR-BT2030C(W)","Camera ","VC1.0.18.2","1",null,null,"+",null,"+",null,null,"1920x1080","640x480","320x240","+",null,"+","+","-","+","+",null,"motion detection","+"]
["iZett","iZett HR-CB1330B(W)","Camera ","VB1.0.40","1",null,null,"+","+","+",null,null,"1280x800","640x480","320x240","+",null,"+","+","-","+","+","-","motion detection","+"]
["iZett","iZett HR-CB6430BP","Camera ","iZett-VB1.0.38_SO-20130823","1",null,null,"+","+","+",null,null,"640x480","640x480","320x240","+",null,"+","+",null,"+","+","-","motion detection","+"]
["iZett","iZett HR-FD2030C(P/VP)","Camera ","VC1.0.18.2","1",null,null,"+",null,"+",null,null,"1920x1080","640x480","320x240","+",null,"+","+","-","+","+","-","motion detection","+"]
["iZett","iZett HR-SD1330X22","Camera ","VB1.0.40.dc ","1",null,null,"+","+","+",null,null,"1280x1024","1280x960","640x480","-",null,"+","+","+.","+","+","-","motion detection","+"]
["J2000IP","J2000IP DWV112-Ir1-PDN / PWH112-Ir4-PDN","Camera ","v1.6_build044014_145","1",null,null,"+",null,"+",null,null,"1920x1080 / 1280x720","1920x1080 / 1280x720","640x360",null,null,"+",{"$nulls":6},"-","Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\nЧастота опорных кадров задается в секундах и может принимать значения от 1 до 3.\nДля корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz.\nМаксимально доступное разрешение в ПО ITV/Axxon зависит от значения настройки Source Resolution в веб-интерфейсе камеры.","To connect to the camera required in connection settings set port 30001 in AxxonSoft products.\nReference frames frequency specified in seconds and can take values ​​from 1 to 3.\nFor FPS settings correct work in AxxonSoft software, recommended to set 60Hz mode in camera's web interface.\nMaximum available resolution AxxonSoft software depends on Source Resolution setting in camera's web-interface."]
["J2000IP","J2000IP DWV120-Ir1DN / DWV120-Ir1-PDN / DWV120-PDN","Camera ","v1.6_build044012_025","1",null,null,"+",null,"+",null,null,"704x576","704x576","352x288",null,null,"+",{"$nulls":6},"-"]
["J2000IP","J2000IP DWV311-Ir3-PDN","Camera ","v1.6_build044014_145","1",null,null,"+",null,"+",null,null,"1280x960 / 1280x720","from WEB / 1280x720","640x480 / 1280x720",null,null,"+",{"$nulls":6},"-","1. Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\n2. Набор разрешений в ПО ITV/Axxon зависит от значения настройки Source Resolution в веб-интерфейсе.\n3. При смене разрешений для кодека H.264 меняется диапазон значений битрейта. Если при переходе на новое разрешение текущий битрейт не попадает в новый диапазон, то настройка не применяется.\n4. Для корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz. ","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. The list of resolution in Axxonsoft SW depends on value of Source Resolution in web interface.\n3. When resolution for H.264 is changed, range of bitrate value is also changed. If there's no current bitrate value for new resolution, in this case setting is not applied.\n4. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["J2000IP","J2000IP mDWV112-Ir1-PDN","Camera ","v1.6_build044014_101","1",null,null,"+",null,"+",null,null,"1920x1080","1920x1080","640x360",null,null,"+",{"$nulls":6},"-","1. Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\n2. Для корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz. \n\n","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["J2000IP","J2000IP PWH121-Ir4-PDN","Camera ","v1.6_build044014_136","1",null,null,"+",null,"+",null,null,"1280x720","1280x720","640x360",null,null,"+",{"$nulls":6},"-"]
["J2000IP","J2000IP PWH312-Ir3-PDN / PWH312-Ir4-PDN / PWH312-Ir5-PDN","Camera ","v1.6_build044014_101","1",null,null,"+",null,"+",null,null,"1920x1080 ","1920x1080 ","640x360",null,null,"+",{"$nulls":6},"-","1. Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\n2. Частота опорных кадров задается в секундах и может принимать значения от 1 до 3.\n3. Для корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz.\n4. Максимальное разрешение в продукте зависит от настройки максимального разрешение на камере\n","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. The frequency of of keyframes is set in seconds and can be from 1 to 3.\n3. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly.\n4. Max resolution in Axxonsoft SW depends on camera max resolution.\n"]
["J2000IP","J2000IP PWH313-Ir5-PDN / J2000IP-PWVH313-Ir4-PDN","Camera ","v1.6_build044014_145","1",null,null,"+",null,"+",null,null,"2048x1536","1280x720","640x480",null,null,"+",{"$nulls":6},"-","1. Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\n2. Максимальное разрешение зависит от настройки Source Resolution в веб-интерфейсе\n3. Для корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz. ","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. Max resolution in Axxonsoft SW depends on value of Source Resolution in web interface.\n3. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["J2000IP","J2000IP SDW112-24x20DN","Camera ","v1.6_build044014_101","1",null,null,"+",null,"+",null,null,"1920x1080","1920x1080","640x360",null,null,"+",null,"+.",{"$nulls":4},"-","1. Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\n2. Частота опорных кадров задается в секундах и может принимать значения от 1 до 3.\n3. Для корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz. ","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. The frequency of of keyframes is set in seconds and can be from 1 to 3.\n3. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["J2000IP","J2000IP SDW121-24x18DN","Camera ","v1.6_build044014_145","1",null,null,"+",null,"+",null,null,"1280x720","1280x720","640x360",null,null,"+",null,"+",{"$nulls":4},"-","1. Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\n2. Для корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz. ","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["Jassun","Jassun JSI-DPV200IR / JSI-XV200IR / JSI-D200IR / JSI-DV200IP / JSI-C200IR","Camera","1.0.5.1.013_20130930","1",null,null,"+","-","+",null,null,"1920x1080","1280x960","640x480","+",null,"+","+","-","+","+","-","-","+"]
["Jassun","Jassun JSI-XV300IR","Camera","1.0.5.1.013","1",null,null,"+","-","+",null,null,"2048x1536","1280x960","640x480","+",null,"-","-","-","-","-","-","-","+"]
["JVC","JVC VN-C20U","Camera ","1.03b","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":4},"-","-",null,"-","-","1. Не работают настройка яркости и цветности в Intellect\n2. Не работает настройка качества записи на диск\n ","1. In Intellect, the brightness and color settings do not work \n2. The recording quality control does not work\n "]
["JVC","JVC VN-C625U","Camera ","02.06","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":3},"+","-","-",null,"-","-","Видео с разрешением \"Стандартное\" (320х240) отображается на экране КПК с задержкой\n ","Video at standard (320х240) resolution is shown with a delay on the pocket PC screen\n "]
["JVC","JVC VN-C655U","Camera ","02.06","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":3},"+","-","-",null,"-","-","Настройка реле/лучей на камере не возможна, управление диафрагмой (Iris) не реализовано.\n ","Cannot configure alarm I/O on the camera, iris control is not implemented.\n "]
["JVC","JVC VN-H137U","Camera ","3.00.261","1",null,null,"+","+","+",null,null,"1920x1080 (MJPEG / H264) / --- (MPEG4)","1280x960","640x480","+",{"$nulls":7},"+","+","1. Телеметрия работает только при выбранном разрешении 640x360 или 640x480. \n2. На разных потоках камера позволяет включать разрешения с одинаковым соотношением сторон: 4:3 (1280x960, 640x480, 320x240) или 16:9 (1920x1080, 1280x720, 640x360).\n3. Максимальная частота кадров в мультипотоковом режим - 15 fps.\n4. В кодеке MPEG4 недоступно разрешение 1920х1080.\n 5. Допустимые комбинации кодеков в мультипотоковом режиме:\n 0/2.h264 + 1.h264\n 0/2.mjpeg + 1.mjpeg\n 0/2.mjpeg + 1.h264\n 0/2.mjpeg (320x240) + 1.mpeg4 (320x240)\n 0/2.mjpeg (640x480) + 1.mpeg4 (640x480)\n 0/2.mjpeg (1280x960) + 1.mpeg4 (320x240)\n 0/2.mjpeg (1280x960) + 1.mpeg4 (640x480) ","1. The telemetry works only with chosen 640x360 or 640x480 resolutions. \n2. For different streams the camera allows enabling resolutions with an identical aspect ratio: 4:3 (1280x960, 640x480, 320x240) or 16:9 (1920x1080, 1280x720, 640x360).\n3. The maximum frame rate in multi-stream mode is 15 fps.\n4. In the MPEG4 codec 1920х1080 resolution is unavailable.\n 5. Admissible combinations of codecs in a multi-stream mode:\n 0/2.h264 + 1.h264\n 0/2.mjpeg + 1.mjpeg\n 0/2.mjpeg + 1.h264\n 0/2.mjpeg (320x240) + 1.mpeg4 (320x240)\n\n 0/2.mjpeg (640x480) + 1.mpeg4 (640x480)\n 0/2.mjpeg (1280x960) + 1.mpeg4 (320x240)\n 0/2.mjpeg (1280x960) + 1.mpeg4 (640x480)\n"]
["JVC","JVC VN-H157WPU","Camera ","4.00.575","1",null,null,"+","+","+",null,null,"1920x1080","1280x960","640x480","+",{"$nulls":3},"+",{"$nulls":3},"-","+","1. Телеметрия работает только при выбранном разрешении 640x360 или 640x480. ","1. The telemetry works only with chosen 640x360 or 640x480 resolutions. "]
["JVC","JVC VN-H237U / VN-H237VPU","Camera ","4.00.314","1",null,null,"+","+","+",null,null,"1920x1080","1280x960","640x480","+",{"$nulls":3},"+",{"$nulls":3},"motion detection","+","1. Телеметрия работает только при разрешениях 640x480 и 640x360.","1. Telemetry works only for 640x480 and 640x360 resolutions."]
["JVC","JVC VN-H257U / VN-H257VPU","Camera ","4.00.575","1",null,null,"+","+","+",null,null,"1920x1080","1280x720","640x480","+",null,"+","+","+","+","+.",null,"motion detection","+","1. Цифровая телеметрия работает только при разрешениях 640x480 и 640x360","1. Digital PTZ works only for 640x480 and 640x360 resolutions."]
["JVC","JVC VN-H37U","Camera ","4.00.314","1",null,null,"+","+","+",null,null,"1920x1080","1280x960","640x480","+",{"$nulls":3},"+",{"$nulls":3},"motion detection","+","1. Телеметрия работает только при разрешениях 640x480 и 640x360.","1. Telemetry works only for 640x480 and 640x360 resolutions."]
["JVC","JVC VN-H57U","Camera ","4.00.575","1",null,null,"+","+","+",null,null,"1920x1080","1280x960","640x480","+",null,"+","+","+","+","+",null,"motion detection","+","1. Зум работает только при разрешении 640x480 или 640x360.","1. Zooms works only for 640x480 and 640x360 resolutions."]
["JVC","JVC VN-H557U","Camera","1.00.524","1","+","3","+",null,"+",null,null,"1920x1080","1280x960","640x360","+",null,"-","-","+","-","-","-","-","+","На втором и третьем потоке нельзя выставить значение разрешения больше чем на первом. ","The second and third streams can’t have resolution higher than the first one.","new"]
["JVC","JVC VN-H657(U) / VN-H657WP(U)","Camera ","2.00.801","1",null,null,"+",null,"+",null,null,"1920x1080","1280x960","640x360","+",{"$nulls":3},"+",{"$nulls":4},"+","На устройстве есть взаимосвязь между разрешением и минимальным битрейтом.","The camera's settings for resolution and bit rate are interdependent."]
["JVC","JVC VN-T216(VPRU) / VN-T16U","Camera ","j.2.2.1980","1",null,null,"+","+","+",null,null,"MJPEG/MPEG4: 1280х720; H.264: 1920x1080","640x480","320x240","+.",null,null,"-",null,"-","-",null,"-","+"]
["JVC","JVC VN-V225U","Camera ","1.01","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+","-",null,"+","+",null,"-","+"]
["JVC","JVC VN-V25U","Camera","2.02","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":4},"+","+",null,"-","+"]
["JVC","JVC VN-V26U","Camera ","2.02","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","352x240","+",null,"+","+",null,"+","+",null,"-","+"]
["JVC","JVC VN-V685U","Camera ","3.04","1",null,null,"+","+.",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","+"]
["JVC","JVC VN-V686BU","Camera ","3.03","1",null,null,"+","+.",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","+"]
["JVC","JVC VN-V686U","Camera ","1.06","1",null,null,"+","-",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":3},"+.","+","+",null,"-","+","1. с прошивкой 1.06 MPEG-4 видео работает с ошибками на самом устройстве","1. With the 1.06 firmware, MPEG-4 video works with errors on the device itself. "]
["JVC","JVC VN-V686WPBU","Camera ","3.05","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":3},"+","+","+",null,"motion detection","+"]
["JVC","JVC VN-V686WPU","Camera ","1.05","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":3},"+.","+","+",null,"-","-"]
["JVC","JVC VN-X235U","Camera ","1.02","1",null,null,"+","+",{"$nulls":3},"1280x960(MJPEG) / 640x480(MPEG-4)","640x480","320x240","+",null,"+","+","+","+","+",null,"+","+","Камера не поворотная, но есть \"цифровая телеметрия\". Начинает работать при достаточном зумировании картинки. В максимальном разрешении 1280x960 недоступна.Поиск в AxxonNext/Next корректно находит камеру, но верную прошивку нужно выбрать самостоятельно.При смене разрешения в одном из видеопотоков, автоматически изменится разрешение и второго потока - особенность камеры. Таким образом, при одновременном использовании обоих видеопотоков, следующие комбинации будут работать:MJPEG: 320x240 - 320x240 MPEG4MJPEG: 640x480 - 640x480 MPEG4MJPEG: 1280x960 - 640x480 MPEG4Для того, чтобы работали все значения параметра \"Скорость затвора\", нужно в веб-интерфейсе присвоить параметру \"Sense Up\" значение \"Off\".Встроенный детектор камеры не всегда работает корректно: иногда он перестает присылать тревоги. Помогает изменение зоны детектирования.","It is not a PTZ camera, but it has digital telemetry. It starts working after you zoom in enough. At max. resolution (1280x960), it is not available. In AN, search detects the camera correctly, but you have to select the right firmware yourself. If you change the resolution of one of the streams, the resolution of the other stream changes automatically; this is a limitation of the camera itself. For this reason, when you use both streams, the following codec combinations are available: MJPEG: 320x240 – 320x240 MPEG4MJPEG: 640x480 – 640x480 MPEG4MJPEG: 1280x960 – 640x480 MPEG4For the Shutter Speed parameter, to ensure that all the values work, go to the web interface and set the Sense Up parameter to Off. The camera's embedded detection tool does not always work correctly: sometimes it stops sending alarms. It helps to modify the detection zone. "]
["JVC","JVC VN-X235VPU","Camera ","0.02с","1",null,null,"+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4)","640x480","320x240","+",null,"+","-","+","+","+",null,"-","+","1) ограничения fps - 15\n2) камера не поворотная, но есть \"цифровая телеметрия\". Начинает работать при достаточном зумировании картинки. В мегапиксельном разрешении недоступна","1. Frame rate limits: 15 fps. \n2) This is not a PTZ camera, but it has digital PTZ. It starts working after you zoom in enough. At megapixel resolutions, it is not available."]
["JVC","JVC VN-X35U","Camera ","2.01","1",null,null,"+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4)","640x480","320x240","+",null,"+","+","+","+","+",null,"-","+","1) максимально доступный fps = 15, ограничение самой камеры\n2) Камера не поворотная, но есть DigitalPTZ","1. The max. frame rate is 15 fps; this is a limitation of the camera itself.\n2. This is not a PTZ camera, but it has digital PTZ."]
["Legrand","Legrand 430632","Camera","2.103.0000.0.R, build : 2013-02-23","1",null,null,"+","-","+","-","-","1280x960","1280x720","352x288(PAL)/352x240(NTSC)","+","-","-","-","-","-","-","-","-","+"]
["Legrand","Legrand 430652","Camera","2.103.0000.0.R, build : 2013-03-06","1",null,null,"+","-","+","-","-","1280x960","1280x720","352x288","-","-","+","+","+","+","+","-","-","+"]
["Legrand","Legrand 430661","Camera","2.103.0000.1.R, build : 2013-02-26","1",null,null,"+","-","+","-","-","2040x1536","1280x960","352x288","+","-","+","+","-","+","+","-","-","+"]
["LevelOne","LevelOne FCS-3091","Camera","2.3.0326_level1","1","+","2","+",null,"+",null,null,"1600x1200","800x600","640x480","+",null,"-","-",null,"-","-","-","-","+",null,null,"new"]
["LG","LG LE5016D","DVR","auto ","18",{"$nulls":4},"+",null,null,"from WEB ","from WEB ","from WEB ",{"$nulls":9},"-","1. В ПО ITV/Axxon нет возможности изменять настройки устройства\n2. Нужно указать порт 9001\n3. Звук проигрывается с того микрофона, который был включен первым. Для проигрывания звука с другого микрофона нужно выключить активный микрофон и включить необходимый\n\n","1. In AxxonSoft software, you cannot change the camera's settings\n2. Specify port 9001\n3. Sound comes from the microphone which was enabled first. To get sound output from another mic, switch off the active mic and switch on the required one."]
["LG","LG LNB3100","Camera ","1826.0.0.1304190","1",null,null,"+",null,"+",null,null,"1280x1024","704x480","352x240 ","+",{"$nulls":8},"+","Максимальное разрешение в ПО Axxon зависит от значения настройки \"Режим захвата видеоизображения\" ","Max Resolution in Axxon SW depends on \"Video Capture Mode\" setting."]
["LG","LG LNB5100 ","Camera ","1794.0.0.1304190 ","1",null,null,"+",null,"+",null,null,"1280x1024","704x480","352x240 ","+",{"$nulls":8},"+","Максимальное разрешение в ПО Axxon зависит от значения настройки \"Режим захвата видеоизображения\" ","Max Resolution in Axxon SW depends on \"Video Capture Mode\" setting."]
["LG","LG LND3100 ","Camera ","1828.0.0.1304190","1",null,null,"+",null,"+",null,null,"1280x1024","704x480","352x240 ","+",{"$nulls":8},"+","Максимальное разрешение в ПО Axxon зависит от значения настройки \"Режим захвата видеоизображения\" ","Max Resolution in Axxon SW depends on \"Video Capture Mode\" setting."]
["LG","LG LND5100","Camera ","1796.0.0.1304190","1",null,null,"+",null,"+",null,null,"1280x1024","704x480","352x240 ","+",{"$nulls":8},"+","Максимальное разрешение в ПО Axxon зависит от значения настройки \"Режим захвата видеоизображения\" ","Max Resolution in Axxon SW depends on \"Video Capture Mode\" setting."]
["LG","LG LNV5100 ","Camera ","1908.0.0.1304190 ","1",null,null,"+",null,"+",null,null,"1280x1024","704x480","352x240 ","+",{"$nulls":8},"+","Максимальное разрешение в ПО Axxon зависит от значения настройки \"Режим захвата видеоизображения\" ","Max Resolution in Axxon SW depends on \"Video Capture Mode\" setting."]
["LG","LG LNU5100R","Camera","1954.0.0.1306100","1",null,null,"+","-","+",null,null,"1280x1024","704x480","320x240","+",null,"-","-","-","-","-","-","-","+","Детектор движения доступен только для H.264. На камера есть встроенная аналитика Smart Analytics.","Motion detector is only available for H.264 codec. Onboard Smart Analytics."]
["LG","LG LRD5080N ","NVR","auto ","8",{"$nulls":4},"+",null,null,"from WEB ","from WEB ","from WEB ",{"$nulls":9},"-","1. В ПО ITV/Axxon нет возможности изменять настройки устройства\n2. Нужно указать порт 9001\n3. Звук проигрывается с того микрофона, который был включен первым. Для проигрывания звука с другого микрофона нужно выключить активный микрофон и включить необходимый\n\n","1. In AxxonSoft software, you cannot change the camera's settings\n2. Specify port 9001\n3. Sound comes from the microphone which was enabled first. To get sound output from another mic, switch off the active mic and switch on the required one."]
["LG","LG LRD5160N","NVR","auto ","16",{"$nulls":4},"+",null,null,"from WEB ","from WEB ","from WEB ",{"$nulls":9},"-","1. В ПО ITV/Axxon нет возможности изменять настройки устройства\n2. Нужно указать порт 9001\n3. Звук проигрывается с того микрофона, который был включен первым. Для проигрывания звука с другого микрофона нужно выключить активный микрофон и включить необходимый\n\n","1. In AxxonSoft software, you cannot change the camera's settings\n2. Specify port 9001\n3. Sound comes from the microphone which was enabled first. To get sound output from another mic, switch off the active mic and switch on the required one."]
["LG","LG LRH7080D","DVR","auto ","16",{"$nulls":4},"+",null,null,"from WEB ","from WEB ","from WEB ",{"$nulls":9},"-","1. В ПО ITV/Axxon нет возможности изменять настройки устройства\n2. Нужно указать порт 9001\n3. Звук проигрывается с того микрофона, который был включен первым. Для проигрывания звука с другого микрофона нужно выключить активный микрофон и включить необходимый\n\n","1. In AxxonSoft software, you cannot change the camera's settings\n2. Specify port 9001\n3. Sound comes from the microphone which was enabled first. To get sound output from another mic, switch off the active mic and switch on the required one."]
["LG","LG LRH7160D","DVR","auto ","24",{"$nulls":4},"+",null,null,"from WEB ","from WEB ","from WEB ",{"$nulls":9},"-","1. В ПО ITV/Axxon нет возможности изменять настройки устройства\n2. Нужно указать порт 9001\n3. Звук проигрывается с того микрофона, который был включен первым. Для проигрывания звука с другого микрофона нужно выключить активный микрофон и включить необходимый\n\n","1. In AxxonSoft software, you cannot change the camera's settings\n2. Specify port 9001\n3. Sound comes from the microphone which was enabled first. To get sound output from another mic, switch off the active mic and switch on the required one."]
["LG","LG LSW2010F-P","Camera ","258.0.0.1107140","1",null,null,"+",null,"+",null,null,"704x576","704x288","352x288","+",null,"+","+",null,"+","+",null,"+","+","Событие об изменении состояния луча приходит с задержкой ~7-10 сек.Встроенный детектор движения работает только с кодеком H264Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства.При наличии нескольких одновременных подключений к камере возможно искажения видео при перезапуске камеры или ПО.Через Onvif работают только видео с настройками, звук и реле.","Notifications on sensor status changes arrive with a delay (around 7 to 10 seconds). The embedded motion detection tool works only with the H.264 codec. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. If you have several connections to the camera at the same time, you may see distorted video after you restart the camera or software. Via the ONVIF protocol only the following works: search, video (+ settings), and audio."]
["LG","LG LSW900P-B","Camera ","2.0.0.1105060","1",null,null,"+",null,"+",null,null,"704x576","704x288","352x288","+",null,"+","+","+","+","+",null,"+","+","Поиск не возвращает прошивку: правильную версию нужно выбрать самостоятельно.Событие об изменении состояния луча приходит с задержкой ~7-10 сек.Встроенный детектор движения работает только с кодеком H264.Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства.При наличии нескольких одновременных подключений к камере возможно искажения видео при перезапуске камеры или ПО.Через Onvif не работают:Датчик (луч)Настройки изображения","Search does not detect the device's firmware: you must yourself select the right version of the camera's software. Notifications on sensor status changes arrive with a delay (around 7 to 10 seconds). The embedded motion detection tool works only with the H.264 codec. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. If you have several connections to the camera at the same time, you may see distorted video after you restart the camera or software. The sensor and video settings do not work over ONVIF."]
["LG","LG LVW700P-B","Camera ","4.0.1.1106150","1",null,null,"+",null,"+",null,null,"704x576","704x288","352x288","+",null,"+","+",null,"+","+",null,"+.","+","1. ползунок \"Качество\" работает в ПО Intellect только для MJPEG-потока\n2. Работа встроенной видеоаналитики (motion detection) доступна только при H.264 видеопотоке\n3. Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства. ","1. In Intellect, the Quality slider works only for the MJPEG stream.\n2. The embedded video analytics (motion detection) are available only for the H.264 video stream.\n3. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. "]
["LG","LG LVW901P-B","Camera","4.1.0.1110260","1","-",null,"+",null,"+",null,null,"704x576","704x288","352x288","+",null,"+","+",null,"+","+","-","+","+","Поиск не возвращает прошивку: правильную версию нужно выбрать самостоятельно.Событие об изменении состояния луча приходит с задержкой ~7-10 сек.Встроенный детектор движения работает только с кодеком H264Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства.При наличии нескольких одновременных подключений к камере возможно искажения видео при перезапуске камеры или ПО.Через Onvif не работают:Датчик (луч)Настройки изображения","Search does not detect the device's firmware: you must yourself select the right version of the camera's software. Notifications on sensor status changes arrive with a delay (around 7 to 10 seconds). The embedded motion detection tool works only with the H.264 codec. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. If you have several connections to the camera at the same time, you may see distorted video after you restart the camera or software. The sensor and video settings do not work over ONVIF.","improved"]
["LG","LG LW332","Camera ","1026.0.0.1107060","1",null,null,"+",null,"+",null,null,"1280x1024","704x480","352x240","+",null,"+","+",null,"+","+",null,"+","+","В MJPEG в первом потоке максимальная частота кадров - 20 fpsПри наличии нескольких одновременных подключений к камере возможно искажения видео при перезапуске камеры или ПО.Событие об изменении состояния луча приходит с задержкой ~7-10 сек.Встроенный детектор движения работает только с кодеком H264Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства.Прошивка 1026.0.0.1107060: При выборе значений яркости <50 картинка становится почти полностью белой. Проблема устройства.Через Onvif работает видео с настройками и звук","With MJPEG (the first stream), the max. frame rate is 20 fps. If you have multiple connections to the camera at the same time, you may see distorted video after you restart the camera or software. Notifications on sensor status changes arrive with a delay (around 7 to 10 seconds). The embedded motion detection tool works only with the H.264 codec. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. 1026.0.0.1107060 firmware: if you set brightness to <50, the image becomes almost white. This is a limitation of the device itself. Via the ONVIF protocol the following works: video (+ settings), and audio."]
["LG","LG LW345(ONVIF)","Camera ","Package_767.0.0.1105130","1",null,null,"+",null,"+",null,null,"1920x1072","1920x1072","1280x720","+",null,"+","-",null,"-","-",null,"+.","+","1. с прошивкой Package_767.0.0.1104141 реле не работает на самой камере","1) With the Package_767.0.0.1104141 firmware, the relay does not work on the camera itself. "]
["LG","LG LW6324","Camera ","1028.0.0.1107060 ","1",null,null,"+",null,"+",null,null,"1280x1024","704x480","352x240","+",null,"+","+",null,"+","+",null,"+","+","В MJPEG в первом потоке максимальная частота кадров - 20 fpsПри наличии нескольких одновременных подключений к камере возможно искажения видео при перезапуске камеры или ПО.Событие об изменении состояния луча приходит с задержкой ~7-10 сек.Встроенный детектор движения работает только с кодеком H264Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства.Прошивка 1028.0.0.1107060: При выборе значений яркости <50 картинка становится почти полностью белой. Проблема устройстваЧерез Onvif работает видео с настройками и звук","With MJPEG (the first stream), the max. frame rate is 20 fps. If you have multiple connections to the camera at the same time, you may see distorted video after you restart the camera or software. Notifications on sensor status changes arrive with a delay (around 7 to 10 seconds). The embedded motion detection tool works only with the H.264 codec. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. 1028.0.1107060 firmware: if you set brightness to <50, the image becomes almost white. This is a limitation of the device itself. Via the ONVIF protocol the following works: video (+ settings), and audio."]
["LG","LG LW6454(ONVIF)","Camera ","Package_767.0.0.1105130","1",null,null,"+",null,"+",null,null,"1920x1072","1920x1072","1280x720","+",null,"+","-",null,"-","-",null,"+.","+","1. с прошивкой Package_767.0.0.1104141 реле не работает на самой камере","1) With the Package_767.0.0.1104141 firmware, the relay does not work on the camera itself."]
["LG","LG LW9228I-AN","Camera ","774.0.0.1107143 ","1",null,null,"+",null,"+",null,null,"704x480","704x240","352x240","+",null,"+","+","+","+.","+",null,"+","+","При наличии нескольких одновременных подключений к камере возможно искажения видео при перезапуске камеры или ПО.Событие об изменении состояния луча приходит с задержкой ~7-10 сек.Встроенный детектор движения работает только с кодеком H264Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства.Прошивка 774.0.0.1107143: Предустановки телеметрии не работают - проблема самого устройства.Прошивка 774.0.0.1107143: Из 4-х лучей работает только первый. Проблема устройстваЧерез Onvif работает видео с настройками, звук, телеметрия без предустановок и реле.\n","If you have multiple connections to the camera at the same time, you may see distorted video after you restart the camera or software. Notifications on sensor status changes arrive with a delay (around 7 to 10 seconds). The embedded motion detection tool works only with the H.264 codec. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. 774.0.0.1107143 firmware: Telemetry presets do not work. This is a problem of the device itself. 774.0.0.1107143 firmware: of the 4 sensors, only the first sensor works. This is a problem of the device itself. Via the ONVIF protocol the following work: video (+ settings), audio, telemetry (without presets), and the relay.\n"]
["LTV","LTV-ISDNO20-M2 ","Camera ","LTV01.2.1055.42","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",null,"+",null,"+.","+","+",null,null,"+"]
["LTV","LTV-ICCM1-B320-F3.8","Camera ","1044-1026-1031-1008","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",null,"+",null,"-","+","+",null,"-","+","При замыкании луча, камера иногда присылает по очереди, что луч замыкают, размыкают и т.д., это проблема производителей.","When a sensor is closed, the camera signals it is open and closed repeatedly. This is a problem with the camera itself."]
["LTV","LTV-ICDM1-423 / LTV-ICDM1-723-V3.3-12","Camera ","LTV01.2.1913.42","1",null,null,"+",null,"+",null,null,"1280x1024","640x480","320x240","+",null,"+","+",null,"+","+",null,"+.","+","Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".\nРазрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В ASI записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле.\nПрошивка 51110.2.1784.100: Не работает аудио выход","Before using the camera, go to the web interface and disable the Installation Mode, i.e. assign \"Off\" to this parameter.\nThe resolution and frame rate are adjusted for both streams at the same time - this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\"). The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF.\nThe 51110.2.1784.100 firmware: The audio output doesn't work\n"]
["LTV","LTV-ICDM1-623LH-V3.3-12","Camera ","51110.2.1784.100","1",null,null,"+",null,"+",null,null,"1280x1024","1280x720","640x480","+",null,"+","+","+.","+","+",null,"+.","+","Камера не поворотная, но есть встроенный трансфокатор.Разрешение меняется одновременно для двух потоков. В настройках указано в виде \"Разрешение 1 потока : Разрешение 2 потока\"Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле.","This is not a PTZ camera, but it has a built-in zoom lens. The resolution is adjusted for both streams at the same time. This setting is represented as \"Resolution, stream 1 : resolution, stream 2 The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF."]
["LTV","LTV-ICDM1-623LH-V3-9","Camera ","LTV01.2.1074.42","1",null,null,"+",null,"+",null,null,"1280x1024","1024x768","640x480","+",null,"+","-","+.","+","+",null,"motion detection","+"]
["LTV","LTV-ICDM1-723(L)-V3-9 / LTV-ICDM1-823LH-V3-9 ","Camera ","LTV01.2.1084.42","1",null,null,"+",null,"+",null,null,"1280x1024","1024x768","640x480","+",null,"+","-","+","+","+",null,"motion detection; ","+"]
["LTV","LTV-ICDM1-823H-V3.3-12","Camera ","51110.2.1784.100","1",null,null,"+",null,"+",null,null,"1280x1024","1024x768","320x240","+",null,"+","+","+.","+","+",null,"+.","+","Камера не поворотная, но есть встроенный трансфокатор.Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В ASI записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")Прошивка 51110.2.1784.100: через Onvif не меняется разрешение в кодеке MJPEG - проблема камеры.Прошивка 51110.2.1784.100: через Onvif не меняется частота кадров - проблема камеры.Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле.","This is not a PTZ camera, but it has a built-in zoom lens. Before using the camera, go to the web interface and disable the Installation Mode, i.e. assign Off to this parameter. The resolution and frame rate are adjusted for both streams at the same time - this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\")The 51110.2.1784.100 firmware: Via the ONVIF protocol, you can not change the resolution for the MJPEG codec - this seems to be the problem with the device. The 51110.2.1784.100 firmware: Via the ONVIF protocol, you cannot change the frame rate - this seems to be the problem with the device. The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF."]
["LTV","LTV-ICDM1-B423L-F3.8","Camera ","1044-1026-1031-1008","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",null,"+","+","-","+","+",null,"-","+","При замыкании луча, камера иногда присылает по очереди что луч замыкают, размыкают и т.д., это баг на самом устройстве.","When a sensor is closed, the camera signals it is open and closed repeatedly. This is a problem with the camera itself."]
["LTV","LTV-ICDM1-B623L-F3.8","Camera ","1044-1026-1031-1008","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",{"$nulls":3},"-","+","+",null,"-","+","При замыкании луча, камера иногда присылает по очереди что луч замыкают, размыкают и т.д., это проблема производителей.","When a sensor is closed, the camera signals it is open and closed repeatedly. This is a problem with the camera itself."]
["LTV","LTV-ICDM1-B723L-F3.8","Camera ","1044-1026-1031-1008","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",null,"+","-","-","+","+",null,"-","+","При замыкании луча, камера иногда присылает по очереди что луч замыкают, размыкают и т.д., это проблема производителей.","When a sensor is closed, the camera signals it is open and closed repeatedly. This is a problem with the camera itself."]
["LTV","LTV-ICDM2-423 / LTV-ICDM2-723-V3.3-12","Camera ","LTV01.2.1913.42","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","320x240","+",null,"+","+",null,"+","+",null,"+.","+"," Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В ASI записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле. \nПрошивка 51110.2.1784.100: Не работает аудио выход","Before using the camera, go to the web interface and disable the Installation Mode, i.e. assign \"Off\" to this parameter. The resolution and frame rate are adjusted for both streams at the same time - this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\")The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF. \nThe 51110.2.1784.100 firmware: The audio output doesn't work\n"]
["LTV","LTV-ICDM2-423-T5","Camera ","LTV01.2.1227.42","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":3},"motion detection","+","В ПО Axxon записаны двойные разрешения (\"разрешение для 1-го потока\" : \"разрешение для 2-го потока\")\nРежим двухпоточности, при котором на каждом потоке установлен кодек MJPEG, не поддерживается.\nДля того, чтобы в ПО ITV видео с кодеком MJPEG шло с корректным разрешением, необходимо сначала выбрать граббер H264, установить требуемое разрешение, а затем изменить тип граббера на MJPEG.\nКамера не поворотная, но есть встроенный трансфокатор.","In the AxxonSoft software are recorded double resolution (\"Resolution for 1st stream\": \"Resolution for 2nd stream\").\nDual-stream mode, where at each stream MJPEG turned on, is not supported.\nTo get video with MJPEG codec and correct resolution in AxxonSoft software, you need firstly to select the grabber H264, set the desired resolution, and then change type of grabber to MJPEG.\nThe camera does not PTZ but it has a built-in zoom lens."]
["LTV","LTV-ICDM2-623L-F.4","Camera ","LTV01.2.1210.42","1",null,null,"+",null,"+",null,null,"1920x1080 ","1024x768","640x480 ","+",{"$nulls":7},"motion detection","+"]
["LTV","LTV-ICDM2-623LH-V3.3-12","Camera ","51110.2.1784.100 ","1",null,null,"+",null,"+",null,null,"1280x720 (MJPEG) / 1920х1080 (H264)","640x480 (MJPEG) / 1024x768 (H264)","320x240 (MJPEG) / 640x480 (H264)","+",null,"+","+","+.","+","+",null,"+.","+","Камера не поворотная, но есть встроенный трансфокатор.Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В Axxon Next записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")Прошивка 51110.2.1784.100: через Onvif не меняется разрешение в кодеке MJPEG - проблема камеры.Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле.","This is not a PTZ camera, but it has a built-in zoom lens. The resolution and frame rate are adjusted for both streams at the same time - this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\")The 51110.2.1784.100 firmware: Viva the ONVIF protocol, you can not change the resolution for the MJPEG codec - this seems to be the problem with the device. The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF.\n"]
["LTV","LTV-ICDM2-623LH-V3-9","Camera ","LTV01.2.1074.42","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",null,"+","-","+","+","+",null,"motion detection","+","Режим двухпоточности, при котором на каждом потоке установлен кодек MJPEG, не поддерживается.\nДля того, чтобы в ПО ITV видео с кодеком MJPEG шло с корректным разрешением, необходимо сначала выбрать граббер H264, установить требуемое разрешение, а затем изменить тип граббера на MJPEG.","Dual-stream mode, where at each stream MJPEG turned on, is not supported.\nTo get video with MJPEG codec and correct resolution in AxxonSoft software, you need firstly to select the grabber H264, set the desired resolution, and then change type of grabber to MJPEG."]
["LTV","LTV-ICDM2-723(L)-V3-9 / LTV-ICDM2-823LH-V3-9 ","Camera ","LTV01.2.1227.42","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",null,"+","-","+","+","+",null,"motion detection; ","+"]
["LTV","LTV-ICDM2-723L-F.4","Camera ","LTV01.2.1210.42","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480 ","+",{"$nulls":7},"motion detection","+"]
["LTV","LTV-ICDM2-823-F2.1","Camera ","LTV01.2.1058.42","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":7},"+","+","1. В Axxon Next записаны двойные разрешения (\"разрешение для 1-го потока\" : \"разрешение для 2-го потока\")\n2. Для корректного отображения видео нельзя ставить MJPEG одновременно на двух потоках ","1. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\")\n2. You cannot have MJPEG video for both streams at the same time.\n"]
["LTV","LTV-ICDM2-823H-V3.3-12","Camera ","LTV01.2.1913.42","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",null,"+","+","+.","+","+",null,"+.","+","Камера не поворотная, но есть встроенный трансфокатор. Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В ASI записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")Прошивка 51110.2.1784.100: через Onvif не меняется разрешение в кодеке MJPEG - проблема камеры.Прошивка 51110.2.1784.100: через Onvif не меняется частота кадров - проблема камеры.Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле.","This is not a PTZ camera, but it has a built-in zoom lens. Before using the camera, go to the web interface and disable the Installation Mode, i.e. assign Off to this parameter. The resolution and frame rate are adjusted for both streams at the same time - this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\")The 51110.2.1784.100 firmware: Viva the ONVIF protocol, you can not change the resolution for the MJPEG codec - this seems to be the problem with the device. The 51110.2.1784.100 firmware: Via the ONVIF protocol, you cannot change the frame rate - this seems to be the problem with the device. The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF."]
["LTV","LTV-ICDV-423 / LTV-ICDV-723-V3.3-12 / LTV-ICDV-623LH-V3.3-12 / LTV-ICDV-823H-V3.3-12","Camera ","LTV01.2.1913.42","1",null,null,"+",null,"+",null,null,"704x576","640x480","320x240","+",null,"+","+",null,"+","+",null,"+.","+"," Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В ASI записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле.","Before using the camera, go to the web interface and disable the Installation Mode, i.e. assign \"Off\" to this parameter. The resolution and frame rate are adjusted for both streams at the same time - this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\")The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF."]
["LTV","LTV LTV-ISDNO20-M2","Camera","LTV01.2.6040.42","1",null,null,"+","-","+","-","-","1920x1080","1024x768","640x480","+",null,"+","-","+","+","+","-",null,"+","Значения разрешения применяются для обоих потоков.На камере нельзя выставить MJPEG на обоих потоках.","Resolution values are applied to both streams. You cannot set the MJPEG on the camera for both streams."]
["LTV","LTV-IWCCM1-B320L-F3.8","Camera ","1044-1026-1031-1008","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+",null,"+","+","-","+","+",null,"-","+","При замыкании луча, камера иногда присылает по очереди что луч замыкают, размыкают и т.д., это проблема производителей.","When a sensor is closed, the camera signals it is open and closed repeatedly. This is a problem with the camera itself."]
["Magic Box","Magic Box (ONVIF 2-channel device)","Encoder ","v2.1321.5776","2",null,null,"+",null,"+",null,null,"720x576","704x288 (MJPEG) / 704x576 (H264)","320x240 (MJPEG) / 352x288 (H264)","+",null,"+","+","+","-","+",null,"+.","+","1. Прошивка 371.2285: MJPEG-видео не работает на самом устройстве.\n2. Прошивка 1055.4380: звук с подключенного микрофона очень тихий.\n3. Прошивка 1055.4380: Лучи инвертированы на самом устройстве\n4. Прошивка 1055.4380: Реле перепутаны на самом устройстве\n5. Прошивка 1055.4380: Видеоканалы перепутаны на самом устройстве\n6. Прошивка 1170.4816: Устройство не поддерживает настройки изображения и фокус (внешняя телеметрия).\n7. Перед работой со встроенной аналитикой в ПО ITV необходимо выполнить предварительную настройку устройства через утилиту ODM:\nУдалить профили axxon0 и axxon1 (если есть)\nНастроить фильтры для аналитики: в разделе Metadata, тип фильтра \"Content ItemFilter\", значение:\nДля первого канала: boolean(//tt:SimpleItem[@Name=\"Source\" and @Value=\"VIDEO_SOURCE_0\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\" and @Value=\"VIDEO_SOURCE_0\"]) or not(boolean(//tt:SimpleItem[@Name=\"Source\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\"]))\nДля второго канала: boolean(//tt:SimpleItem[@Name=\"Source\" and @Value=\"VIDEO_SOURCE_1\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\" and @Value=\"VIDEO_SOURCE_1\"]) or not(boolean(//tt:SimpleItem[@Name=\"Source\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\"]))\n8. С прошивкой v2.1321.5776 не работают лучи","1. The 371.2285 firmware: MJPEG video does not work on the device.\n2. The 1055.4380 firmware: with the external microphone, the sound volume is very low. \n3. The 1055.4380 firmware: The sensors are reversed i.e closed show open and vice versa on the device itself. The 1055.4380 firmware: The relays are reversed on the device itself. The 1055.4380 firmware: The video channels are mixed up on the device itself. The 1055.4380 firmware: The device does not support the video settings and focus (pan/tilt drive). \n7. Before using embedded video analytics in the AxxonSoft software, configure the device using the ODM utility\nDelete the axxon0 and axxon1 profiles (if they exist) \n Set up the video analytics filters: go to the Metadata section, find the Content Item Filter type, and set the following value:\nFor the first channel: boolean(//tt:SimpleItem[@Name=\"Source\" and @Value=\"VIDEO_SOURCE_0\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\" and @Value=\"VIDEO_SOURCE_0\"]) or not(boolean(//tt:SimpleItem[@Name=\"Source\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\"]))\nFor the second channel: boolean(//tt:SimpleItem[@Name=\"Source\" and @Value=\"VIDEO_SOURCE_1\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\" and @Value=\"VIDEO_SOURCE_1\"]) or not(boolean(//tt:SimpleItem[@Name=\"Source\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\"]))\n8. In the v2.1321.5776 firmware, the sensors do not work."]
["Mango DSP","Mango Pegasus-M","Encoder ","3.2.7.10","1",null,null,"+","+","+",null,null,"720x576","704x576","352x288","+",null,"+","-","+","+","+",null,"-","+","Изменение некоторых параметров требует перезагрузки устройства (~1 мин).При максимальном качестве возможны задержки видеопотока.При минимальном качестве возможна потеря видеопотока. Нужно перезагрузить устройство.Реле устройства по-умолчанию замкнуто. Это проявляется при добавлении устройства, а также при изменении некоторых настроек. После замыкания - размыкания его через наше ПО дальнейшая работа проходит корректно.","For some settings, after you change them, you must restart the device (around 1 minute). At max. quality, the video stream may come with delays or the video stream may stop. Restart the device. By default, the device's relay is closed. This creates problems when adding the device or changing some of the settings. To make the relay work correctly, open/close the relay in the AxxonSoft software."]
["March Networks","VideoSphere MegaPX 720p","Camera ","1.8.5","1",null,null,"-",null,"+",null,null,"1280x720","720x576","352x288","+",null,"-","-",{"$nulls":4},"-","+","из-за отсутствия документации не реализовано:\n1. MJPEG\n2. audio in\n3. audio out","Due to the fact that there is no documentation, the following was not implemented: \n1. MJPEG\n2. Audio in\n3. Audio out"]
["March Networks","VideoSphere MiniDome PTZ","Camera ","2.4.0","1",{"$nulls":3},"+","-",null,null,"720х288","720х288","352x288","+",null,"-",null,"+","-","-",null,null,"+"]
["MBK","MBK-IP67-CMOS-1.3Mp (ONVIF 1-channel device)","Camera","106.2232","1",null,null,"+",null,"+",null,null,"1280x720","1280x720","1280x720","+.",{"$nulls":7},"+.","+","1. Само устройство выдает только ~15 fps и в MJPEG и в H.264\n2. С прошивкой 106.2232 настройка насыщенности цвета работает наоборот на самом устройстве\n","1. The device itself allows around 1 fps, both with MJPEG and H.264.  With the 106.2232 firmware, the saturation control works the other way around on the device itself. \n"]
["Mediatronix","Mediatronix AVSR1","Encoder ","auto","1",{"$nulls":3},"+.",{"$nulls":3},"352x288","352x288","352x288","-",{"$nulls":3},"-","-","-",null,null,"-","В настройках подключения к устройству нужно указывать порт \"20\"","When configuring the connection to the device, set the port number to 20. "]
["Mediatronix","Mediatronix IPCAM_OVT2715","Camera","F106_009 28A3","1",null,null,"-","-","+",null,null,"1920x1080","1920x1080","640x368","-",null,"-","-","-","-","-","-","-","-"]
["Merit Lilin","Merit Lilin IPD112ESX","Camera ","0.0.64","1",null,null,"+",null,"+",null,null,"1280x768","1280x768","640x384","+",null,"-","-",null,"-","+",null,"+","-","Максимальная частота кадров: 20 fps в H264, 10 fps в mjpegИзменение настроек происходит достаточно долго: камера каждый раз перезагружается. Особенность устройства.С прошивками 0.0.60, 0.0.62 и 0.0.64 луч(датчик) не работают на самом устройствеС прошивками 0.0.60 и 0.0.64 настройки изображения (яркость, контраст и т.д) через протокол ONVIF не меняются на самом устройствеДоступность кодеков, разрешений, значений частоты кадров в разных потоках взаимозависима. Пользователю придется самостоятельно следить за совместимостью и при необходимости включать/выключать потоки/профили из веб-интерфейса.","Max. frame rate: 20 fps for H.264, 10 fps for MJPEG. Applying changes to settings takes a lot of time: the camera restarts every time. This is a limitation of the device itself. With the 0.0.60, 0.0.62, and 0.0.64 firmware, the sensor does not work on the device itself. With 0.0.60 and 0.0.64, if you use the ONVIF protocol, the video settings (brightness, contrast, and so on) do not change on the device itself. The availability of codecs, resolutions, and frame rates for one stream depends on the current settings of the other. Users must manually check whether the settings are compatible and use the web interface to enable/disable streams/profiles if needed. "]
["Merit Lilin","Merit Lilin IPD2220ES3 / IPR320ESX3","Camera ","1.0.490","1",null,null,"+",null,"+",null,null,"from WEB","from WEB","from WEB","+.",null,"-",null,"+",{"$nulls":3},"-","-","1. Профили настраиваются вручную в веб-интерфейсе камеры. В ПО ITV/Axxon нужно выбирать соответствующий кодек, чтобы работали настройки.","1. You can configure profiles in the web interface. In the AxxonSoft software, you have to select an appropriate codec to comply with settings."]
["Merit Lilin","Merit Lilin IPD552EX","Camera ","0.3.38","1",null,null,"+",null,"+",null,null,"720x576(H.264) / 352 x 288(MJPEG)","720x576(H.264) / 352 x 288(MJPEG)","352 x 288(H.264) / 352 x 288(MJPEG)","+",null,"-",{"$nulls":5},"-","-","1) В ПО ITV следует выбирать граббер Merit Lilin\n2) для MJPEG есть только одно разрешение 352*288\n3) для MJPEG максимальное значение fps = 1-2","1. In the AxxonSoft software, select the Merit Lilin grabber.\n2. For MJPEG, you have only one resolution, 352*288.\n3. For MJPEG, the max. frame rate is 1–2 fps."]
["Merit Lilin","Merit Lilin IPR712S","Camera ","0.0.66","1",null,null,"+",null,"+",null,null,"1280x768","1280x768","from WEB ","+",{"$nulls":7},"+","-","Изменение настроек видео приводит к перезагрузке камеры (~1 минута)Перед переключением кодека/разрешения нужно убедиться, что в веб-интерфейсе включен соответствующий видео-профиль.Максимальные значения частоты кадров достигаются при отключении неиспользуемых видео-профилей (в веб-интерфейсе).Через Onvif работает только получение видео, смена частоты кадров и транспортного протокола","If you change video settings, the camera must restart (1 minute). Before switching to a certain codec/resolution, go to the web interface and make sure that the relevant video profile is enabled. To reach the max. frame rate, go to the web interface and disable the video profiles that are not in use. Via the ONVIF protocol, you can only receive video, change the frame rate, and change the transport protocol."]
["Merit Lilin","Merit Lilin IPR7428ESX / IPR7424ESX","Camera ","1.0.506","1",null,null,"-",null,"+",null,null,"1920х1080(H264)","1920х1080(H264)","1920х1080(H264)","+",null,"-","-","+","-","-",null,"-","-","1. Профили настраиваются вручную в веб-интерфейсе камеры. В ПО ITV/Axxon нужно выбирать соответствующий кодек, чтобы работали настройки.","1. You can configure profiles in the web interface. In the AxxonSoft software, you have to select an appropriate codec to comply with settings."]
["Merit Lilin","Merit Lilin IPS0258","Camera ","0.3.49a","1",null,null,"+",null,"+",null,null,"352x288(MJPEG) / 720x576(H.264)","352x288(MJPEG) / 720x576(H.264)","352x288","+",{"$nulls":3},"+","+.",null,null,"-","-","1) для MJPEG есть только одно разрешение 352*240\n2) для MJPEG максимальное значение fps = 1-2\n3) Реле только как реакция на замыкание Луча, поэтому в ПО ITV не реализовано\n4) Лучи в ПО ITV правильно работают только \"на замыкание\", особенность самой камеры\n5) не работает луч №6 - по заявлению от производителя оборудований данный порт зарезервирован.\n6) после изменения настроек (разрешение, качество, fps) на восстановление видеопотока может потребовать до 50 секунд времени.","1. For MJPEG, you have only one resolution, 352*240\n2. For MJPEG, the max. frame rate is 1-2 fps\n3. The relay works only as a response to a Sensor tripwire; for this reason, it is not implemented in the AxxonSoft software\n4) In the AxxonSoft software, the sensors work properly only as a tripwire, this is a limitation of the camera itself\n5. Sensor 6 does not work - according to the vendor, this port is reserved.\n6. After you change the settings (resolution, quality, frame rate), the video stream may take up to 50 seconds to restart."]
["Merit Lilin","Merit Lilin IPS1354N","Camera ","0.3.41a","1",null,null,"+",null,"+",null,null,"352x240(MJPEG)/720x480(H.264)","352x240(MJPEG)/720x480(H.264)","352x240","+",{"$nulls":4},"-",null,null,"-","-","1) для MJPEG есть только одно разрешение 352*240\n2) для MJPEG максимальное значение fps = 1-2\n3) Реле только как реакция на замыкание Луча, поэтому в ПО ITV не реализовано","1. For MJPEG, you have only one resolution, 352*240.\n2. For MJPEG, the max. frame rate is 1–2 fps.\n3. The relay works only as a response to the Sensor getting closed; for this reason, it is not implemented in the AxxonSoft software."]
["Merit Lilin","Merit Lilin IPS1354N (ONVIF)","Camera ","0.3.41a","1",null,null,"+",null,"+",null,null,"720x480","720x480","352x240","-",{"$nulls":7},"-","+","1) работает по ONVIF\n2) для MJPEG есть только одно разрешение 352*288\n3) для MJPEG максимальное значение fps = 1-2\n4) Реле только как реакция на замыкание Луча, поэтому в ПО ITV не реализовано\n5) разрешения необходимо переключать через родной веб-интерфейс камеры. Особенность самого устройства","1. Works via the ONVIF protocol.\n2. For MJPEG, you have only one resolution: 352*288.\n3. For MJPEG, the max. frame rate is 1–2 fps.\n4. The relay works only when Sensor is on a closed circuit; for this reason, it is not implemented in the AxxonSoft software.\n5. Resolutions can be switched only in the camera's web interface. This is a limitation of the device itself."]
["Merit Lilin","Merit Lilin IPS1358","Camera ","V0.3.28c","1",null,null,"+",null,"+",null,null,"352x288(MJPEG)/720x576(H.264)","352x288(MJPEG)/720x576(H.264)","352x288","+",{"$nulls":3},"+","+.",null,null,"-","-","1) В ПО ITV следует выбирать граббер Merit Lilin\n2) для MJPEG есть только одно разрешение 352*288\n3) для MJPEG значение fps = 1-2\n4) Реле только как реакция на замыкание Луча, поэтому в ПО ITV не реализовано\n5) не работает луч №6 - по заявлению от производителй зарезервирован для чего-то","1. In the AxxonSoft software, select the Merit Lilin\n grabber.\n2. For MJPEG, you have only one resolution: 352*288.\n3. For MJPEG, the frame rate is 1–2 fps.\n4. The relay works only as a response to the Sensor getting closed; for this reason, it is not implemented in the AxxonSoft software.\n5. Sensor 6 does not work: according to the vendor, this port is reserved for something else."]
["Merit Lilin","Merit Lilin LR7722EX3.6","Camera","1.1.12","1","-",null,"+",null,"+",null,null,"1920x1080","1280x720(MJPEG) / 1920x1080(H264)","352x240(MJPEG) / 720x480(H.264)","+",null,"+","-",null,"-","+",null,"motion detection","-","Значение настройки RTSP порт должно соответствовать значению аналогичной настройки, выставленному в веб-интерфейсе на странице Network → HTTP/RTSP Service.Особенность прошивки камеры не позволяет провести полноценную интеграцию настроек видео без необходимости совершения дополнительных действий в веб-интерфейсе камеры. Для корректной работы настроек в ПО ITV/Axxon необходимо, настройки \"Видеокодек\" и \"Разрешение\" в ПО ITV/Axxon соответствовали аналогичным настройкам в веб-интерфейсе камеры, где они зависят от значения параметра Profile (Settings → Video / Audio).Для того, чтобы в ПО Интеллект работали настройки видео, а также разрешения соответствовали указанным в текущих результатах, необходимо соблюдать следующее соответствие между выбранными параметрами в ПО Интеллект и значением настройки Profile в веб-интерфейсе камеры:Разрешение в ПО ИнтеллектMJPEGH.264СтандартноеProfile 2Profile 1ВысокоеProfile 1Profile 2ПолноеProfile 1Profile 1","The value of RTSP port setting is to correspond to the value of the similar setting set in the web interface on the Network → HTTP/RTSP Service page. Camera firmware does not allow integrating video settings without other actions in the camera web interface. For proper operation of settings in Axxon software, the Video codec and Resolution settings in Axxon software are to correspond to the similar settings in the camera web interface where they depend on the Profile (Settings → Video / Audio) parameter. For video settings to operate and resolutions to correspond to those specified in the results in Intellect, you are to keep the following correspondence of selected parameters in Intellect and Profile setting in the camera web interface: Resolution in Intellect MJPEGH.264 Standard Profile 2 Profile 1 High Profile 1 Profile 2 Full Profile 1 Profile 1","improved"]
["Merit Lilin","Merit Lilin PIH-7625PFIP","Camera ","2.40 R07.2.T","1",null,null,"+",{"$nulls":4},"704x576","352x288","176x144","+",{"$nulls":3},"+","-","-",null,"-","-","1. В ПО ITV следует выбирать граббер Lilin\n2. В поле \"Скорость\" на панели телеметрии следует вводить числа меньше 8.","1. In the AxxonSoft software, select the Lilin grabber.\n2. In the Telemetry Control Panel's Speed field, enter a number less than 8. "]
["Merit Lilin","Merit Lilin VS012","Camera ","0.3.48","1",null,null,"+",null,"+",null,null,"704x576","704x576","352x288","+",null,"-",null,"+.","+","+",null,"-","-","1) для MJPEG есть только одно разрешение 352*288\n2) для MJPEG значение fps = 1-2\n3) после изменения настроек (разрешение, качество, fps) на восстановление видеопотока может потребовать до 50 секунд времени.","1. For MJPEG, you have only one resolution, 352*288.\n2. For MJPEG, the frame rate is 1–2 fps.\n3. After you change the settings (resolution, quality, frame rate), the video stream may take up to 50 seconds to restart."]
["Messoa","Messoa NCB855pro / NCR875pro","Camera ","AP_01-00-59-07_2M_MS03","1",null,null,"+","+","+",null,null,"1920x1080","1024x768","640x480","+",null,"+","+",null,"+","+",null,"+","+","Прошивка AP_01-00-58_2M_MS03: Настройки на камере применяются довольно долго - после нажатия кнопки Применить камера уходит в ребут и настройки применяются примерно через минуту.Прошивка AP_01-00-59-07_2M_MS03: Чтобы работал втроенный детектор движения необходимо, чтобы на одном из потоков был выбран кодек MJPEG, а на другом - MPEG4 либо H264.Прошивка AP_01-00-59-07_2M_MS03: На камере не работает настройка FPS с кодеками H264 и MPEG4. Независимо от значения параметра реально FPS всегда примерно равен 17.Параметр ТВ-стандарт интегрирован, но на аналогичную настройку в вебе не влияет. Он нужен для работы с камерами -HN5 и -HP5 (они отличаются только ТВ-стандартом, значениями разрешений и FPS). Т.е. при изменении этой настройки в AxxonNext/Next меняется список доступных разрешений и значений FPS и больше ничего.Прошивка AP_01-00-59-07_2M_MS03: Через ONVIF у камеры не работают никакие настройки потока и изображения, кроме смены протокола. Также не работают датчики, реле и встроенная аналитика. Это вина прошивки, а не интеграции.","AP_01-00-58_2M_MS03: The camera takes a lot of time to apply changes to settings: after you click Apply, the camera is restarted, so the changes are applied in around 1 minute. AP_01-00-59-07_2M_MS03 firmware: to make the embedded motion detection tool work, select the MJPEG codec for one of the streams and select MPEG4 or H.264 for the other stream. AP_01-00-59-07_2M_MS03 firmware: With the H.264 or MPEG4 codec, setting the frame rate does not work on the camera itself. No matter what you set, the actual frame rate is always around 17 fps. The TV standard parameter is integrated, but it does not affect the corresponding parameter in the web interface. This parameter is only needed for -HN5 and -HP5 cameras (these models differ only in available TV standards, resolutions, and frame rates). That is, if you change these settings in AN, you change the list of available resolutions and frame rates, but nothing else. AP_01-00-59-07_2M_MS03 firmware: The camera does not allow changing video or stream settings via the ONVIF protocol, except for switching protocols. The sensors, relays, and embedded video analytics do not work either. The firmware has nothing to do with it; the integration was done incorrectly. "]
["Messoa","Messoa NCB858","Camera ","AP_01-00-61-02_MS05","1",null,null,"+","+","+",null,null,"MJPEG/H.264: 2592x1944; MPEG4: 1920х1080","1024x768","640x480","+.",{"$nulls":3},"-",{"$nulls":4},"+","1. В Интеллекте значению Частоты опорных кадров \"0\" соответствует значение \"1/2\" из веб-интерфейса","1. In Intellect, the keyframe rate of 0 corresponds to that of 1/2 in the camera's web interface."]
["Messoa","Messoa NCR870","Camera ","AP_01-00-60-25_MS00","1",null,null,"+","+","+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":7},"-","+","1. Второй поток не доступен при одновременном выборе кодека MPEG4/H264 и разрешения 1920х1080 в первом потоке\n2. Третий поток не доступен при одновременном выборе кодека MJPEG и разрешения 1920х1080 в первом потоке ","1. If you select the MPEG4/H.264 codec and 1920x1080 resolution for the first stream, the second stream is not available. \n2. If you select the MPEG4 codec and 1920x1080 resolution for the first stream, the third stream is not available. "]
["Messoa","Messoa NDF821 / NDF820 / NDF831 / NDR891 / NCR870","Camera ","AP_01-00-59-07_2M_MS02","1",null,null,"+","+","+",null,null,"1920x1080","1024x768","640x480","+",null,"+","+",null,"+","+",null,"+","+","Прошивка AP_01-00-55_2M_MS02: Настройки на камере применяются довольно долго - после нажатия кнопки Применить камера уходит в ребут и настройки применяются примерно через минуту.Прошивка AP_01-00-55_2M_MS02: При отключении питания на камере для нее останавливается время. При включении питания на камере установлено время ее отключения.Прошивка AP_01-00-59-07_2M_MS02: Чтобы работал втроенный детектор движения необходимо, чтобы на одном из потоков был выбран кодек MJPEG, а на другом - MPEG4 либо H264.Прошивка AP_01-00-59-07_2M_MS02: На камере не работает настройка FPS с кодеками H264 и MPEG4. Независимо от значения параметра реально FPS всегда примерно равен 17.Параметр ТВ-стандарт интегрирован, но на аналогичную настройку в вебе не влияет. Он нужен для работы с камерами -HN5 и -HP5 (они отличаются только ТВ-стандартом, значениями разрешений и FPS). Т.е. при изменении этой настройки в AxxonNext/Next меняется список доступных разрешений и значений FPS и больше ничего.Прошивка AP_01-00-59-07_2M_MS02: Через ONVIF у камеры не работают никакие настройки потока и изображения, кроме смены протокола. Также не работают датчики, реле и встроенная аналитика. Это вина прошивки, а не интеграции.","AP_01-00-55_2M_MS02 firmware: The camera takes a lot of time to apply changes to settings: after you click Apply, the camera is restarted, so the changes are applied in around 1 minute. AP_01-00-55_2M_MS02 firmware: When you power the camera off, its time freezes. When you power it on again, the camera's time is the time when it was powered off. AP_01-00-59-07_2M_MS02 firmware: To make the embedded motion detection tool work, select the MJPEG codec for one of the streams and select MPEG4 or H.264 for the other stream. AP_01-00-59-07_2M_MS02 firmware: With the H.264 or MPEG4 codec, setting the frame rate does not work on the camera itself. No matter what you set, the actual frame rate is always around 17 fps. The TV standard parameter is integrated, but it does not affect the corresponding parameter in the web interface. This parameter is only needed for -HN5 and -HP5 cameras (these models differ only in available TV standards, resolutions, and frame rates). That is, if you change these settings in AN, you change the list of available resolutions and frame rates, but nothing else. AP_01-00-59-07_2M_MS02 firmware: The camera does not allow changing video or stream settings via ONVIF, except for switching protocols. The sensors, relays, and embedded video analytics do not work either. The firmware has nothing to do with it; the integration was done incorrectly."]
["Messoa","Messoa NIC830","Camera ","X.2.1.17","1",null,null,"+",{"$nulls":4},"1280x960","640x480","320x240","+",{"$nulls":5},"+",null,"-","+"]
["Messoa","Messoa NIC835","Camera ","X.2.1.17","1",null,null,"+",{"$nulls":4},"1280x960","640x480","320x240","+",{"$nulls":7},"-","+"]
["Messoa","Messoa NIC836","Camera ","X.2.1.10","1",null,null,"+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4","640x480","320x240","+",null,"+.","+.",null,"+","+",null,"-","+","1. при разрешении 1280х960 максимальный fps равен 12-15 fps, ограничение самой камеры\n2. автоматический поиск устройства в сети в ПО ITV  не может быть реализован \n\n","1. At 1280x960 resolution, the max. frame rate is 12–15 fps; this is a limitation of the camera itself.\n2. Automatic detection of the device cannot be implemented in AxxonSoft software. \n\n"]
["Messoa","Messoa NIC990","Camera ","M.0.2.7 ","1",null,null,"+",null,"+",null,null,"1280x720 (MJPEG) / 1920x1080 (H264)","640x480","320x240","+",null,"-","-","+.",{"$nulls":3},"-","+","1. Камера не поддерживает управление зумом/фокусом/диафрагмой с различной скоростью. В Axxon Next это проявляется в том, что нужно отклонять джойстик на максимальный угол.\n2. Прошивка M.0.2.5: видео в кодеке h264 при использовании протокола TCP идет с задержками. Рекомендуется использовать UDP.\n3. В многопоточном режиме настройки потоков зависят друг от друга. Ниже приведена таблица совместимости разрешений:\nH264 / MJPEG:\n1080P / -\n720P / 720P\n720P / CIF\n720P / QVGA\n480P / 480P\nVGA / VGA\nVGA / QVGA\nQVGA / QVGA","1. The camera does not support Zoom/Focus/Iris control at various speeds. In AN, this makes you bend you joystick at a max. angle.\n2. The M.0.2.5 firmware: H.264 video under TCP is lagging. We recommend using UDP.\n3. In Multistreaming mode, the streams' parameters are interdependent. Here below is compatibility table for resolutions:\nH264 / MJPEG:\n1080P / -\n720P / 720P\n720P / CIF\n720P / QVGA\n480P / 480P\nVGA / VGA\nVGA / QVGA\nQVGA / QVGA\n"]
["MicroDigital (MDi)","MicroDigital MDC-i4020C / MDC-i4020CTD / MDC-i7020VTD-30 / MDC-i7020FTD-30 / MDC-i7020F / MDC-i8020V-H / MDC-i8020VTD-30H / MDC-i8020VTD-H","Camera ","4.19-75-ds-Ivgsm","1","+.",null,"+",null,"+",null,null,"720x480","720x480","352x240","+",null,"+",null,null,"+","+",null,null,"+"]
["MicroDigital (MDi)","MicroDigital MDC-i4060C / MDC-i4060CTD / MDC-i7060VTD-30 / MDC-i7060FTD-30 / MDC-i7060F / MDC-i8060V-H / MDC-i8060VTD-30H / MDC-i8060VTD-H","Camera ","4.19-75-ds-Ivgsm","1","+.",null,"+",null,"+",null,null,"1280x1024","704x480","320x240","+",null,"+",null,null,"+","+",null,null,"+"]
["MicroDigital (MDi)","MicroDigital MDC-i4090C / MDC-i4090CTD / MDC-i7090VTD-30 / MDC-i7090FTD-30 / MDC-i7090F / MDC-i8090V-H / MDC-i8090VTD-30H / MDC-i8090VTD-H","Camera ","4.19-34-ds","1","+.",null,"+",null,"+",null,null,"1920x1072","1280x720","640x352","+",null,"+",null,null,"+","+",null,null,"+"]
["MicroDigital (MDi)","MicroDigital MDC-i4220CDN","Camera ","4.19-75-ds-Ivgsm","1","+.",null,"+",null,"+",null,null,"720x576","704x576","352x288","+",null,"+","-","+","+","+",null,"-","+","В NTSC-стандарте видео с камеры поступает только черно-белое - особенность устройства.Значение частоты кадров во втором видеопотоке задается не абсолютно, а относительно частоты кадров в первом потоке при помощи соответствующего параметра.","With NTSC, the camera sends only black-and-white video. This is a problem of the camera. For the second stream, the frame rate is set not as an absolute value, but relative to the frame rate of the first stream; use the relevant parameter."]
["MicroDigital (MDi)","MicroDigital MDC-i4230C","Camera ","4.01-14","1","+.",null,"+",null,"+",null,null,"640x480","640x480","320x240","+",null,"+","-",null,"+","-",null,"-","+","1. звук есть только с потоком MJPEG\n2. чтобы настроить работу Луча в ПО ITV. Необходимо после создания объекта \"Луч\" в ПО ITV в веб-интерфейсе камеры переключить состояние Input Type из Normal Open в Normal Close и обратно.\n ","1. Audio works only with the MJPEG stream.\n2. To make a sensor work in the AxxonSoft software, first create a Sensor object in the AxxonSoft software, then go to the camera's web interface, switch Input Type from Normal Open to Normal Close, and then switch it back to Normal Open. \n "]
["MicroDigital (MDi)","MicroDigital MDC-i4240 /-W","Camera ","4.19-75-ds-Ivgsm","1","+.",null,"+",null,"+",null,null,"640x480","640x480","320x240","+",null,"+","-","-","+","+",null,"-","+"]
["MicroDigital (MDi)","MicroDigital MDC-i4240C","Camera ","4.06","1","+.",null,"+",null,"+",null,null,"640x480","640x480","320x240","+",null,"+","-",null,null,"+",null,"-","+"]
["MicroDigital (MDi)","MicroDigital MDC-i4250C / MDC-i4250CTD","Camera ","4.11-75md-d1","1","+.",null,"+",null,"+",null,null,"1280x720","1280x720","640x352","-",null,"+","-","-","+","+",null,"-","+","Значение частоты кадров во втором видеопотоке задается не абсолютно, а относительно частоты кадров в первом потоке при помощи соответствующего параметра.","For the second stream, the frame rate is set not as an absolute value, but relative to the frame rate of the first stream; use the relevant parameter."]
["MicroDigital (MDi)","MicroDigital MDC-i4260/C/CTD","Camera ","4.19-75-ds-Ivgsm","1","+.",null,"+",null,"+",null,null,"1280x1024","704x480","320x240","-",null,"+","-",null,"+","+",null,"-","+","1. Прошивка 4.01-14: Чтобы настроить работу луча в ПО ITV. Необходимо после создания объекта \"Луч\" в ПО ITV в веб-интерфейсе камеры переключить состояние Input Type из Normal Open в Normal Close и обратно.\n2. Прошивка 4.11-63: камера интегрирована как MDi4260/C/CTD - именно такой индекс модели имеет устройство и так обнаруживается поиском.\n3. Камера имеет ограничение для мультипотокового режима: с двух потоков нельзя одновременно получать видео в кодеке MJPEG, в H264 - можно.","1. 4.01-14 firmware: To make a sensor work in the AxxonSoft software, first create a Sensor object in the AxxonSoft software, then go to the camera's web interface, switch Input Type from Normal Open to Normal Close, and then switch it back to Normal Open. \n2. 4.11-63 firmware: The camera is integrated as MDi4260/C/CTD: this is the model number of the device and how it is detected by search. \n3. The camera has a limitation on multi-streaming mode: you cannot have MJPEG video for both streams at the same time. There is no such limitation for H.264 video. "]
["MicroDigital (MDi)","MicroDigital MDC-i4270C","Camera ","4.07-06","1","+.",null,"+",null,"+",null,null,"720x576","704x576","352x288","+",null,"+","-","-","+","+",null,"-","+","Значение частоты кадров во втором видеопотоке задается не абсолютно, а относительно частоты кадров в первом потоке при помощи соответствующего параметра.","For the second stream, the frame rate is set not as an absolute value, but relative to the frame rate of the first stream; use the relevant parameter. "]
["MicroDigital (MDi)","MicroDigital MDC-i6060VTD-24H","Camera ","4.19-75-ds-Ivgsm","1","+.",null,"+",null,"+",null,null,"1280x1024","704x480","320x240","+",{"$nulls":8},"+","Устройство определяется в продукте, как MDi6060VTDd ","Camera is identified as MDi6060VTDd ."]
["MicroDigital (MDi)","MicroDigital MDC-i6090FTD-24H / MDC-i6090VTD-24H","Camera ","4.19-34-ds","1","+.",null,"+",null,"+",null,null,"1920x1072","1280x720","640x352","+",{"$nulls":8},"+"]
["MicroDigital (MDi)","MicroDigital MDC-i6261VTD(W)-66H","Camera ","4.19-79m-ds-iv ","1","+.",null,"+",null,"+",null,null,"1280x720","1280x720","640x352","+",{"$nulls":7},"-","+","1. В ПО ITV/Axxon камеры определяются как MDi6261VTDa / MDi6261VTDWa.","1. In the AxxonSoft products, the cameras are identified as MDi6261VTDa / MDi6261VTDWa."]
["MicroDigital (MDi)","Microdigital MDC-i6290VTD-10H","Camera","4.19-96-ds","1","+",2,"+","-","+","-","-","1920x1080","1280x720","640x352","-","-","-","-","-","-","-","-","-","+"]
["MicroDigital (MDi)","MicroDigital MDC-i7020FTD-12 / MDC-i6020FTD-24H / MDC-i6020VTD-24H","Camera ","4.19-75-ds-Ivgsm","1","+.",null,"+",null,"+",null,null,"720x480","720x480","352x240","+",{"$nulls":8},"+"]
["MicroDigital (MDi)","MicroDigital MDC-i7060FTD-12 / MDC-i6060FTD-24H / MDC-i6060VTD-24H","Camera ","4.19-75-ds-Ivgsm","1","+.",null,"+",null,"+",null,null,"1280x1024","704x480","320x240","+",{"$nulls":8},"+"]
["MicroDigital (MDi)","MicroDigital MDC-i8250V / MDC-i8250VTD ","Camera ","4.19-75-ds-IVgsm ","1","+.",null,"+",null,"+",null,null,"1280x720","1280x720","640х352","+",null,"+","-",null,"+","+",null,"-","+"]
["MicroDigital (MDi)","MicroDigital MDC-i8270V","Camera ","4.11-14","1","+.",null,"+",null,"+",null,null,"960x720","640x480","320x240","+",null,"+","-","-","+","+",null,"-","+","Значение частоты кадров во втором видеопотоке задается не абсолютно, а относительно частоты кадров в первом потоке при помощи соответствующего параметра.","For the second stream, the frame rate is set not as an absolute value, but relative to the frame rate of the first stream; use the relevant parameter."]
["MicroDigital (MDi)","MicroDigital MDC-i8270VTD","Camera ","4.11-14","1","+.",null,"+",null,"+",null,null,"960x720","640x480","320x240","+",null,"+","-","-","+","+",null,"-","+","Значение частоты кадров во втором видеопотоке задается не абсолютно, а относительно частоты кадров в первом потоке при помощи соответствующего параметра. После перезагрузки камера иногда перестает транслировать видео. Нужно повторно перезагрузить камеру.","For the second stream, the frame rate is set not as an absolute value, but relative to the frame rate of the first stream; use the relevant parameter. Sometimes, after the camera restarts, it stops sending video. Restart the camera again."]
["MicroDigital (MDi)","MicroDigital MDS-i101 / MDS-i3621Н / MDS-i3621WН","Camera ","4.19-75-ds-Ivgsm","1","+.",null,"+",null,"+",null,null,"720x576","704x576","352x288","+",null,"+","-","+","+","+",null,"-","+"]
["MicroDigital (MDi)","MicroDigital MDS-i1220 / MDS-i1220А / MDS-i1220Н","Camera ","4.19-75-ds-Ivgsm","1","+.",null,"+",null,"+",null,null,"720x576","720x576","352x288","+",null,"+",null,"+",{"$nulls":4},"+"]
["MicroDigital (MDi)","MicroDigital MDS-i301","Camera ","4.11-63","1","+.",null,"+",null,"+",null,null,"720x576","704x576","352x288","+",null,"+","-","+","+","+",null,"-","+","Значение частоты кадров во втором видеопотоке задается не абсолютно, а относительно частоты кадров в первом потоке при помощи соответствующего параметра.","For the second stream, the frame rate is set not as an absolute value, but relative to the frame rate of the first stream; use the relevant parameter."]
["Mobotix","Mobotix D12D","Camera ","MX-V3.4.5.18","1",null,null,"+",{"$nulls":3},"+.","2048x1536","1024x768","640x480","+",null,"+","-",null,"+","+",null,"-","+","1. в Intellect 4.7.6 Release поддержки кодека MxPEG нет. В Intellect 4.7.8/4.7.6. SP1 MxPEG поддерживается\n 2. звук с камеры можно получить, только если видео идет в формате MxPEG - особенность самой камеры\n 3. у самой камеры есть ограничение по fps для мегапиксельных разрешений:\n-Полное(2048х1536) - max. fps = 4(для MJPEG) / 7 (для MxPEG)\n-Высокое(1024х768) - max. fps =15 (для MJPEG) / 17 (для MxPEG)","1. Intellect 4.7.6 Release does not support the MxPEG codec. Intellect 4.7.8/4.7.6. SP1 does support MxPEG \n2. The camera sends audio only if video is in the MxPEG format. This is a limitation of the camera itself.\n3. For megapixel resolutions, the camera itself has frame rate limits:\n-Full (2048х1536) – max. fps = 4 (for MJPEG) / 7 (for MxPEG)\n-High (1024х768) – max. fps =15 (for MJPEG) / 17 (for MxPEG)"]
["Mobotix","Mobotix D14D","Camera ","MX-V4.1.4.11","1",null,null,"+",{"$nulls":3},"+","2048x1536","1024x768","640x480","+",null,"+","-","+",{"$nulls":3},"-","+"]
["Mobotix","Mobotix D15D / M15D / S15D / V15D","Camera","MX-V4.1.10.28","1",null,null,"+","-","-",null,"+","2048x1536","1024x768","640x480","+",null,"+","-","+","-","-","-","-","+"]
["Mobotix","Mobotix D22M","Camera ","MX-V3.5.2.23","1",null,null,"+",{"$nulls":3},"+.","2048x1536","1024x768","640x480","+",null,null,"-",{"$nulls":4},"-","+","1. в Intellect 4.7.6 Release поддержки кодека MxPEG нет. В Intellect 4.7.8/4.7.6 SP1 MxPEG работает, правда пока с проблемами\n2. для получения звука с данной камеры необходимо подключать сторонний ммикрофон у которого специфичные разьемы. Такого микрофона у нас нет, поэтому проверить звук с данной модели нельзя\n3. у самой камеры есть ограничение по fps для мегапиксельных разрешений:\n-Полное(2048х1536) - max. fps = 4(для MJPEG) / 7 (для MxPEG)\n-Высокое(1024х768) - max. fps =15 (для MJPEG) / 17 (для MxPEG)\n ","1. Intellect 4.7.6 Release does not support the MxPEG codec. In Intellect 4.7.8/4.7.6 SP1,  MxPEG does work, but there are still some problems.\n2. To get audio from this camera, you need to connect a third-party microphone by using special connectors. Because we do not have such a microphone, we cannot test audio for this camera.\n3. For megapixel resolutions, the camera itself has frame rate limits:\n-Full (2048х1536) – max. fps = 4 (for MJPEG) / 7 (for MxPEG)\n-High (1024х768) – max. fps =15 (for MJPEG) / 17 (for MxPEG)\n "]
["Mobotix","Mobotix D24M","Camera ","MX-V4.0.4.28","1",null,null,"+",{"$nulls":3},"+","2048x1536","1024x768","640x480","+",null,null,"-","+",{"$nulls":3},"-","+","Передача аудио доступна с помощью специального расширения.","You can get audio if you use a special plug-in. "]
["Mobotix","Mobotix M12D","Camera ","MX-V3.4.5.18","1",null,null,"+",{"$nulls":3},"+.","2048x1536","1024x768","640x480","+",null,"+","-",null,"+","+",null,null,"+","1. в Intellect 4.7.6 Release поддержки кодека MxPEG нет. В Intellect 4.7.8/4.7.6. SP1 MxPEG работает, правда пока с проблемами\n2. звук с камеры можно получить, только если видео идет в формате MxPEG - особенность самой камеры\n3. у самой камеры есть ограничение по fps для мегапиксельных разрешений:\n-Полное(2048х1536) - max. fps = 4(для MJPEG) / 7 (для MxPEG)\n-Высокое(1024х768) - max. fps =15 (для MJPEG) / 17 (для MxPEG)","1. Intellect 4.7.6 Release does not support the MxPEG codec. In Intellect 4.7.8/4.7.6 SP1, MxPEG does work, but there are still some problems.\n2. The camera sends audio only if video is in the MxPEG format. This is a limitation of the camera itself.\n3. For megapixel resolutions, the camera itself has frame rate limits:\n-Full (2048х1536) – max. fps = 4 (for MJPEG) / 7 (for MxPEG)\n-High (1024х768) – max. fps = 15 (for MJPEG) / 17 (for MxPEG)"]
["Mobotix","Mobotix M22M","Camera ","MX-V3.5.2.23","1",null,null,"+",{"$nulls":3},"+.","2048x1536","1024x768","640x480","+",null,null,"-",{"$nulls":4},"-","+","1. в Intellect 4.7.6 Release поддержки кодека MxPEG нет. В Intellect 4.7.8/4.7.6 SP1 MxPEG работает\n 2. у самой камеры есть ограничение по fps для мегапиксельных разрешений:\n-Полное(2048х1536) - max. fps = 4(для MJPEG) / 7 (для MxPEG)\n-Высокое(1024х768) - max. fps =15 (для MJPEG) / 17 (для MxPEG)","1. Intellect 4.7.6 Release does not support the MxPEG codec. In Intellect 4.7.8/4.7.6 SP1, MxPEG does work\n 2. For megapixel resolutions, the camera itself has frame rate limits:\n-Full (2048х1536) – max. fps = 4 (for MJPEG) / 7 (for MxPEG)\n-High (1024х768) – max. fps = 15 (for MJPEG) / 17 (for MxPEG)"]
["Mobotix","Mobotix M24M","Camera ","MX-V4.0.4.28","1",null,null,"+",{"$nulls":3},"+","2048x1536","1024x768","640x480","+",null,"+",null,"+",{"$nulls":3},"-","+","1. Звук с камеры есть только если видео идет в формате MxPEG. Это особенность самой камеры.\n2. Камера не PTZ, но у неё есть \"виртуальная\" телеметрия\n3. у самой камеры есть ограничение по fps для мегапиксельных разрешений:\n-Полное(2048х1536) - max. fps = 4(для MJPEG) / 7 (для MxPEG)\n-Высокое(1024х768) - max. fps =15 (для MJPEG) / 17 (для MxPEG)","1. The camera sends audio only if video is in the MxPEG format. This is a limitation of the camera itself.\n2. This is not a PTZ camera, but it has virtual PTZ support.\n3. For megapixel resolutions, the camera itself has frame rate limits:\n-Full (2048х1536) – max. fps = 4 (for MJPEG) / 7 (for MxPEG)\n-High (1024х768) – max. fps = 15 (for MJPEG) / 17 (for MxPEG)"]
["Mobotix","Mobotix Q22M","Camera ","MX-V3.4.5.10 (2009-03-02)","1",null,null,"+",{"$nulls":3},"+.","2048x1536","1024x768","640x480","+",null,"+",null,"+",{"$nulls":3},"-","+","1) максимальное разрешене 2048*1536 или 1456x1088, в зависимости от режима выбранного в камере INTL-7404\n2) Звук с камеры есть только если видео идет в формате MxPEG. Это особенность самой камеры.\n3) Камера не PTZ, но у неё есть \"виртуальная\" телеметрия\n ","1. The max. resolution is 2048*1536 or 1456x1088, depending on which mode you select on the INTL-7404 camera.\n2. The camera sends audio only if video is in the MxPEG format. This is a limitation of the camera itself.\nThis is not a PTZ camera, but it has virtual PTZ. \n "]
["Mobotix","Mobotix Q24M","Camera ","MX-V4.1.4.11 ","1",null,null,"+",{"$nulls":3},"+.","2048x1536","1024x768","640x480","+",null,"+","-","+",{"$nulls":3},"-","+","1. Звук с камеры есть только если видео идет в формате MxPEG. Это особенность самой камеры.\n2. Камера не PTZ, но у неё есть \"виртуальная\" телеметрия 3. Частота кадров сильно зависит от разрешения. При максимальном разрешении частота кадров составляет 1-2 кадра в секунду.\n4. При интенсивном движении в поле зрения камеры частота кадров может снижаться почти вдвое. ","1. The camera sends audio only if video is in the MxPEG format. This is a limitation of the camera itself.\n2. This is not a PTZ camera, but it has virtual PTZ. 3. The frame rate very much depends on the resolution settings. If you set the max. resolution, the frame rate drops to around 1-2 fps.\n4. Heavy motion in the FoV causes the frame rate to drop by half. "]
["Mobotix","Mobotix S14D / S14M","Camera ","V4.1.4.11","1",null,null,"+",{"$nulls":3},"+","2048x1536","1024x768","640x480","+",null,"+","-","+",{"$nulls":3},"-","+","1. Audio Input работает только, если для видео выбран кодек MxPEG","1. Audio Input works only if video is selected in MxPEG codec "]
["Mobotix","Mobotix T24M","Intercom ","MX-V4.1.1.21","1",null,null,"+",{"$nulls":3},"+","2048x1536","1024x768","640x480","+",null,null,"-","+",{"$nulls":4},"+"]
["MOXA","MOXA Vport 461","Encoder ","3.1 Build 11080216","1",null,null,"+",null,"+",null,null,"720x576","704x576","640x480","+",null,"+","-","-","+","+",null,"-","+","В процессе работы с устройством обнаружилась такая особенность: иногда (примерно раз в сутки, может реже) устройство зависает и становится недоступным. Помогает перезагрузка.Телеметрию не удалось заставить работать даже через веб-интерфейс.Чтобы сработал датчик, на его вход необходимо подать напряжение от 13В до 30В (в соответствии с мануалом).","While using the camera, we discovered the following problem: sometimes (approx. once per day, sometimes less often) the device freezes and becomes unavailable. It helps to restart the device. We did not manage to make telemetry work, even in the web interface. To make the sensor go off, energize it (13–30 V, according to the guide)."]
["NexusIP ","NexusIP 1MP-NEX-BOX","Camera ","v1.1.0_20130109","1",null,null,"+","+","+",null,null,"1280x720 (H264) / 720x576 (MJPEG / MPEG4) ","720x576","352x288","+",{"$nulls":8},"-"]
["NexusIP ","NexusIP 1MP-NEX-DOME ","Camera ","v1.1.0_20130109","1",null,null,"+","+","+",null,null,"1280x720","720x576","352x288","+",{"$nulls":8},"-"]
["NexusIP ","NexusIP 2MP-NEX-BOX","Camera ","v1.1.0_20130109","1",null,null,"+","+","+",null,null,"H.264: 1920x1080; MJPEG / MPEG4: 1280x720","H.264: 1280x720; MJPEG / MPEG4: 720x576","352x288",{"$nulls":9},"-"]
["NexusIP ","NexusIP 2MP-NEX-DOME ","Camera ","v1.1.0_20130109","1",null,null,"+","+","+",null,null,"H.264: 1920x1080; MJPEG / MPEG4: 1280x720;","H.264: 1280x720; MJPEG / MPEG4: 720x576","352x288",{"$nulls":9},"-"]
["Novus","Novus NVIP-2C2011D-P ","Camera ","nv20111011NSA","1",null,null,"+",null,"+",null,null,"1920x1080","800x600","640x480","+",null,"+",{"$nulls":5},"+","+","Поиск может обнаружить устройство как Onvif-совместимое, но работать через Onvif оно не будет.Доступные кодеки, разрешения и значения частоты кадров в разных потоках зависят друг от друга.","Search detects the camera as an ONVIF-conformant device, but the camera does not work via the ONVIF protocol. The Codec and Resolution parameters for different streams are interdependent."]
["Novus","Novus NVIP-2DN2001D-2P","Camera ","nv20111110NSA","1",null,null,"+",null,"+",null,null,"1920x1080","800x600","640x480","+",null,"+","-",null,"+","+",null,"+","+","Доступные кодеки, разрешения и значения частоты кадров в разных потоках зависят друг от друга.Поиск может обнаружить устройство как Onvif-совместимое, но работать через Onvif оно не будет.","The Codec and Resolution parameters for different streams are interdependent. Search detects the camera as an ONVIF-conformant device, but the camera does not work via the ONVIF protocol. "]
["Novus","Novus NVIP-2DN2001D-P/GO","Camera ","NVS01.2.1061.46","1",null,null,"+",null,"+",null,null,"1920х1080","1024x768","640x480","+",{"$nulls":7},"motion detection; ","+"]
["Novus","Novus NVIP-2DN5001С-1P / NVIP-2DN3001H/IR-2P / NVIP-2DN4001V/IRH","Camera ","nv20111110NSA","1",null,null,"+",null,"+",null,null,"1920x1080","800x600","640x480","+",null,"+","-",null,"+","+",null,"+","+","Доступные кодеки, разрешения и значения частоты кадров в разных потоках зависят друг от друга.Поиск может обнаружить устройство как Onvif-совместимое, но работать через Onvif оно не будет.","Which codecs, resolutions, and frame rates are available for one stream depends on those for the other stream. Search detects the camera as an Onvif-conformant device, but the camera does not work via the ONVIF protocol "]
["Novus","Novus NVIP-2DN5005CZ-P/GO","Camera ","NVS01.2.1061.46","1",null,null,"+",null,"+",null,null,"1920х1080","1024x768","640x480","+",{"$nulls":7},"motion detection; ","+"]
["Novus","Novus NVIP-2DN5018CZ-2P","Camera ","nv20130115NSA ","1",null,null,"+",null,"+",null,null,"1920x1080 ","800x600","640x480","+",{"$nulls":3},"+.",{"$nulls":4},"+","Из функционала телеметрии интегрированы только зум, фокус и пресеты.","For PTZ (telemetry) only interated zoom, focus, presets."]
["Novus","Novus NVIP-2DN6020SD","Camera ","V1.202R05-T320","1",null,null,"+",null,"+",null,null,"1920x1080(H.264)/720x576(mjpeg)","1024x768(H.264)/352x480(mjpeg)","640x480(H.264)/352x240(mjpeg)","+",{"$nulls":3},"+","+","+",null,null,"+"]
["Novus","Novus NVIP-2DN6020SD-2P","Camera ","nv20130115NSA ","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","-",null,"+","-","+","+","+",null,"motion detection; ","+"]
["Novus","Novus NVIP-5DN2021D/IR-2P","Camera ","nv20130115NSA ","1",null,null,"+",null,"+",null,null,"1920x1080(MJPEG) 2592x1944(H264)","1024x768 ","640x480 ","+",null,"+",null,null,"+",null,null,"motion detection; ","+","Разрешение на втором потоке камеры зависит от разрешения на первом потоке, при работе с двумя потоками необходимо проверять в веб интерфейсе существует ли необходимая комбинация разрешений. ","Resolution on the second stream of camera depends on resolution of the first stream. Using two streams, please check in web interface if there's a required combination of resolution."]
["Novus","Novus NVIP-5DN5001C-1P","Camera ","nv20130115NSA","1",null,null,"+",null,"+",null,null,"2592x1944 (H264) / 1920x1080 (MJPEG)","1024x768","640x480","+",null,"+","-",null,"+","+",null,"motion detection; ","+"]
["Novus","Novus NVIP-DN6137SD","Camera ","V1.110R02-T322","1",null,null,"+",null,"+",null,null,"720x576","352x480","352x240","+",null,"+","+","+","-","-",null,"-","+","Звук с микрофона не идет, если видео получается со второго потока ","If video comes from stream 2, the mic fails to deliver audio. "]
["Novus","Novus NVIP-TDN3401H/IR/MPX2.0","Camera ","v1.0.28_NV","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+",null,null,"+","+",null,"motion detection","+","1. В ПО Intellect камера обнаруживается поиском как FineCCTV IPCam.","1. In Intellect, the search finds the camera as FineCCTV IPCam."]
["Novus","Novus NVIP-TDN5401C/MPX2.0 ","Camera ","V1.0.42_NV","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+","+",null,"+","+",null,"motion detection; ","+"]
["Oncam Grandeye","Oncam Grandeye EVO-05NCD","Fisheye Camera","1.2.2.S","1",null,null,"+",null,"+",null,null,"2144x1944","1488x1360","528x480","+",{"$nulls":8},"+","1. Камера интегрирована в ПО ITV/Axxon как OncamGrandeye Evolution series.\n2. Для корректной работы настройки качества с кодеком H264 необходимо выбрать значение off настройки bitrate control. ","1. Camera is integrated in Axxonsoft SW as OncamGrandeye Evolution series.\n2. Please select value of bitrate control \"off\" to work with quality setting of H.264 correctly."]
["Oncam Grandeye","Oncam Grandeye Halocam IPC","Fisheye Camera","2.1.3","1","+","4","+",{"$nulls":4},"2144x1944","1024x768","640x480","+",{"$nulls":3},"-","-","-",null,"-","+",null,null,"new"]
["Optelecom-NKF","Siqura BC24 WDR","Camera ","s20091022NS","1",null,null,"+","+",{"$nulls":3},"1280x960(MJPEG) / 640x480(MPEG-4)","1280x960(MJPEG) / 352x288(MPEG-4)","640x480(MJPEG) / 320x240(MPEG-4)","+",null,"+","-",null,"+","+",null,"-","+"]
["Optelecom-NKF","Siqura C-50 E-MC encoder","Encoder ","2.5.0","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","320x240","+",null,"+","-","+","+","+",null,"-","-"]
["Optelecom-NKF","Siqura C-60 E-MC encoder","Encoder ","2.5.0","1",null,null,"+","+","+",null,null,"720x576","640x480","320x240","+",null,"+","-","+","+","+",null,null,"-"]
["Optelecom-NKF","Siqura S-54 E encoder","Encoder ","2.5.0","4",null,null,"+","+",{"$nulls":3},"720x576","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","-","1. fps видеопотока сильно зависит от разрешения и качества видео\n2. видеоформат (MJPEG/MPEG-4) и fps видеопотока в Intellect меняется сразу для всех 4-х каналов.\n ","1. The frame rate very much depends on the video resolution and quality\n2. in Intellect, when you change the codec (MJPEG/MPEG-4) or frame rate, you change it for all 4 channels at once. \n "]
["Optelecom-NKF","Siqura S-64 E encoder","Encoder ","3.0.1","4",{"$nulls":4},"+",null,null,"720x576","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","-"]
["Optelecom-NKF","Siqura V-30 E-MSA encoder","Encoder ","2.5.0","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","320x240","+",{"$nulls":3},"+","+","+",null,"-","-","1. После смены граббера(MJPEG/MPEG-4) в  ПО ITV, следует то же самое сделать и в веб-интерфейсе самого ip-устройства.","1. After you change the grabber (MJPEG/MPEG-4) in the AxxonSoft software, do the same in the device's web interface."]
["Panasonic (BB/BL)","Panasonic BB-HCM311","Camera ","1.34","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",null,"+","-","+","+","+",null,"-","-","1. При Полном разрешении камера способна выдавать только 12-14 fps (в зависимости откачества). Это особенность самой камеры, описана в документации на камеру\n2. У самой камеры всего 3 положения качества, а в Intellect их 5, поэтому некоторые будут повторяться","1. With the Full resolution, the frame rate is limited to 12 -14 fps (depending on the quality). This is a limitation of the device itself (described in the camera's documentation) \n2. The camera itself has 3 positions for quality. Because Intellect has 5, some of the positions in Intellect mean one and the same quality. "]
["Panasonic (BB/BL)","Panasonic BB-HCM331","Camera ","1.34","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",null,"+","-","+","+","+",null,"-","-"]
["Panasonic (BB/BL)","Panasonic BB-HCM381","Camera ","1.34","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",null,"+","-","+.","+","+.",null,"-","-"]
["Panasonic (BB/BL)","Panasonic BB-HCM511CE/515CE","Camera ","3.5100R","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+","-","+","+","+",null,"-","+","1) для потока MJPEG нельзя изменить fps, такой настройки нет у самой камеры. Значения такие:\nразрешение 640*480 - 10 fps\nразрешение 320*240 - 29-30 fps\n2) у камеры есть только 3 фиксировыых значения качества - потому некоторые значения на ползунке качество в Intellect не отрабатывают","1) for the MJPEG stream, you cannot change the frame rate, because the camera itself does not have this setting. Frame rate values: \nthe 640*480 resolution - 10 fps\nthe 320*240 resolution - 29-30 fps\n2) the camera itself has 3 positions for quality. For this reason, some of the positions do not work on Intellect's quality slider. "]
["Panasonic (BB/BL)","Panasonic BB-HCM531CE","Camera ","3.60R00","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+","-","+","+","+",null,"-","+","1) для потока MJPEG нельзя изменить fps, такой настройки нет у самой камеры. Значения такие:\nразрешение 640*480 - 10 fps\nразрешение 320*240 - 29-30 fps\n2) у камеры есть только 3 фиксированных значения качества - потому некоторые значения на ползунке качество в Intellect не отрабатывают\n \n ","1) for the MJPEG stream, you cannot change the frame rate, because the camera itself does not have this setting. Frame rate values:\nthe 640*480 resolution - 10 fps\nthe 320*240 resolution - 29-30 fps\n2) the camera itself has 3 positions for quality. For this reason, some of the positions do not work on Intellect's quality slider. \n \n "]
["Panasonic (BB/BL)","Panasonic BB-HCM580CE/581CE","Camera ","3.60R00","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+","-","+","+","+",null,"-","+","1) у камеры есть только 3 фиксированных значения качества при MJPEG - поэтому некоторые значения на ползунке качество в Intellect будут совпадать","1) for MJPEG, the camera itself has 3 positions for quality. For this reason, some of the positions do not work on Intellect's quality slider."]
["Panasonic (BB/BL)","Panasonic BB-HCM715CE","Camera"," 4.31R03","1",null,null,"+","+","+","-","-","1280x960","640x480","320x240","+","-","+","-","+","+","+","-","-","+","Включение/выключение максимального разрешения 1280х960 и применение некоторых других настроек видео требует перезагрузки устройства.В многопоточном режиме смена разрешения на одном из потоков изменяет список доступных разрешений на другом потоке. Нужно самостоятельно исключать конфликты выбранных параметров.Разрешение 192х144 во втором потоке недоступно для кодека H264.Прошивка 4.31R00: Изображение в кодеке H264 искажено.Реле имеет выходное напряжение 10.5-13 В DC","After you switch the max. resolution (1280x960) on/off or apply certain video settings, you have to restart the device. In multistream mode, when you change the resolution for one of the streams, you change the list of resolutions available for another stream. You have to avoid conflicts of selected parameters yourself. For the second stream, the 192x144 resolution is not available with H.264.The 4.31R00 firmware: With H.264, video is distorted. The relay's output voltage is 10.5-13 V DC."]
["Panasonic (BB/BL)","Panasonic BL-C1","Camera ","1.34","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":7},"-","+","1. При Полном разрешении камера способна выдавать только 7-10 fps (в зависимости от качества). Это особенность самой камеры, при Стандартном разрешении - 15 fps\n2. У самой камеры всего 3 положения качества, а в Intellect их 5, поэтому некоторые будут повторяться\n","1. With the Full resolution, the camera allows 7 -10 fps max. (depending on the quality). This is a limitation of the device itself; with the Standard resolution, the camera allows 15 fps. The camera itself has 3 positions for quality. Because Intellect has 5, some of the positions in Intellect mean one and the same quality.\n"]
["Panasonic (BB/BL)","Panasonic BL-C10","Camera ","1.25","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":4},"-","1. При Полном разрешении камера способна выдавать только 7-10 fps (в зависимости от качества). Это особенность самой камеры, описана в документации на камеру, при Стандартном разрешении - 15 fps\n2. У самой камеры всего 3 положения качества, а в Intellect их 5, поэтому некоторые будут повторяться","1. With the Full resolution, the camera allows 7 -10 fps max. (depending on the quality). This is a limitation of the device itself (described in the camera's documentation); with the Standard resolution, the camera allows 15 fps.\n2. The camera itself has 3 positions for quality. Because Intellect has 5, some of the positions in Intellect mean one and the same quality."]
["Panasonic (BB/BL)","Panasonic BL-C111","Camera ","3.60R00","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+",null,"+",{"$nulls":3},"-","+","1. Из мануала на камеру «Частота 30 кадров/сек. невозможна при просмотре изображений MJPEG с разрешением 640 × 480»\n2. У самой камеры всего 3 положения качества, а в Intellect их 5, поэтому некоторые будут повторяться\n\n","1. According to the camera's guide, the 30 fps frame rate is not available when viewing videos with MJPEG and the 640 x 480 resolution\n2. The camera itself has 3 positions for quality. Because Intellect has 5, some of the positions in Intellect mean one and the same quality.\n\n"]
["Panasonic (BB/BL)","Panasonic BL-C131","Camera ","3.60R00","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+",null,"+",{"$nulls":3},"-","+","1. Из мануала на камеру «Частота 30 кадров/сек. невозможна при просмотре изображений MJPEG с разрешением 640 × 480»\n2. У самой камеры всего 3 положения качества, а в Intellect их 5, поэтому некоторые будут повторяться","1. According to the camera's guide, the 30 fps frame rate is not available when viewing videos with MJPEG and the 640 x 480 resolution\n2. The camera itself has 3 positions for quality. Because Intellect has 5, some of the positions in Intellect mean one and the same quality."]
["Panasonic (BB/BL)","Panasonic BL-C160","Camera ","3.60R00","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":7},"-","+"]
["Panasonic (BB/BL)","Panasonic BL-C20","Camera ","1.34","1",null,null,"+",{"$nulls":4},"640x480","640x480","352x240","+",{"$nulls":7},"-","+","1. При Полном разрешении камера способна выдавать только 7-10 fps (в зависимости от качества). Это особенность самой камеры, описана в документации на камеру, при Стандартном разрешении - 15 fps\n2. У самой камеры всего 3 положения качества, а в Intellect их 5, поэтому некоторые будут повторяться","1. With the Full resolution, the camera allows 7 -10 fps max. (depending on the quality). This is a limitation of the device itself (described in the camera's documentation); with the Standard resolution, the camera allows 15 fps.\n2. The camera itself has 3 positions for quality. Because Intellect has 5, some of the positions in Intellect mean one and the same quality."]
["Panasonic i-Pro","Panasonic AW-HE60SN/SE/HN/HE","Camera","V03.06","1",null,null,"+","-","+","-","-","640x480","640x480","640x480","-","-","-","-","+","-","-","-",null,"+","Для получения видео в ПО ITV/Axxon c кодеком H.264 необходимо в web-интерфейсе камеры включить настройки \"H.264 transmission\" и \"Internet mode (over HTTP)\"","To receive video in Axxon software with H.264 codec, enable \"H.264 transmission\" and \"Internet mode (over HTTP)\" settings in the camera web interface."]
["Panasonic i-Pro","Panasonic WJ-GXE500","Encoder ","1.11","4","+.",null,"+","+","+.",null,null,"640x480 / 640x360 / 720x576","640x480 / 640x360 / 720x576","320x240 / 320x180 / 720x576","+",null,"+","-","+","+","+",null,"+","+","1. При задействовании на камере H.264 или MPEG-4 на MJPEG-видеопоток накладывается ограничение в 15 fps max\n2. fps для MJPEG потока зависит от количества одновременно задействованных видеоканалов\n3. При выборе других ТВ-стандартов кроме PAL в настройках в ПО Axxon будет доступен MPEG-4, хотя фактически на камере он будет заблокирован\n4. При выборе MPEG-4 в настройках в ПО Axxon будет доступно мегапиксельное разрешение, хотя при MPEG-4 фактически камера его не поддерживает","1. If you enable H.264 or MPEG-4 on the camera, the MJPEG video stream is limited to 15 fps max.\n2. For MJPEG, the frame rate very much depends on how many video channels are used at the same time\n3. If you select any ***TV standard*** other than PAL, the AxxonSoft software shows MPEG-4 as an available option, but the camera itself does not allow this codec. \n4. If you select any MPEG-4, the AxxonSoft software shows a megapixel resolution as an available option, but the camera itself does not allow this resolution for MPEG-4. "]
["Panasonic i-Pro","Panasonic WJ-ND400","NVR","Software version 1: V3.30, Software version 2: V1.20","64",null,null,"+","+","+",null,null,"auto","auto","auto",null,null,"-",null,"+.","-","+","+.",null,"-","В веб-интерфейсе есть настройка пресетов, но пресеты не работают.Реле замыкается на промежуток времени, настраиваемый в веб-интерфейсе, по истечении которого реле автоматически размыкается.","The web interface allows you to configure presets, but presets do not work. The relay stays closed for the time that you set in the web interface; after that time elapses, the relay opens automatically."]
["Panasonic i-Pro","Panasonic WJ-NT304 encoder","Encoder ","1.12","4",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+","-","-","+.","+",null,"-","+","1. для MPEG-4 ползунок \"Скорость\" регулирует битрейт видеопотока, поэтому вместе с изменением fps меняется и качество видеоизображения - так сделано потому что у самой камеры нет настройки \"Скорость\" в чистом виде для MPEG-4 видепотока\n2. Лучи на размыкание не работают в Intellect - особенность интеграции в Intellect\n3. Телеметрия не проверялась из-за проблем с подключением","1. for MPEG-4, the ***Rate*** slider changes the bit rate of the video stream; for this reason, when you adjust the frame rate, you adjust the image quality too: it was done like this, because for MPEG-4 the camera itself doe not have a \"pure\" Rate setting\n2. In Intellect, the sensors do not go off when you close them - this is how the integrated was done in Intellect\n3. We did not test telemetry, because of connection problems. "]
["Panasonic i-Pro","Panasonic WV-NF284(E)","Camera ","1.60E4","1","+.",null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+",null,null,"+","+",null,"-","+","1. при включении одновременно MJPEG и MPEG-4, на MJPEG накладывается ограничение по скорости в 5(10) fps - особенность самой камеры, Intellect не причем.\n2. для MPEG-4 ползунок \"Скорость\" регулирует битрейт, поэтому вместе с изменением fps меняется и качество - особенность интеграции в Intellect.\n3. Реле подключается к OUT-GND (срабатывает с задержкой ~5 секунд)","1. when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself, Intellect has nothing to do with it.\n2. for MPEG-4, the ***Rate*** slider changes the bit rate; for this reason, when you adjust the frame rate, you adjust the image quality too - this is how the integration was done in Intellect. \n3. Connect relays to OUT-GND (it works with a delay of around 5 seconds)"]
["Panasonic i-Pro","Panasonic WV-NP1000(E)/1004(E)","Camera ","1.24E2","1",null,null,"+","+",{"$nulls":3},"1280x960или960x720(MJPEG)/640x480(MPEG-4)","640x480","320x240","+",null,"+",null,null,"+.","+",null,"-","-","1. при включении в настройках камеры одновременно MJPEG и MPEG-4 видеопотока, на MJPEG-поток накладывается ограничение по скорости в 5(10) fps - это особенность самой камеры, так камера работает и в \"родном\" софте и в Intellect\n2. для MPEG-4 ползунок \"Скорость\" регулирует битрейт видеопотока, поэтому вместе с изменением fps меняется и качество видеоизображения - так сделано потому что у самой камеры нет настройки \"Скорость\" в чистом виде для MPEG-4 видепотока\n3. Лучи на размыкание не работают в Intellect - особенность интеграции в Intellect\n4. У камеры есть два режима. Partial и Full Scanning, в первом \"Полное\" разрешение равно 960x720, во втором - 1280x960\n\n5. Реле подключается к AUX-GND","1. when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself, the camera works like this both in its own software and in Intellect. \n2. for MPEG-4, the ***Rate*** slider changes the bit rate of the video stream; for this reason, when you adjust the frame rate, you adjust the image quality too: it was done like this, because for MPEG-4 the camera itself doe not have a \"pure\" Rate setting\n3. In Intellect, the sensors do not go off when you close them - this is how the integrated was done in Intellect\n4. The camera has two modes: Partial Scanning and Full Scanning; the Full resolution is 960x720 for the first mode and 1280x960 for the second mode\n\n5. Connect relays to AUX-GND"]
["Panasonic i-Pro","Panasonic WV-NP240(E)/244(E)","Camera ","1.80E4","1","+.",null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+",null,null,"+","+",null,"-","+","1. при включении в настройках камеры одновременно MJPEG и MPEG-4 видеопотока, на MJPEG-поток накладывается ограничение по скорости в 5(10) fps - это особенность самой камеры, так камера работает и в \"родном\" софте и в Intellect\n2. для MPEG-4 ползунок \"Скорость\" регулирует битрейт видеопотока, поэтому вместе с изменением fps меняется и качество видеоизображения - так сделано потому что у самой камеры нет настройки \"Скорость\" в чистом виде для MPEG-4 видепотока \n3. У MPEG-4 всего 3 положения кач-ва, а в Intellect их 5, поэтому некотрые будут повторятся - особенность интеграции в Intellect\n4. Реле подключается к OUT-GND","1. when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself, the camera works like this both in its own software and in Intellect. \n2. for MPEG-4, the ***Rate*** slider changes the bit rate of the video stream; for this reason, when you adjust the frame rate, you adjust the image quality too: it was done like this, because for MPEG-4 the camera itself doe not have a \"pure\" Rate setting \n3. For MPEG-4, the camera itself has 3 positions for quality. Because Intellect has 5, some of the positions in Intellect mean one and the same quality - this is how the integration was done.\n4. Connect relays to OUT-GND"]
["Panasonic i-Pro","Panasonic WV-NP472(E)","Camera ","2.21/E","1",null,null,"+",{"$nulls":4},"752x560","752x272","368x272","+",{"$nulls":4},"-","+",null,"-","-","1. Скорость видео сильно зависит от качества и разрешения. Например примаксимальном разрешении и качестве ограничение по скорости составляет 7 fps, при максимальном разрешении и средней скорости - 10 fps. Высокое разрешение и максимальное качество - 15 fps, Высокое разрешение и среднее качество - 20 fps.\n\n2.После нажатия \"Применить\" видео в течении 2-2,5 секунд продолжает идти со старыми настройками, и лишь затем по камере отображается деттач и новые настройки применяются. Особенность камеры","1. The frame rate very much depends on the video resolution and quality. For example, with the max. resolution and quality, the max. frame rate is 7 fps and with the max. resolution and average quality, the max. frame rate is 10 fps. The high resolution and max. quality - 15 fps; the high resolution and average quality - 20 fps. \n\n2.After you click Apply, for 2-2.5 seconds video does not change; only after that the camera shows a detach and new settings are applied. This is a limitation of the camera itself."]
["Panasonic i-Pro","Panasonic WV-NP502(E)/NW502S(E)","Camera ","1.44","1","+.",null,"+","+","+",null,null,"PAL (4:3, 3MP): 2048x1536 (MJPEG) / 1280x960 (H264) / --- (MPEG4) | NTSC (16:9, 3MP): 1920x1080 (MJPEG, H264) / --- (MPEG4)","PAL (4:3, 3MP): 1280x960 (MJPEG) / 640x480 (H264) / 640x480 (MPEG4) | NTSC (16:9, 3MP): 1920x1080 (MJPEG, H264) / --- (MPEG4)","PAL (4:3, 3MP): 640x480 (MJPEG) / 320x240 (H264) / 320x240 (MPEG4) | NTSC (16:9, 3MP): 640x360 (MJPEG, H264) / --- (MPEG4)","+.","+","+","-",null,"+","+",null,"+","+","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.В кодеках MPEG4 и H264 при получении видео по протоколу UDP возможны потери пакетов и рывки видео. В таких случаях рекомендуется использовать протокол RTSP over TCP.Набор разрешений зависит от выбранного режима (1.3 MP, 3MP) и соотношения сторон (4:3, 16:9). В нашем ПО эти настройки реализованы через параметр \"ТВ-стандарт\".Настройки видео (кодек, разрешение, частота кадров) в потоках взаимозависимы. Следить за их совместимостью пользователь должен самостоятельно.Кодеки в потоках 1 и 2 должны совпадать. Одновременно получать с камеры и MPEG4, и H264 нельзя.MPEG4 доступен только в режимах 4:3_3MP и 4:3_1.3MP (PAL)Смена режима 1.3MP - 3MP требует перезагрузки устройства.Для поиска камеры в сети необходимо предварительно настроить постоянную, не ограниченную по времени видимость камеры. Эта настройка осуществляется через веб-интерфейс камеры.Находится в списке неподдерживаемых устройств (общая проблема камер Panasonic). То есть найти устройство можно, но добавить из результатов поиска в конфигурацию нельзя. Добавлять устройство нужно вручную.Из встроенной аналитики в настоящий момент интегрирован детектор лиц, детектор движения не интегрирован.На камере есть 3 программируемых IO-порта. 1й и 3й используются в нашем ПО как лучи, 2й - как реле.","Video transmission (mpeg4/h.264) is implemented via the following protocols: the Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP In Intellect, these protocols correspond to the unicast, tcp, udp, and multicast ***Windows Registry keys***, respectively. For MPEG4 and H.264, when receiving video via the UDP protocol, packets may get lost, video may stop for some time and then continue again. To fix this, use RTSP over TCP. The set of resolutions depends on which mode (1.3 MP, 3MP) and aspect ratio (4:3, 16:9) are selected. Our software implements these settings with the ***TV Standard*** parameter. The video settings (codec, resolution, frame rate) for different streams are interdependent. The user must himself ensure that the settings are compatible. You have to use the same codecs for stream 1 and 2. You cannot get MPEG4 and H.264 streams from the camera at the same time.MPEG4 is available only in 4:3_3MP and 4:3_1.3MP (PAL) modes After you switch resolutions (1.3 MP - 3MP) ), you must restart the device (around 1 minute).To be able to search for the device, set the camera to ***permanent visibility***. Do it in the camera's web interface. This is an unsupported device (a problem shared by Panasonic cameras). That is, the search finds the device, but you cannot add the device directly from the search results. You must add it manually. Of the embedded video analytics, the ***face detector*** is integrated; the motion detector is not integrated. The camera has 3 programmable I/O ports. Our software uses ports 1 and 3 for sensors and port 2 for relays. "]
["Panasonic i-Pro","Panasonic WV-NS202A(E)","Camera ","2.70P7","1","+.",null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+","-","+","+","+",null,"-","+","1. при включении в настройках камеры одновременно MJPEG и MPEG-4 видеопотока, на MJPEG-поток накладывается ограничение по скорости в 5(10) fps - это особенность самой камеры, так камера работает и в \"родном\" софте и в Intellect \n2. Реле подключается к OUT-GND\n","1. when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself, the camera works like this both in its own software and in Intellect. \n2. Connect relays to OUT-GND\n"]
["Panasonic i-Pro","Panasonic WV-NS950(E)/954(E)","Camera ","1.60E3","1","+.",null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+.","-","+","+","+",null,"-","+","1. при вкл. одновременно MJPEG и MPEG-4, на MJPEG накладывается ограничение по скорости в 5(10) fps - особенность самой камеры\n2. для MPEG-4 ползунок \"Скорость\" регулирует битрейт видеопотока, поэтому вместе с изменением fps меняется и качество видеоизображения - так сделано потому что у самой камеры нет настройки \"Скорость\" в чистом виде для MPEG-4 видепотока\n3. Ползунок \"Качество\" для MPEG-4 видеопотока не работает - особенность интеграции в ПО ITV\n4. Реле подключается к OUT-GND","1. when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself\n2. for MPEG-4, the ***Rate*** slider changes the bit rate of the video stream; for this reason, when you adjust the frame rate, you adjust the image quality too: it was done like this, because for MPEG-4 the camera itself doe not have a \"pure\" Rate setting\n3. For MPEG-4, the Quality slider does not work - this is how the integration was done in the AxxonSoft software\n4. Connect relays to OUT-GND"]
["Panasonic i-Pro","Panasonic WV-NW484S(E)","Camera ","1.60E5","1","+.",null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":4},"+","+",null,"-","+","1. при включении в настройках камеры одновременно MJPEG и MPEG-4 видеопотока, на MJPEG-поток накладывается ограничение по скорости в 5(10) fps - это особенность самой камеры, так камера работает и в \"родном\" софте и в Intellect\n2. для MPEG-4 ползунок \"Скорость\" регулирует битрейт видеопотока, поэтому вместе с изменением fps меняется и качество видеоизображения - так сделано потому что у самой камеры нет настройки \"Скорость\" в чистом виде для MPEG-4 видепотока \n3. Реле подключается к OUT-GND","1) when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself, the camera works like this both in its own software and in Intellect. \n2. for MPEG-4, the ***Rate*** slider changes the bit rate of the video stream; for this reason, when you adjust the frame rate, you adjust the image quality too: it was done like this, because for MPEG-4 the camera itself doe not have a \"pure\" Rate setting \n3. Connect relays to OUT-GND"]
["Panasonic i-Pro","Panasonic WV-NW960(E)/964(E)","Camera ","1.60E3","1","+.",null,"+","+",{"$nulls":3},"640x480","640x480","352x240","+",null,"+.","-","+","+","+",null,"-","+","1. при вкл. одновременно MJPEG и MPEG-4, на MJPEG накладывается ограничение по скорости в 5(10) fps - особенность самой камеры\n2. для MPEG-4 ползунок \"Скорость\" регулирует битрейт видеопотока, поэтому вместе с изменением fps меняется и качество видеоизображения - так сделано потому что у самой камеры нет настройки \"Скорость\" в чистом виде для MPEG-4 видепотока\n3. Ползунок \"Качество\" для MPEG-4 видеопотока не работает - особенность интеграции в ПО ITV\n4. Реле подключается к OUT-GND","1. when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself\n2. for MPEG-4, the ***Rate*** slider changes the bit rate of the video stream; for this reason, when you adjust the frame rate, you adjust the image quality too: it was done like this, because for MPEG-4 the camera itself doe not have a \"pure\" Rate setting\n3. For MPEG-4, the Quality slider does not work - this is how the integration was done in the AxxonSoft software\n4. Connect relays to OUT-GND"]
["Panasonic i-Pro","Panasonic WV-SC385(E)","Camera ","1.05","1","+.",null,"+","+","+.",null,null,"1280x960(MJPEG)/640x480(MPEG-4)/1280x960(H.264)","640x480","320x240","+","+","+",null,"+","+","+",null,"+","+","1. При задействовании на камере H.264 или MPEG-4 на MJPEG-видеопоток накладывается ограничение в 15 fps max\n2. Под значениями PAL и NTSC настройки \"ТВ-стандарт\" в ПО ITV/Axxon понимаются форматы видео 4:3 и 16:9 соответственно\n3. При выборе других ТВ-стандартов кроме PAL в настройках в ПО Axxon будет доступен MPEG-4, хотя фактически на камере он будет заблокирован\n4. При выборе MPEG-4 в настройках в ПО Axxon будет доступно мегапиксельное разрешение, хотя при MPEG-4 фактически камера его не поддерживает\n ","1. If you enable H.264 or MPEG-4 on the camera, the MJPEG video stream is limited to 15 fps max.\n2. In the AxxonSoft software, ***TV standard*** means aspect ratio (PAL for 4:3 and NTSC for 16:9).\n3. If you select any ***TV standard*** other than PAL, the AxxonSoft software shows MPEG-4 as an available option, but the camera itself does not allow this codec. \n4. If you select any MPEG-4, the AxxonSoft software shows a megapixel resolution as an available option, but the camera itself does not allow this resolution for MPEG-4.\n "]
["Panasonic i-Pro","Panasonic WV-SC386(E)","Camera","1.81 ","1","+.",null,"+","+","+",null,null,"from WEB","from WEB","from WEB","+","+","-","-","+","-","-","-","-","+","Набор доступных разрешений в ПО ITV зависит от настройки \"Image Capture mode\" в веб-интерфейсе.","In AxxonSoft products available permissions depends on \"Image Capture mode\" in camera's web interface."]
["Panasonic i-Pro","Panasonic WV-SC386 (ONVIF) ","Camera ","V.1.61","1",null,null,"+",null,"+",null,null,"1280x960 ","640x480","320x240","+",{"$nulls":3},"+",null,null,"+",null,"+"]
["Panasonic i-Pro","Panasonic WV-SC588","Camera","1.08","1","+","3","+",null,"+",null,null,"1280x720","1280x720","640x360","+","+","+","+","+","+","+","-","-","+","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.Набор разрешений зависит от выбранного режима (1.3 MP, 2MP) и соотношения сторон (4:3, 16:9). В ПО Axxon эти настройки реализованы через параметр \"ТВ-стандарт\".","Video transmission (mpeg4/h.264) is implemented via the following protocols: the Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. In Intellect, these protocols correspond to the unicast, tcp, udp, and multicast registry keys, respectively. The set of resolutions depends on which mode (1.3 MP, 2MP) and aspect ratio (4:3, 16:9) are selected.  Axxon software implements these settings with the TV Standard parameter.","improved"]
["Panasonic i-Pro","Panasonic WV-SF132(E)","Camera ","1.03","1","+.",null,"+",null,"+",null,null,"PAL: 640x480, NTSC: 640x360","PAL: 640x480, NTSC: 640x360","PAL: 320x240, NTSC: 640x360","+","+",{"$nulls":6},"other detectors","+","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.Поиск устройств и в AxxonNext/Next и в Интеллект обнаруживает камеру, как неподдерживаемое устройство. Это вина камеры - она присылает некорректные данные.FPS на потоке MJPEG зависит от состояние потоков H264. Если хотя бы один из них включен, FPS с MJPEG не будет превышать 5 кадров в секунду.Чтобы работал встроенный детектор через Onvif необходимо в настройках устройства указать логин и пароль.","Video transmission (mpeg4/h.264) is implemented via the following protocols: the Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP In Intellect, these protocols correspond to the unicast, tcp, udp, and multicast ***Windows Registry keys***, respectively. Both in AN and Intellect, Search detects the camera as an unsupported device. This is the camera's fault: it sends wrong data. For the MJPEG stream, the frame rate very much depends on the status of the H.264 streams If at least one of them is enabled, MPEG video comes with 5 fps matzo make the embedded detector work via the ONVIF protocol, go to the devices settings and enter the login and password"]
["Panasonic i-Pro","Panasonic WV-SF135(E)","Camera ","1.03","1","+.",null,"+",null,"+",null,null,"PAL: 1280x960, NTSC: 1280x720","PAL: 640x480, NTSC: 640x360","PAL: 320x240, NTSC: 640x360","+","+",{"$nulls":6},"+.","+","Поиск устройств и в AxxonNext/Next и в Интеллект обнаруживает камеру, как неподдерживаемое устройство. Это вина камеры - она присылает некорректные данные.FPS на потоке MJPEG зависит от состояние потоков H264. Если хотя бы один из них включен, FPS с MJPEG не будет превышать 5 кадров в секунду.Чтобы работал встроенный детектор через Onvif необходимо в настройках устройства указать логин и пароль.","Both in AN and Intellect, Search detects the camera as an unsupported device. This is the camera's fault: it sends wrong data. For the MJPEG stream, the frame rate very much depends on the status of the H.264 streams If at least one of them is enabled, MPEG video comes with 5 fps matzo make the embedded detector work via the ONVIF protocol, go to the devices settings and enter the login and password"]
["Panasonic i-Pro","Panasonic WV-SF332(E)","Camera ","1.03","1","+.",null,"+",{"$nulls":4},"640x480 (PAL) / 640x360 (NTSC)","640x480 (PAL) / 640x360 (NTSC)","320x240 (PAL) / 640x360 (NTSC)","+","+",{"$nulls":6},"-","+"]
["Panasonic i-Pro","Panasonic WV-SF335(E) / WV-SF336(E) / WV-SF346","Camera","1.61","1","+","3","+","+","+",null,null,"PAL: 1280x960 (H264/MJPEG); 640x480 (MPEG4) / NTSC: 1280x720","PAL: 640x480 / NTSC: 1280x720","PAL: 320x240 / NTSC: 640x360","+","+","+","+","+","+","+","-","other detectors","+","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.Кодеки в потоках 1 и 2 должны совпадать. Одновременно получать с камеры и MPEG4, и H264 нельзя.MPEG4 доступен только в режиме PALДля поиска камеры в сети необходимо предварительно настроить постоянную, не ограниченную по времени видимость камеры. Эта настройка осуществляется через веб-интерфейс камеры.Находится в списке неподдерживаемых устройств (общая проблема камер Panasonic). То есть найти устройство можно, но добавить из результатов поиска в конфигурацию нельзя. Добавлять устройство нужно вручную.Из встроенной аналитики интегрирован детектор лиц.","Video transmission (mpeg4/h.264) is implemented via the following protocols: the Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. In Intellect, these protocols correspond to the unicast, tcp, udp, and multicast Windows registry keys, respectively.\nCodecs for streams 1 and 2 have to be the same. \nYou can not get both MPEG4 and H264 video from this camera at the same time. \nMPEG4 video is available inly in PAL mode.\n To be able to discover the device, set the camera to Permanent Visibility. Do it in the camera's web interface.\nThis is an unsupported device (a problem shared by Panasonic cameras). That is, the search finds the device, but you cannot add the device directly from the search results. You must add it manually.\nOnly embedded Facial Recognition has been integrated.","improved"]
["Panasonic i-Pro","Panasonic WV-SF538","Camera","1.31","1","-",null,"+",null,"+",null,null,"1280x720","1280x720","640x360","+","+","-","-","+","-","-",null,"-","+","На камере присутствует встроенный детектор лиц. ","There is an on-board Face detection tool."]
["Panasonic i-Pro","Panasonic WV-SP105(E)","Camera ","1.46","1","+.",null,"+",null,"+",null,null,"1280x960 (PAL) / 1280x720 (NTSC)","640x480 (PAL) / 1280x720 (NTSC)","320x240 (PAL) / 640x360 (NTSC)","+","+",{"$nulls":6},"-","+","Настройки видео (кодек, разрешение, частота кадров) в потоках взаимозависимы. Следить за их совместимостью пользователь должен самостоятельно.\nНаходится в списке неподдерживаемых устройств (общая проблема камер Panasonic). То есть найти устройство можно, но добавить из результатов поиска в конфигурацию нельзя. Добавлять устройство нужно вручную.Для поиска камеры в сети необходимо предварительно настроить постоянную, не ограниченную по времени видимость камеры. Эта настройка осуществляется через веб-интерфейс камеры.","Video settings (codec, resolutions, picture frequency) are interdependent in flows. User shall itself to track their compatibility.\nIt's in the list of unsupported devices (a common problem of the cameras Panasonic). It's possible to find the device but impossible to add it from search results in a configuration. Add the device manually.\nTo find camera on a network it's necessary to set up beforehand the constant which hasn't been restricted on time visibility of the camera. This setup is carried out via the camera web interface."]
["Panasonic i-Pro","Panasonic WV-SP302(E)","Camera ","1.03","1","+.",null,"+",{"$nulls":4},"-","640x480 (PAL) / 640x360 (NTSC)","320x240 (PAL) / 640x360 (NTSC)","+","+",{"$nulls":6},"-","+"]
["Panasonic i-Pro","Panasonic WV-SP305(E)","Camera ","1.50","1","+.",null,"+","+","+",null,null,"1280x960 (PAL) / 1280x720 (NTSC)","640x480 (PAL) / 1280x720 (NTSC)","320x240 (PAL) / 640x360 (NTSC)","+.","+","+","+.","+","+","+",null,"+.","+","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.\nВ кодеках MPEG4 и H264 при получении видео по протоколу UDP возможны потери пакетов и рывки видео. В таких случаях рекомендуется использовать протокол RTSP over TCP.\nНастройки видео (кодек, разрешение, частота кадров) в потоках взаимозависимы. Следить за их совместимостью пользователь должен самостоятельно.\nКодеки в потоках 1 и 2 должны совпадать. \nОдновременно получать с камеры и MPEG4, и H264 нельзя.\nНаходится в списке неподдерживаемых устройств (общая проблема камер Panasonic). То есть найти устройство можно, но добавить из результатов поиска в конфигурацию нельзя. Добавлять устройство нужно вручную.Для поиска камеры в сети необходимо предварительно настроить постоянную, не ограниченную по времени видимость камеры. Эта настройка осуществляется через веб-интерфейс камеры.\nИз встроенной аналитики в настоящий момент интегрирован детектор лиц, детектор движения не интегрирован. Детектор движения работает через Onvif.\nЗвук из динамика камеры начинает воспроизводиться с задержкой в несколько секунд. ","In MPEG4 and H264 codecs when obtaining video according to the UDP protocol are possible losses of packets and video breakthroughs. In such cases it is recommended to use the RTSP over TCP protocol.\nVideo settings (the codec, permission, picture frequency) for streams are interdependent. To track their compatibility the user shall independently.\nCodecs in streams 1 and 2 shall match. \nIt is impossible to receive from the camera and MPEG4, and H264 at the same time.\nIs in the list of unsupported devices (a common problem of the cameras Panasonic). It is possible to find the device , but impossible to add from search results in a configuration . To add the device it is necessary manually. For camera search on a network it is necessary to set up beforehand the constant which has not been restricted on time visibility of the camera. This setup is carried out via the camera web interface.\nFrom built-in analytics the face detector is integrated at the moment, motion detector isn't integrated. The motion detector works through Onvif.\nThe sound from the speaker of the camera starts to be reproduced with a time delay in some seconds."]
["Panasonic i-Pro","Panasonic WV-SP306(E)","Camera ","1.04","1","+.",null,"+","+","+",null,null,"PAL (4:3): 1280x960 (MJPEG/H264) / 640x480 (MPEG4) | NTSC (16:9): 1280x720 (MJPEG/H264)","PAL (4:3): 640x480 (MJPEG/H264/MPEG4) | NTSC (16:9): 1280x720 (MJPEG/H264)","PAL (4:3): 320x240 (MJPEG/H264/MPEG4) | NTSC (16:9): 640x360 (MJPEG/H264)","+","+","+.","-",null,"+","+",null,"-","+","В камере 3 стримминга, однако 2 из них - неполноценные, у них один кодек на двоих (MPEG4/H264) . Одновременно получать с камеры и MPEG4, и H264 нельзя.В кодеке H264 возможны задержки и \"рывки\" видео. Для поиска камеры в сети необходимо предварительно настроить постоянную, неограниченную видимость камеры. Эта настройка осуществляется через веб-интерфейс камеры.Поиск обнаруживает камеру как неподдерживаемое устройство - особенность камер Panasonic i-Pro.","The cameras has 3 streams; however, two of them are not full-fledged, they share a codec (MPEG4/H.264). You cannot get MPEG4 and H.264 streams from the camera at the same time. With H.264, sometimes video stops for a while, then starts again. To be able to search for the device, set the camera to ***permanent visibility***. Do it in the camera's web interface. Search detects the camera as unsupported device - this is a limitation of Panasonic i-Pro cameras."]
["Panasonic i-Pro","Panasonic WV-SP509(E) / WV-SF539(E) / WV-SW559(E) / WV-SP508 / WV-SF549 / WV-SF548 / WV-SW558","Camera","1.30","1","+","3","+",null,"+",null,null,"from WEB","from WEB","from WEB","+","+","+","+","+","+","+",null,"-","+","Набор доступных разрешений в ПО ITV зависит от настройки \"Image Capture mode\" в веб-интерфейсеНа камере есть 3 программируемых IO-порта. 1й и 3й используются в нашем ПО как лучи, 2й - как реле.Для работы с MJPEG по ONVIF нужно включить в веб-интерфейсе поток H.264, а затем выключить его","1. In AxxonSoft software, the choice of resolutions depends on Image Capture Mode settings in the camera's web interface.\n2. The camera has 3 programmable I/O ports. Our software uses ports 1 and 3 for sensors and port 2 for relays.\n3. To work with MJPEG via ONVIF enable H.264 in the camera's web interface and then disable it.","improved"]
["Panasonic i-Pro","Panasonic WV-SW152(E)/-M(E)","Camera ","1.03","1","+.",null,"+",null,"+",null,null,"PAL: 800x600 NTSC: 640x360","PAL: 640x480 NTSC: 640x360","PAL: 320x240 NTSC: 640x360","+","+",{"$nulls":6},"+.","+","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.Поиск устройств и в AxxonNext/Next и в Интеллект обнаруживает камеру, как неподдерживаемое устройство. Это вина камеры - она присылает некорректные данные.FPS на потоке MJPEG зависит от состояние потоков H264. Если хотя бы один из них включен, FPS с MJPEG не будет превышать 5 кадров в секунду.Чтобы работал встроенный детектор через Onvif, необходимо в настройках устройства указать логин и пароль.","Video transmission (mpeg4/h.264) is implemented via the following protocols: the Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP In Intellect, these protocols correspond to the unicast, tcp, udp, and multicast ***Windows Registry keys***, respectively. Both in AN and Intellect, Search detects the camera as an unsupported device. This is the camera's fault: it sends wrong data. For the MJPEG stream, the frame rate very much depends on the status of the H.264 streams If at least one of them is enabled, MPEG video comes with 5 fps matzo make the embedded detector work via the ONVIF protocol, go to the devices settings and enter the login and password"]
["Panasonic i-Pro","Panasonic WV-SW155(E)/-M(E)","Camera ","1.03","1","+.",null,"+",null,"+",null,null,"PAL: 1280x960 NTSC: 1280x720","PAL: 640x480 NTSC: 640x360","PAL: 320x240 NTSC: 640x360","+","+",{"$nulls":6},"+.","+","Поиск устройств и в AxxonNext/Next и в Интеллект обнаруживает камеру, как неподдерживаемое устройство. Это вина камеры - она присылает некорректные данные.FPS на потоке MJPEG зависит от состояние потоков H264. Если хотя бы один из них включен, FPS с MJPEG не будет превышать 5 кадров в секунду.Чтобы работал встроенный детектор через Onvif, необходимо в настройках устройства указать логин и пароль.","Both in AN and Intellect, Search detects the camera as an unsupported device. This is the camera's fault: it sends wrong data. For the MJPEG stream, the frame rate very much depends on the status of the H.264 streams If at least one of them is enabled, MPEG video comes with 5 fps matzo make the embedded detector work via the ONVIF protocol, go to the devices settings and enter the login and password"]
["Panasonic i-Pro","Panasonic WV-SW158 / WV-SF138","Camera","1.05","1","+.",null,"+","-","+",null,null,"from WEB","from WEB","from WEB","-","+","+","-","-","-","-","-","-","+"]
["Panasonic i-Pro","Panasonic WV-SW316(E)/L(E)","Camera ","1.61","1","+.",null,"+","-","+",null,null,"1280x720(NTSC)/1280x960(PAL)","1280x720(NTSC)/640x480(PAL)","640x360(NTSC)/320x240(PAL)","+","+","+","+.","+","+","+",null,"other detectors","+","1. Для включения реле через ONVIF необходимо настроить Alarm Terminal 3 в режим AUX output\n2. Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.\n3. Кодеки в потоках 1 и 2 должны совпадать. Одновременно получать с камеры и MPEG4, и H264 нельзя.\n4. MPEG4 доступен только в режиме PAL\n5. Для поиска камеры в сети необходимо предварительно настроить постоянную, не ограниченную по времени видимость камеры. Эта настройка осуществляется через веб-интерфейс камеры.\n6. Находится в списке неопределяемых устройств (общая проблема камер Panasonic). То есть найти устройство можно, но добавить из результатов поиска в конфигурацию нельзя. Добавлять устройство нужно вручную.\n7. Из встроенной аналитики интегрирован детектор лиц.","1. To connect the relay through ONVIF, set up Alarm Terminal 3 to AUX output\n2. Video transmission (mpeg4/h.264) is implemented via the following protocols: the Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP In Intellect, these protocols correspond to the unicast, tcp, udp, and multicast Windows registry keys, respectively.\n3. Codecs for streams 1 and 2 have to be the same. You can not get both MPEG4 and H264 video from this camera at the same time.\n4. MPEG4 video is available inly in PAL mode\n5. To be able to discover the device, set the camera to Permanent Visibility. Do it in the camera's web interface.\n6. This is an unsupported device (a problem shared by Panasonic cameras). That is, the search finds the device, but you cannot add the device directly from the search results. You must add it manually.\n7. Only embedded Facial Recognition has been integrated."]
["Panasonic i-Pro","Panasonic WV-SW316L (ONVIF) ","Camera ","1.66 ","1",null,null,"+",null,"+",null,null,"1280x960","640x480","320x240 ","+",null,"+","+",null,null,"+","+",null,"+","По ONVIF не работает кодек MPEG4 (особенность устройства).","Via the ONVIF protocol, the MPEG4 codec does not work."]
["Panasonic i-Pro","Panasonic WV-SW355(E)","Camera ","1.49","1","+.",null,"+","+","+",null,null,"1280x960 (PAL) / 1280x720 (NTSC)","640x480 (PAL) / 1280x720 (NTSC)","320x240 (PAL) / 640x360 (NTSC)","+.","+","+","+.","+","+","+",null,"+.","+","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.\nВ кодеках MPEG4 и H264 при получении видео по протоколу UDP возможны потери пакетов и рывки видео. В таких случаях рекомендуется использовать протокол RTSP over TCP.\nНастройки видео (кодек, разрешение, частота кадров) в потоках взаимозависимы. Следить за их совместимостью пользователь должен самостоятельно.\nКодеки в потоках 1 и 2 должны совпадать. Одновременно получать с камеры и MPEG4, и H264 нельзя.\nНаходится в списке неподдерживаемых устройств (общая проблема камер Panasonic). То есть найти устройство можно, но добавить из результатов поиска в конфигурацию нельзя. Добавлять устройство нужно вручную.\nИз встроенной аналитики в настоящий момент интегрирован детектор лиц, детектор движения не интегрирован. Детектор движения работает через Onvif.\nЗвук из динамика камеры начинает воспроизводиться с задержкой в несколько секунд. ","In MPEG4 and H264 codecs when obtaining video according to the UDP protocol are possible losses of packets and video breakthroughs. In such cases it is recommended to use the RTSP over TCP protocol.\nVideo settings (the codec, permission, picture frequency) for streams are interdependent. To track their compatibility the user shall independently.\nCodecs in streams 1 and 2 shall match. \nIt is impossible to receive from the camera and MPEG4, and H264 at the same time.\nIs in the list of unsupported devices (a common problem of the cameras Panasonic). It is possible to find the device , but impossible to add from search results in a configuration . To add the device it is necessary manually. For camera search on a network it is necessary to set up beforehand the constant which has not been restricted on time visibility of the camera. This setup is carried out via the camera web interface.\nFrom built-in analytics the face detector is integrated at the moment, motion detector isn't integrated. The motion detector works through Onvif.\nThe sound from the speaker of the camera starts to be reproduced with a time delay in some seconds."]
["Panasonic i-Pro","Panasonic WV-SW396(E) / WV-SW395(E) / WV-SW396A / WV-SW395A","Camera","1.44","1","+","3","+","+","+",null,null,"PAL (4:3, 3MP): 1280x960 (MJPEG, H264) / --- (MPEG4) | NTSC (16:9, 3MP): 1280x720 (MJPEG, H264) / --- (MPEG4)","PAL (4:3, 3MP): 640x480 (MJPEG, H264, MPEG4) | NTSC (16:9, 3MP): 1280x720 (MJPEG, H264) / --- (MPEG4)","PAL (4:3, 3MP): 320x240 (MJPEG, H264, MPEG4) | NTSC (16:9, 3MP): 640x360 (MJPEG, H264) / --- (MPEG4)","+","+","+","-","+","+","+","-","-","+","Если включен один из потоков H264/MPEG4, на первом потоке (MJPEG) действует ограничение в 5 fps.","If one of the H.264/MPEG4 streams are enabled, the frame rate for the first stream (MJPEG) is 5 fps max. ","improved"]
["Panasonic i-Pro","Panasonic WV-SW458(M) / WV-SF438","Fisheye Camera","1.04","1","+",3,"+","-","+","-","-","from WEB","from WEB","from WEB","+","+","-","-","+","+","+","+","others","+","Набор доступных разрешений в ПО ITV зависит от настройки \"Image Capture mode\" в веб-интерфейсеНа камере есть встроенный детектор лиц","In AxxonSoft products available resolutions depend on the Image Capture mode setting in camera web interface. The camera has an on-board Face detection tool."]
["Panasonic i-Pro","Panasonic WV-SW598","Camera ","0.0A","1","+.",null,"+",null,"+",null,null,"from WEB","from WEB","from WEB","+","+",null,null,"+",{"$nulls":4},"+","Набор доступных разрешений в ПО ITV зависит от настройки \"Image Capture mode\" в веб-интерфейсе.","The set of available resolution in Axxon software depends on the \"Image Capture mode\" setting in the web interface."]
["Partizan","Partizan ADF-14S DVR","DVR","1.0.0. build 22","4",{"$nulls":4},"+",null,null,"704x480","704x480","352x240","+.",null,"-","-","-",null,null,"+.","-","-"]
["Partizan","Partizan DVR ADH-18V","DVR","1.0.0 build 32","8",{"$nulls":4},"+",null,null,"704x576","-","352x288","-",null,"+","-","-","-","-","+.","-","-"]
["Pelco","Pelco IDE20DN","Camera ","1.7.8.9111-O3.5288","1","+.",null,"+",null,"+",null,null,"1600x1200","1280x960","640x480","+",null,"-","-",null,"+","+",null,"-","+","Изменение настроек принимается камерой достаточно долго (~1 мин.)Настройки сильно зависят друг от друга. Параметры \"битрейт\", \"интервал включения ключевых кадров\", \"fps\", \"разрешение\" все взаимозависимые: при изменении одного меняются значения всех остальных.В ПО Axxon все настройки установлены от минимального до максимального значения. Поэтому иногда могут возникать несоответствия между настройками в ПО и реальными параметрами видеопотока - особенность интеграции.В Интеллекте в зависимости от выбранных параметров некоторые значения других настроек могут оказаться недоступны. В частности, при максимальной частоте кадров будет недоступна смена разрешений. При необходимости можно настраивать поток в веб-интерфейсе и получать видео в Интеллекте.","The camera takes quite a lot of time to apply changes to video settings (1 minute).The settings depends on each other very much. The Bit Rate, Keyframes Interval, Frame Rate, and Resolution parameters all depends on each other: if you change one of them, all the others change too. In the AxxonSoft software, ***for each parameter, you can set any value, from min. to max [This is how I understand the original sentence, but I am not 100% sure]***. For this reason, sometimes you may get a mismatch between the software's settings and the actual parameters of the video stream - this is how the integration was done. In Intellect, depending on the selected values, some values for some settings are not available. For example, if you select the max. frame rate, then you cannot switch resolutions. If needed, you can configure the stream in the web interface and use Intellect to view video. "]
["Pelco","Pelco IEE20DN","Camera ","1.7.8.8111-03.5288","1","+.",null,"+",null,"+",null,null,"1600x1200","1280x960","640x480","+",{"$nulls":7},"-","+"]
["Pelco","Pelco IL10","Camera ","1.8.2.4.8310-O3.9119","1","+.",{"$nulls":3},"+",null,null,"1280x720 ","1280x720 ","640x352","+",{"$nulls":8},"+"]
["Pelco","Pelco IX10 / ID10 / IE10 / IM10 ","Camera ","1.8.2.11.9080","1","+.",null,"+",null,"+",null,null,"1280x1024","1280x960","640x480","+.",{"$nulls":7},"-","+","На камере есть зависимости между разрешением, частотой кадров и битрейтом. Нужно отслеживать зависимости в веб-интерфейсе.","The camera has a few joint settings for resolution, frame rate and bit rate. Check the dependent settings in the web interface."]
["Pelco","Pelco IX30 / ID30 / IE30","Camera ","1.8.2.11.9080","1","+.",null,"+",null,"+",null,null,"2048x1536","1280x960","640x480","+",{"$nulls":7},"-","+"]
["Pelco","Pelco IXE20 / IDE20 / IEE20 ","Camera ","1.8.2.11.9081","1","+.",null,"+",null,"+",null,null,"1600x1200","1280x960","640x480","+",null,null,"-",{"$nulls":4},"-","+","1. Видео в ПО ITV/Axxon можно получать либо только с первого потока, либо одновременно с первого и второго. Получать видео только со второго потока - невозможно, это особенность камеры.\n2. Набор доступных настроек видеопотока (кодек, разрешение, фпс, битрейт) сильно взаимозависим.","1. In the AxxonSoft products, video is available either from stream 1 only, or from stream 1 & 2 at the same time. You cannot get video stream 2 only.\n2. The camera has a few pretty rigid settings for resolution, frame rate, codec and bit rate."]
["Pelco","Pelco Sarix IM10C10","Camera ","1.7.41.9261-O2.6725","1","+.",null,"-",null,"+",null,null,"1280x1024","1280x960","640x480","+.",{"$nulls":7},"-","+","1. В ПО ITV нет возможности получать видео только со второго потока. Можно либо только с первого, либо одновременно с обоих потоков.","1. In the AxxonSoft software, you cannot receive video from stream 2 only. Either you get stream 1 or both stream 1 and 2.\n"]
["Pelco","Pelco Sarix IMS0C10-1","Camera ","1.7.8.9260-O2.5288","1","+.",null,"+","+","+",null,null,"800x600","704x480","352x240","+",null,"-","-",{"$nulls":4},"-","+","Изменение настроек принимается камерой достаточно долго (~1 мин.)Настройки сильно зависят друг от друга. Параметры \"битрейт\", \"интервал включения ключевых кадров\", \"fps\", \"разрешение\" все взаимозависимые: при изменении одного меняются значения всех остальных.  В ПО Axxon все настройки установлены от минимального до максимального значения. Поэтому иногда могут возникать несоответствия между настройками в ПО и реальными параметрами видеопотока - особенность интеграции.","The camera takes quite a lot of time to apply changes to video settings (1 minute).The settings depends on each other very much. The Bit Rate, Keyframes Interval, Frame Rate, and Resolution parameters all depends on each other: if you change one of them, all the others change too.  In the AxxonSoft software, ***for each parameter, you can set any value, from min. to max [This is how I understand the original sentence, but I am not 100% sure]***. For this reason, sometimes you may get a mismatch between the software's settings and the actual parameters of the video stream - this is how the integration was done."]
["Pelco","Pelco Spectra 1080P (S5230)","Camera ","1.9.2.1-20130620-1.9330-A1.9822","1","+.",null,"+",null,"+",null,null,"1920x1080","800x448","480x272","+",{"$nulls":3},"+",{"$nulls":4},"+","Параметры \"битрейт\", \"интервал включения опорных кадров\", \"fps\", \"разрешение\" все взаимозависимые: при изменении одного меняется список доступных значений всех остальных. Набор доступных в текущей конфигурации значений этих настроек можно посмотреть в веб-интерфейсе.","Parameters \"bit rate\", \"reference frames range\", \"fps\", \"resolution\" are all interdependent: when you change the list of available values ​​change all the rest. The available values ​​of current configuration can be found in the web interface."]
["Pelco","Pelco Spectra HD 720p (D5118)","Camera ","1.8.2.11-20120623-1.9310-A1.8120","1","+.",null,"+",null,"+",null,null,"1280x960","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":4},"+","В Интеллекте не применяется максимальное значение FPS. В ПО ITV/Axxon камера интегрирована как D5118 ","1. In AxxonSoft Intellect, you cannot get the max. fps. 2. Camera has been integrated as D5118 in Axxon software."]
["Pelco","Pelco Spectra IV IP (MPEG4)","Camera ","01.00.0015","1",null,null,"+","+",{"$nulls":3},"704x576","704x576","704х576(MJPEG)/352х288(MPEG-4)","+",{"$nulls":3},"+",{"$nulls":4},"-","1. При MJPEG камера поддерживает только 704х576 разрешение. Соответственно в Intellect будет Стандартное\"=\"Высокое\"=\"Полное\"=704 x 576\n\n","1. For MJPEG, the camera support only the 704x576 resolution. For this reason, in Intellect, you have Standard = High = Full= 704 x 576. \n\n"]
["Pelco","Pelco Spectra IV / Exsite IP (TXB-N) ","Camera ","1.8.2.11-20120623-1.2084-O1.8120","1","+.",null,"+","+","+",null,null,"704x480","704x480","352x240","+.",null,"+","-","+","+","-",null,null,"+","1. Во втором потоке в разрешении 704x576 частота кадров ограничена: не более 12.5 fps для MJPEG, не более 5 fps для MPEG4/H264.\n2. В ПО ITV нет возможности получать видео только со второго потока. Можно либо только с первого, либо одновременно с обоих потоков. \n3. При добавлении устройства всегда создаются 7 лучей. Все 7 лучей поддерживает модель SD4E35. \nУ модели SD4E23 работает только 1 луч\n4. Настройки видеопотока в продуктах работают только при правильно указанном ТВ-стандарте 5. Для включения/выключения дворника необходимо перейти на пресет №86. Для повторной активации пресета необходимо перейти сначала на любой другой пресет, а затем снова на пресет №86.\n6. Максимальное количество пресетов на камере - 80.","1. For the second stream, if you select the 704x576 resolution, the frame rate is limited: max. 12.5 fps for MJPEG and max. 5 fps for MPEG4/H264.\n2. In the Axxonsoft software, you cannot receive video from stream 2 only. Either you get stream 1 or both stream 1 and 2 at the same time. \n3. When you add the camera, 7 sensors are created. All 7 sensors are supported by SD4E35. \nThe SD4E23 supports only 1 sensor.\n4. Video parameters can be applied only if you select the right TV standard. 5. To turn on/off \"Wash and Wipe\", please go to the preset number 86. To repeat the action, please go to any other preset, and then again to the preset number 86.\n6. The maximum number of presets on the camera is 80."]
["Pelco","Pelco TI3","Thermal Imaging Camera","1.8.2.13-20120816-1.9441-O4.8287","1","+.",null,"+",null,"+",null,null,"384x288","384x288","320x240 ","-",{"$nulls":7},"-","+"]
["Pinetron","Pinetron PDR-X7008","DVR","X7K-APP-1.0.3.6","8",{"$nulls":4},"+",null,null,"704x576","704x288","352x288","-",null,"-","-","-","-","-",null,null,"+","Разрешение изменяется только через веб-интерфейс (Установки->Запись)","Resolution changes only via the web interface (Installations-> Record)"]
["Pinetron","Pinetron PDR-XM3104","DVR","XM314-APP-B090910.1880","4",{"$nulls":4},"+.",null,null,"-","720х288","352x288","+.",null,"-","-","-","-","-","-","-","+","1. Параметры живого потока зависят от настроек потока на запись.\n2. Разрешение изменяется только через веб-интерфейс (Установки->Система) 3. Для корректного отображения видео в ПО ITV необходимо в реестре в папке HKLM/SOFTWARE/ITV/INTELLECT/Video создать ключ MonitorFrameBuffer (строковый параметр) и придать ему значение 5. ","1. Parameters of a live stream depend on settings of a stream for record. \n2. Resolution changes only via the web interface (Installations-> System)"]
["PixEYE","PixEYE MEGA","Camera ","1.4.99","1",null,null,"+",{"$nulls":4},"1600x1200","852x480","320x240","+.",{"$nulls":8},"+","При смене разрешения возможны кратковременные искажения видеопотока - особенность устройства.","When you switch resolutions, video may get distorted for some time - this is a limitation of the device itself. "]
["PixEYE","PixEYE SD1","Camera ","1.4.99","1",null,null,"+",{"$nulls":4},"720x576","640x480","320x240","+",{"$nulls":7},"-","+","1) данная камера - аналог камеры PixEYE Mega, отличается от неё только отсутствием мегапиксельных разрешений","1) this camera is very similar to the PixEYE Mega camera; the only difference is that this camera does not megapixel resolutions."]
["Planet","Planet ICA-350","Camera ","3.0.2.2457","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"-","-",{"$nulls":4},"-","+"]
["Planet","Planet ICA-HM230","Camera ","5.0.1.3576","1",null,null,"+","+","+",null,null,"1280x1024(MJPEG/H.264)/640x480(MPEG-4)","640x480","320x240","+",null,"+","-","+",{"$nulls":3},"-","+"]
["Planet","Planet ICA-M230","Camera ","3.0.2.3083","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240(MJPEG)/640x480(MPEG-4)","+",null,"+","-","+",{"$nulls":3},"-","+"]
["Probe","Probe PIC-H1300","Camera ","v1.0.0_20110523","1",null,null,"+","+.","+",null,null,"1280x720","720x480","352x240","+",null,null,"-",{"$nulls":4},"-","-"]
["Probe","Probe PIC-H1310T","Camera ","v0.0.1_20110909","1",null,null,"+",null,"+.",null,null,"H264: 1280x720; MJPEG: 720x576","720x576","352x288","+",null,"+","-",null,"+","+",null,"+","-","На камере перепутаны микрофон и динамик: микрофон надо подключать к разъему с надписью audio out, а динамик - к audio in.","On the camera the microphone and the loudspeaker are entangled: the microphone is to be connected to the socket with audio out inscription, and the loudspeaker - to audio in."]
["Probe","Probe PIC-H2000T","Camera ","v1.0.4_20120717","1",null,null,"+","+","+",null,null,"H.264: 1920x1080; MJPEG / MPEG4: 1280x720","H.264: 1280x720; MJPEG / MPEG4: 720x576","352x288","+",{"$nulls":7},"motion detection","-"]
["Probe","Probe PID-H1000","Camera ","v1.0.1_20110823","1",null,null,"+","+","+",null,null,"1280x720","720x576","352x288","+",null,"+","+",null,"+","+",null,"+","-","1. Для второго потока (MJPEG) при максимальном разрешении (1280x720) максимальный fps составляет 20 кадров в секунду.\n2. \"На размыкание\" луч срабатывает с задержкой в 5-6 секунд - это особенность камеры.","1. The max. fps for stream 2(MJPEG) at max. resolution 1280x720) is 20.\n2. The normally-closed Alarm Input work with a delay (around 5-6 seconds), this is the limitation of the camera.\n"]
["Probe","Probe PIN-H2000","Camera ","1.0.4","1",null,null,"+","+","+",null,null,"1920x1080(H264) / 1280x720(MJPEG/MPEG4)","1280x720(H264) / 720x576(MJPEG/MPEG4)","352x288","+",{"$nulls":8},"-"]
["Probe","Probe PMI-400","Camera ","0.10.27_20110819","1",null,null,"+","+","+",null,null,"704x480","704x480","320x240","+",null,null,"-","+",{"$nulls":3},"-","-"]
["Probe","Probe PMI-H2000","Camera ","1.1.0_20130305","1",null,null,"+","+","+",null,null,"1920x1080(H.264) / 1280x720(MJPEG, MPEG-4)","1280x720(H264) / 740x480(MJPEG, MPEG-4)","352x240","-",null,"+","+","+","+","+",null,"motion detection","-","С прошивкой 1.1.0_20130305 камера интегрирована как N1P1-S10H2N_TF01\nС разрешением 1920х1080 максимальный fps составляет 15 кадров в секунду\nДопустимые диапазоны настроек на том или ином стримминге зависят от текущей конфигурации других стриммингов, зависимость необходимо отслеживать через веб-интерфейс. \n ","1. With firmware 1.1.0_20130305 camera integrated as N1P1-S10H2N_TF01\n2. Max fps with max resolution 1920x1080 is 15 fps.\n3. Valid ranges of settings for a particular strimming depend on current configuration of other streams, this relationship should be monitored via web-interface."]
["Probe","Probe PTI-503","Camera ","v0.10.15_20110221","1",null,null,"+","+.","+",null,null,"704x576","704x576","352x288","+",null,null,"-","+",{"$nulls":3},"-","-"]
["QNAP","QNAP VS-12164U-RP Pro / VS-12164U-RP Pro+","NVR","4.0.2","64",null,null,"+","+","+",null,null,"from WEB","from WEB","from WEB",null,null,"+",null,"+",null,null,"+",null,"+","1. Все настройки видеопотока и видеоизображения настраиваются из веб-интерфейса NVR (ограниченный ряд настроек), а также из веб-интерфейса устройств, подключенных к NVR\n2. Через ПО ITV нельзя узнать, что за устройства подключены к NVR\n3. К NVR можно подключить устройства, которые есть у него в списке доступных.","1. All stream settings, however with limitations, are available in the NVR web interface as well as from the web interface of the devices connected to the NVR.\n2. In AxxonSoft software, you can not see what devices are connected to the NVR.\n3. You can connect to the NVR only compatible equipment."]
["QNAP","QNAP VS-xx12Pro / VS-4012U-RP Pro / VS-2112Pro+ / VS-4112Pro+ / VS-4112U-RP Pro+ / VS-6112Pro+ ","NVR","4.0.0","12",null,null,"+","+","+",null,null,"from WEB","from WEB","from WEB",null,null,"+.","-","+",null,null,"+","-","+","1. Обозначение модели - xx может принимать значения: 20,21,40,41,60,61\n2. Все настройки видеопотока и видеоизображения настраиваются из веб-интерфейса NVR (ограниченный ряд настроек), а также из веб-интерфейса устройств, подключенных к NVR\n3. Через наше ПО нельзя узнать, что за устройства подключены к NVR\n4. К NVR можно подключить устройства, которые есть у него в списке доступных.","1. The model number - xx and currently is: 20,21,40,41,60,61\n2. All stream settings are available in the NVR web interface as well as from the web interface of the devices connected to the NVR.\n3. In the AxxonSoft products, you can not see what devices are connected to the NVR.\n4. You can connect to the NVR only compatible equipment."]
["QNAP","QNAP VS-xx16Pro / VS-4016U-RP Pro / VS-4116Pro+ / VS-4116U-RP Pro+ / VS-6116Pro+","NVR","3.6.0","16",null,null,"+","+","+",null,null,"from WEB","from WEB","from WEB",null,null,"+.","-","+",null,null,"+","-","+","1. Обозначение модели - xx может принимать значения: 40,41,61\n2. Все настройки видеопотока и видеоизображения настраиваются из веб-интерфейса NVR (ограниченный ряд настроек), а также из веб-интерфейса устройств, подключенных к NVR\n3. Через наше ПО нельзя узнать, что за устройства подключены к NVR\n4. К NVR можно подключить устройства, которые есть у него в списке доступных.","1. The model number - xx and currently is: 40,41,61\n2. All stream settings are available in the NVR web interface as well as from the web interface of the devices connected to the NVR.\n3. In the AxxonSoft products, you can not see what devices are connected to the NVR.\n4. You can connect to the NVR only compatible equipment."]
["RIVA","RIVA RC2102HD-5511","Camera ","1.4.0.12","1",null,null,"+",null,"+",null,null,"1920x1080","800x450","480x270","+",{"$nulls":8},"+"]
["RIVA","RIVA RC3302HD-5344 / RC3702HD-5314","Camera ","1.4.0.12","1",null,null,"+",null,"+",null,null,"1920x1080","800x450","480x270 ","+",{"$nulls":8},"+","Видеопотоки и встроенные детекторы зависят от ресурсов камеры. В зависимости от конфигурации видеопотока используется определенное количество ресурсов (отображается в вебе, в настройках видеопотока). Включенная VCA аналитика съедает 50% ресурсов. ","Video streams and on-board detection tools depend on camera resources. Different amounts of camera resources are used by different video stream configurations (shown in the camera web interface, in the video stream settings). VCA analytics consume 50% of resources when enabled. "]
["RIVA","RIVA RC3502HD-5311 / RC3502HD-5311IR","Camera","1.5.0.12","1",null,null,"+","-","+","-","-","1920x1080","960x540","480x270","+","-","-","-","-","-","-","-","-","+","На камере присутствует видеоаналитика VCA. Видеопотоки и встроенные детекторы зависят от ресурсов камеры. В зависимости от конфигурации видеопотока используется определенное количество ресурсов (отображается в вебе, в настройках видеопотока). Включенная VCA аналитика отнимает 50% ресурсов.","Camera has VCA video analytics. Video streams and on-board detection tools depend on camera resources. Different amounts of camera resources are used by different video stream configurations (shown in the camera web interface, in the video stream settings). VCA analytics consume 50% of resources when enabled."]
["RIVA","RIVA RC5500","Camera ","1.06.05","1",null,null,"+","+","+",null,null,"720x576 (PAL) / 720x480 (NTSC)","640x576 (PAL) / 640x480 (NTSC)","320x288 (PAL) / 320x240 (NTSC)","+",null,"+.","+","+","+","+",null,null,"+","В MJPEG максимальная частота кадров - 5 fps.\nНастройки для аудиовыхода и аудиовхода должны быть одинаковыми.\nЛуч приходит в положение готовности спустя 10-50 секунд после включения в нашем ПО. В дальнейшем замыкание/размыкание луча отрабатывается без задержек.\nАудио-выход камеры воспроизводит звук с задержкой в 5 секунд - проблема камеры.\nЧтобы заработал звук, нужно выставить максимальный уровень громкости на динамике. ","Max frame rate for MJPEG codec is 5 fps.\nSettings for Audio Input and Audio Output should be the same.\nAlarm In comes to a standby position after 10-50 seconds after applying in ITV | AxxonSoft software. Later, closing / opening of Alarm In works without delay.\nAudio Output plays the sound with 5 seconds delay - it's camera's feature."]
["RIVA","RIVA RC6602HD-5311 ","Camera ","1.4.0.11 ","1",null,null,"+",null,"+",null,null,"1920x1080 ","800x450","480x270 ","+",{"$nulls":8},"+","Видеопотоки и встроенные детекторы зависят от ресурсов камеры. В зависимости от конфигурации видеопотока используется определенное количество ресурсов (отображается в вебе, в настройках видеопотока). Включенная VCA аналитика съедает 50% ресурсов. ","Video streams and on-board detection tools depend on camera resources. Different amounts of camera resources are used by different video stream configurations (shown in the camera web interface, in the video stream settings). VCA analytics consume 50% of resources when enabled."]
["RIVA","RIVA RC6802HD-6211","Camera","1.5.0.12","1",null,null,"+","-","+","-","-","1920x1080","960x540","480x270","+","-","-","-","-","-","-","-","motion detection","+","На камере присутствует видеоаналитика VCA. Видеопотоки и встроенные детекторы зависят от ресурсов камеры. В зависимости от конфигурации видеопотока используется определенное количество ресурсов (отображается в вебе, в настройках видеопотока). Включенная VCA аналитика отнимает 50% ресурсов.","Camera has VCA video analytics. Video streams and on-board detection tools depend on camera resources. Different amounts of camera resources are used by different video stream configurations (shown in the camera web interface, in the video stream settings). VCA analytics consume 50% of resources when enabled."]
["RIVA","RIVA RE1000 / RE110","Encoder ","1.7.0","1",null,null,"+","+","+",null,null,"720x576 (PAL) / 720x480 (NTSC)","640x576 (PAL) / 640x480 (NTSC)","320x288 (PAL) / 320х240 (NTSC)","+",{"$nulls":3},"+",{"$nulls":4},"+","Значение параметра \"ТВ-сандарт\" в нашем ПО нужно выбирать в соответствии с реальным ТВ-стандартом видеосигнала, подаваемого на устройство.","In our software, select the value of the ***TV standard*** parameter so that it corresponds to the actual ***TV standard*** of the device's input video signal. "]
["RIVA","RIVA RE4000","Encoder ","1.7.0","4",null,null,"+","+","+",null,null,"720x576 (PAL) / 720x480 (NTSC)","640x576 (PAL) / 640x480 (NTSC)","320x288 (PAL) / 320х240 (NTSC)","+",{"$nulls":3},"+",{"$nulls":4},"+","Устройство представляет собой 4-канальный видеосервер. Однако каждый канал имеет отдельный ip-адрес. Поэтому в нашем ПО каждому каналу сервера соответствует независимое ip-устройство. То есть для получения видео со всех 4-х каналов нужно создать 4 устройства \"RIVA RE4000\".При этом управление внешним поворотным устройством поддерживает только первый канал видеосервера.Значение параметра \"ТВ-сандарт\" в нашем ПО нужно выбирать в соответствии с реальным ТВ-стандартом видеосигнала, подаваемого на устройство.","This device is a 4-channel video encoder. However, each channel has its own IP address. For this reason, in our software, each channel corresponds to a separate IP device. That is, to receive video from all 4 channels, you must create 4 RIVA RE4000 devices. Only the first channel supports pan/tilt drives. In our software, select the value of the ***TV standard*** parameter so that it corresponds to the actual ***TV standard*** of the device's input video signal."]
["RVi","RVi R16LB-PRO","DVR","2.610.0000.0 2012-07-25","16",null,null,"+","-","+",null,null,"704x576","352х576","352x288","-",null,"+","-","-","+","-","-","-","+","Луч работает следующим образом: При его замыкании на устройстве включается таймер, по завершению которого луч автоматически размыкается. Пока таймер включен, повторно луч сработать не может. Время таймера настраивается в веб-интерфейсе устройства в интервале 5-600 сек.Диапазон битрейта на камере зависит от комбинации кодека, разрешения и значения fps. В ПО Axxon для каждого потока прописаны максимальные диапазоны.","Sensor works as follows: when it is closed, the timer on the device is activated, after timer stopped, sensor is automatically opened. While the timer is active, sensor doesn not work. The timer is configured in the web interface  in  range of 5-600 seconds. Bit rate range depends on combination of codec, resolution, an ​​fps. value. In the AxxonSoft products for each stream maximum flow ranges are prescribed."]
["RVi","RVi-HR16/4","DVR","2.610.0000.0 Build 2013-4-12","16",{"$nulls":4},"+",null,null,"704x576","352х576","352х288","+",null,"+","-","+.","+","+","-","-","+"]
["Samsung electronics","Samsung SNC-B2315","Camera ","2.10_090521","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","640x480","+.",null,"+","-",null,"+","+",null,"-","+"]
["Samsung electronics","Samsung SNC-B2331P","Camera ","v1.00-090910","1",null,null,"+","+","+",null,null,"704x576","640x480","640x480","+",{"$nulls":4},"+.","+",null,"-","+"]
["Samsung electronics","Samsung SNC-B2335P","Camera ","1.10_100129","1",null,null,"+","+","+",null,null,"704x576","640x480","352x288","+",null,"+","-",null,"+","+",null,"-","+","1. Камера может выдавать два независимых видеопотока с различыми настройками. Для этого в ПО ITV создаются два граббера и настраиваются они независимо друг от друга.","1. The camera supports two independent video streams, with different settings. For this, create 2 grabbers in Intellect and configure the grabbers independently. "]
["Samsung electronics","Samsung SNC-B5368P","Camera ","v1.00-090910","1",null,null,"+","+","+",null,null,"704x576","640x480","640x480","+",{"$nulls":4},"+","+",null,"-","+"]
["Samsung electronics","Samsung SNC-B5395P","Camera ","v2.10_090521","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","640x480","+.",null,"+","-",null,"+","+",null,"-","+"]
["Samsung electronics","Samsung SNC-B5399P","Camera ","1.10_100129","1",null,null,"+","+","+",null,null,"704x576","640x480","352x288","+",null,"+","-",null,"+","+",null,"-","+","1. Камера может выдавать два независимых видеопотока с различыми настройками. Для этого в ПО ITV создаются два граббера и настраиваются они независимо друг от друга.","1. The camera supports two independent video streams, with different settings. For this, create 2 grabbers in Intellect and configure the grabbers independently."]
["Samsung electronics","Samsung SNC-C6225P","Camera ","1.01","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","352x288","+",null,null,"-","+","+","+",null,"-","+","Звук остался непроверенным (микрофон подключается через спецразьем, которого у нас нет).Тревога по замкнутому лучу поступает с перебоями.","We did not manage to test audio (the microphone connects via a special connector, which we do not have).When you close the sensor, it does send alarms, but not always."]
["Samsung electronics","Samsung SNC-C7225P","Camera ","1.01","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","352x288","+",null,null,"-","+","+","+",null,"-","+","1. Звук остался непроверенным (микрофон подключается через спецразьем, которого у нас нет)","1. We did not manage to test audio (the microphone connects via a special connector, which we do not have)."]
["Samsung electronics","Samsung SNC-C7478P","Camera ","v1.01_090625","1",null,null,"+","+",{"$nulls":3},"720x576","640x480","640x480","+",null,"+","-","+.","+","+",null,"-","+","1) Рекомендуется в настройках самой камеры отключить режим De-Interlace, иначе при Высоком разрешении видео в Inellecte искажено (эффект ступенек)\n2) Настройки Яркость и Контраст не работают на самой камере","1) In the camera's settings, disable the De-Interlace mode; otherwise, with the Full resolution, video is distorted in Intellect (aliasing)\n2) The Brightness and Contrast settings do not work on the camera itself"]
["Samsung electronics","Samsung SNC-M300P","Camera ","2.10_090521","1",null,null,"+","+",{"$nulls":3},"2048*1536(MJPEG)/640*480(MPEG-4)","1600*1200(MJPEG)/640*480(MPEG-4)","1280x1024(MJPEG)/640*480(MPEG-4)","+",null,"+","-",null,"+","+",null,"-","+","1) в MPEG-4 есть только одно разрешение 640*480\n2) fps в MPEG-4 и MJPEG зависят друг от друга (т.е. что бы получить максимум fps в MJPEG нужно выставить минимум fps в MPEG-4 и наоборот)\n ","1) for MPEG-4, you have only one resolution, 640*480\n2) the frame rates for MPEG-4 and MJPEG depend on each other (that is, to get the max. frame rate for MJPEG, you must set the min. frame rate for MPEG-4, and the other way around)\n "]
["Samsung Techwin","Samsung SNB-1000(P)","Camera ","1.00_100715","1","+.",null,"+","+","+",null,null,"640x480","640x480","320x240","+",{"$nulls":5},"-",null,"-","+"]
["Samsung Techwin","Samsung SNB-1001","Camera ","1.00_111226","1","+.",null,"+",null,"+",null,null,"640x480","640x480","320x240","+",null,"+","+",null,"+",null,null,"+","+"]
["Samsung Techwin","Samsung SNB-2000(P)","Camera ","1.41","1","+.",null,"+","+","+",null,null,"704x576","640x480","352x288","+",{"$nulls":4},"+","+",null,"+","+","Прошивка 1.41: камера должна работать через Onvif, но не работает - проблема устройства.","The 1.41 firmware: the camera is supposed to work via the ONVIF protocol, but it does not - this is a problem of the device itself. "]
["Samsung Techwin","Samsung SNB-3000(P)","Camera ","1.41","1","+.",null,"+","+","+",null,null,"704x576","640x480","352x288","+",null,"+","-",null,"+","+",null,"+","+"]
["Samsung Techwin","Samsung SNB-3002","Camera ","1.00_120114","1","+.",null,"+","+","+",null,null,"704x576","640x480","320x240","+",null,"+","+",null,"+","+",null,"+","+","ТВ-стандарт интегрирован для поддержки моделей с разными ТВ-стандартами. Сами камеры поддерживают либо только PAL либо только NTSC.","TV standard is integrated to support models with different TV standards. Cameras support either PAL or SECAM."]
["Samsung Techwin","Samsung SNB-5000","Camera ","1.20_101018","1","+.",null,"+","+","+",null,null,"1280x1024","800x600","640x480","+",null,"+","-",null,"+","+",null,"-","+"]
["Samsung Techwin","Samsung SNB-5001 / SND-5011 / SND-5061","Camera","1.00_120521","1","+","4","+",null,"+",null,null,"1280x1024","1024x768","640x480","+",{"$nulls":4},"+",null,"-","+","+",null,null,"improved"]
["Samsung Techwin","Samsung SNB-5004 / SNB-5003 / SNV-5084 / SND-5084 / SND-5083","Camera","1.11_131011","1","+",2,"+","-","+","-","-","1280x1024","1024x768","640x480","+","-","+","+","+","+","+","-","motion detection; audio detection; tampering detection; others","+","Диапазон битрейта зависит от значения разрешенияДля настройки профиль нельзя выставить режим базовый если для настройки статическая кодировка стоит режим CAVLCНа камере есть детектор лиц, анализ ситуацииИз двух детекторов: \"детектор ситуации\" и \"анализ ситуации\" одновременно можно создать только один","Bitrate range depends on the resolution. You cannot set the base mode for the Profile setting, if there is CAVLC mode for the static coding. There are Situational Analysis and Face detection tools. You can create only one detection tool: either Situational Analysis or Face detection tool."]
["Samsung Techwin","Samsung SNB-6004 / SNB-6003 / SND-6084 / SND-6083","Camera","1.00_130412","1","+","4","+",null,"+",null,null,"1920x1080","1024x768","640x480","+",null,"+","+","+","+","+","+","motion detection; audio detection; tampering detection; other detectors","+","Прочие встроенные детекторы:Появление / исчезновение объекта в областиВход / выход объекта из областиПересечение линииДетектор лицПри работе со встроенным детектором \"Анализ ситуации\" нужно иметь в виду, что он позволяет детектировать либо появление/исчезновение объекта в заданной области, либо вход/выход объекта из области. И то и другое одновременно детектировать нельзя, это особенность прошивки.","Other on-board detection tools: Object appearance/disappearance from area, Object entry/exit from area, Line crossing and Face detection tool. When using the on-board Situational Analysis detection tool, remember that it allows detecting either appearance/disappearance of an object in a selected area or the entry/exit of an object from an area. But it is not possible to detect both at the same time, due to firmware limitations.","improved"]
["Samsung Techwin","Samsung SNB-7000","Camera ","1.10_110725","1","+.",null,"+",null,"+",null,null,"2048x1536","1024x768","640x480","+",null,"+","+","-","+","+",null,"+","+","По Onvif работает только в режиме совместимости. Работает только получение H264 видео, звука и релеПосле смены ТВ-стандарта нужно заново настраивать параметры видео, изображения, встроенной аналитикиПри первом использовании аудио-выхода звук камерам начинает воспроизводить звук через ~5 секунд - особенность интеграции.","Via the ONVIF protocol, it works only in compatibility mode. Only the following works: H.264 video, audio, and the relay After you switch ***TV standards***, you have to configure video and embedded video analytics again. When you use the audio output for the first time, you hear audio only after around 5 seconds - this is how the integration was done."]
["Samsung Techwin","Samsung SNB-7001 / SND-7011 / SND-7061 ","Camera","1.00_120622","1","+",2,"+","-","+","-","-","2048x1536","1024x768","640x480","+","-","-","-","-","+","-","-","+","+"]
["Samsung Techwin","Samsung SNB-7002 / SND-7082 / SNV-7082 / SNO-7082R","Camera","1.00_121005","1","+",2,"+","-","+","-","-","2048x1536","1024x768","640x480","+","-","+","+","-","+","+","-","motion detection; tampering detection; others","+","Встроенные детекторы: Анализ ситуации, Детектор лицКамера не поворотная, но имеет встроенный трансфокатор ","On-board detection tools: Situational Analysis and Face detection tool. This is not a PTZ camera, but it has a built-in zoom lens."]
["Samsung Techwin","Samsung SND-1010(P)","Camera ","1.02_101122","1","+.",null,"+","+","+",null,null,"640x480","640x480","320x240","-",{"$nulls":5},"-",null,"-","+"]
["Samsung Techwin","Samsung SND-1011 ","Camera ","1.00_111226 ","1","+.",null,"+",null,"+",null,null,"640x480","640x480","320x240","+",{"$nulls":4},"+",null,null,"+","+"]
["Samsung Techwin","Samsung SND-1080 / SNV-1080 / SNV-1080R","Camera ","2.00_121027","1","+.",null,"+",null,"+",null,null,"640x480","640x480","320x240","+",null,"+","+",null,"+",null,null,"+","+"]
["Samsung Techwin","Samsung SND-3080C","Camera ","1.41","1","+.",null,"+","+","+",null,null,"704x576","640x480","352x288","+",{"$nulls":4},"+.","+",null,"-","+"]
["Samsung Techwin","Samsung SND-3080F","Camera ","1.30","1","+.",null,"+","+","+",null,null,"704x576","640x480","352x288","+",{"$nulls":4},"+","+",null,"-","+","Прошивка 1.30: устройство обнаруживается поиском как поддерживающее Onvif, но работать через Onvif не будет. Проблема самого устойства.При добавлении устройства с помощью поиска прошивку нужно выбирать вручную: автоматически она не определяется.При максимальных настройках камера передает видео с максимальной частотой кадров ~15-20 fps. Ограничение самого устройства. ","The 1.30 firmware: Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. This is a problem of the device itself. If you add the device using the search, you must select the firmware manually: it is not detected automatically. With the max. settings, the camera send video at around 15-20 fps.  This is a limitation of the device itself. "]
["Samsung Techwin","Samsung SND-3082 / SNV-3082","Camera ","1.00_111204","1","+.",null,"+","+","+",null,null,"704x576","640x480","320x240","+",null,"+","+",null,"+","+",null,"+","+","ТВ-стандарт интегрирован для поддержки моделей с разными ТВ-стандартами. Сами камеры поддерживают либо только PAL либо только NTSC.","TV standard is integrated to support models with different TV standards. Cameras support either PAL or SECAM."]
["Samsung Techwin","Samsung SND-5010","Camera ","1.00_120626","1","+.",null,"+",null,"+",null,null,"1280x1024","1024x768","640x480","+",{"$nulls":7},"motion detection, tampering detection","+"]
["Samsung Techwin","Samsung SND-5080","Camera ","1.33_110218","1","+.",null,"+","-","-",null,null,"1280x1024","800x600","640x480","+",null,"+.","-",null,"+","+",null,"-","+"]
["Samsung Techwin","Samsung SND-6084 / SND-6084R / SNV-6084R / SNO-6084R","Camera","2.21_131008","1","+","4","+",null,"+",null,null,"1920x1080","1024x768","640x480","+",null,"+","+","-","+","+","-","motion detection; audio detection; tampering detection; other detectors","+","Диапазон битрейта зависит от значения разрешенияДля настройки профиль нельзя выставить режим базовый если для настройки статическая кодировка стоит режим CAVLCНа камере присутствует встроенная аналитика:Детектор лицАнализ ситуации ","Bit rate range depends on the resolution. You cannot set the base mode for the Profile setting, if there is CAVLC mode for the static coding. There are Situational Analysis and Face detection tools.","improved"]
["Samsung Techwin","Samsung SND-7080 /SND-7080F / SNO-7080R / SNV-7080R ","Camera ","1.20_111227","1","+.",null,"+",null,"+",null,null,"2048x1536","1024x768","640x480","+",null,"+","+",null,"+","+",null,"+","+"]
["Samsung Techwin","Samsung SNF-7010(V) ","Camera","1.00_130806","1","+.",null,"+","-","+",null,null,"2048x1536","1024x768","640x480","+","-","-","-","-","-","-","-",null,"+","Если в ПО, после создания зоны детектирования, менять настройки \"отразить вертикально\" и \"отразить горизонтально\", то созданная на камере зона также отобразиться зеркально/вертикально и перестанет соответствовать зоне, установленной в продукте. ","If in AxxonSoft products, after area zone detection created, you will change the settings \"vertical reflect\" and \"horizontal reflect\", then created area zone will also be changed to mirror/vertical display and will not longer match the zone established in the product."]
["Samsung Techwin","Samsung SNO-1080R","Camera ","1.00_111226","1","+.",null,"+",null,"+",null,null,"640x480","320x240","640x480","+",{"$nulls":4},"+",null,null,"+","+"]
["Samsung Techwin","Samsung SNO-5080R","Camera ","0.17_110222","1","+.",null,"+","+","+",null,null,"1280x1024","1024x768","640x480","+",{"$nulls":7},"+","+"]
["Samsung Techwin","Samsung SNO-6011R / SND-6011R","Camera","1.11_131011","1","+",2,"+","-","+","-","-","1920x1080","1024x768","640x480","+","-","-","-","-","-","-","-","motion detection; tampering detection; others","+","Диапазон битрейта зависит от значения разрешенияДля настройки профиль нельзя выставить режим базовый если для настройки статическая кодировка стоит режим CAVLCНа камере есть детектор лиц, анализ ситуации","Bitrate range depends on the resolution. You cannot set the base mode for the Profile setting, if there is CAVLC mode for the static coding. There are Situational Analysis and Face detection tools."]
["Samsung Techwin","Samsung SNP-3120V","Camera ","1.22_110120_1","1","+.",null,"+","+","+",null,null,"704x576","640x480","320x240","+",{"$nulls":3},"+","+","+",null,"-","+","Событие о срабатывании лучей приходит с задержкой (~5 сек.) - особенность камеры.","Notifications on a sensor going off arrive with a delay (around 5-10 seconds). This is a limitation of the camera itself."]
["Samsung Techwin","Samsung SNP-3302(H) / SNP-3371(H/TH) ","Camera ","1.01_111121","1","+.",null,"+","+","+",null,null,"704x576","640x480","320x240","+",null,null,"+","+","+","+",null,"+","+","1. Поиск не возвращает прошивку. Правильную версию нужно выбрать самостоятельно.\n2. Луч срабатывает с задержкой (1 сек).\n3. В мультипотоковом режиме максимальная суммарная частота кадров с обоих потоков - 25 fps.\n4. Через Onvif работает получение видео с некоторыми настройками видео и изображения, телеметрия. На сайте onvif.org камера официально не заявлена как поддерживающая Onvif.","1. Search doesn't restore a firmware. It's necessary to choose the correct version of firmware manually.\n2. Alarm in triggers with a delay (1 second).\n3. In a multi-stream mode the maximum total frame rate from both streams is 25 fps.\n4. Video receiving with some settings of video and the image, telemetry works via Onvif. At www.onvif.org the camera isn't officially declared as Onvif-supporting.\n"]
["Samsung Techwin","Samsung SNP-3370","Camera ","1.20_101006","1",null,null,"+","+","+",null,null,"704x576","704x576","352x288","+",null,"+","-","+","+","+",null,"+.","+","Перед работой с реле необходимо в веб-интерфейсе параметру \"duration\" присвоить значение \"always\"При работе со встроенным детектором зоны детектирования приходится создавать через веб-интерфейс.По утверждению производителя интеграция настроек изображения сейчас невозможна.В видеопотоке \"0. MJPEG\" максимальная частота кадров 10 fps доступна для выбора только в том случае, когда в потоке \"1. MPEG4/H.264 \" выбран кодек MPEG4","Before using the camera, go to the web interface and set the Duration parameter to \"always \"When working with the embedded detector, you have to use the web interface to create detection areas. According to the vendor, currently it is not possible to integrate ***basic video settings*** (?).For the 0. MJPEG stream, you can select the max. frame rate (10 fps) only after you select the MPEG4 codec for the 1.MPEG4/H.264 codec."]
["Samsung Techwin","Samsung SNP-3430H","Camera ","1.11_111104","1","+.",null,"+","+","+",null,null,"704x576","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"+","+"]
["Samsung Techwin","Samsung SNP-5200(H)","Camera ","1.00_110309","1","+.",null,"+","+","+",null,null,"1280x1024","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":4},"+"]
["Samsung Techwin","Samsung SNP-5300/H","Camera ","1.10_130523","1","+.",null,"+",null,"+",null,null,"1280x1024","1024x768","640x480","+",null,"+","+","+","+","+",null,"motion detection; audio detection; tampering detection; and others","+","На камере присутствуют детектор лиц и детектор \"анализ ситуации\" .","On-board detection tools: Situational Analysis, Face Detection Tool."]
["Samsung Techwin","Samsung SNP-6200 / SNP-6200H","Camera ","1.00_120302","1","+.",null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",null,"+","+.","+","+","+",null,"+","+","1. Список встроенных детекторов камеры:\nИзменение положения\nВход в область\nВыход из области\nИсчезновение из области\nПоявление в области\nПересечение линии","1. Video analytics embedded in the cameras include:\nTampering\nEnter/Exit\nAppear/Disappear\nVirtual Line\n"]
["Samsung Techwin","Samsung SNP-6200RH","Camera","1.11_131002","1","+.",null,"+","-","+",null,null,"1920x1080","1024x768","640x480","+",null,"-","-","+","-","-","-",null,"+"]
["Samsung Techwin","Samsung SNV-3080P","Camera ","1.13","1","+.",null,"+","+","+",null,null,"704x576","640x480","352x288","+",null,"+","+",null,"+","+",null,"+","+"]
["Samsung Techwin","Samsung SNV-3120P","Camera ","1.20_101123","1","+.",null,"+","+","+",null,null,"704x576","640x480","320x240","+",null,"+","-","+.","+","+",null,"-","+","Камера не PTZ, телеметрия цифроваяЦифровое увеличение иногда срабатывает с ошибками: сразу в максимум. Проблема устройства.","This is not a PTZ camera, but it has digital telemetry Sometimes digital zoom does not work correctly: it goes to the max. zoom from the start. This is a limitation of the device itself."]
["Samsung Techwin","Samsung SNV-5080R","Camera ","1.00_110421","1","+.",null,"+","+","+",null,null,"1280x1024","1024x768","640x480","+",{"$nulls":8},"+"]
["Samsung Techwin","Samsung SNV-6012M","Camera","1.11_131011","1",null,null,"+","-","+",null,null,"1920x1080","1024x768","640x480","+",null,"-","-","-","-","-","-","motion detection; tampering detection; others","+"]
["Samsung Techwin","Samsung SNV-6084","Camera","1.11_131011","1","+",2,"+","-","+","-","-","1920x1080","1024x768","640x480","+","-","+","+","-","+","+","-","motion detection; audio detection; tampering detection; others","+"]
["Samsung Techwin","Samsung SNZ-5200","Camera ","1.00_110218","1","+.",null,"+","+","+",null,null,"1280x1024","1024x768","640x480","+",{"$nulls":8},"+"]
["Samsung Techwin","Samsung SPE-100P","Encoder ","1.21_101213","1","+.",null,"+","+","+",null,null,"640x480","640x480","320x240","+",null,"+","-","+","+","+",null,"-","+"]
["Samsung Techwin","Samsung SPE-101","Encoder ","1.00_110829","1","+.",null,"+","+","+",null,null,"704x576","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"+","+","Настройка ТВ-стандарта сделана для поддержки моделей с разными ТВ-стандартами.","The TV-standard is configured to support models with different TV-standards"]
["Samsung Techwin","Samsung SPE-400","Encoder ","1.00_110114","4","+.",null,"+","+","+",null,null,"704x576","640x480","320x240","+",{"$nulls":8},"+","1. устройство представляет из себя 4-х канальный ip-видеосервер, причем каждый канал имеет свой ip-адрес, а значит является отдельным граббером в ПО ITV/Axxon\n2. Задать области детектированя встроенной аналитики в ПО Axxon нельзя. Особенность интеграции","1. the device is a 4-channel video encoder; because each channel has its own IP address, it has a separate grabber in the AxxonSoft software.\n2. In AxxonSoft software, you cannot set detection areas for the embedded video analytics. This is how the integration was done."]
["Santec","Santec SNC-637ID","Camera ","3.8.4","1",null,null,"+","+",{"$nulls":3},"720x576","720x576 (MJPEG) / 720x288 (MPEG4)","720x576 (MJPEG) / 352x288 (MPEG4)","+",{"$nulls":3},"+","+","+",null,"-","+","Событие о прекращении тревоги по лучу приходит с ~10-секундной задержкой. Особенность камеры.","Notifications on a sensor going off arrive with a delay (around 10 seconds). This is a limitation of the camera itself."]
["Sanyo","Sanyo VCC-HD2100P","Camera ","Main 1.02-02 & Sub 1.01-00 & 2.03-08","1",null,null,"+",null,"+",null,null,"2288x1712(MJPEG)/1600x1200(H.264)","1024x768","640x480","+",{"$nulls":3},"+","+","+",null,"-","+","1. ограничение fps самого устройстваMJPEG:\n-Полное 3-5 fps (в завис. от кач-ва)\n-Высокое 10-12 fps (в завис. от кач-ва)\n-Стандартное 25 fps\nH.264:\n-во всех разрешениях при любом качестве 25 fps\n2. Полноценная работа видео реализована только в режиме \"4:3\". В режиме \"16:9\" может быть недоступным максимальное разрешение.\n3. Камера не PTZ, но есть настраиваемый фокус, в ПО ITV работает в телеметрии.\n","1. The camera itself has the following frame rate limits: MJPEG:\n- Full resolution 3-5 fps (depending on the quality)\n- High resolution 10-12 fps (depending on the quality)\n- Standard resolution 25 fps\nH.264:\n25 fps for any resolution and any quality\n2. Full-fledged video is implemented only for 4:3 mode. In 16:9 mode, the max. resolution is not available sometimes. \n3. This is not a PTZ camera, but it has adjustable zoom; in the AxxonSoft software, telemetry works. \n"]
["Sanyo","Sanyo VCC-HD2300P","Camera ","Main 2.03-02 & Sub 1.01-00","1",null,null,"+",null,"+",null,null,"2288x1712(MJPEG)/1600x1200(H.264)","1024x768","640x480","+",{"$nulls":4},"+","+",null,"-","+","Ограничение fps самого устройстваMJPEG:Полное 3-5 fps (в завис. от кач-ва)Высокое 10-12 fps (в завис. от кач-ва)Стандартное 25 fpsH.264:Во всех разрешениях при любом качестве 25 fpsПереключение соотношения сторон 4:3 - 16:9 релизовано в AxxonNext/Next (и только в AxxonNext/Next) посредством смены ТВ-стандарта.Камера поддерживает управление фокусом - это интегрировано как частичная телеметрия.","The camera itself has the following frame rate limits: MJPEG:- Full resolution 3-5 fps (depending on the quality)- High resolution 10-12 fps (depending on the quality)- Standard resolution 25 fpsH.264:25 fps for any resolution and any quality Switching aspect ratios (4:3 - 16:9) is implemented in AN (and only in AN) as switching ***TV standards***.The camera supports zoom - this is integrated as partial telemetry."]
["Sanyo","Sanyo VCC-HD2500P","Camera ","1.00-08 (100107-02)","1",null,null,"+",null,"+",null,null,"2280x1712(MJPEG)/1600x1200(H264);","1024x768 (MJPEG), 1280x960 (H264);","640x480","+",null,"+","-",null,"+","+",null,"-","+"]
["Sanyo","Sanyo VCC-HD4600P","Camera ","CAM MAIN Ver. 1.02-00 (100604-00) & CAM SUB Ver. 1.01-00 (100528-00)","1",null,null,"+",null,"+",null,null,"2288x1712(MJPEG) / 1600x1200(H.264)","1024x768","640x480","+",null,"+","-","+","+","+",null,"-","+","1. ограничение fps самого устройстваMJPEG:\n-Полное 3-5 fps (в завис. от кач-ва)\n-Высокое 10-12 fps (в завис. от кач-ва)\n-Стандартное 25 fps\nH.264:\n-во всех разрешениях при любом качестве 25 fps\n2. Полноценная работа видео реализована только в режиме \"4:3\". В режиме \"16:9\" может быть недоступным максимальное разрешение.","1. The camera itself has the following frame rate limits: MJPEG:\n- Full resolution 3-5 fps (depending on the quality)\n- High resolution 10-12 fps (depending on the quality)\n- Standard resolution 25 fps\nH.264:\n25 fps for any resolution and any quality\n2. Full-fledged video is implemented only for 4:3 mode. In 16:9 mode, the max. resolution is not available sometimes. "]
["Sanyo","Sanyo VCC-HD5600P","Camera ","2.03-05","1",null,null,"+",null,"+",null,null,"1600x1200","1024x768","640x480","+",null,"+","-","+","+","+",null,"-","+","Зум срабатывает с задержкой - особенность камерыВ Интеллекте скорость поворота (телеметрии) нужно устанавливать в диапазоне [1,8] - особенность устройства.В H264 при высоких разрешениях (начиная с 1024х768) набор допустимых значений параметра \"Интервал включения опорных кадров\" сужается до [15, 100]Ограничения частоты кадров при высоких разрешениях:MJPEG:800x600: 12.5 fps1024x768: 12.5 fps1280x960: 10 fps1600x1200: 5 fpsH264: в зависимости от текущего выбранного разрешения в MJPEGначиная с DP 3.2.4.643 в ПО Intellect можно получить одновременно два независимых виодеопотока с камеры, для этого на одном граббере необходимо создать 2 камеры с номерами каналов 1 и 2, но надо помнить что в возмодность открытия очередного видеопотока на самой камере очень сильно зависит от настроек уже существующих видеопотоков, таким образом сама камера не позволяет создать много независимых видеопотоков с максимальными настройками.","Zoom works with a delay - this is a limitation of the camera itself In Intellect, set the PTZ (telemetry) speed to a value between 1 and 8 - this is a limitation of the camera itself. For H.264, for high resolutions (starting from 1024x768), the range of the available values for the Keyframes Interval parameter becomes as narrow as [15, 100]Frame rate limits for high resolutions:MJPEG:800x600: 12.5 fps1024x768: 12.5 fps1280x960: 10 fps1600x1200: 5 fpsH264: depends on the currently selected resolution for MJPEGstarting from DP 3.2.4.643, in Intellect, you can get two independent video streams at the same time; to do this, for the same grabber create 2 cameras and set their channel numbers to 1 and 2; note that whether you can open a new stream on the camera itself depends very much on the settings of the already existing streams; thus, the camera itself does not allow you to create many independent streams with max. settings."]
["Sanyo","Sanyo VCC-N6695P","Camera ","1.01-00<08102300>","1",null,null,"+",null,"-",null,null,"720x576","640x480","640x480","+",{"$nulls":4},"-","+",null,null,"+"]
["Sanyo","Sanyo VDC-HD3100P","Camera ","Main 1.02-02 & Sub 1.01-00","1",null,null,"+",null,"+",null,null,"2288x1712(MJPEG) / 1600x1200(H.264)","1024x768","640x480","+",{"$nulls":3},"+","+","+",null,"-","+","1. ограничение fps самого устройстваMJPEG:\n-Полное 3-5 fps (в завис. от кач-ва)\n-Высокое 10-12 fps (в завис. от кач-ва)\n-Стандартное 25 fps\nH.264:\n-во всех разрешениях при любом качестве 25 fps\n2. Полноценная работа видео реализована только в режиме \"4:3\". В режиме \"16:9\" может быть недоступным максимальное разрешение.\n3. Камера не PTZ, но есть настраиваемый фокус, в ПО ITV работает в телеметрии.","1. The camera itself has the following frame rate limits: MJPEG:\n- Full resolution 3-5 fps (depending on the quality)\n- High resolution 10-12 fps (depending on the quality)\n- Standard resolution 25 fps\nH.264:\n25 fps for any resolution and any quality\n2. Full-fledged video is implemented only for 4:3 mode. In 16:9 mode, the max. resolution is not available sometimes. \n3. This is not a PTZ camera, but it has adjustable zoom; in the AxxonSoft software, telemetry works."]
["Sentry360","Sentry360 FS-IP3000","Fisheye Camera","sr20130717NSA","1",null,null,"+",null,"+",null,null,"2048x1536(H.264) / 1920x1080(MJPEG)","1024x768","640x480","+",{"$nulls":8},"+","После смены режима ТВ-стандарта камера перезагружается.","After TV-standard changing the camera will be rebooted."]
["Sentry360","Sentry360 FS-IP5000","Camera ","442 ","1",null,null,"+",null,"+",null,null,"2560x1920","1024x768","640x480","+",{"$nulls":7},"-","+","Частота кадров сильно зависит от настроек видео и изображения. Максимальная частота кадров - 15 fps.","The frame rate very much depends on the video settings. The max. frame rate is 15 fps. "]
["Sentry360","Sentry360 IS-DM 220","Camera ","y20120224ANS","1",null,null,"+",null,"+",null,null,"1920x1080","640x480 (1280х720 with ONVIF)","320x240(720x576 with ONVIF)","+",null,"+","+",null,"+","+",null,"+","+","1. В разрешении 1920х1080 максимальный fps на камере равен 12.\n2. Настройки аудио-входа и аудио-выхода должны быть одинаковыми.","1. With the 1920x1080 resolution, the camera allows max. 12 fps. \n2. Settings of an audio input and audio output shall be identical."]
["Sentry360","Sentry360 IS-IP14K-DN","Camera","462","1",null,null,"+","-","+","-","-","4592x3280","3440x2448","1152x816","+",null,"-","-","-","-","-","-","-","+","Максимальное значение FPS зависит от выбранного значения разрешения.Значение разрешения в продукте зависит от значения настройки Size, в веб-интерфейсе камеры.","The max. fps rate depends on the selected resolution. Resolution depends on the Size setting in the camera web interface. "]
["SimpleIP Cam","SimpleIP Cam SPC series","Camera ","06.00.03.02","1",null,null,"+",null,"+",null,null,"704x576","704x288","320x240","+",null,"+","-",null,"-","+",null,"+","-","1. Количество реле зависит от конкретной модели подключаемой камеры\n2. Ползунок \"Качество\" в ПО Intellect регулирует битрейт видеопотока","1. The number of relays depends on the model of a particular camera. In Intellect, the Quality slider adjusts the video bit rate. "]
["SimpleIP Cam","SimpleIP Cam SPC series","Camera ","06.00.16.03","1",null,null,"+",null,"+",null,null,"704x576","704x288","320x240","+",null,"-","-","+",{"$nulls":3},"-","-","1. Ползунок \"Качество\" в ПО Intellect регулирует битрейт видеопотока\n","1. In Intellect, the Quality slider adjusts the video bit rate.\n"]
["SimpleIP Cam","SimpleIP Cam SPC series","Camera ","06.00.10.03","1",null,null,"+",null,"+",null,null,"704x576","704x288","352x288","+",null,"-","-",null,"-","+",null,"-","-"]
["SimpleIP Cam","SimpleIP Cam SPCHD series","Camera ","1.2.24","1",null,null,"+","+.","+",null,null,"2048x1536(MJPEG) / 1280x960(MPEG-4) / 1920x1072(H.264)","1600x1200(MJPEG) / 1280x720(MPEG-4) / 1280x720(H.264)","720x480(MJPEG) / 720x480(MPEG-4) / 720x480(H.264)","+",null,"+.",null,null,"-","-",null,null,"+","1.  настройки яркость, контраст, резкость, цветность не работают на самой камере с прошивкой 1.2.24\n2. в MJPEG при 2048х1536 максимальный fps = 15 (ограничение самой камеры)\n3. в H.264 при 1920х1080 максимальный fps = 10 (ограничение самой камеры)\n4. С прошивкой 1.2.24 аудио не работает на самой камере (шум вместо звука). Проблема устройства.\n5. С прошивкой 1.2.24 после перезагрузки камера вместо видео транслирует зеленый экран - проблема самого устройства ","1.  With the 1.2.24 firmware, the Brightness, Contrast, Sharpness, and Saturation settings do not work on the camera itself\n2. with MJPEG and 2048x1536 resolution, the max. frame rate is 15 fps (this is a limitation of the device itself)\n3. with H.264 and 1920x1080 resolution, the max. frame rate is 10 fps (this is a limitation of the device itself)\n4. With the 1.2.24 firmware, audio does not work on the camera itself (noise instead of audio) This is a problem of the device itself.\n5. With the 1.2.24 firmware, after you restart the camera, it shows a green screen instead of video - this is a problem of the device itself "]
["SimpleIP Cam","SimpleIP Cam SPCHD series","Camera ","1.2.24","1",null,null,"+","+.","+",null,null,"2048x1536(MJPEG) / 1920x1072(MPEG-4) / 1920x1072(H.264)","1600x1200(MJPEG) / 1280x960(MPEG-4) / 1280x720(H.264)","720x480(MJPEG) / 720x480(MPEG-4) / 720x480(H.264)","+",null,"+.","-",null,"+","-",null,null,"+","1.  настройки яркость, контраст, резкость, цветность не работают на самой камере с прошивкой 1.2.24\n2. в MJPEG при 2048х1536 максимальный fps = 15 (ограничение самой камеры)\n3. в H.264 при 1920х1080 максимальный fps = 10 (ограничение самой камеры)\n4. С прошивкой 1.2.24 аудио не работает на самой камере (шум вместо звука). Проблема устройства.\n5. С прошивкой 1.2.24 после перезагрузки камера вместо видео транслирует зеленый экран - проблема самого устройства ","1.  With the 1.2.24 firmware, the Brightness, Contrast, Sharpness, and Saturation settings do not work on the camera itself\n2. with MJPEG and 2048x1536 resolution, the max. frame rate is 15 fps (this is a limitation of the device itself)\n3. with H.264 and 1920x1080 resolution, the max. frame rate is 10 fps (this is a limitation of the device itself)\n4. With the 1.2.24 firmware, audio does not work on the camera itself (noise instead of audio) This is a problem of the device itself.\n5. With the 1.2.24 firmware, after you restart the camera, it shows a green screen instead of video - this is a problem of the device itself "]
["SimpleIP Cam","SimpleIP SPCHD-200SA","Camera ","1.0.7","1",null,null,"+",null,"+",null,null,"h.264: 1920x1080, mjpeg: 640x352","h.264: 1280x720, mjpeg: 640x352","h264: 720x480, mjpeg: 640x352","+",{"$nulls":4},"+.","-",null,"+.","+","Реле и телеметрия не работает на самой камереЧтобы работал встроенный детектор движения, необходимо выбрать режим Dual или Tri-stream. Из-за этого в Интеллекте детектор не работает - адаптер при любых комбинациях кодека и разрешения выбирает режим Single.При максимальном разрешении и/или качестве fps падает до 2-5 кадров в секундуВстроенный детектор лиц не работает на самой камереМикрофон интегрирован, т.к. он описан в SDK, но фактически на камере нет ни встроенного микрофона, ни аудио-входа.На запросы IP-wizard'a наших продуктов камера вместо имени модели возвращает \"SPCHD series\". Т.к. устройство с таким именем прописано в нашем драйвере совершенно по-другому, в AxxonNext/Next камеру нужно добавлять обязательно только вручную, а в Интеллекте при добавлении обязательно указывать модель \"SPCHD-200SA\".firmware v1.0.7: продолжительность тревоги от встроенного детектора устанавливается в веб-интерфейсе (\"Потеря соединения\" -> \"Последнее событие\").","The relays and telemetry do not work on the camera itself To make the embedded motion detector work, select Dual or Tri-stream mode. For this reason, the detector does not work in Intellect: the adapter selects Single mode for any codec and any resolution. If you set the max. resolution and/or quality, the frame rate drops to around 2-5 fps. The embedded face recognition detector does not work on the camera itself. The microphone is integrated, because it is described in the SDK, but in reality the camera has neither a microphone, nor an audio input. In our software products, IP-wizard's requests return \"SPCHD series\" instead of the model name. A device with this name is supported by our driver in a different way. For this reason, in AN you must add the camera manually and in Intellect when adding the camera you must specify the model as SPCHD-200SA.The v1.0.7 firmware: You can configure how long an alarm from the embedded detection tools is active in the camera web interface.(\"Connection lost\" -> \"Last event\")"]
["SimpleIP Cam","SimpleIP SPCHD-241VDS","Camera","2.8.1.0O_201309111214_P4P","1","-",{"$nulls":3},"+",null,null,"1920x1080","1920x1080","352x288","+",{"$nulls":7},"-","+",null,null,"improved"]
["SimpleIP Cam","SimpleIP SPCHD-260VO.IRS / SPCHD-231VBIRS / SPCHD-221VDIRS","Camera","2.8.2.0O_201309111214_P2P","1","-",{"$nulls":3},"+",null,null,"1280x720","1280x720","352x288","+",{"$nulls":7},"-","+",null,null,"improved"]
["Sinkross","Sinkross UID-01","Camera ","v.01","1",null,null,"+",{"$nulls":4},"800x600","800x600","800x600",{"$nulls":8},"motion detection; others","+","На камере два сетевых интерфейса. При подключении нужно указывать порт 1100.\nНа камере есть детектор огня, движения и дыма\nНастройки камеры и детекторов необходимо производить в вебе.","There are two network interfaces. For connection required to set port 1100. The camera has fire, motion and smoke detection. Camera's settings and detection should be performed using web-interface."]
["SNR","SNR SNR-CI-DW3.0I","Camera","2.211.0000.0.T, build : 2013-10-15","1",null,null,"+","-","+","-","-","2048x1536","1280x960","352x288","+","-","-","-","-","-","-","-","-","+"]
["Smartec","Smartec STC-IP2070/1","Camera ","A1D-M2N-V2.09.11-NB","1",{"$nulls":3},"+",{"$nulls":3},"720x576","720x576","352x288","+",{"$nulls":4},"-","-",null,"-","-","За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream."]
["Smartec","Smartec STC-IP2070A/1","Camera ","A1D-M2N-V2.09.11-NB","1",{"$nulls":3},"+",{"$nulls":3},"720x576(PAL)/720x480(NTSC)","720x576(PAL)/720x480(NTSC)","352x288(PAL)/352x240(NTSC)","+",null,"+",null,null,"-","-",null,null,"-","1. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","1) The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream."]
["Smartec","Smartec STC-IP2571A/1","Camera ","A1D-M2N-V2.09.11-NB","1",{"$nulls":3},"+",{"$nulls":3},"720x576(PAL)/720x480(NTSC)","720x576(PAL)/720x480(NTSC)","352х272(PAL)/320x240(NTSC)","+","+","+","-",null,"+","+",null,null,"-","1. За неимением на самом устройства настройки качества видеоизображения, ползунок \"Качество\" в Intellecte регулирует bit rate видеопотока.Если выбрать неверный тип цветопередачи (ТВ-стандарт), возможна потеря части изображения.\n2. Для отображения видео в ПО ITV необходимо использовать протокол TCP.","1. The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream. If you select an incorrect color rendering (TV standard), parts of the image may be lost. \n2. For video display in a software of ITV it is necessary to use the TCP protocol."]
["Smartec","Smartec STC-IP2580/1","Camera ","A1D-220-V3.08.08-NB","1",null,null,"+","+",{"$nulls":3},"704x576","640x480","352x288","+",null,"+","-",{"$nulls":4},"-","-","1. За неимением на самом устройстве настройки качества видеоизображения при MPEG-4, ползунок \"Качество\" в Intellect регулирует bit rate mpeg-4 видеопотока.","1) With MPEG-4, the device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream."]
["Smartec","Smartec STC-IP3070/1","Camera ","A1D-M2N-V2.09.11-NB","1",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352х288(PAL)/352x240(NTSC)","+",{"$nulls":4},"-","+",null,"-","-","1. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока","1) The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream."]
["Smartec","Smartec STC-IP3070A/1","Camera ","A1D-M2N-V2.09.11-NB","1",{"$nulls":3},"+",{"$nulls":3},"720x576","720x576","352x288","+",null,"+",null,null,"-","+",null,null,"-","За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока","The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream."]
["Smartec","Smartec STC-IP3570A/1","Camera ","A1D-M2N-V2.06.12-NB","1",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352x288(PAL)/352x240(NTSC)","+",null,"+","-",null,"+","+",null,"-","-","1. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока","1) The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream."]
["Smartec","Smartec STC-IP3975A/2","Camera ","A1D-M2N-V2.09.11-NB","1",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352х288(PAL)/352x240(NTSC)","+",null,"+","-","+","-","-",null,"-","-","1. Для работы телеметрии в настройках самой камеры необходимо проставить протокол-Pelco D,скорость-2400, адрес-001\n2. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока\n","1) When configuring telemetry devices in Intellect, choose the protocol Pelco D, Baud Rate -2400, adress -001\n2) The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream.\n"]
["Smartec","Smartec STC-IP3985A/2","Camera ","A1D-M2N-V2.09.11-NB","1",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352х288(PAL)/352x240(NTSC)","+",null,"+","-","+","-","-",null,"-","-","1. Для работы телеметрии при выборе протокола \"Ip camera\" будет работать по протоколу Pelco-D с адресом 1 и baud rate'ом 2400\nПри выборе протокола \"Pelco-D\" или \"Dynacolor\" будет работать по выбранному протоколу с выбраным baud rate'ом и адресом\n2. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока\n","1) When configuring telemetry devices in Intellect, choose the protocol \"Ip camera\", telemetry will be work by protocol Pelco D, Baud Rate -2400, adress-001\n2) The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream.\n"]
["Smartec","Smartec STC-IP3988A/2","Camera ","A1D-M2N-V2.08.11-NB","1",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352х288(PAL)/352x240(NTSC)","+",{"$nulls":3},"+",{"$nulls":3},"-","-","1. Для работы телеметрии в настройках самой камеры необходимо проставить протокол-Pelco D,скорость-2400, адрес-001\n2. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока\n","1) When configuring telemetry devices in Intellect, choose the protocol Pelco D, Baud Rate -2400, adress -001\n2) The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream.\n"]
["Smartec","Smartec STC-IPM2090A","Camera ","A1D-220-V3.08.08-NB","1",null,null,"+","+",{"$nulls":3},"1280x1024","1280x720","640x480","+",null,"+","-",null,"+","+",null,"-","-","1. При \"Полном\" разрешении (1280х1024) камера способна выдавать максимум 8 fps\n2. При MPEG-4 за неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока","1) With the Full resolution (1280х1024), the camera allows 8 fps max. \n2. For MPEG-4, the device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream."]
["Smartec","Smartec STC-IPM3077A / STC-IPM3578A / STC-IPM3577A","Camera ","BgWT8130035N04 V24 1211052A","1",null,null,"+","+","+",null,null,"1280x1024","1280x960","720x480","+",{"$nulls":8},"+"]
["Smartec","Smartec STC-IPM3086A, STC-IPM3186A, STC-IPM3586A","Camera ","BgWT8202715N03 V23 1208153A","1",null,null,"+","+","+",null,null,"1920x1072","1280x1024","720x480","+",null,"+","-","-","+","+.",null,"motion detection; ","+"]
["Smartec","Smartec STC-IPM3090A","Camera ","A1D-220-V3.09.14-NB","1",null,null,"+","+",{"$nulls":3},"1280x1024","640x480","640x480","+",null,"+","-",null,"+","+.",null,"-","-","Интегрировано в Intellect 4.7.6.125 и старше. Т.е. в Intellect 4.7.6 Release камера работать не будет.","Already integrated in Intellect 4.7.6.125 and above. i.e. this camera is not going to work in Intellect 4.7.6."]
["Smartec","Smartec STC-IPMX3593A/1","Camera ","1.3.0","1",null,null,"+",null,"+",null,null,"1920x1080","1280x720","480x270","+",null,"+","+",null,"+.","+",null,"Motion, Presence, Enter, Exit, Appear, Disappear, Stopped, Dwell, Direction filter, Speed Filter, Tailgating \n","+","1. Список детекторов встроенной аналитики: Presence Enter Exit Appear Disappear Stopped Dwell Direction filter Speed Filter Tailgating","1. List of detectors of built-in analytics: Presence Enter Exit Appear Disappear Stopped Dwell Direction filter Speed Filter Tailgating"]
["Smartec","Smartec STC-IPMX3693A","Camera ","1.4.0.12","1",null,null,"+",null,"+",null,null,"1920x1080","800x450","480x270","+",null,"+","+",null,"+","+",null,"motion detection.; tampering detection; others.;","+","Список детекторов встроенной аналитики:\nPresence\nEnter\nExit\nAppear\nDisappear\nStopped\nDwell\nDirection filter\nSpeed Filter\nTailgating","In-built detectors:\nPresence\nEnter\nExit\nAppear\nDisappear\nStopped\nDwell\nDirection filter\nSpeed Filter\nTailgating"]
["Smartec","Smartec STC-IPX3630A / STC-IPX3561A ","Camera ","1.6.7","1",null,null,"+","+","+",null,null,"720x576","640x576","320x288","+",null,"+","+",{"$nulls":5},"+","1. Для корректной работы динамика и микрофона в ПО ITV/Axxon необходимо, чтобы их настройки совпадали.\n2. Кодек G.711 работает только с частотой дискретизации 8 КГц, частота 16 кГц не поддерживается. ","1. To work with the speaker and the microphone in Axxon SW correctly, their settings must be the same.\n2. G.711 codec works only with a sampling rate of 8 kHz. 16 kHz is not supported."]
["Smartec","Smartec STS-IPT160 encoder","Encoder ","A1D-M2N-V2.05.12-NB","1",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352х288(PAL)/352x240(NTSC)","+",{"$nulls":3},"+","+","+",null,"-","-","1. При настройке телеметрии в настройках Intellecta протокол следует выбирать не \"IPCamera\", а тот, по-которому работает подключенная поворотная камера (Pelco-D, DynaColor, Panasonic-850 проч.). Также необходимо указывать настройку \"Скорость\" (Boud Rate)\n2. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","1) When configuring telemetry devices in Intellect, choose the protocol that the newly plugged camera (Pelco-D, DynaColor, Panasonic-850 etc.) supports. Do not choose the \"IPCamera\" protocol. Then specify the Baud Rate. 2 The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream."]
["Smartec","Smartec STS-IPT180 encoder","Encoder ","A1D-M2N-V2.09.11-NB","1",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352х288(PAL)/352x240(NTSC)","+",null,"+","-","+","+.","+.",null,"-","-","1. При настройке телеметрии в настройках Intellecta протокол следует выбирать не \"IPCamera\", а тот, по-которому работает подключенная поворотная камера (Pelco-D, DynaColor, Panasonic-850 проч.). Также необходимо указывать настройку \"Скорость\" (Boud Rate)\n2. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n","1) When configuring telemetry devices in Intellect, choose the protocol that the newly plugged camera (Pelco-D, DynaColor, Panasonic-850 etc.) supports. Do not choose the \"IPCamera\" protocol. Then specify the Baud Rate. 2 The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream.\n"]
["Smartec","Smartec STS-IPT260 encoder","Encoder ","A2D-P2N-V2.01.00-NB","2",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352х288(PAL)/352x240(NTSC)","+",{"$nulls":3},"+","+","+",null,"-","-","1. При настройке телеметрии в настройках Intellecta протокол следует выбирать не \"IPCamera\", а тот, по-которому работает подключенная поворотная камера (Pelco-D, DynaColor, Panasonic-850 проч.). Также необходимо указывать настройку \"Скорость\" (Boud Rate)\n2. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","1) When configuring telemetry devices in Intellect, choose the protocol that the newly plugged camera (Pelco-D, DynaColor, Panasonic-850 etc.) supports. Do not choose the \"IPCamera\" protocol. Then specify the Baud Rate. 2 The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream."]
["Smartec","Smartec STS-IPT280 encoder","Encoder ","A2D-P2N-V2.02.09-NB","2",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352х288(PAL)/352x240(NTSC)","+",null,"+","-","+","+","+",null,"-","-","1. При изменении некоторых настроек в Intellect (а именно: тип сигнала \"PAL/NTSC\", разрешение видео, качество видео - bitrate, скорости видео - fps) и последующего нажатия кнопки \"Применить\" ip-сервер перезагружается для применения настроек. \n2. При настройке телеметрии в настройках Intellecta протокол следует выбирать не \"IPCamera\", а тот, по-которому работает подключенная поворотная камера (Pelco-D, DynaColor, Panasonic-850 проч.). Также необходимо указывать настройку \"Скорость\" (Boud Rate)\n3. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n","1) If you change some settings in Intellect e.g. PAL/NTSC, resolution, bit rate and fps of the video stream, and then click Apply, the IP server will reboot to enable these settings. \n2) When configuring telemetry devices in Intellect, choose the protocol that the newly plugged camera (Pelco-D, DynaColor, Panasonic-850 etc.) supports. Do not choose the \"IPCamera\" protocol. Then specify the Baud Rate. 3 The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream.\n"]
["Smartec","Smartec STS-IPT460 encoder","Encoder ","A4Q-T2N-V2.01.03-NB","4",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352х288(PAL)/352x240(NTSC)","+",{"$nulls":3},"+","+","+",null,null,"-","1. По информации от Nextec для устройства STS-IPT460 с прошивкой  A4Q-T2N-V2.03.05-NB нужно выбрать в Интеллекте устройство STS-IPT480, никаких обновлений прошивки НЕ требуется.\n2. При настройке телеметрии в настройках Intellecta протокол следует выбирать не \"IPCamera\", а тот, по-которому работает подключенная поворотная камера (Pelco-D, DynaColor, Panasonic-850 проч.). Также необходимо указывать настройку \"Скорость\" (Boud Rate)\n3. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","1) As per Nextec briefing on STS-IPT460 with the A4Q-T2N-V2.03.05-NB firmware, you only need to select the STS-IPT480 device in Intellect and don't need to update the firmware.\n2) When configuring telemetry devices in Intellect, choose the protocol that the newly plugged camera (Pelco-D, DynaColor, Panasonic-850 etc.) supports. Do not choose the \"IPCamera\" protocol. Then specify the Baud Rate. 3 The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream."]
["Smartec","Smartec STS-IPT480 encoder","Encoder ","A4Q-T2N-V2.03.05-NB","4",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720х480(NTSC)","720х576(PAL)/720х480(NTSC)","352х288(PAL)/352х240(NTSC)","+",null,"+","-","+","+","+",null,"-","-","1. У устройства 4 канала, но видео можно получать одновременно только с одного (любого) канала, либо сразу со всех четырех (так называемый Quad-режим) В Intellect это будет соответственно каналы 1-4 и 5-ый для Quad-режима\n \n\n2. При настройке телеметрии в настройках Intellecta протокол следует выбирать не \"IPCamera\", а тот, по-которому работает подключенная поворотная камера (Pelco-D, DynaColor, Panasonic-850 проч.). Также необходимо указывать настройку \"Скорость\" (Boud Rate)\n\n3. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n ","1) The device offers 4 channels. Video is streamed either via any one of the channels or via all of them in the s.c. Quad mode. The corresponding channels in Intellect will be 1-4 and 5 for the Quad mode. When configuring telemetry devices in Intellect, choose the protocol that the newly plugged camera (Pelco-D, DynaColor, Panasonic-850 etc.) supports. Do not choose the \"IPCamera\" protocol. Then specify the Baud Rate. 3. The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream.\n "]
["Smartec","Smartec STS-IPT880 encoder","Encoder ","A8D-R2N-V2.02.07-NB","8",{"$nulls":3},"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)","720х576(PAL)/720x480(NTSC)","352х288(PAL)/352x240(NTSC)","+",null,"+","-","+","+.","+",null,"-","-","1. При настройке телеметрии в настройках Intellecta протокол следует выбирать не \"IPCamera\", а тот, по-которому работает подключенная поворотная камера (Pelco-D, DynaColor, Panasonic-850 проч.). Также необходимо указывать настройку \"Скорость\" (Boud Rate)\n2. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n3.Луч работает только по активному каналу (т.е. если видео идет только по 1-му каналу, то и лучи будут работать только те, которые относятся к 1-му каналу)\n","1) When configuring telemetry devices in Intellect, choose the protocol that the newly plugged camera (Pelco-D, DynaColor, Panasonic-850 etc.) supports. Do not choose the \"IPCamera\" protocol. Then specify the Baud Rate. \n2 The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream.\n3. The sensor works only with the active channel i.e. if video is streamed via channel 1, then only the sensors allocated for channel 1 will work.\n"]
["Smartec_G2","Smartec STC-IPM3095A/3","Camera ","X.2.1.8","1",null,null,"+","+",{"$nulls":3},"1280x960","640x480","320x240","+",null,"+.","+.",null,"+","+",null,"-","+","1. при разрешении 1280х960 максимальный fps равен 12-15 fps, ограничение самой камеры\n2. автоматический поиск устройства в сети в ПО ITV  не может быть реализован ","1) With the 1280x960 resolution, the max. frame rate is 12-15 fps; this is a limitation of the camera itself in the AxxonSoft software, the automatic search for the device cannot be implemented. "]
["Smartec_G2","Smartec STC-IPM3096A/3","Camera ","X.2.1.10","1",null,null,"+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4)","640x480","320x240","+",null,"+.","-",null,"+","+",null,"-","+","1. при разрешении 1280х960 максимальный fps равен 12-15 fps, ограничение самой камеры","1. With the 1280x960 resolution, the max. frame rate is12-15 fps; this is a limitation of the camera itself"]
["Smartec_G2","Smartec STC-IPM3097A / STC-IPM3597A","Camera ","gWT8300036NO0001 V21 1202024F","1",null,null,"+","+","+",null,null,"2048x1536 (MJPEG, H264) / 1920x1072 (MPEG4)","1920x1072 (MJPEG) / 1280x1024 (H264, MPEG4)","720x480","+",null,"-",null,"-","-","-",null,"-","+","Получать несколько независимых потоков с камеры нельзя. Потоки в AxxonNext/Next по сути представляют собой различные профили получения видео.Настройки видео применяются с небольшой задержкой (~ 5-10 секунд)Максимальная частота кадров в MJPEG - 15 fps в минимальном разрешении и 5-8 fps в высоких разрешениях.Устройство находится поиском как Onvif, но работать через Onvif не будет.Прошивка gWT8300036NO0001 V21 1202024F: в потоках 5 и 6 в кодеках mpeg4.1 и h264.1 в разрешении QVGA видео идет в 320х240.","No multistreaming for that camera. Video streams in AN are basically different profiles for video. Video settings are applied with a delay of 5 to 10 sec. Max frame rate in MJPEG is 15 fps under min. resolution and 5 to 8 fps with high resolution. Device discovery mistakenly shows this device as ONVIF ready. Firmware gWT8300036NO0001 V21 1202024F: video is streamed at 320 [240 when via channels 5 and 6 and coded in MPEG4 and H264 with the QVGA resolution."]
["Smartec_G2","Smartec STC-IPM3595A/3","Camera ","X.1.15.1","1",null,null,"+","+",{"$nulls":3},"1280x960(MJPEG)","640x480","320x240","+",null,"+","-",null,"+","+",null,"-","+","1. при разрешении 1280х960 максимальный fps равен 12-15 fps, ограничение самой камеры\n2. автоматический поиск устройства в сети в ПО ITV  не может быть реализован \n","1) With the 1280x960 resolution, the max. frame rate is12-15 fps; this is a limitation of the camera itself\n2. in the AxxonSoft software, the automatic search for the device cannot be implemented. \n"]
["Sony","Sony SNC-CH110 / SNC-DH110(T)","Camera ","1.78.00","1",null,null,"+","+","+",null,null,"1280x960","1024x768","640x480","+","+",null,null,"+","+",null,null,"motion detection; ","+","1. При максимальных разрешениях и качестве камера имеет ограничения, накладываемые на частоту кадров (см. инструкцию к камере)\n2. Во втором потоке камера имеет ограничения на частоту кадров и набор разрешений в зависимости от текущих настроек первого потока (см. инструкцию к камере)\n3. При изменении \"ТВ-стандарта\" происходит сброс на значения по умолчанию настроек видео, встроенного детектора \"Интеллектуальное обнаружение\", предустановок телеметрии.\n4. Изменение \"ТВ-стандарта\" происходит с задержкой (~1 минута) - камера перезагружается.\n5. Цифровая PTZ-телеметрия камеры работает только при выбранном \"ТВ-стандарте\" \"PAL, 4:3\"\n6. Встроенный детектор \"Интеллектуальное обнаружение\" будет работать при использовании только нулевого видеопотока и только при выключенной \"Цифровой PTZ-телеметрии\"\nПри включенной \"Цифровой PTZ-телеметрии\" максимальное разрешение - \"768x576\"\n7. При включении двух стриммингов и выборе для обоих кодека MJPEG камера перестает присылать видео по второму стриммингу. Проблема самой камеры с текущей прошивкой 1.27.02","1. For max. resolutions and video quality settings the camera is limited in fps. (see the camera manual).\n For stream 2 the camera fps and resolution limitation depend on stream 1 settings. (see the camera manual). \n3. When you change the TV standard, video parameters, telemetry presets and Next Detection settings are reset to the default values.\n4. Changes to TV standard are applied with a delay (around 1 min) while the camera is rebooted.\n5. Digital PTZ-works only with PAL 4:3\n6. Embedded Next Detection works only with stream 0 and when Digital PTZ is disabled \nIf the Digital PTZ is enabled, then the max resolution is \"768x576\"\n7. If you choose MJPEG for both streams In the dual stream mode, the camera fails to feed stream 2. This is a bug of the camera's current firmware 1.27.02"]
["Sony","Sony SNC-CH120 / SNC-CH160","Camera ","1.78.00","1",null,null,"+","+","+",null,null,"1280x1024","1024x768","640х480","+","+",null,null,"+","+","+",null,"motion detection; onboard tracker","+","1. Камера не поворотная, но есть цифровая телеметрия (solidPTZ)\n2. При включении телеметрии на камеру накладывается ограничение по разрешению (макс. разрешение - 768х576). 3 Для включения мультикаста в Интеллекте необходимо открыть редактор реестра, перейти по пути \\HKEY_LOCAL_MACHINE\\SOFTWARE\\Wow6432Node\\ITV\\INTELLECT\\Video\\ создать там каталог TransportProtocols и в этом каталоге создать строковый параметр SonyIpela со значением multicast \n\n","1. This is not a PTZ camera, but it has digital telemetry (solidPTZ) 2. When you enable telemetry, the camera's resolution will be limited to ( max.768х576)."]
["Sony","Sony SNC-CH140 / SNC-CH180","Camera ","1.77.00","1",null,null,"+","+","+",null,null,"1280x1024","640x480","320x240","+","+","+.","+","+","+","+",null,"motion detection; ","+","1. При изменение настроек встроенного детектора устанавливается максимальное разрешение","1. If you change the embedded detection settings, then the max. resolution is applied."]
["Sony","Sony SNC-CH210 / SNC-DH210(T)","Camera ","1.78.00","1",null,null,"+","+","+",null,null,"MJPEG: 2048x1536; H.264/MPEG4: 1600х1200","1024x768","640x480","+","+",null,null,"+",{"$nulls":3},"motion detection; onboard tracker","+","1. При максимальных разрешениях и качестве камера имеет ограничения, накладываемые на частоту кадров (см. инструкцию к камере)\n2. Во втором потоке камера имеет ограничения на частоту кадров и набор разрешений в зависимости от текущих настроек первого потока (см. инструкцию к камере)\n3. При изменении \"ТВ-стандарта\" происходит сброс на значения по умолчанию настроек видео, встроенного детектора \"Интеллектуальное обнаружение\", предустановок телеметрии.\n4. Изменение \"ТВ-стандарта\" происходит с задержкой (~1 минута) - камера перезагружается.\n5. Цифровая PTZ-телеметрия камеры работает только при выбранном \"ТВ-стандарте\" \"PAL, 4:3\"\n6. Встроенный детектор \"Интеллектуальное обнаружение\" будет работать при использовании только нулевого видеопотока и только при выключенной \"Цифровой PTZ-телеметрии\"\n7. При включенной \"Цифровой PTZ-телеметрии\" максимальное разрешение - \"768x576\"","1. For max. resolutions and video quality settings the camera is limited in fps. (see the camera manual). For stream 2 the camera fps and resolution limitation depend on stream 1 settings. (see the camera manual). \n3. When you change the TV standard, video parameters, telemetry presets and Next Detection settings are reset to the default values.\n4. Changes to TV standard are applied with a delay (around 1 min) while the camera is rebooted.\n5. Digital PTZ works only with PAL 4:3 \n6. Embedded Next Detection works only with stream 0 and when Digital PTZ is disabled.\n7. If the Digital PTZ is enabled, then the max resolution is \"768x576\""]
["Sony","Sony SNC-CH220 / SNC-CH260","Camera","1.80.00","1",null,null,"+","+","+",null,null,"1920x1440 / 1920x1080","640x480","320x240","+","+","-","-","+","-","-","-","motion detection; tampering detection; on-board tracker","+","Максимально доступное разрешение (1920x1080 / 1920x1440) зависит от значения настройки Maximum image size в веб-интерфейсе. При максимальных разрешениях и качестве камера имеет ограничения, накладываемые на частоту кадров (см. инструкцию к камере). Во втором потоке камера имеет ограничения на частоту кадров и набор разрешений в зависимости от текущих настроек первого потока (см. инструкцию к камере). Изменение \"ТВ-стандарта\" происходит с задержкой (~1 минута) - камера перезагружается. Цифровая PTZ-телеметрия камеры работает только при выбранном \"ТВ-стандарте\" \"PAL, макс. разрешение 1920х1440\". Встроенный детектор \"Интеллектуальное обнаружение\" будет работать при использовании только нулевого видеопотока и только при выключенной \"Цифровой PTZ-телеметрии\" ","Maximum available resolution (1920x1080 / 1920x1440) depends on from Maximum image size setting in web interface of device. With maximum resolution and quality value of camera, frame rate setting has limitations (look into camera's instructions). At second stream, it is limitations of frame rate and permissions sets, it depends on from current settings of first stream (look into instructions).  \"TV standard\" changing is delayed (about 1 minute) - the camera is rebooting. Digital PTZ: camera's telemetry works only when selected TV standard is PAL and resolution 1920x1440 resolution .\" Built-in detector \"Intelligent detection\" will work only with selected zero stream of video and switched off \" Digital PTZ- telemetry \"."]
["Sony","Sony SNC-CH240 / SNC-CH280","Camera","1.77.00","1","-",null,"+","+","+",null,null,"1920x1440","1024x768","640x480","+","+","-","-","+","-","-",null,"motion detection; inbuilt tracker","+","1. У камеры цифровая телеметрия - ePTZ \n2. Для того, чтобы на камере были доступны разрешения больше 1920*1080, нужно в веб-интерфейсе на вкладке Installation выбрать max image size 1920*1440\n","1. The camera offers digital telemetry (ePTZ) 2. To make camera resolutions over 1920x1080 available, select max image size 1920x1440 on the Installation tab  in the camera web interface. ","improved"]
["Sony","Sony SNC-CM120","Camera ","1.10","1",null,null,"+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4)","960x720(MJPEG)/384x288(MPEG-4)","640x480(MJPEG)/320x240(MPEG-4)","+",null,"+","-",null,"+","+",null,"motion detection; onboard tracker","+","1) реле требуют предварительного включения в web-интерфейсе камеры\n2) у камеры есть функция Light Funnel\n - при включенной функции, значения fps в Intellect максимум 30, но нельзя выставить мегапиксельное разрешение в потоке MJPEG\n - при выключеной функции значения fps в Intellect максимум 10, но можно выставить мегапиксельное разрешение в потоке MJPEG\n","1) Enable the relay in the camera web interface \n2) the camera offers the Light Funnel function. \nIf you enable it, the max. fps in Intellect will be 30, and no mega pixel resolutions in MJPEG. \nIf you disable it, the max fps will be 10, but you can set the mega pixel resolution in MJPEG.\n"]
["Sony","Sony SNC-CS10Р/11P","Camera ","1.06","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",null,"+.","+.",null,"+","+",null,"-","+"]
["Sony","Sony SNC-CS20","Camera ","1.10","1",null,null,"+","+",{"$nulls":3},"640x480","640x480(MJPEG) / 384x288(MPEG-4)","320x240","+",null,"+","-",null,"+","+",null,"motion detection; onboard tracker","+"]
["Sony","Sony SNC-CS50P","Camera ","2.32","1",null,null,"+","+","+",null,null,"640x480","384x288","320x240","+",null,"+","-",null,"+","+",null,"motion detection; onboard tracker","+","1. У самой камеры в родном вебе есть настройка Image mode и три положения для неё (Field, Frame и Auto). Frame – для неподвижных изображений, Field – для движущейся картинки, Auto –камера сама распознает режим .  Поэтому если в Intellect вы увидите эффект похожий на интерлейсинг (лесенка) – это не баг скорее всего, просто проверьте параметр Image mode в родном вебе\n ","1) The camera's web interface offers 3 settings (Field, Frame and Auto) in the Image mode. Frame - is for still images, Filed - is for video and Auto is when the camera switches to the appropriate mode itself.  For that reason if you see saw-tooth / interlacing artifacts, check the Image mode settings.\n "]
["Sony","Sony SNC-CX600(W)","Camera","1.9.2","1","-",null,"+",null,"+",null,null,"1280x720","704x576","640x480","+",null,"+","-","+",null,null,"-","motion detection; inbuilt tracker","+","На камере есть встроенный детектор лиц.","There is an on-board Face detection tool.","improved"]
["Sony","Sony SNC-DF40P","Camera ","1.18","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",null,"+","-",null,"+","+",null,"-","-"]
["Sony","Sony SNC-DF70P","Camera ","1.18","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",null,"+","-",null,"+","+",null,"-","-"]
["Sony","Sony SNC-DF80P","Camera ","1.22","1",null,null,"+","+","+",null,null,"640x480","384x288","320x240","+",{"$nulls":7},"motion detection; onboard tracker","+","1. Ползунок \"Качество\" для MPEG и H.264 регулирует bit rate видеопотока\n2. Звук, Лучи и Реле не проверены, т.к. нет необходимых для этого разъемов.\n3. При H.264 сама камера выдает только 8-12 fps","1. For MPEG-4 and H.264 use the Quality slider to adjust the video stream bit rate. \n2. Sound, Sensors and Relays haven't been checked so far since there are no suitable connectors at the moment.\n3. With H.264, the camera is capable of running at 8-12 fps max."]
["Sony","Sony SNC-DF85P","Camera ","1.20","1",null,null,"+","+","+",null,null,"640x480","640x480","320x240","+",null,null,"-",{"$nulls":4},"motion detection; onboard tracker","+","ауди, лучи и реле не проверены т.к. с камерой не предоставили нужных переходников","Sound, Sensors and Relays haven't been checked so far since there are no no adapters for that camera in the test kit."]
["Sony","Sony SNC-DH120(T) / SNC-DH160 ","Camera","1.80.00","1",null,null,"+","+","+",null,null,"1280x1024","1024x768","640x480","+","+","-","-","+","-","-","-","motion detection; tampering detection; on-board tracker","+","Разрешение на втором потоке должно быть меньше, чем на первом. Для включения мультикаста в Интеллекте необходимо открыть редактор реестра, перейти по пути \\HKEY_LOCAL_MACHINE\\SOFTWARE\\Wow6432Node\\ITV\\INTELLECT\\Video\\ , создать каталог TransportProtocols и в этом каталоге создать строковый параметр SonyIpela со значением \"multicast\".","The resolution for stream 2 should be lower than or equal to one for stream. To use the camera in Axxon Intellect with multicast you need to launch registry editor, move to \\HKEY_LOCAL_MACHINE\\SOFTWARE\\Wow6432Node\\ITV\\INTELLECT\\Video\\, create directory TransportProtocols and create there link parameter SonyIpela with value multicast "]
["Sony","Sony SNC-DH140(T) / SNC-DH180 ","Camera ","1.73.01","1",null,null,"+","+","+",null,null,"1280x1024","1024x768","640x480","+","+","+","+","+",{"$nulls":3},"motion detection; onboard tracker","+"," 1. Максимальное разрешение в Intellect зависит от настройки Maximum image size"," 1. The max. resolution in AxxonSoft Intellect depends on the Maximum Image Size setting."]
["Sony","Sony SNC-DH240(T) / SNC-DH280","Camera ","1.73.01","1",null,null,"+","+","+",null,null,"1920x1440","1024x768","640x480","+","+",null,null,"+",{"$nulls":3},"motion detection; onboard tracker","+","1. У камеры цифровая телеметрия - ePTZ\n2. Для того, чтобы на камере были доступны разрешения больше 1920*1080, нужно в вебе на вкладке Installation выбрать max image size 1920*1440\n3. Видео в ПО Intellect с \"Полным\" разрешением будет только если в веб-интерфейсе на вкладке Installation выбрать max image size 1920*1440","1. The camera offers digital telemetry (ePTZ)\n2. To make camera resolutions over 1920x1080 available, select max image size 1920x1440 on the Installation tab in the camera web interface. 3. Intellect offers the Full resolution video only if you select max image size 1920x1440 on the Installation tab in the camera web interface."]
["Sony","Sony SNC-DM110","Camera ","1.10","1",null,null,"+","+",{"$nulls":3},"1280x960(MJPEG) / 640x480(MPEG-4)","960x720(MJPEG) / 384x288(MPEG-4)","640х480(MJPEG) / 320х240(MPEG-4)","+",null,"+","-","+","+","+",null,null,"+","1. У камеры есть функция Light Funnel:\n - при включенной функции, значения fps в Intellect максимум 30, но нельзя выставить мегапиксельное разрешение в потоке MJPEG\n - при выключеной функции значения fps в Intellect максимум 15, но можно выставить мегапиксельное разрешение в потоке MJPEG\n2. При включении функции Light Funnel нельзя менять разрешение MJPEG-видео через Intellect\n3. Реле требуют предварительного включения в web-интерфейсе камеры\n4. Камера не поворотная, но есть solidPTZ","1. The camera has the Light Funnel function:\n If you enable it, the max. fps in Intellect will be 30, and no mega pixel resolutions in MJPEG. \nIf you disable it, the max fps will be 15, but you can set the mega pixel resolution in MJPEG. \n2. If enabled, Light Funnel makes it impossible to change MJPEG resolution via Intellect. \n3. Enable the relay in the camera web interface \n4. This is not a PTZ camera, but it has digital telemetry (solidPTZ)."]
["Sony","Sony SNC-DM160","Camera ","1.11","1",null,null,"+","+",{"$nulls":3},"1280x960(MJPEG) / 640x480(MPEG-4)","960x720(MJPEG) / 384x288(MPEG-4)","640х480(MJPEG) / 320х240(MPEG-4)","+",{"$nulls":7},"motion detection; onboard tracker","+","1. у камеры есть функция Light Funnel:\n- при включении функции нельзя менять разрешение MJPEG-видео через Intellect\n- при включенной функции значения fps в Intellect максимум 30, но нельзя выставить мегапиксельное разрешение в потоке MJPEG\n- при выключеной функции значения fps в Intellect максимум 15, но можно выставить мегапиксельное разрешение в потоке MJPEG \n2. при включении функции Light Funnel нельзя менять разрешение MJPEG-видео через Intellect","1. The camera has the Light Funnel function:\nIf you enable it, the max. fps in Intellect will be 30, and no mega pixel resolutions in MJPEG. If you disable it, the max fps will be 15, but you can set the mega pixel resolution in MJPEG. \n2. If enabled, Light Funnel makes it impossible to change MJPEG resolution via Intellect. "]
["Sony","Sony SNC-EB520 / SNC-EM521","Camera ","1.78.00","1",null,null,"+","+","+",null,null,"800x600","640x480","320x240","+","+",null,null,"+","+","+",null,"motion detection, tampering detection; onboard tracker","+","1. Чтобы работала цифровая телеметрия, нужно включить соответствующую настройку объекта камеры.\n2. Разрешение на втором потоке не может быть больше, чем на первом.","1. To make digital PTZ work, enable the relevant setting for the camera object.\n2. The resolution for stream 2 should be lower than or equal to one for stream 1."]
["Sony","Sony SNC-EB600(B) / SNC-EM600 / SNC-EM601 / SNC-EM602R","Camera","1.9.2","1","-",null,"+",null,"+",null,null,"1280x1024","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":3},"-","+","Настройка \"Поворот видеоизображения\" актуальна только для камеры SNC-EM600","Video rotation setting is relevant only for SNC-EM600 camera.","improved"]
["Sony","Sony SNC-EM520","Camera ","1.78.00","1",null,null,"+","+","+",null,null,"800x600","640x480","320x240","+","+",null,null,"+",{"$nulls":4},"+","1. Чтобы работала цифровая телеметрия, нужно включить соответствующую настройку объекта камеры.\n2. Разрешение на втором потоке не может быть больше, чем на первом. ","1. To make digital PTZ work, enable the relevant setting for the camera object.\n2. The resolution for stream 2 should be lower than or equal to one for stream 1."]
["Sony","Sony SNC-EP520, SNC-EP521, SNC-ER520, SNC-ER521","Camera ","1.78.00 ","1",null,null,"+","+","+",null,null,"720x576","640x480","320x240","+","+","+","+","+","+","+",null,"motion detection, tampering detection","+","1. Разрешение на втором потоке не может быть больше, чем разрешение на первом потоке.\n2. При изменение настроек встроенного детектора устанавливается максимальное разрешение","1. The resolution for stream 2 should be lower than or equal to one for stream 1.\n2. If you change the embedded detection settings, then the max. resolution is applied."]
["Sony","Sony SNC-EP550 / SNC-ER550 / SNC-ZR550 / SNC-ZP550","Camera ","v1.70.00","1",null,null,"+","+","+",null,null,"1280x720","800x600","640x480","+","+",null,null,"+",{"$nulls":3},"onboard tracker","+"]
["Sony","Sony SNC-ER580 / SNC-EP580 / SNC-ER585 / SNC-ER585H ","Camera ","1.78.00","1",null,null,"+","+","+",null,null,"1920x1080","1024x768","640x480","+","+",null,null,"+",{"$nulls":3},"motion detection; ","+","1. Чтобы заработал встроенный детектор движений нужно отключить 2 поток, Letterbox и Cropping в веб-интерфейсе\n2. При изменении настроек встроенного детектора устанавливается максимальное разрешение.\n3. Значение частоты FPS зависит от разрешения","1. To enable embedded motion detection, you should disable stream 2, Letterbox and Cropping in the web interface.\n2. If you change the embedded detection settings, then the max. resolution is applied.\n3. FPS value depends on resolution"]
["Sony","Sony SNC-P1","Camera ","1.30","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",null,"+.","+.",null,"+","+",null,"-","+","При разрешении 640х480 максимально 15-18 fps","With the 640x480 resolution, the camera allows 15-18 fps max."]
["Sony","Sony SNC-P5","Camera ","1.29","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","+","1. У камеры нет настройки фокуса. Поэтому в Intellect не будут работать кнопки Focus+, Focus-, AutoFocus\n2. При разрешении 640х480 максимально 15-18 fps","1. The camera doesn't offer Focal Length adjustment. This is why in Intellect the Focus+, Focus-, AutoFocus buttons will be disabled.\n2. With the 640x480 resolution, the camera allows 15-18 fps max."]
["Sony","Sony SNC-RH124 / SNC-RH164","Camera ","1.73.00","1",null,null,"+","+","+",null,null,"1280x720","800x600","640x480","+","+",null,null,"+",{"$nulls":3},"motion detection; onboard tracker","+"]
["Sony","Sony SNC-RS44N/P, SNC-RS46N/P, SNC-RS84N/P, SNC-RS86N/P","Camera ","1.73.00","1",null,null,"+","+","+",null,null,"720x576 (PAL) / 720x480 (NTSC)","640x480","320x240","+","+",null,null,"+",{"$nulls":3},"motion detection; onboard tracker","+","1. SNC-RS44/46/84/86N и SNC-RS44/46/84/86P отличаются друг от друга ТВ-стандартом.","1. SNC-RS44/46/84/86N differs from SNC-RS44/46/84/86P by the TV standard they use."]
["Sony","Sony SNC-RX530N/P","Camera ","3.01","1",null,null,"+","+","+",null,null,"640x480","384x288","320x240","+",{"$nulls":3},"+.",{"$nulls":3},"motion detection; onboard tracker","+"]
["Sony","Sony SNC-RX550P","Camera ","3.10","1",null,null,"+","+","+",null,null,"640x480","384x288","320x240","+",null,"+",null,"+","+","+",null,"motion detection; onboard tracker","+","1. Реле требуют предварительного включения в web-интерфейсе камеры \n2. добавилось новое разрешение 704x576 ( после прошивки на 3.10, если прошивка ниже, то максимальное (полное) разрешение 640*480) - ждем его добавления и выбора в качестве полного разрешения\n3. Настройка качества видео есть только для потока MJPEG (в web-интерфейсе камеры так же)","1. Enable the relay in the camera web interface. 2. New 704x576 resolution is available now after firmware update to 3.10. \nFor older versions the max. resolution is 640x480. We are expecting it to be added and being available for the Full resolution choice. \n3. You can configure video quality only for MJPEG streams (same in camera interface)"]
["Sony","Sony SNC-RX570P","Camera ","3.10","1",null,null,"+","+","+",null,null,"640x480","640x480","320x240","+",null,"+","-","+","+","+",null,"motion detection; onboard tracker","+","1. Видео в формате H.264 может отображаеться с максимальной частотой 8-15 fps (в зависимости от Bit rate видеопотока). Ограничение самой камеры.\n2. Чтобы можно было управлять настройкой фокуса, необходимо в веб-интерфейсе камеры выставить Focus mode=Manual","1. H.264 video is available only with the 8-15 fps max. depending on the bit rate. This is a limitation of the camera itself.\n2. To be able to adjust the focal length, select Manual in the Focus mode in the camera web interface."]
["Sony","Sony SNC-RZ25P","Camera ","1.40","1",null,null,"+","+",{"$nulls":3},"640x480","480x360","320x240","+",null,"+.","+.","+","+","+",null,"-","+","1. При разрешении 640х480 достижимы максимально 15-18 fps","1) With the 640x480 resolution, the camera allows 15-18 fps max."]
["Sony","Sony SNC-RZ30P/N","Camera ","3.14","1",null,null,"+",{"$nulls":4},"736х544","640x480","320x240","+",{"$nulls":3},"+","+","+",null,"-","-","1. Чтобы работало управление фокусом, в веб-интерфейсе необходимо выставить Focus mode=Manual. \n2. Лучи следует замыкать под напряжением","1. To be able to adjust the focal length, select Manual in the Focus mode in the camera web interface. \n2. Close the sensors when they are energized."]
["Sony","Sony SNC-RZ50P","Camera ","2.42","1",null,null,"+","+","+",null,null,"640x480","384x288","320x240","+",null,"+","-","+","+","+",null,"motion detection; onboard tracker","+","1. Ползунок \"Качество\" для MPEG и H.264 регулирует bit rate видеопотока\n2. При H.264 сама камера выдает только 8-12 fps","1. For MPEG-4 and H.264 use the Quality slider to adjust the video stream bit rate. \n2. With H.264, the camera is capable of running at 8-12 fps max."]
["Sony","Sony SNC-VB600 / SNC-VM600 / SNC-VM601 / SNC-VM602R","Camera","1.12.0","1",null,null,"+","-","+","-","-","1280x1024","1024x768","640x480","+","-","+","+","+","+","+","-","motion detection; tampering detection; others; on-board tracker","+","Значение 60 FPS для Интеллект применяется через веб, а в AN включением настройки \"режим высокой частоты кадров\"Прочие встроенные детекторы:Детектор лиц","You can set 60 fps for Intellect in the camera's web interface, while in Axxon Next you have to enable high frame rate mode to get 60 fps. Other on-board detection tools: Face detection tool."]
["Sony","Sony SNC-VB600B / SNC-VM600B / SNC-VM601B","Camera","1.12.0","1",null,null,"+","-","+","-","-","1280x1024","1024x768","640x480","+","-","+","+","+","+","+","-","motion detection; tampering detection; others; on-board tracker","+","Прочие встроенные детекторы:Детектор лиц","Other on-board detection tools: Face detection tool"]
["Sony","Sony SNC-VB630 / SNC-VB635 / SNC-VM630 / SNC-VM631 / SNC-VM632R","Camera","1.9.2","1","-",null,"+",null,"+",null,null,"1920x1080","720x576","640x480","+",null,"+",null,"+","+","-","-","motion detection; tampering detection; other detectors; inbuilt tracker","+","Значение 60 FPS для Интеллект применяется через веб, а в AN включением настройки \"режим высокой частоты кадров\"Прочие встроенные детекторы:Детектор лиц","You can set 60 fps for Intellect in the camera's web interface, while in Axxon Next you have to enable high frame rate mode to get 60 fps. Other on-board detection tools: Face detection tool.","improved"]
["Sony","Sony SNC-Z20P","Camera ","1.06","1",null,null,"+",{"$nulls":4},"736х544","640x480","320x240","+",{"$nulls":3},"+","+","+",null,"-","-","Просто в качестве информации:\n1. Камера не PTZ, т.е. не вращается. Но есть оптический зум и фокус.\n2. В родном вебе должен стоять Focus mode=Manual, чтобы можно было управлять фокусом\n","FYI\n1. This is not a PTZ camera. But it has optical zoom and focus. \n2. To be able to adjust the focal length, select Manual in the Focus mode in the camera web interface. 2.\n"]
["Sony","Sony SNT-EX154","Encoder ","1.77.03 ","1",null,null,"+","+","+",null,null,"704x576","640x480","320x240","+","+",{"$nulls":6},"onboard tracker","+","1. Устройство представляет из себя 4-канальный сервер, но у каждого из каналов - свой сетевой адрес.","1. This is a 4 channel server, where each channel has its own IP address."]
["ST","ST ST-170 IP","Camera","H18C01-B.771","1","-",{"$nulls":3},"+",null,null,"1280x720","1280x720","640x360","+",{"$nulls":7},"-","-","В продукте, для подключения камеры, необходимо ввести номер порта 9000 (значение по-умолчанию для камеры)","To connect a camera, specify 9000 port (default value for the camera).","improved"]
["ST","ST ST-171 IP / ST-172 IP / ST-181 IP / ST-182 IP","Camera","H18C01-C.889","1","-",{"$nulls":3},"+",null,null,"1920x1080","1920x1080","480x270","+",{"$nulls":7},"-","-","В продукте, для подключения камеры, необходимо ввести номер порта 9000 (значение по-умолчанию для камеры)","To connect a camera, specify 9000 port (default value for the camera).","improved"]
["ST","ST ST-180 IP","Camera","H18C01-B.774","1","-",{"$nulls":3},"+",null,null,"1280x960","1280x960","640x480","+",{"$nulls":6},"-","-","-","В продукте, для подключения камеры, необходимо ввести номер порта 9000 (значение по-умолчанию для камеры)","To connect a camera, specify 9000 port (default value for the camera).","improved"]
["StarDot","NetCam SC 1.3 MP IR","Camera ","1.1.66","1",null,null,"+",{"$nulls":4},"1296x960","1024x768","640x480","+",{"$nulls":4},"-","-",null,"-","+","1. Fps при максимальном разрешении очень сильно зависит от размера фрейма, а размер фрейма в свою очередь зависит от качества,  движения в кадре, освещенности и т.д. У меня fps был от 4 до 12.","1) Frame rate at max. resolution depends heavily on the frame size, which in turn is a function of video quality, motion in the scene and lighting conditions etc. We experienced fps from 4 to 12."]
["StarDot","StarDot SDH300VN / SDH300BN ","Camera ","1.1.78","1",null,null,"+",null,"+",null,null,"2048x1536","1024x768","640x480","+",{"$nulls":8},"+","1. В ПО ITV/Axxon камеры интегрированы как серия \"3MP\"\n2. Для корректной работы двухпоточности в ПО Axxon в настройках обоих потоков должно быть установлено одно и то же значение разрешения ","1. Cameras has been integrated as the series \"3MP\" in Axxon SW.\n2. To work correctly with dual-stream in the Axxon, the same resolution should be set in the settings of both streams."]
["Stream Labs","WaveCam MX","Camera ","Ubicom 2.1.0.0; PNX Bios 2.4.0.0; PNX Main 2.6.1.0","1",{"$nulls":5},"+",null,"768х576(PAL)/640х480(NTSC)","704х544(PAL)/640х480(NTSC)","384х288(PAL)/320x240(NTSC)","+",{"$nulls":8},"-"]
["Stream Labs","WaveCam MX-A","Camera ","Ubicom 2.1.0.0; PNX Bios 2.4.0.0; PNX Main 2.6.1.0","1",{"$nulls":5},"+",null,"768х576(PAL)/640х480(NTSC)","704х544(PAL)/640х480(NTSC)","384х288(PAL)/320x240(NTSC)","+",null,"+","+.",{"$nulls":5},"-"]
["Stream Labs","WaveCam MXE","Camera ","Ubicom 2.1.0.0; PNX Bios 2.4.0.0; PNX Main 2.6.1.0","1",{"$nulls":5},"+",null,"768х576(PAL)/640х480(NTSC)","704х544(PAL)/640х480(NTSC)","384х288(PAL)/320x240(NTSC)","+",{"$nulls":3},"-",{"$nulls":4},"-"]
["Stream Labs","WaveCam MX-M","Camera ","Ubicom 2.1.0.0; PNX Bios 2.4.0.0; PNX Main 2.6.1.0","1",{"$nulls":5},"+",null,"768х576(PAL)/640х480(NTSC)","704х544(PAL)/640х480(NTSC)","384х288(PAL)/320x240(NTSC)","+",{"$nulls":8},"-","Для корректной работы устройства в ПО ITV рекомендуется в настройках камеры поле декомпрессор оставлять пустым, либо указывать декомпрессор Wavelet 2. При выборе других декомпрессоров корректная работа ПО не гарантируется. ","For correct works between the device and ITV | AxxonSoft software is recommended to leave fiend decompressor blank in camera settings, or specify the decompressor \"Wavelet\" 2. When choosing other decompressors correct work of Software is not guaranteed."]
["Stream Labs","WaveCam Q1","Camera ","Ubicom 1.6.5.1\\PNX Bios 1.6.2.0\\PNX Main 1.6.5.0","1",{"$nulls":5},"+",null,"1280x960","1280x720","1280x720","+",null,"+.",null,"+.","+","+",null,null,"-","1. Ограничение по fps:\n1280x720 - 12 fps1280x960 - 10 fps\n2. Лучи необходимо замыкать под напряжением\n3. Камера сама по себе не поворотная, но имеет RS-485 порт для подключения сторонней поворотной платформы.\n4. Камера не поворотная, но у неё есть оптический зум и фокус, но работает этот фунционал только со спец. объективом, которого у нас сейчас нет. Таким образом данный функционал пока остался непроверенным","1. Frame rate limits:\n1280x720 - 12 fps1280x960 - 10 fps\n2. Close the sensors when they are energized\n3. This is not a PTZ camera, but it has a RS-485 port to connect a third-party pan/tilt drive. \n4. This is not a PTZ camera, but it has optical zoom and focus. However, this functionality requires a special lens, which we do not have at the moment. For this reason, we did not manage to test this functionality"]
["Stream Labs","WaveCam QX","Camera ","Ubicom 1.8.1.0\\PNX Bios 1.6.2.0\\PNX Main 1.8.3.0","1",{"$nulls":5},"+",null,"768х576(PAL)/640х480(NTSC)","704х544(PAL)/640х480(NTSC)","352х272(PAL)/320x240(NTSC)","+",null,"+","-","-","+","+",null,null,"-","1. Лучи необходимо замыкать под напряжением\n2. Камера сама по себе не поворотная, но имеет RS-485 порт для подключения сторонней поворотной платформы.\n3. Камера не поворотная, но у неё есть оптический зум и фокус, но работает этот фунционал только со спец. объективом","1. Close the sensors when they are energized\n2. This is not a PTZ camera, but it has a RS-485 port to connect a third-party pan/tilt drive.\n3. This is not a PTZ camera, but it has optical zoom and focus. However, this functionality requires a special lens. "]
["Stream Labs","WaveServer 1501A encoder","Encoder ","Ubicom 2.0.0.0; PNX Bios 2.0.3.0; PNX Main 2.3.0.0","1",{"$nulls":5},"+",null,"768х576(PAL)/640х480(NTSC)","704х544(PAL)/640х480(NTSC)","352x272(PAL)/320x240(NTSC)","+",null,"+","+.","+","+","+",null,null,"-","Для того, чтобы в Интеллект заработал аудио-выход, нужно присвоить параметру \"Частота дискретизации\" значение \"16000\". Для корректной работы устройства в ПО ITV рекомендуется в настройках камеры поле декомпрессор оставлять пустым, либо указывать декомпрессор Wavelet 2. При выборе других декомпрессоров корректная работа ПО не гарантируется. ","To activate the audio output in Intellect, set Sampling Rate at 16000. For correct works between the device and ITV | AxxonSoft software is recommended to leave fiend decompressor blank in camera settings, or specify the decompressor \"Wavelet\". When choosing other decompressors correct work of Software is not guaranteed."]
["Stream Labs","WaveServer 1504R encoder","Encoder ","Ubicom 0.8.0.0; PNX BIOS 0.8.1.0; PNX Main 1.4.0.0","4",{"$nulls":5},"+",null,"768x576(PAL) / 640x480(NTSC)","704x544(PAL) / 640x480(NTSC)","352x272(PAL) / 640x480(NTSC)","+",null,"+",{"$nulls":6},"-","1. Если настроен один канал, то у него 25 fps. Если задействован мультиплекс(т.е. два или более каналов), то 16 fps на все каналы - это значит, если два канала, то на каждый приходится 16/2=8 fps, если четыре канала, то на каждый приходится 16/4=4 fps","1. If only one channel is enabled, its max. frame rate is 25 fps. If multiplex is enabled (that is, two channels or more), you have 16 fps for all the channels - this mean: if you have two channels, each gets 16/2=8 fps, if you have four channels, each gets 16/4=4 fps"]
["Stream Labs","WaveServer 1554 encoder","Encoder ","Ubicom 2.0.0.0 \\ PNX Bios 2.0.3.0 \\ PNX Main 2.3.0.0","4",{"$nulls":5},"+",null,"768x576(PAL) / 640x480(NTSC)","704x544(PAL) / 640x480(NTSC)","384x288(PAL) / 320x240(NTSC)","+",null,"+","+.","+","+","+",null,null,"-","1. Если настроен один канал, то у него 25 fps. Если задействован мультиплекс(т.е. два или более каналов), то 16 fps на все каналы - это значит, если два канала, то на каждый приходится 16/2=8 fps, если четыре канала, то на каждый приходится 16/4=4 fps\n2. Телеметрия в ПО Axxon не реализована. При настройке телеметрии в Intellecte в настройках объекта \"Контроллер телеметрии\" протокол следует выбирать \"в явном виде\" (напр. Peclo-D, Panasonic-850), а не \"IPCamera\" как на большинстве других ip-устройств\nДля корректной работы устройства в ПО ITV рекомендуется в настройках камеры поле декомпрессор оставлять пустым, либо указывать декомпрессор Wavelet 2. При выборе других декомпрессоров корректная работа ПО не гарантируется. \n \n2. При настройке телеметрии в Intellect в настройках объекта \"Контроллер телеметрии\" протокол следует выбирать \"в явном виде\" (напр. Peclo-D, Panasonic-850), а не \"IPCamera\" как на большинстве других ip-устройств\n ","1. If only one channel is enabled, its max. frame rate is 25 fps. If multiplex is enabled (that is, two channels or more), you have 16 fps for all the channels - this mean: if you have two channels, each gets 16/2=8 fps, if you have four channels, each gets 16/4=4 fps\n2. The AxxonSoft software does not implement telemetry\n \n2. When you are configuring telemetry settings in the the Telemetry Controller object in Intellect, choose one of Pelco-D, Panasonic-850 etc. protocols. Do not choose the IPCamera protocol as you do with most other IP devices. \n "]
["Stream Labs","WaveServer 1554H encoder (ONVIF)","Encoder ","0.10.2.0","4",null,null,"+",null,"+",null,null,"768x576","640x480","320x240","+.",null,"+","-","-","-","+.",null,null,"-","1. Устройство выдает 50 fps, эта частота кадров будет \"делиться\" между задействованными каналами\n2. Лучи необходимо замыкать под напряжением\n3. в Intellect настройки \"Кодек\" и \"fps\" применяются одновременно для всех каналов, Axxon Next такого ограничения лишен.\n4. Для получения звука необходимо использовать активный микрофон\n5. Телеметрия реализована через serial port, а serial port в свою очередь не поддерживается ONVIF'ом в нашем ПО. Т.о. телеметрия не работает ни в Axxon Next ни в Intellect\n6. Через ONVIF реализованы только два Луча и два Реле из 4-х и 3-х соответственно имеющихся на самом устройстве","1) If the device is running at 50 fps, then the total fps is distributed between the streams. Close the sensors when they are energized\n3. The Codec and Fps settings are applied simultaneously for all channels in Intellect. Axxon Next let you configure them individually.\n4) Use only active mics to get sound. 5. Telemetry is implemented via serial port. Serial ports are not not ONVIF ready in the AxxonSoft software. So telemetry doesn't work neither in Axxon Next nor in Intellect. 6. Only 2 sensors and 2 relays out of 4 and 3 correspondingly are supported via ONVIF"]
["Stream Labs","WaveServer 1554H encoder","Encoder ","Ubicom 2.4.0.0; PNX Bios 2.5.0.0; PNX Main 2.9.0.0","4",{"$nulls":5},"+",null,"768x576(PAL) / 640x480(NTSC)","704x544(PAL) / 640x480(NTSC)","384x288(PAL) / 320x240(NTSC)","+",null,"+",null,null,"-","+.",null,"-","-","Для корректной работы устройства в ПО ITV рекомендуется в настройках камеры поле декомпрессор оставлять пустым, либо указывать декомпрессор Wavelet 2. При выборе других декомпрессоров корректная работа ПО не гарантируется.\nОграничение 50 fps в сумме на 4 канала.","It is limitation in the amount of 50 fps for 4 channels.For correct works between the device and ITV | AxxonSoft software is recommended to leave fiend decompressor blank in camera settings, or specify the decompressor \"Wavelet\". When choosing other decompressors correct work of Software is not guaranteed."]
["Stream Labs","WaveServer 1554S encoder","Encoder ","Ubicom 2.1.0.0; PNX Bios 2.4.0.0; PNX Main 2.6.1.0","4",{"$nulls":5},"+",null,"768х576(PAL)/640х480(NTSC)","704х544(PAL)/640х480(NTSC)","384х288(PAL)/320x240(NTSC)","+",null,"+","+.","+","+","+",null,null,"-","1. Лучи следует замыкать под напряжением.\n2. Звук только с активными микрофоном и динамиком\n3. ограничение 25 fps суммарно на 4 канала","1. Close the sensors when they are energized\n2. Use only active mic and speakers to get sound. \n3. The max fps is 25 for 4 streams combined."]
["Stream Labs","WaveServer 2554H encoder (Onvif)","Encoder ","PNX BIOS: 2.5.0.0 PNX MAIN: 0.16.1.0 UBICOM: 0.21.0.0","4",null,null,"+.",null,"+.",null,null,"768x576","640x480","320x240","+",null,"+",null,null,"-","+.",null,null,"-","Устройство работает только по протоколу ONVIF.","We checked this device only via Onvif."]
["Stream Labs","WaveServer Enterprise 19' rack","Encoder ","0.34.1","4",{"$nulls":5},"+",null,"768х576(PAL)/640х480(NTSC)","704х544(PAL)/640х480(NTSC)","352х272(PAL)/320x240(NTSC)","+",null,"+",null,"+","+","+",null,null,"-","1. Если настроен один канал, то у него 25 fps. Если задействован мультиплекс(т.е. два или более каналов), то 16 fps на все каналы - это значит, если два канала, то на каждый приходится 16/2=8 fps, если четыре канала, то на каждый приходится 16/4=4 fps\n2. При настройке телеметрии в Intellect в настройках объекта \"Контроллер телеметрии\" протокол следует выбирать \"в явном виде\" (напр. Peclo-D, Panasonic-850), а не \"IPCamera\" как на большинстве других ip-устройств. Для корректной работы устройства в ПО ITV рекомендуется в настройках камеры поле декомпрессор оставлять пустым, либо указывать декомпрессор Wavelet 2. При выборе других декомпрессоров корректная работа ПО не гарантируется. ","1. If only one channel is enabled, its max. frame rate is 25 fps. If multiplex is enabled (that is, two channels or more), you have 16 fps for all the channels - this mean: if you have two channels, each gets 16/2=8 fps, if you have four channels, each gets 16/4=4 fps\n2. When you are configuring telemetry settings in the the Telemetry Controller object in Intellect, choose one of Pelco-D, Panasonic-850 etc. protocols. Do not choose the IPCamera protocol as you do with most other IP devices. Peclo-D, Panasonic-850), а не \"IPCamera\" как на большинстве других ip-устройств"]
["Stretch","Stretch VRC6004 card","Video Capture Board ","SDK 7.4.1","4",null,null,"+","+","+",null,null,"PAL 720x576; NTSC 720x480","PAL 528х384; NTSC 528x320","PAL 352х288; NTSC 352x240","+",{"$nulls":3},"+","+.","+.",null,"+.","-","На одной платформе работает только одна плата Stretch.Для переключения стандартов PAL/NTSC требуется перезапуск ПО ITV.В intellect для корректной работы лучей/реле необходимо подключенное видео.PTZ-устройство подключается через RS485-разъем на дополнительной IO-плате.","Only 1 Stretch card works on the same platform To switch between PAL and NTSC, apply the changes and restart the AxxonSoft software. In Intellect, connect a video channel for sensors and relays to operate properly. Connect PTZ devices via RS485 in the additional IO card."]
["Stretch","Stretch VRC6008 card","Video Capture Board ","SDK 7.4.1","8",null,null,"+","+","+",null,null,"PAL 720х576; NTSC 720x480","PAL 528х384; NTSC 528x320","PAL 352х288; NTSC 352x240","+",null,"+",null,"+","+.","+.",null,"+.","-","На одной платформе работает только одна плата Stretch.Для переключения стандартов PAL/NTSC требуется перезапуск ПО ITV.В intellect для корректной работы лучей/реле необходимо подключенное видео.PTZ-устройство подключается через RS485-разъем на дополнительной IO-плате.","Only 1 Stretch card works on the same platform To switch between PAL and NTSC, apply the changes and restart the AxxonSoft software. In Intellect, connect a video channel for sensors and relays to operate properly. Connect PTZ devices via RS485 in the additional IO card."]
["Stretch","Stretch VRC6404HD card","Video Capture Board ","SDK 7.4.1","4",null,null,"+","+","+.",null,null,"1920x1072","960x528","480x256","+",{"$nulls":3},"+","+","+",null,"-","-","На одной платформе работает только одна плата Stretch. Настройка изображения недоступна из ПО ITV. При изменении разрешения на камере (например, с 1080p на 720p) необходимо перезапустить ПО ITV. ","Only 1 Stretch card works on the same platform. You can't configure video in the AxxonSoft software. After you change the resolution e.g. from 1080 to 720, restart the AxxonSoft software to apply the changes. "]
["Stretch","Stretch VRC6416 card","Video Capture Board ","SDK 7.4.1","16",null,null,"+","+","+",null,null,"PAL 720х576; NTSC 720x480","PAL 528х384; NTSC 528x320","PAL 352х288; NTSC 352x240","+",null,"+",null,"+","+.","+.",null,"+.","-","На одной платформе работает только одна плата Stretch.Для переключения стандартов PAL/NTSC требуется перезапуск ПО ITV.В intellect для корректной работы лучей/реле необходимо подключенное видео.PTZ-устройство подключается через RS485-разъем на дополнительной IO-плате.","Only 1 Stretch card works on the same platform To switch between PAL and NTSC, apply the changes and restart the AxxonSoft software. In Intellect, connect a video channel for sensors and relays to operate properly. Connect PTZ devices via RS485 in the additional IO card."]
["Stretch","Stretch VRC7008L card","Video Capture Board ","SDK 7.4.1","8",null,null,"+","+","+",null,null,"PAL 720х576; NTSC 720x480","PAL 528х384; NTSC 528x320","PAL 352х288; NTSC 352x240","+",null,"+",null,null,"+","+",null,"+.","-","На одной платформе работает только одна плата Stretch.Для переключения стандартов PAL/NTSC требуется перезапуск ПО ITV.В intellect для корректной работы лучей/реле необходимо подключенное видео.","Only 1 Stretch card works on the same platform To switch between PAL and NTSC, apply the changes and restart the AxxonSoft software. In Intellect, connect a video channel for sensors and relays to operate properly. "]
["Stretch","Stretch VRC7016LX card","Video Capture Board ","SDK 7.4.1","16",null,null,"+","+","+",null,null,"PAL 720х576; NTSC 720x480","PAL 528х384; NTSC 528x320","PAL 352х288; NTSC 352x240","+",null,"+",null,"+","+","+",null,"+.","-","На одной платформе работает только одна плата Stretch. Для переключения стандартов PAL/NTSC требуется перезапуск ПО ITV. В intellect для корректной работы лучей/реле необходимо подключенное видео.","Only 1 Stretch card works on the same platform. After you change the resolution e.g. from 1080 to 720, restart the AxxonSoft software to apply the changes. In Intellect, connect a video channel for sensors and relays to operate properly. "]
["Sunell","Sunell SN-IPR54/14ALDN","Camera","v1.6_build044014_216","1","+","3","+",null,"+",null,null,"1920x1080","1920x1080","640x360","-",null,"-","-",{"$nulls":4},"-","-","Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.При смене разрешений для кодека H.264 меняется диапазон значений битрейта. Если при переходе на новое разрешение текущий битрейт не попадает в новый диапазон, то настройка не применяется.Частота опорных кадров задается в секундах и может принимать значения от 1 до 3.","To connect to camera in Axxonsoft, please specify 30001 port. If you change the resolution for the H.264 codec, value of bit rate will be changed. If you select a new resolution, a new bit rate misses the new range, the setting will not be applied. Key frame rate is set in seconds and can have value from 1 to 3.","improved"]
["Sunell","Sunell SN-IPR54/31AKDN","Camera ","v1.6_build044014_148","1",null,null,"+",null,"+",null,null,"2048x1536 / 1920x1080 / 1280x720","2048x1536 / 1920x1080 / 1280x720","640x480 / 1920x1080 / 1280x720 ","-",{"$nulls":8},"-","Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\nНабор разрешений в ПО ITV/Axxon зависит от значения настройки Source Resolution в веб-интерфейсе.\nПри смене разрешений для кодека H.264 меняется диапазон значений битрейта. Если при переходе на новое разрешение текущий битрейт не попадает в новый диапазон, то настройка не применяется.\nДля корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz.","To connect to camera in Axxonsoft SW, please specify 30001 port. Resolution set in ITV | AxxonSoft software depends on setting Source Resolution in web-interface. If you change the resolution for the H.264 codec, value of bit rate will be changed. If you select a new resolution, a new bit rate misses the new range, the setting will not be applied.Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["Sunell","Sunell SN-IPV54/31UDR","Camera ","v1.6_build044014_148","1",null,null,"+",null,"+",null,null,"2048x1536 / from web","2048x1536 / from web","640x480 / from web",{"$nulls":9},"-","Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\nНабор разрешений и значение максимального fps в ПО ITV/Axxon зависит от значения настройки Source Resolution в веб-интерфейсе.\nПри смене разрешений для кодека H.264 меняется диапазон значений битрейта. Если при переходе на новое разрешение текущий битрейт не попадает в новый диапазон, то настройка не применяется.\nДля корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz.","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. The list of resolution in Axxonsoft SW depends on value of Source Resolution in web interface.\n3. When resolution for H.264 is changed, range of bitrate value is also changed. If there's no current bitrate value for new resolution, in this case setting is not applied.\n4. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["Tamron","Tamron 300QV-P-CM","Fisheye Camera","AXXON-TEST-002","1",null,null,"+","+","+",null,null,"640x640 (H.264) / 1280x960 (mjpeg) / 1280x960 (mpeg4)","640x480","320x240","+",null,"+",{"$nulls":6},"+","В ПО ITV при переходе на полное разрешение, на камере происходит переключение профиля камеры с compensated на original.\nВ ПО Axxon для того чтобы получать видео с 3, 4 и 6 потоков, необходимо в веб-интерфейсе камеры для настройки split выбрать соответствующий режим.\n","In SW AxxonSoft, when you change resolution to full value, the camera switches profile from compensated to original.\nIn SW AxxonSoft, to receive video from 3, 4 and 6 streams, you should select the appropriate mode for setting 'Split' in web-interface of the camera."]
["Tantos","Tantos TSi-C211F","Camera"," v3.3.2.1","1",null,null,"+","+","+",null,null,"1920x1080","1024x768","640x480","+",null,"+","-","-","-","-","-","-","+"]
["Tantos","Tantos TSi-SDW211Z22","Camera","v1.6_build044014_213","1",null,null,"+","-","+",null,null,"1920x1080","1920x1080","640x360","-",null,"-","-","+","-","-","-","-","-","Настройка \"Частота опорных\" в Интеллекте задается в секундах и может принимать значения от 1 до 3.","In Axxon Intellect \"Reference rate\" setting is expressed in seconds and can take values ​​from 1 to 3."]
["Tattile","Tattile Vega 2HD / Vega Access / Vega III","Camera ","10.21.2","1",null,null,"+",{"$nulls":4},"from WEB","from WEB","from WEB",{"$nulls":9},"+","1. Данное устройство интегрировано для использования в вертикальном решении Авто-Интеллект.\n2. Устройство присылает следующие метаданные: таймстемп(дата и время),номер, страна, надежность распознавания, скорость, класс траспортного средства, направление, картинка\n3. Настройка устройства производится через веб интерфейс ","1. This device has been integrated for using it in Auto Intellect. \n2. Camera can send to Intellect following metadata: timestamp (date and time), number, country, recognition reliability, speed, vehicle type, direction, picture.\n3. Device should be configure via its web interface. "]
["TBK","TBK DVR PLUS 4","DVR","V2.2.4 build 130702","4",{"$nulls":4},"+",null,null,"704x576","704x288","352x288","+",{"$nulls":8},"-"]
["TEDD_G1","TEDD TCC-IP-4002","Camera ","A1D-220-V3.05.05-NB","1",{"$nulls":3},"+",{"$nulls":3},"640x480","640x480","352x288","+",null,"+","-",{"$nulls":4},"-","-","1.  ползунок \"Качество\" в Intellect регулирует bit rate видеопотока","1)  You may use the Quality slider to adjust the video stream bit rate."]
["Tiandy","Tiandy TC-NC9000S3-2MP-E","Camera","NVSSv5.2.0_20121109","1",null,null,"+","-","+",null,null,"1920x1080","1280x960","640x480","+",null,"-","-","-","-","-","-","-","+"]
["Tiandy","Tiandy TC-NC9000S3-2MP-E","Camera","NVSSv5.2.0_20121109","1",null,null,"+","-","+",null,null,"1920x1080","1280x960","640x480","+",null,"-","-","-","-","-","-","-","+"]
["Tiandy","Tiandy TC-NC9100S3-2MP-E-IR30","Camera","5.2.0_20121109","1",null,null,"+","-","+","-","-","1920x1080","1280x960","640x480","+",null,"-","-","-","-","-","-","-","-"]
["Tiandy","Tiandy TC-NC9200S3-2MP-E-IR30","Camera","5.2.0_20121109","1",null,null,"+","-","+","-","-","1920x1080","1280x960","640x480","+",null,"-","-","-","-","-","-","-","-"]
["Tiandy","Tiandy TC-NC9500S3E-MP-IR30","Camera","V6.0.0_20130115","1",null,null,"+","-","+","-","-","1280x960","704x576","640x480","+",null,"-","-","-","-","-","-","-","-"]
["TRENDnet","TRENDNet TV-IP100W","Camera ","3.12 (2005-08-18)","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":7},"-","-","1. При разрешении 640х480на скорость видео накладывется ограничение в 10 fps. Ограничение самой камеры, а не нашего ПО","1) With the 640x480 resolution, the frame rate is limited to 10 fps. This is a limitation of the camera itself, not of our software. "]
["TRENDnet","TRENDnet TV-IP110","Camera ","1.0.0.57","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":8},"-","1.Настройки fps, качество и разрешение принимаются после 30 сек ребута.\n","1. After you change the settings (resolution, quality, frame rate), the camera may take up to 30 seconds to restart.\n"]
["TRENDnet","TRENDNet TV-IP201","Camera ","2.00 build: 110","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",null,"+",null,null,"-","+",null,null,"-","1. Интегрирован только PCM аудиокодек. ADPCM пока не интегрирован\n ","1) The PCM audio codec is integrated. ADPCM is not integrated yet.\n "]
["TRENDnet","TRENDNet TV-IP212W","Camera ","1.0.0 build: 18","1",null,null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",null,"+","-",{"$nulls":4},"-","-","1.Настройки fps, качество и разрешение принимаются после 30 сек ребута. Особенность камеры2. Настройка цветности не работает на самой камере. Т.е. даже в родном вебе значение цветности меняется, но картинка не меняется\n","1. After you change the settings (resolution, quality, frame rate), the camera may take up to 30 seconds to restart. This is a limitation of the camera itself.2 The Color setting on the camera does not work . i.e. it is applied in the web interface, but the video image doesn't change.\n"]
["TRENDnet","TRENDNet TV-IP301","Camera ","1.00 build: 37","1",null,null,"+","-",{"$nulls":3},"640x480(MJPEG) / MPEG-4 no test","640x480(MJPEG) / MPEG-4 no test","320x240(MJPEG)/MPEG-4 no test","+",null,"+","-",null,null,"+",null,"-","-","1. Интегрирован только PCM (8 Kbps) аудиокодек","1) The PCM audio codec (8Kbps) is integrated."]
["TRENDnet","TRENDNet TV-IP312W","Camera ","1.0.0 build: 56","1",null,null,"+","+.",{"$nulls":3},"640x480","640x480","320x240(MJPEG)/640х480(MPEG-4)","+",null,"+","-",{"$nulls":4},"-","-","1.Настройки fps, качество и разрешение принимаются после 30 сек ребута. Особенность камеры\n","1. After you change the settings (resolution, quality, frame rate), the camera may take up to 30 seconds to restart. This is a limitation of the camera itself.\n"]
["TRENDnet","TRENDNet TV-IP400","Camera ","3.36","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","-","1. При разрешении 640х480 накладывается ограничение на скорость видео в 10 fps. Ограничение самой камеры, а не нашего ПО\n2. У камеры нет оптических зума и фокуса, поэтому кнопки управления \"Масштаб\" и \"Фокус\" на Панели Телеметрии работать не будут.\n3. У камеры нет настройки скорости поворота в чистом виде, поэтому настройка \"Скорость\" на Панели Телеметрии изменяет не скорость, а угол поворота.","1) With the 640x480 resolution, the frame rate is limited to 10 fps. This is a limitation of the camera itself, not of our software. \n2. Since the camera doesn't have optical zoom and focus controls, the Zoom and Focus control buttons do not work in the PTZ Control Panel.\n3) Since the camera doesn't have the Pan Speed control as such, you can use the Speed setting in he PTZ Control Panel to change its pan angle."]
["TRENDnet","TRENDnet TV-IP410","Camera ","1.1.0 build: 53","1",null,null,"+",{"$nulls":4},"640x480","640x480","320x240","+.",{"$nulls":3},"+.","-","+",null,"-","-","Изменение настроек видео приводит к перезагрузке устройства.","If you change video settings, the camera restarts."]
["TRENDnet","TRENDnet TV-IP422","Camera ","1.1.0 build: 68","1",null,null,"+","-",{"$nulls":3},"640x480","640x480","320x240","+.",null,"+","-","+","-","+",null,"-","-","Изменение настроек видео приводит к перезагрузке устройства.","If you change video settings, the camera restarts."]
["TVT","TVT TD2304SS-B","DVR","3.2.0.P-3520A-00","4",null,null,"-","-","+","-","-","704x480","704x480","704x480","-",null,"-","-","-","-","-","-","-","-","При настройке параметров подключения в ПО Axxon / ITV необходимо указывать порт, соответствующий аналогичной настройке в веб-интерфейсе устройства (CONFIG → Network → Server Port). По умолчанию значение порта - 6036.","When setting the connection parameters in Axxonsoft, specify the port corresponding to the similar setting in the camera web interface (CONFIG → Network → Server Port). Default value of the port is 6036."]
["UDP","UDP IPE5500","Camera","1.06.05 ","1",null,null,"+","+","+",null,null,"720x576 (PAL) / 720x480 (NTSC)","640x576 (PAL) / 640x480 (NTSC)","320x288 (PAL) / 320x240 (NTSC)","+",null,"+.","+","+","+","+","-","-","+","В MJPEG максимальная частота кадров - 5 fps.Настройки для аудиовыхода и аудиовхода должны быть одинаковыми.Луч приходит в положение готовности спустя 10-50 секунд после включения в нашем ПО. В дальнейшем замыкание/размыкание луча отрабатывается без задержек.Аудио-выход камеры воспроизводит звук с задержкой в 5 секунд - проблема камеры.Чтобы заработал звук, нужно выставить максимальный уровень громкости на динамике.","With MJPEG, maximum frame rate is 5fps. The audio input and output settings must be identical. It takes a sensor 10 to 50 seconds to activate after it has been enabled in the AxxonSoft software. After that, the sensor opens and closes with no delay. The problem is that audio output on the camera is delayed by 5 seconds. To get audio, you need to tune max volume value at audio out."]
["UDP","UDP NVC1000","Encoder ","1.06.05","1",null,null,"+","+","+",null,null,"720x576 (PAL) / 720x480 (NTSC)","640x576 (PAL) / 640x480 (NTSC)","320x288 (PAL) / 320x240 (NTSC)","+",null,"+.","+","+","+","+",null,"+","+","В кодеке MJPEG возможны задержки видео и падение частоты кадров, чем выше качество видео, тем они сильнее. В веб-интерфейсе поведение такое же.Настройки для аудиовыхода и аудиовхода должны быть одинаковыми.Луч приходит в положение готовности спустя 10-50 секунд после включения в нашем ПО. В дальнейшем замыкание/размыкание луча отрабатывается без задержек.Аудио-выход камеры воспроизводит звук с задержкой в 5 секунд - проблема камеры.","With MJPEG, video is delayed the frame rate drops, this all the more frequent and steep when you want better quality video. Same in the web interface. The audio input and output settings must be identical. It takes a sensor 10 to 50 seconds to activate after it has been enabled in the AxxonSoft software. After that, the sensor opens and closes with no delay. The problem is that audio output on the camera is delayed by 5 seconds."]
["UDP","UDP NVC4000L","Encoder ","1.2.0","4",{"$nulls":4},"+",null,null,"720x480","640x480","320x240","+",{"$nulls":8},"+"]
["V1netIP","V1netIP-220N","Camera ","2.2.2","1",{"$nulls":3},"+",{"$nulls":3},"704x576","704x288","352x288","+",null,"+","-",null,"+","+",null,"-","+"]
["V1netIP","V1netIP-230N","Camera ","2.2.2","1",{"$nulls":3},"+",{"$nulls":3},"720x576","720х288","352x288","+",null,"+","-",null,"+","+",null,"-","+","1) для нормальной работы камеры в ПО ITV необходимо в настройках камеры (в родном веб-интерфейсе) выставлять ограничение подключений строго больше 1. При ограничении =1 камера в ПО ITV не работает","1) Make sure the number of connections as configured in the web interface is greater than 1. If you set it to 1, the camera doesn't work."]
["V1netIP","V1netIP-240-26S","Camera ","2.2.4","1",{"$nulls":3},"+",{"$nulls":3},"720x576","720х288","352x288","+",null,"+","-","+","+","+",null,"-","+","из-за специфики кодека, после включени/выключения цвета возможно незначительное искажение картинки на 1-2 секунды","The codec may cause the image to garble for 1-2 seconds."]
["V1netIP","V1netIP-270H","Camera ","2.2.4","1",{"$nulls":3},"+",{"$nulls":3},"720x576","720х288","352x288","+",null,"+.","-","+","-","+",null,"-","+"]
["V1netIP","V1netServer-510 encoder","Encoder ","2.2.2","1",{"$nulls":3},"+",{"$nulls":3},"720*576(PAL)/720*480(NTSC)","720*288(PAL)/720*240(NTSC)","352*288(PAL)/352*240(NTSC)","+",null,"+","-","+","+","+",null,"-","+"]
["V1netIP","V1netServer-540 encoder","Encoder ","3.4.2","4",{"$nulls":3},"+",{"$nulls":3},"704x576(PAL)/704x480(NTSC)","704x576(PAL)/704x480(NTSC)","352x288(PAL)/352x240(NTSC)","+",null,"+.","-","+","+","+",null,"-","+"]
["Veilux","Veilux VVIP-2L2812","Camera","v1.6_build044014_117","1","-",null,"+",null,"+",null,null,"1920x1080 / 1280x720","1920x1080 / 1280x720","640x360",null,null,"-","-",null,"-","-","-",null,"-","Максимальное разрешение (1920х1080 или 1280х720) зависит от настройки Source Resolution в веб-интерфейсеВ настройках подключения в ПО ITV/Axxon нужно указывать порт, соответствующий значению поля Control Port в веб-интерфейсе камерыИзменение ТВ-стандарта нужно делать через веб-интерфейс","1. The max. resolution (1920х1080 or 1280х720) depends on the Source Resolution setting in the camera web interface.\n2. Specify  Control Port in the VMS settings\n3. You can configure TV standard via web interface.","improved"]
["Videosec","Videosec ICS-20F","Camera ","vt20120525NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":8},"+"]
["Videosec","Videosec ICS-20W","Camera ","vt20120525NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":8},"+"]
["Videosec","Videosec ICS-50W","Camera ","vt20120525NSA","1",null,null,"+",null,"+",null,null,"2592x1944(H264)/1920x1080(MJPEG)","800x600","640x480","+",{"$nulls":8},"+"]
["Videosec","Videosec ID-20","Camera ","vt20120525NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":8},"+"]
["Videosec","Videosec IPTZ-20","Camera ","vt20120525NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":3},"+",{"$nulls":4},"+"]
["Videosec","Videosec IRD-20W","Camera ","vt20120525NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":8},"+"]
["Videosec","Videosec IRW-20W","Camera ","vt20120525NSA","1",null,null,"+",null,"+",null,null,"1920x1080","1024x768","640x480","+",{"$nulls":8},"+"]
["ViDigi","ViDigi S-2101 / S-2103f / S-2104v / S-2105v / S-2106v","Camera","1.0.5.1.019","1","-",null,"+",null,"+",null,null,"1920x1080","1280x960","640x480","+",null,"+","+","-","+","+",null,"motion detection","+",null,null,"improved"]
["VIDO","VIDO G70HD820","Camera ","2.7.5 May 28 2012","1",null,null,"+",null,"+",null,null,"1920x1072","1280x720","352x288","+",null,"-","-","+","-","-",null,null,"-","1. Для работы фокуса необходимо для настройки Focus установить значение Manual.\n2. Для работы с нашим ПО нужно указывать Dev Port из вкладки Settings -> ServerParam\n3. В ПО ITV/Axxon устройство определяется как EH4300.","1. To make Focus work, set its settings to Manual.\n2. To make it work with AxxonSoft software, you have to select Dev Port in the Settings -> ServerParam\n3. In the AxxonSoft products, this camera is identified as EH4300."]
["VIDO","VIDO HX600HD / IRC600HD / IRC650HD","Camera ","2.7.5","1",null,null,"+",null,"+",null,null,"1920х1072","1280x720","352x288","+",null,"-","-","+","-","-",null,null,"-","1. В ПО ITV/Axxon модели определяются как VIDO SE600.","1. In the AxxonSoft products, the cameras are identified as VIDO SE600."]
["Visiocom","Visiocom VR-9632NI-ST","NVR","V2.1.0 build 111017","32",{"$nulls":4},"+",null,null,"2048x1536","1600x1200","320x240",{"$nulls":7},"+",null,"-"," Для подключения к устройству используется порт 8000 "," Please use port 8000 to connect to device."]
["Vision","VISIONxIP PM2Ti","Camera","1.1.3.3 20130620","1",null,null,"+","-","+",null,null,"1280х720(H264) / 720x480(MJPEG)","320x192(H264) / 640x480(MJPEG)","from WEB","-",null,"-","-","+","-","-","-","-","+","В ПО ITV со стандартным разрешением камера не показывает видео, особенность работы камеры.","In AxxonSoft products, standard camera resolution doesn't show video (camera's feature)."]
["Vision","Vision VC58SM3i","Camera ","1.1.0.16 20120316","1",null,null,"+",null,"+",null,null,"H264: 1920x1080 MJPEG: 1280x720","640x480","320x240","+.",null,"-","-",null,"-","-",null,"-","+","1. Разрешение на втором потоке не может быть больше, чем на первом. Например, если на первом стоит 320x240, то на втором не применяется 640x480 .Если на первом потоке выбрано разрешение 640x480, то на втором автоматически тоже устанавливается 640x480 и никакие другие не применяются.\n2. На камере не работает настройка яркости.","1. Resolution on the second stream can't be more than on the first. For example, if on the first costs 320x240, on the second it is not applied 640x480. If on the first stream resolution 640x480 is chosen, on the second automatically too is established 640x480 and any others aren't applied.\n2. Brightness control doesn't work at the camera."]
["Vision","Vision VDA110SM3i-IR","Camera ","1.1.0.16 20120316","1",null,null,"+",null,"+",null,null,"H264: 1920x1080 MJPEG: 1280x720","640x480","320x240","+.",null,"-","-",null,"-",null,null,"-","+","1. Разрешение на втором потоке не может быть больше, чем на первом. Например, если на первом стоит 320x240, то на втором не применяется 640x480 .Если на первом потоке выбрано разрешение 640x480, то на втором автоматически тоже устанавливается 640x480 и никакие другие не применяются.","1. Resolution on the second stream can't be more than on the first. For example, if on the first costs 320x240, on the second it is not applied 640x480. If on the first stream resolution 640x480 is chosen, on the second automatically too is established 640x480 and any others aren't applied."]
["Vision","Vision VDA50SMi","Camera ","1.1.0.16 20120316 ","1",null,null,"+",null,"+",null,null,"1280x720","640x480","320x240","+.",{"$nulls":7},"-","+","1. Разрешение на втором потоке не может быть больше, чем на первом. Например, если на первом стоит 320x240, то на втором не применяется 640x480 .Если на первом потоке выбрано разрешение 640x480, то на втором автоматически тоже устанавливается 640x480 и никакие другие не применяются.","1. Resolution on the second stream can't be more than on the first. For example, if on the first costs 320x240, on the second it is not applied 640x480. If on the first stream resolution 640x480 is chosen, on the second automatically too is established 640x480 and any others aren't applied."]
["Vitek","Vitek VT-PTZ220NP","Camera ","4.16-B0-ds-VI","1",null,null,"+",null,"+",null,null,"1920х1072","1280x720","640x352","+",{"$nulls":3},"+","-","-",null,"-","+"]
["Vitek","Vitek VTD-MV20VRN","Camera ","4.18-B1-ds","1",null,null,"+",null,"+",null,null,"1920x1080","1280x720","640x35","+",{"$nulls":8},"-"]
["Vitek","Vitek VTC-IR402","Camera ","4.16-B2-ds-VI","1",null,null,"+",null,"+",null,null,"1280x720 ","1280x720 ","640x352 ","+.",{"$nulls":8},"+"]
["Vivotek","Vivotek CC8130","Camera ","CC8130-VVTK-0200c","1","+",null,"+",null,"+",null,null,"1280x800","1280x800","640x400","+",null,"+",{"$nulls":5},"motion detection; tampering detection","-","Цифровая телеметрия работает только на первом потоке.","Digital PTZ works only on first stream."]
["Vivotek","Vivotek FD7131","Camera ","0201c","1","+",null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":8},"-"]
["Vivotek","Vivotek FD7141","Camera ","0101b","1","+",null,"+",{"$nulls":4},"720x480","720x480","360x240","+",{"$nulls":7},"-","-"]
["Vivotek","Vivotek FD8131/V","Camera ","0100e","1","+",null,"+","+","+",null,null,"1280x800","1280x800","640x400","+",{"$nulls":3},"+",{"$nulls":4},"-"]
["Vivotek","Vivotek FD8133(V) / FD8134(V)","Camera","FD8134-VVTK-0109a","1","+",4,"+","+","+","-","-","1280x800","1280x720","640x480","+","-","-","-","-","+","-","-","motion detection; tampering detection","-","Частота опорных в Интеллекте указывается в миллисекундах.","In Intellect, you can set up the key frame rate in milliseconds."]
["Vivotek","Vivotek FD8135H","Camera ","FD8135_VVTK_0201a","1","+",null,"+","+","+",null,null,"1280x800","1280x800","640x400","+",null,"+.","+","+","+","+",null,"motion detection; tampering detection","-"]
["Vivotek","Vivotek FD8136","Camera ","FD8136-VVTK-0101a","1","+",null,"+","+","+",null,null,"1280x800","1280x800","640x400","+",null,"+",null,"+","+",null,null,"motion detection; tampering detection","-"]
["Vivotek","Vivotek FD8137H / FD8137HV","Camera","FD8137-VVTK-0101a","1","+",2,"+","-","+","-","-","1280x800","1280x720","640x360","+","-","-","-","+","-","-","-","motion detection","-"]
["Vivotek","Vivotek FD8151V","Camera ","FD8151V-VVTK-0103a","1","+",null,"+",null,"+",null,null,"1280x1024","960x768","320x256","+",null,"+",null,"+","+",null,null,"motion detection; tampering detection","-","Цифровая телеметрия работает только на первом потоке.","Digital PTZ works only on first stream."]
["Vivotek","Vivotek FD8161","Camera ","0105b ","1","+",null,"+","+","+",null,null,"1600x1200","800x600","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","-","1. Особенность данной камеры: потоки (streams) управления телеметрией. Для каждого из них свой набор пресетов. ","1) This is a peculiarity of the camera itself. PTZ control panel settings. Each stream has a range of presets of its own. "]
["Vivotek","Vivotek FD8162","Camera ","0103a","1","+",null,"+","+","+",null,null,"1920x1080","1360x768","640x360","+",null,"+",null,"+",{"$nulls":3},"+","-"]
["Vivotek","Vivotek FD8335H","Camera","FD8335-VVTK-0202c","1","+","2","+","+","+",null,null,"1280x800","1280x800","640x400","+",null,"+","-","+","+","+","-","motion detection; tampering detection","-"]
["Vivotek","Vivotek FD8361","Camera ","0200b","1","+",null,"+",{"$nulls":4},"1280x720","1280x720","640x360","+",{"$nulls":3},"+.",{"$nulls":3},"-","-","1. Особенность данной камеры: потоки (streams) управления телеметрией. Для каждого из них свой набор пресетов.","1) This is a peculiarity of the camera itself. Telemetry control streams. Each stream has a range of presets of its own."]
["Vivotek","Vivotek FD8362(E)","Camera","FD8362E-VVTK-0103f","1","+","4","+","+","+",null,null,"1920x1080","1360x768","640x360","+",null,"+",null,"+","+","+","-","motion detection; tampering detection","-",null,null,"improved"]
["Vivotek","Vivotek FE8171V","Fisheye Camera","0100d","1","+",null,"+","+","+",null,null,"1536x1536","1056x1056","384х384","+",null,"-",null,null,"+","+",null,"-","-","Через Onvif работает видео и звук.","Video and audio streams works via ONVIF."]
["Vivotek ","Vivotek FE8172 / FE8172V","Fisheye Camera","FE8172-VVTK-0100g","1","+",null,"+","+","+",null,null,"1920 x 1080 (FullHD) / 1920 x 1920 (Fisheye)","1360 x 768 (FullHD) / 1056 x 1056 (Fisheye) ","640 x 360 (FullHD) / 384 x 384 (Fisheye)","+",null,"+",null,null,"+","+",null,"motion detection; tampering detection","-","В Интеллекте интервал включения опорных кадров задается в миллисекундах и может принимать следующие значения: 250, 500, 1000, 2000, 3000, 4000.","In Intellect, you can set up the keyframe rate in milliseconds at: 250, 500, 1000, 2000, 3000, 4000."]
["Vivotek","Vivotek IP6112/6122","Camera ","0105b","1",null,null,"+","+",{"$nulls":3},"704x576","704x576","352x288","+",null,"-","-",null,"-","+",null,"-","-","1) для камеры с прошивкой 0101e следует использовать граббер Vivotek, для камеры с прошивкой 0105b - Vivotek(mjpeg) и Vivotek(mpeg4)","1) For cameras with the 0101e firmware use the Vivotek, grabber, for version 0105b - Vivotek(mjpeg) and Vivotek(mpeg4)"]
["Vivotek","Vivotek IP7130","Camera ","0101b","1","+",null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":8},"-"]
["Vivotek","Vivotek IP7133","Camera ","0200b","1","+",null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":3},"-",{"$nulls":4},"-","у камеры Digital PTZ","The camera has Digital PTZ (digital telemetry)."]
["Vivotek","Vivotek IP7138","Camera ","0300a","1","+",null,"+","+",{"$nulls":3},"1280x1024(MJPEG) / 800x600(MPEG-4)","800x600","640x480","+",null,"+.","-",null,"+","+",null,"-","-","1. У самой камеры в Полном разрешении есть ограничение на частоту кадров, равное 8 fps","1. With the Full resolution, the camera itself allows 8 fps max. "]
["Vivotek","Vivotek IP7139","Camera ","0201b","1","+",null,"+","+",{"$nulls":3},"1280x1024(MJPEG) / 800x600(MPEG-4)","640x480","320x240","+",null,"+.","-",null,"+","+",null,"-","-","1. У самой камеры в Полном разрешении есть ограничение на частоту кадров, равное 8 fps","1. With the Full resolution, the camera itself allows 8 fps max."]
["Vivotek","Vivotek IP7154","Camera ","0200a","1","+",null,"+",{"$nulls":4},"640x480","640x480","320x240","+",null,null,"-",{"$nulls":5},"-"]
["Vivotek","Vivotek IP7160","Camera ","0103c","1","+",null,"+","+",{"$nulls":3},"1280x720","1280x720","640x360","+",null,"+.","-","+",{"$nulls":3},"-","-","1. Камера не поворотная, но есть Digital Telemetry","1. This is not a PTZ camera, but it has Digital Telemetry. "]
["Vivotek","Vivotek IP7161","Camera ","0103b","1","+",null,"+",{"$nulls":4},"1600x1200","800x600","320x240","+",{"$nulls":3},"+",{"$nulls":3},"-","-"]
["Vivotek","Vivotek IP7330","Camera ","0200b","1","+",null,"+","+",{"$nulls":3},"640x480","640x480","320x240","+",{"$nulls":4},"+",null,null,"-","-"]
["Vivotek","Vivotek IP7361","Camera ","0200b","1","+",null,"+",{"$nulls":4},"1280x720","1280x720","640x360","+",null,"+",null,"+",{"$nulls":4},"-","камера поддерживает только Digital PTZ","The camera supports only Digital PTZ. "]
["Vivotek","Vivotek IP8133/W","Camera ","0102a","1","+",null,"+","+","+",null,null,"1280x800","1280x720","640x400","+",{"$nulls":7},"+","-"]
["Vivotek","Vivotek IP8151","Camera ","0301e","1","+",null,"+","+","+",null,null,"1280x1024","800x600","640x480","+",null,"+","+","+","+","+",null,"+","-","В мануале написано, что камера поддерживает аналоговую телеметрию (внешнее поворотное устройство). Заставить ее работать не удалось.","According to the guide, the camera supports analog telemetry (a pan/tilt drive). We did not manage to make it work. "]
["Vivotek","Vivotek IP8151P","Camera ","0300f","1","+",null,"+","+","+",null,null,"1280x1024","800x600","640x480","+",{"$nulls":3},"+",{"$nulls":3},"+","-","Камера отличается от IP8151 списком настроек, т.к. тестирование производилось на разных версиях прошивки. Физически камеры различаются только параметрами оптики (судя по спецификации).","The list of settings for that camera is different from the one of IP8151 as we tested the cameras with different firmware versions. According the specs, the cameras differ in the optics."]
["Vivotek","Vivotek IP8152","Camera ","IP8152-VVTK-0101b","1","+",null,"+",null,"+",null,null,"1280x1024","960x768","320x256","+",null,"+","+","+","+",null,null,"motion detection; tampering detection","-","Цифровая телеметрия работает только на первом потоке.","Digital PTZ works only on first stream."]
["Vivotek","Vivotek IP8161","Camera ","0103a","1","+",null,"+","+","+",null,null,"1600x1200","800x600","640x480","+",{"$nulls":3},"+",{"$nulls":3},"-","-"]
["Vivotek","Vivotek IP8162/-P","Camera ","0100f","1","+",null,"+","+","+",null,null,"1920x1080","1360x768","800x450","+",null,"+",null,"+",{"$nulls":3},"+","-"]
["Vivotek","Vivotek IP8172(P)","Camera","IP8172-VVTK-0102b","1","+",3,"+","+","+","-","-","from WEB","from WEB","from WEB","+","-","+","-","+","+","+","-","motion detection; tampering detection","-","Доступный набор разрешений в Интеллекте зависит от настройки в веб интерфейсе камеры ( Configuration > Media  > Video > FOV).","The list of available resolutions in Intellect depends on the settings of camera web interface (Configuration > Media  > Video > FOV)."]
["Vivotek","Vivotek IP8330","Camera ","0100g","1","+",null,"+",{"$nulls":4},"640x480","640x480","320x240","+",{"$nulls":8},"-"]
["Vivotek","Vivotek IP8332 / IP8332-C","Camera","IP8332-VVTK-0200d","1","+",4,"+","+","+","-","-","1280x800","1280х720","640х400","+","-","-","-","-","-","-","-","motion detection; tampering detection","-","\nЧастота опорных кадров в Интеллекте указывается в миллисекундах. ","In Intellect, you can set up the key frame rate in milliseconds."]
["Vivotek","Vivotek IP8335H","Camera ","0100h","1","+",null,"+","+","+",null,null,"1280x800","1280x800","640x400","+",null,"+","+","+","+","+",null,"+","-"]
["Vivotek","Vivotek IP8352","Camera ","0102a","1","+",null,"+","+","+",null,null,"1280x1024","1280x720 (MJPEG / H264) / 960x768 (MPEG4)","320x256","+",null,"+","+.","+","+","+",null,"+","-","Аудио-выход не работает, если выбран кодек MJPEG.","If you select the MJPEG codec, the audio output does not work."]
["Vivotek","Vivotek IP8362","Camera ","0101b","1","+",null,"+","+","+",null,null,"1920x1080","1360х768","640x360","+",null,"-","-","+","+","+",null,"-","-","Через Onvif не работают лучи.","Via the ONVIF protocol, the sensors do not work. "]
["Vivotek","Vivotek IP8371E","Camera","IP8371E-VVTK-0100j","1","+","4","+","+","+",null,null,"2048x1536(3mp)/1920x1080(Full HD)","800x600","640x480","+",null,"-","-","+","-","-",null,"-","-",null,null,"improved"]
["Vivotek","Vivotek MD7560D","Camera ","MD7560-VVTK-0100e","1","+",null,"+","+",{"$nulls":3},"1600x1200","800x600","640x480","+",null,null,"-","+",{"$nulls":3},"-","-"]
["Vivotek","Vivotek MD8562","Camera ","0102a","1","+",null,"+","+","+",null,null,"1920x1080","1360x768","640x360","+",{"$nulls":3},"+",{"$nulls":3},"+","-"]
["Vivotek","Vivotek PT8133/W","Camera ","0100e","1","+",null,"+","+","+",null,null,"1280x800","1280x720","640x400","+",{"$nulls":3},"+",{"$nulls":3},"+","-"]
["Vivotek","Vivotek PZ7111","Camera ","0200a","1","+",null,"+",{"$nulls":4},"704x480","704x480","352x240","+",{"$nulls":3},"+.",{"$nulls":4},"-"]
["Vivotek","Vivotek PZ7131","Camera ","0200a","1","+",null,"+",{"$nulls":4},"640x480","640x480","320x240","+",null,null,"-","+",{"$nulls":3},"-","-"]
["Vivotek","Vivotek PZ81x1/W","Camera ","0100e","1","+",null,"+","+","+",null,null,"720x480","704x480","352x240","+",{"$nulls":3},"+",{"$nulls":3},"+","-"]
["Vivotek","Vivotek SD73x3 series","Camera ","0103c","1","+",null,"+",{"$nulls":4},"704x480","704x480","352x240","+",{"$nulls":3},"+.",{"$nulls":4},"-"]
["Vivotek","Vivotek SD81x1","Camera ","0103c","1","+",null,"+","+","+",null,null,"720x480(NTSC)/720x576(PAL)","704x480(NTSC)/704x576(PAL)","352x240(NTSC)/352x288(PAL)","+",{"$nulls":3},"+",{"$nulls":4},"-"]
["Vivotek","Vivotek SD8362E","Camera ","SD8362-VVTK-0203d","1","+",null,"+","+","+",null,null,"1920x1080","1360x768","640x360","+",null,"+","+","+","+","+",null,"+","-"]
["Vivotek","Vivotek SD8363E","Camera","SD8363-VVTK-0200d","1","+","4","+","+","+",null,null,"1920x1080","1280x720","640x360","+",null,"+","+","-","+","+","-","motion detection","-","Кодек SVC не интегрирован. Максимальное разрешение и FPS в ПО ITV, зависит от выбранного значения(Full HD (MAX1080P 30fps) или Exceptional frame rate ( 720P 60fps)) в разделе FOV веб-интерфейса камеры. При смене этих режимов в веб-интерфесе камеры, для первого потока автоматически применяется кодек SVC.","SVC codec is not integrated. In AxxonSoft products, maximum resolution and FPS products depends on value (Full HD (MAX1080P 30fps) or Exceptional frame rate (720P 60fps)) in FOV section of web-interface. When you change the modes in camera web interface, SVC codec will be automatically applied on first stream."]
["Vivotek","Vivotek SD83X2","Camera ","SD83X3-VVTK-0202b","1","+",null,"+","+","+",null,null,"720x576","704x576","352x288","+",{"$nulls":3},"+",{"$nulls":3},"motion detection","-","ТВ-стандарт нужно выбирать в соответствии с модификацией камеры:\nSD8322 - PAL\nSD8312 - NTSC","TV-standart should be selected in accordance with camera's modification: SD8322- PAL, SD8312- NTSC."]
["Vivotek","Vivotek SD83X3","Camera ","SD83X3-VVTK-0202b","1","+",null,"+","+","+",null,null,"720x576","720x576","352x288","+",null,"-","-","+","+","+",null,"motion detection","-","ТВ-стандарт нужно выбирать в соответствии с модификацией камеры:SD8323 - PAL; SD8313 - NTSC","Select the TV standard as follows: SD8323 - PAL, SD8313 - NTSC"]
["Vivotek","Vivotek SF8172 / SF8172V","Fisheye Camera","SF8172-VVTK-0100d","1","+","3","+","+","+",null,null,"1920x1920","1056x1056","384x384","+",null,"+","-","+","+","+",null,"motion detection; tampering detection","-","В Интеллекте частота опорных кадров задается в миллисекундах и может принимать следующие значения: 250, 500, 1000, 2000, 3000, 4000.Для данной камеры реализована функция Panoramic PTZ. Для ее работы требуется поворотная камера Vivotek SD8362E. Более подробную информацию можно найти на сайте Vivotek.","In Intellect, you can set up the keyframe rate in milliseconds at: 250, 500, 1000, 2000, 3000 and 4000. Panoramic PTZ feature is enabled for this camera. Vivotek SD8362E PTZ camera is required. You can find details at Vivotek website. ","new"]
["Vivotek","Vivotek VS2403 coder","Encoder ","VS2403-VVTK-0103e","4",null,null,"+",{"$nulls":4},"704x576","704x288","352x288","+",null,"-","-","+","+","+",null,null,"-","Видеосервер физически имеет 4 канала. Но интегрирован в наше ПО как 5-канальный. Через 5-й канал идет видео со всех камер сразу в режиме 4-кратора.Настройки изображения работают только при выключенном веб-интерфейсе.Удалять предустановки телеметрии через ПО ITV нельзя.","Physically, the video encoder has 4 channels. But our software integrates it as a 5-channel device. Channel 5 feeds video from all cameras simultaneously in the Quad mode. Video settings are available only if the web interface is disabled. You can not delete presets via the AxxonSoft software."]
["Vivotek","Vivotek VS8102 encoder","Encoder ","0200c5","1","+",null,"+",{"$nulls":4},"720x480","704x480","352x240","+",{"$nulls":8},"-"]
["Vivotek","Vivotek VS8401 encoder","Encoder ","0200a","4","+",null,"+","+","+",null,null,"720x480/640х480","704x480/640х480","352x240/320х240","+",null,"-","-","-","-","-",null,"-","-","1. Частота опорных кадров в Интеллекте задается в миллисекундах.","1. In Intellect, you set the keyframe rate in milliseconds."]
["Vivotek","Vivotek VS8801 encoder","Encoder ","0200a","8",null,null,"+","+","+",null,null,"720x480","704x480","352x240","+",null,"-","-","-","-","-",null,"-","-"]
["WuT","WuT WEB-IO","I/O Module","3.40","0",{"$nulls":7},"from WEB","from WEB","from WEB",{"$nulls":5},"+","+",null,null,"+","1. 12 Input x 12 Output Нумерация в Интеллекте начинается с 1 (единицы), а на устройстве - с 0 (нуля).\n2. При включении/выключении всех реле одновременно (макрокомандой, например) некоторые могут не сработать и остаться в предыдущем состоянии.","1. 12 Input x 12 Output. Intellect's numbering tart with 1, whereas the device's range starts with 0.\n2. If you enable/disable all relays at a time e.g. with a macro, some will fail to switch to the new status."]
["Y-cam ","Y-cam Bullet HD 1080","Camera ","1.3057","1",null,null,"+",null,"+",null,null,"1920x1080","1920x1080","1920x1080","+",{"$nulls":8},"+"]
["Y-cam","Y-cam Cube HD 1080","Camera","5.46","1",null,null,"+","+","+",null,null,"1920x1080","768x432","480x270","-",null,"-","-","-","-","-","-","-","+"]
["Y-cam","Y-cam Cube HD 720","Camera","5.46","1",null,null,"+","+","+",null,null,"1280x720","640x480","480x270(H264/MPEG4)/ MJPEG: from Web","-",null,"+","-","-","-","-","-","-","+"]
["Yudor Technologies","Yudor CO-i03MY1 (YUC-HS94)","Camera ","V1.0.32_Y ","1",null,null,"+","-","+",null,null,"640x480","640x480","320x240","+",null,"+","+",{"$nulls":4},"+","+"]
["Yudor Technologies","Yudor CO-i04DY2(3.7-12) (YUC-HM93-312)","Camera ","V1.0.32_Y","1",null,null,"+","-","+",null,null,"720x576","704x576","352x288","+",null,"+","+",null,"+","+",null,"+","+","Между переходами луча в состояние \"замкнуто\" должен соблюдаться временной интервал, настраиваемый через веб-интерфейс. Минимальное значение - 10 секунд.Через Onvif камера работает только в режиме совместимости. Видео и звук идут, но никакие настройки не применяются.В Интеллекте поиск находит камеру как FineCCTV.","You can configure the delay before a sensor closes. Min 10 seconds. The camera works via the ONVIF protocol, but only in compatibility mode Video and audio streams are there but changes can't be applied. Intellect identifies the camera as FineCCTV."]
["Yudor Technologies","Yudor CO-i13MY1 (CO-YUC-HS95)","Camera ","V1.0.32_Y","1",null,null,"+","-","+",null,null,"1280x1024","1280x960","640x480","+",null,"+","+",{"$nulls":4},"+","+","На камере есть ограничение FPS в зависимости от разрешения:\n Для разрешений не больше 640x480 ограничение составляет 30 fps, для больших разрешений - 15. Ограничение включается для всех потоков, если разрешение >640x480 установлено хотя бы на одном из двух потоков.","The camera has frame rate limits (depending on the resolution):\n For resolutions lower than 640x480 the max fps is 30, fro greater resolutions it is 15. This limitation applies to all streams if a resolution greater than 640x480 is set for any of the 2 streams."]
["Yudor Technologies","Yudor CO-i20DY2(2,7-9) (CO-YUC-HM96-279)","Camera ","V1.0.32_Y","1",null,null,"+","-","+",null,null,"1600x1200","1280x960","640x480","+",null,"+","+",null,"+","+",null,"+","+","Поиск в AxxonNext/Next не определяет прошивку: ее нужно выбрать самостоятельно.Между переходами луча в состояние \"замкнуто\" должен соблюдаться временной интервал, настраиваемый через веб-интерфейс. Минимальное значение - 10 секунд.Прошивка V1.0.32_Y: через Onvif камера работает только в режиме совместимости. Видео и звук идут, но никакие настройки не применяются. Поиском не находится.В Интеллекте поиск находит камеру как FineCCTV.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AxxonNext/Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.","In AN, the search does not find the device's firmware. You must select the right firmware yourself. You can configure the delay before a sensor closes. Min 10 seconds. With firmware V1.0.32_Y and via the ONVIF protocol, the camera works only in the compatibility mode. Video and audio streams are there but changes can't be applied. The camera can't be located by search. Intellect device discovery identifies it as Fine CCTV. The camera offers the Video Parameters option (the max. resolution and max. frame rate). In AN, you must make sure that there is not conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value."]
["Yudor Technologies","Yudor CO-i20DY2IRPV (CO-YUC-Hi96RP)","Camera ","V1.0.32_Y","1",null,null,"+","-","+",null,null,"1600x1200","1280x960","640x480","+",null,"+","+",null,"+","+",null,"+","+","Настройка \"Параметры видео\" определяет ограничение FPS в зависимости от разрешения. Для получения максимального FPS необходимо следить за тем, чтобы разрешение настройки \"Параметры видео\" было не больше, чем выбренное разрешение получаемого видео.После размыкания датчика реакция на следующее замыкание может произойти не раньше, чем через 10 секунд.","The Video Parameters setting is used to limit fps depending on the resolution: To get the maximum frame rate, make sure that the Video Parameters setting has the the same or lower resolution than you selected for your video. After opening, the sensor can close in not earlier than 10 seconds."]
["Yudor Technologies","Yudor CO-YUC-H696","Camera ","V1.0.26_Y","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+","-","+","+","+",null,"+","+","Поиск в AxxonNext/Next не определяет прошивку: ее нужно выбрать самостоятельно.Прошивка V1.0.26_Y: камера работает по Onvif только в режиме совместимости, поиском как Onvif не находится.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AxxonNext/Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.","In AN, the search does not find the device's firmware. you must select the right firmware yourself. The V1.0.26_Y firmware: Via the ONVIF protocol, the camera works only in compatibility mode; the search does not find the camera as a device that supports ONVIF. The camera has the ***Video Parameters *** option (the max. resolution and max. frame rate). In AN, you must make sure that there is not conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value."]
["Yudor Technologies","Yudor CO-YUC-H696P","Camera ","V1.0.26._Y","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+","-","+","+","+",null,"+","+","Поиск в AxxonNext/Next не определяет прошивку: ее нужно выбрать самостоятельно.Прошивка V1.0.26_Y: камера работает по Onvif только в режиме совместимости, поиском как Onvif не находится.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AxxonNext/Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.","In AN, the search does not find the device's firmware. you must select the right firmware yourself. The V1.0.26_Y firmware: Via the ONVIF protocol, the camera works only in compatibility mode; the search does not find the camera as a device that supports ONVIF. The camera has the ***Video Parameters *** option (the max. resolution and max. frame rate). In AN, you must make sure that there is not conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value."]
["Yudor Technologies","Yudor CO-YUC-H696RP","Camera ","V1.0.26_Y","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+","-","+","+","+",null,"+","+","Поиск в AxxonNext/Next не определяет прошивку: ее нужно выбрать самостоятельно.Прошивка V1.0.26_Y: камера работает по Onvif только в режиме совместимости, поиском как Onvif не находится.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AxxonNext/Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.","In AN, the search does not find the device's firmware. you must select the right firmware yourself. The V1.0.26_Y firmware: Via the ONVIF protocol, the camera works only in compatibility mode; the search does not find the camera as a device that supports ONVIF. The camera has the ***Video Parameters *** option (the max. resolution and max. frame rate). In AN, you must make sure that there is not conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value."]
["Yudor Technologies","Yudor CO-YUC-H696RW","Camera ","V1.0.20_Y","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"+","-","+","+","+",null,"+","+","Поиск в AxxonNext/Next не определяет прошивку: ее нужно выбрать самостоятельно.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AxxonNext/Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.","In AN, the search does not find the device's firmware. you must select the right firmware yourself. The camera has the ***Video Parameters *** option (the max. resolution and max. frame rate). In AN, you must make sure that there is not conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value."]
["Yudor Technologies","Yudor YUC-H796R","Camera ","1.0.38_Y","1",null,null,"+",null,"+",null,null,"1600x1200","800x592","640x480","+",null,"-","-",null,"+","+",null,"motion detection; ","+","1. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект после добавления камеры необходимо выбрать нужное значение в веб-интерфейсе.\n2. Протокол ONVIF: при переключение кодека с MJPEG на H.264 - нет видео. Проблема устройства. Чтобы получить видео необходимо выставить кодек в веб-интерфейсе и перезапустить продукт\n","1. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, after adding the camera, go to the web interface and select the required value.\n2. ONVIF: when you switch from MJPEG to H.264, video stream is lost. This is a problem of the camera itself. To get video, go to the camera's web interface, select a codec and restart the VMS.\n"]
["ZAVIO ","ZAVIO F3115","Camera ","M2.1.6.02 ","1",null,null,"+","+","+",null,null,"1280x800 ","640x480","320x240 ","+",{"$nulls":8},"-"]
["ZAVIO ","ZAVIO B5111 ","Camera ","M2.1.6.03C019","1",null,null,"+","+","+",null,null,"from WEB ","from WEB ","from WEB ","+",{"$nulls":8},"-"," Разрешение в ПО ITV/Axxon меняется только после смены кодека. Это особенность текущей прошивки. \n\n","Resolution in Axxon SW changes only after codec changing. This is a limitation of the current firmware."]
["ZAVIO ","ZAVIO F531E ","Camera ","LM.1.6.18P10","1",{"$nulls":3},"+",{"$nulls":3},"640x480 ","640x480 ","320x240","+",{"$nulls":8},"-"]
["ZAVIO ","ZAVIO F7210 ","Camera ","M2.1.6.01C2 ","1",null,null,"+","+","+",null,null,"1920x1080 ","1024x768 ","640x480","+",{"$nulls":8},"-"]

{"sheet":"Intellect (ONVIF)","index":3,"n_rows":248,"n_cols":5,"rows_kept":248,"flags":["formulas_cached_only"]}
["Vendor","Model ","Firmware version","Notes","Notes in English"]
["3S Vision","3S Vision N1011","V1.03_STD-1"]
["3S Vision","3S Vision N1031","V1.02_STD-1"]
["3S Vision","3S Vision N1072","V1.09_STD-1"]
["3S Vision","3S Vision N3011","V1.03_STD-1"]
["3S Vision","3S Vision N3031","V1.02_STD-1"]
["3S Vision","3S Vision N3072","V1.07_STD-1"]
["3S Vision","3S Vision N5011","V1.05_STD-1"]
["3S Vision","3S Vision N5012","V1.05_STD-1"]
["3S Vision","3S Vision N5013","V1.01_STD-1"]
["3S Vision","3S Vision N6013","V1.03_STD-1"]
["3S Vision","3S Vision N6033","V1.02_STD-1"]
["3S Vision","3S Vision N6076","V1.07_STD-1"]
["3S Vision","3S Vision N8012","V1.03_STD-1"]
["3S Vision","3S Vision N8032","V1.02_STD-1"]
["3S Vision","3S Vision N8072","V1.07_STD-1"]
["3S Vision","3S Vision N9071","V1.10_STD-1"]
["3S Vision","3S Vision S2071","V1.06_STD-1"]
["3S Vision","3S Vision S4071","V1.06_STD-1"]
["Acumen","Acumen AiP-B34","1.0.496(Ai)"]
["Acumen","Acumen AiP-M53","1.1.004(Ai)"]
["Avigilon","Avigilon xx-H3PTZ-xx","2.4.4.26(7969) "]
["Avigilon","Avigilon xx-H3-xx","2.4.2.16(7966)"]
["Canon","Canon VB-H41","1.0.0"]
["Canon","Canon VB-H410","1.0.0"]
["Canon","Canon VB-H6100D","1.0.0"]
["Canon","Canon VB-H6100VE","1.0.0"]
["Canon","Canon VB-H610D","1.0.0"]
["Canon","Canon VB-H610VE","1.0.0"]
["Canon","Canon VB-H7100F","1.0.0"]
["Canon","Canon VB-H710F","1.0.0"]
["Canon","Canon VB-S300D","1.0.0"]
["Canon","Canon VB-S30D","1.0.0"]
["Canon","Canon VB-S310D","1.0.0"]
["Canon","Canon VB-S31D","1.0.0"]
["Canon","Canon VB-S8000D","1.0.0"]
["Canon","Canon VB-S800D","1.0.0"]
["Canon","Canon VB-S9000F","1.0.0"]
["Canon","Canon VB-S900F","1.0.0"]
["Dahua","Dahua DH-IPC-HD2100","V4.1.1"]
["Dahua","Dahua DH-IPC-HD3100","V4.1.1"]
["Dahua","Dahua DH-IPC-HD3200","V4.1.1"]
["Dahua","Dahua DH-IPC-HDB3100","V4.1.1"]
["Dahua","Dahua DH-IPC-HDB3101","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDB3110","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDB3200","V4.1.1"]
["Dahua","Dahua DH-IPC-HDB3200C","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDB3202","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDB3300","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDBW3100","V4.1.1"]
["Dahua","Dahua DH-IPC-HDBW3101","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDBW3110","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDBW3200","V4.1.1"]
["Dahua","Dahua DH-IPC-HDBW3300","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDW2100","V4.1.1"]
["Dahua","Dahua DH-IPC-HDW3100","V4.1.1"]
["Dahua","Dahua DH-IPC-HDW3200S","V4.1.1"]
["Dahua","Dahua DH-IPC-HF3100","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HF3101","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HF3110","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HF3200","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HF3211","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HF3300","V2.103.02"]
["Dahua","Dahua DH-IPC-HF3500","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HFW2100","V4.1.1"]
["Dahua","Dahua DH-IPC-HFW3110","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HFW3200C","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HFW3200S","V4.1.1"]
["Dahua","Dahua DH-IPC-HFW3202C","V4.1.1"]
["Dahua","Dahua DH-IPC-HFW3300","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HFW3300C","V2.2.6.1"]
["Dahua","Dahua DH-IPC-K100A","V4.1.1"]
["Dahua","Dahua DH-SD6580C-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6580-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6581-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6582A-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6582-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6582-HNI","V2.2.6.1"]
["Dahua","Dahua DH-SD65XX-HN","V2.103.02"]
["Dahua","Dahua DH-SD6980C-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6980-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6981-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6982A-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6982-HN","V2.2.6.1"]
["Dahua","Dahua DH-SDZ1018","V4.1.1"]
["Dahua","Dahua DH-SDZ2020","V4.1.1"]
["Dahua","Dahua HD-IPC-HDW3200","V4.1.1"]
["Dahua","Dahua IPC-HDBW3202","V2.2.6.1"]
["Dahua","Dahua IPC-HFW3101C","V2.2.6.1"]
["Digimerge ","Digimerge DNB14TL2","v1.6_build044014_104 "]
["Digimerge ","Digimerge SyncroIP (DNB14TL2, DNB13TL2, DND13TL2, DNE14TL2, DNV14TL2 )","v1.6_build044014_148"]
["FLIR","FLIR A310PT","Nexus v2.5.16.0"]
["FLIR","FLIR D-Series","Nexus v2.5.16.0 "]
["FLIR","FLIR F-Series","Nexus v2.5.16.0  "]
["FLIR","FLIR FC-Series","Nexus v2.5.15.0"]
["FLIR","FLIR F-Series","Nexus v2.5.16.0"]
["FLIR","FLIR PT-Series","Nexus v2.5.16.0"]
["FLIR","FLIR SyncroIP (DNB14TL2, DNB13TL2, DND13TL2, DNE14TL2, DNV14TL2 )","v1.6_build044014_148"]
["FLIR","FLIR TrafiBot","4.13.0"]
["FLIR","FLIR Traficon VIP-TX","4.13.0"]
["GeoVision ","GeoVision GV-BL1200","v2.059"]
["GeoVision ","GeoVision GV-BL120D","v2.059"]
["GeoVision ","GeoVision GV-BL1210","v2.059"]
["GeoVision ","GeoVision GV-BL1300","v2.059"]
["GeoVision ","GeoVision GV-BL130D","v2.059"]
["GeoVision ","GeoVision GV-BL1500","v2.059"]
["GeoVision ","GeoVision GV-BL220D","v2.059"]
["GeoVision ","GeoVision GV-BL2400","v2.059"]
["GeoVision ","GeoVision GV-BL2410","v2.059"]
["GeoVision ","GeoVision GV-BL2500","v2.09"]
["GeoVision ","GeoVision GV-BL320D","v2.059"]
["GeoVision ","GeoVision GV-BL3400","v2.059"]
["GeoVision ","GeoVision GV-BL3410 ","v2.059"]
["GeoVision ","GeoVision GV-BL5310","v2.059"]
["GeoVision ","GeoVision GV-BX120D","v2.059"]
["GeoVision ","GeoVision GV-BX1300","v2.059"]
["GeoVision ","GeoVision GV-BX130D","v2.059"]
["GeoVision ","GeoVision GV-BX140DW","v2.059"]
["GeoVision ","GeoVision GV-BX1500 ","v2.059"]
["GeoVision ","GeoVision GV-BX1500-E","v2.059"]
["GeoVision ","GeoVision GV-BX220D","v2.059"]
["GeoVision ","GeoVision GV-BX2400","v2.059"]
["GeoVision ","GeoVision GV-BX2500","v2.09"]
["GeoVision ","GeoVision GV-BX320D","v2.059"]
["GeoVision ","GeoVision GV-BX3400","v2.059"]
["GeoVision ","GeoVision GV-BX520D","v2.059"]
["GeoVision ","GeoVision GV-BX5300","v2.059"]
["GeoVision ","GeoVision GV-CA120","v2.059"]
["GeoVision ","GeoVision GV-CA220","v2.059"]
["GeoVision ","GeoVision GV-CAW120","v2.059"]
["GeoVision ","GeoVision GV-CAW220","v2.059"]
["GeoVision ","GeoVision GV-CB120","v2.059"]
["GeoVision ","GeoVision GV-CB220","v2.059"]
["GeoVision ","GeoVision GV-CBW120","v2.059"]
["GeoVision ","GeoVision GV-CBW220 ","v2.059"]
["GeoVision ","GeoVision GV-CR420","v1.019"]
["GeoVision ","GeoVision GV-EBL1100","v1.00"]
["GeoVision ","GeoVision GV-EBX1100","v1.00"]
["GeoVision ","GeoVision GV-EFD1100","v1.00"]
["GeoVision ","GeoVision GV-FD1200","v2.059"]
["GeoVision ","GeoVision GV-FD120D","v2.059"]
["GeoVision ","GeoVision GV-FD1500","v2.059"]
["GeoVision ","GeoVision GV-FD1510","v2.09"]
["GeoVision ","GeoVision GV-FD220D","v2.059"]
["GeoVision ","GeoVision GV-FD2400","v2.059"]
["GeoVision ","GeoVision GV-FD2500","v2.09"]
["GeoVision ","GeoVision GV-FD2510","v2.09"]
["GeoVision ","GeoVision GV-FD3400","v2.059"]
["GeoVision ","GeoVision GV-FD5300 ","v2.059"]
["GeoVision ","GeoVision GV-FE2301","v2.059"]
["GeoVision ","GeoVision GV-FE420 ","v2.059"]
["GeoVision ","GeoVision GV-FE4301","v2.059"]
["GeoVision ","GeoVision GV-FE520 ","v2.059"]
["GeoVision ","GeoVision GV-FER521 ","v2.059"]
["GeoVision ","GeoVision GV-Hybrid","v1.019"]
["GeoVision ","GeoVision GV-MDR120","v2.059"]
["GeoVision ","GeoVision GV-MDR220","v2.059"]
["GeoVision ","GeoVision GV-MDR2400 ","v2.059"]
["GeoVision ","GeoVision GV-MDR320 ","v2.059"]
["GeoVision ","GeoVision GV-MDR3400","v2.059"]
["GeoVision ","GeoVision GV-MDR520 ","v2.059"]
["GeoVision ","GeoVision GV-MFD120","v2.059"]
["GeoVision ","GeoVision GV-MFD130","v2.059"]
["GeoVision ","GeoVision GV-MFD1501","v2.059"]
["GeoVision ","GeoVision GV-MFD220 ","v2.059"]
["GeoVision ","GeoVision GV-MFD2501","v2.09"]
["GeoVision ","GeoVision GV-MFD320","v2.059"]
["GeoVision ","GeoVision GV-MFD520","v2.059"]
["GeoVision ","GeoVision GV-PT130D","v2.099"]
["GeoVision ","GeoVision GV-PT220D","v2.099"]
["GeoVision ","GeoVision GV-PT320D","v2.099"]
["GeoVision ","GeoVision GV-SD200 ","V103"]
["GeoVision ","GeoVision GV-SD200-S","V103"]
["GeoVision ","GeoVision GV-SD220","v1.009"]
["GeoVision ","GeoVision GV-SD220-S ","v1.009"]
["GeoVision ","GeoVision GV-UBL3401","v2.059"]
["GeoVision ","GeoVision GV-UBX1301","v2.059"]
["GeoVision ","GeoVision GV-UBX2301 ","v2.059"]
["GeoVision ","GeoVision GV-UBX3301 ","v2.059"]
["GeoVision ","GeoVision GV-UFD1501","v2.09"]
["GeoVision ","GeoVision GV-UFD2501","v2.09"]
["GeoVision ","GeoVision GV-VD1200 ","v2.059"]
["GeoVision ","GeoVision GV-VD120D","v2.059"]
["GeoVision ","GeoVision GV-VD1500","v2.059"]
["GeoVision ","GeoVision GV-VD1540","v2.09"]
["GeoVision ","GeoVision GV-VD1540-E","v2.09"]
["GeoVision ","GeoVision GV-VD220D","v2.059"]
["GeoVision ","GeoVision GV-VD2400","v2.059"]
["GeoVision ","GeoVision GV-VD2430","v2.09"]
["GeoVision ","GeoVision GV-VD2500","v2.09"]
["GeoVision ","GeoVision GV-VD320D","v2.059"]
["GeoVision ","GeoVision GV-VD3400","v2.059"]
["GeoVision ","GeoVision GV-VD3440","v2.09"]
["GeoVision ","GeoVision GV-VD3440-E","v2.09"]
["GeoVision ","GeoVision GV-VD5300","v2.059"]
["GeoVision ","GeoVision V-FD320D ","v2.059"]
["Honeywell","Honeywell H3D1F1X ","40.0.6"]
["Honeywell","Honeywell H4D2F1X","40.0.6"]
["Honeywell","Honeywell HCD2FX ","40.0.6"]
["Honeywell","Honeywell HDZ20HDEX","HS20131118NSA"]
["Legrand","Legrand Seried3:IP Speed Domes","2.103.General 00.0.R, build: 2013-07-17(V4.1.1)"]
["Legrand","Legrand Series 1: IP Cameras","2.103.General 00.0.R, build: 2013-07-27(V4.1.1)"]
["Legrand","Legrand Series 2: IP Cameras","2.103.General 00.0.R, build: 2013-07-27(V4.1.1) "]
["Legrand","Legrand Series 4: IP Cameras","2.103.General 00.0.R, build: 2013-07-27(V4.1.1)"]
["Legrand","Legrand Series 5 : IP Speed Domes","2.211.General 00.0.R, build: 2013-10-08(V4.1.1) "]
["NEXCOM ","NEXCOM NCb-301","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCb-311","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCi-301-V","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCi-311","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCi-311-R","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCi-312","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCm-301-2V","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCM-301-V","NexWare_01.00.0009"]
["NEXCOM ","NEXCOM NCo-301-VHR","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCr-301-VHR","NexWare_01.00.0010"]
["Qihan","Qihan IPCamera","v2.3.4"]
["RVi","RVi RVi-IPC12","6.C.2.11896"]
["RVi","RVi RVi-IPC12W","6.C.2.11896"]
["RVi","RVi RVi-IPC20DN","V045_1"]
["RVi","RVi RVi-IPC21","V017_1"]
["RVi","RVi RVi-IPC21DN","V047_1"]
["RVi","RVi RVi-IPC21DNL","V082_1"]
["RVi","RVi RVi-IPC22DN","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)"]
["RVi","RVi RVi-IPC23DN","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)"]
["RVi","RVi RVi-IPC23DN","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)  "]
["RVi","RVi RVi-IPC31DN","V053_1"]
["RVi","RVi RVi-IPC31DNL","V110_1"]
["RVi","RVi RVi-IPC32DNS","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)  "]
["RVi","RVi RVi-IPC32M","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)"]
["RVi","RVi RVi-IPC41DNL","V0114_1"]
["RVi","RVi RVi-IPC41DNS","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)  "]
["RVi","RVi RVi-IPC42DN","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1) "]
["RVi","RVi RVi-IPC42DNS","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)  "]
["RVi","RVi RVi-IPC50DN36","V035_1"]
["RVi","RVi RVi-IPC51DN18","V069_1"]
["RVi","RVi RVI-IPC52DN20","2.103.Group 00.0.R, build: 2013-08-22(V4.1.1)  "]
["RVi","RVi RVi-IPS125","V029_1"]
["RVi","RVi RVi-IPS125A","2.608.GP00.0.T,Build:2013-11-4(V2.2.5.1)  "]
["RVi","RVi RVi-IPS4100A","2.608.GP00.0.T,Build:2013-11-4(V2.2.5.1)  "]
["Stream Labs","Stream Labs WaveCam S1","0.2.0.0"]
["Stream Labs","Stream Labs WaveCam S1V","2.13.7.10"]
["Stream Labs","Stream Labs WaveServer 3554","2.13.7.10"]
["Stream Labs","Stream Labs WaveServer R3554","2.13.7.10"]
["Surveon","Surveon 2301A","V2.1.E04"]
["Surveon","Surveon 4321","V2.1.E04"]
["Surveon","Surveon 4361","V2.1.E04"]
["Surveon","Surveon CAM6181","fr20130223NSA"]
["Surveon","Surveon CAM6351","fr20130223NSA"]

{"sheet":"AxxonNext","index":4,"n_rows":1123,"n_cols":23,"rows_kept":1123,"flags":["formulas_cached_only"]}
["Vendor","Model","Type","Firmware","Channel","Streams","MJPEG","MPEG","H264","Wavelet","MxPEG","Max resolution","Settings","Multicast","Audio IN","Audio Out","PTZ","Alarm IN","Alarm OUT","Analytics","Notes","Notes in English"]
["!ONVIF","1-channel device",null,"Onvif Spec v.1.02","1","2","+","+","+",null,null,"from device","+",null,"+","-","+.","+","+","motion detection.","1. Список устройств, поддерживающих ONVIF, перечислен на официальном сайте форума:\nhttp://www.onvif.org/ConformantProducts/ProductList.aspx \nОбращайте внимание на наименование модели и прошивку. 2. Работа устройства Onvif за NAT не поддерживается. Устройство должно быть с отдельным внешним IP адресом. 3. В продукте доступны два вендора, ONVIF(однопоточный) и ONVIF 2.X(двухпоточный)","1. A list of ONVIF-conformant devices may be found at ONVIF's official website:\nhttp://www.onvif.org/ConformantProducts/ProductList.aspx\nPay attention to the model names and firmware. 2. It's not supported if device is connected via NAT. It must have separate external IP address."]
["!PSIA","1-channel device",null,"PSIA spec. 1.1","1","2","+","-","+",null,null,"depending on the device","+",null,"+","-","-","-","-","-",null,null,"improved"]
["360Vision","360Vision Predator Pred-XX-IP","Camera ","1.3/20090127","1","4",null,"+",{"$nulls":3},"720x576","+",{"$nulls":3},"+",null,null,"-"]
["3S Vision","3S Vision S4071","Camera ","V1.03_STD-1","4","3","+",null,"+",null,null,"704x480","+",null,null,"-","+","-","-","-"]
["3S Vision","3S Vision N1011","Camera"," V1.04_STD-1","1","3","+",null,"+",null,null,"QSXGA Mode: 2560x1920(h.264)/1280x960(mjpeg). FullHD Mode:1920x1080","+",null,"+","-","-","-","-","-","Значения битрейта зависят от значения разрешенияНа третьем потоке потоке нельзя выставить значение разрешения 1600x1200 если на первом потоке стоит значение разрешения выше 1600x1200","Bit rate values depend on the selected resolution. It is impossible to set 1600x1200 resolution on the third stream, if the resolution is higher than 1600x1200 on the first stream.","new"]
["3S Vision","3S Vision N1031","Camera","V1.04_STD-1","1","3","+",null,"+",null,null,"QXGA Mode: 2560x1920(h.264)/1280x960(mjpeg). FullHD Mode:1920x1080","+",null,"+","-","-","-","-","-","Значения битрейта зависят от значения разрешенияНа третьем потоке потоке нельзя выставить значение разрешения 1600x1200 если на первом потоке стоит значение разрешения выше 1600x1200","Bit rate values depend on the selected resolution. It is impossible to set 1600x1200 resolution on the third stream, if the resolution is higher than 1600x1200 on the first stream.","new"]
["3S Vision","3S Vision N1072","Camera","V1.09.1_STD-1","1","3","+",null,"+",null,null,"UXGA Mode : 1600x1200 / WXGA Mode: 1280x720","+",null,"+","-","-","-","-","-","Значения битрейта зависят от значения разрешения","Bit rate values depend on the selected resolution.","new"]
["3S Vision","3S Vision N4012 / N5012","Camera","V1.04_STD-1.20131127","1","3","+",null,"+",null,null,"1920x1080","+",null,"+","-","+","-","-","-",null,null,"improved"]
["3S Vision","3S Vision N6071","Camera ","V1.10_STD-1","1","3","+",null,"+",null,null,"1600x1200","+",{"$nulls":7},"1. Диапазон доступных значений битрейта меняется в зависимости от значения выбранного разрешения.\n2. Диапазон доступных разрешений меняется в зависимости от значения настройки sensor-mode.","1. The range of available bit rate values ​​vary depends on the selected resolution.\n2. The range of available permits varies depends on the sensor-mode setting value."]
["3S Vision","3S Vision N8071","Camera","V1.08.1_STD-1","1","3","+",null,"+",null,null,"UXGA Mode : 1600x1200 / WXGA Mode: 1280x720","+",null,"+","-",{"$nulls":3},"-","Значения битрейта зависят от значения разрешенияВ ПО ITV смену режима Sensor mode следует производить в веб-интерфейсе камеры","Bit rate values depend on the selected resolution. In Axxon software the Sensor mode is to be changed in the camera web interface.","new"]
["3S Vision","3S Vision N9018","Fisheye Camera","V1.00.1_STD-1","1","3","+",null,"+",null,null,"1920x1080","+",null,"-","-","-","-","-","-","Настройка битрейта имеет динамический диапазон, который зависит от текущих значений настроек разрешений, частоты кадров, частоты включения опорных кадров, ТВ-стандарта.","Bit rate has a dynamic value range that depends on current resolution, fps, key frame rate and TV standard.","new"]
["Abron","Abron ABC-i422VR","Camera","C1.0.20.2_Y",1,"2","+","-","+","-","-","1920x1080","+","-","+","+","-","+","+","motion detection","Диапазон значений битрейта зависит от значения FPSВ ПО ITV настройку опорных кадров следует производить в веб-интерфейсе камеры.","Bitrate range depends on FPSB value. Key frames are to be set in the camera web interface."]
["ACTi","ACTi ACD-2000Q encoder","Encoder","V3.04.08","4","1","+","+","-","-","-","720x480","+",null,"-","-","-","-","+","-"]
["ACTi","ACTi ACD-2100 encoder","Encoder ","A1D-220-V3.14.19-AC","1",null,"+","+",{"$nulls":3},"720x576",null,null,"+","-","+","+","+","motion detection","1. при MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","1. With MPEG-4, in Intellect, you may use the Quality slider to adjust the video stream bit rate. "]
["ACTi","ACTi ACD-2400 encoder","Encoder ","firmware system AGD-R2N-V2.06.00-AC; firmware channel A1D-220-V3.12.13-AC","16",null,"+","+",{"$nulls":3},"720x576",null,null,"+","-","+","+.","+.","-","1. При задействовании сразу большого количества каналов устройству неоходимо окоо 2-х минут на старт после запуска Intellect.\n2. телеметрия будет пока что работать только с камерами с протоколом Pelco-D, 9600. В Intellect следует выбирать телеметрию \"IPCamera\"","1. When using multiple channels simultaneously, the device needs about 2 minutes to start up, after Intellect is started up. \n2. So far, telemetry only works with cameras that support the Pelco-D protocol, 9600 bps. In Intellect, select IPCamera telemetry."]
["ACTi","ACTi ACM-1101P","Camera ","A1D-220-V3.09.14-AC","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","-",{"$nulls":3},"-","при MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","in MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate."]
["ACTi","ACTi ACM-1231","Camera ","A1D-V3.11.13","1",null,"+","+",{"$nulls":3},"1280x1024",null,null,"+","-",{"$nulls":3},"-","1. У самой камеры есть ограничение на fps:\n-при размершении 1280x1024 максимально 8 fps\n2. За неимением на самом устройства настройки качества видеоизображения, ползунок \"Качество\"  в Intellect регулирует bit rate MPEG-4 видеопотока","1. The camera itself has frame rate limits: \n1280x1024 resolution, max. 8 fps.\n2. The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream."]
["ACTi","ACTi ACM-1431","Camera ","A1D-V3.11.13","1",null,"+","+",{"$nulls":3},"720x576",null,null,"+","-",{"$nulls":3},"-","для MPEG-4 за неимением на самом устройства настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","For MPEG-4, the device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream."]
["ACTi","ACTi ACM-1511","Camera ","A1D-V3.11.13","1",null,"+","+",{"$nulls":3},"1280x1024",null,null,"+","-",{"$nulls":3},"-","1. У самой камеры есть ограничение на fps:\n-при размершении 1280x1024 максимально 8 fps\n2. За неимением на самом устройства настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate MPEG-4 видеопотока.","1) The camera itself has frame rate limits:\n- 1280x1024 resolution, max. 8 fps. The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream."]
["ACTi","ACTi ACM-3001","Camera ","V3.11.13-AV","1","1","+","+",{"$nulls":3},"640x480",{"$nulls":5},"-","-","-"]
["ACTi","ACTi ACM-3011","Camera ","V3.11.13-AV","1","1","+","+",{"$nulls":3},"640x480",{"$nulls":5},"-","-","-"]
["ACTi","ACTi ACM-3401","Camera ","A1D-220-V3.12.13-AC","1",null,"+","+",{"$nulls":3},"1280x1024",null,null,"+","-",{"$nulls":3},"-","1. после переподключения питания камере видеопоток всегда восстанавливается в разрешении 1280x1024\n2. У самой камеры есть ограничение на fps:\n-при размершении 1280х720 максимально 10 fps\n-при размершении 1280x1024 максимально 8 fps\n3. для MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","1) After you reconnect the power adapter, the video stream always restarts with 1280x1024 resolution. The camera itself has frame rate limits:\nat 1280x720 resolution, max. 10 fps\nat 1280x1024 resolution, max. 8 fps\n3. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate."]
["ACTi","ACTi ACM-3411","Camera ","A1D-V3.11.13","1",null,"+","+",{"$nulls":3},"1280x1024",null,null,"+","-",{"$nulls":3},"-"]
["ACTi","ACTi ACM-3511","Camera ","A1D-220-V3.12.15-AC","1","1","+","+",{"$nulls":3},"1280x1024",{"$nulls":7},"-"]
["ACTi","ACTi ACM-3601","Camera ","V3.11.13-AV","1","1","+","+",{"$nulls":3},"640x480",{"$nulls":7},"-"]
["ACTi","ACTi ACM-3701 / ACM-3703","Camera ","V3.12.13-AC","1","1","+","+",{"$nulls":3},"1280x1024",{"$nulls":7},"-"]
["ACTi","ACTi ACM-4000","Camera ","A1D-220-V3.12.13-AC","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","-",{"$nulls":3},"-"]
["ACTi","ACTi ACM-4001","Camera ","A1D-V3.11.13","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","-",{"$nulls":3},"-"]
["ACTi","ACTi ACM-4200","Camera ","A1D-220--V3.12.13-AC","1",null,"+","+",{"$nulls":3},"1280x1024",null,null,"+","-",{"$nulls":3},"-","1. У самой камеры есть ограничение на fps:\n-при размершении 1280х720 максимально 10 fps\n-при размершении 1280x1024 максимально 8 fps\n2. для MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n","1) The camera itself has frame rate limits:\nat 1280x720 resolution, max. 10 fps\nat 1280x1024 resolution, max. 8 fps\n2. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate.\n"]
["ACTi","ACTi ACM-4201","Camera ","A1D-220--V3.12.13-AC","1",null,"+","+",{"$nulls":3},"1280x1024",null,null,"+","-",{"$nulls":3},"-","1. У самой камеры есть ограничение на fps:\n-при размершении 1280х720 максимально 10 fps\n-при размершении 1280x1024 максимально 8 fps\n2. для MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n\n","1. The camera itself has frame rate limits:\nat 1280x720 resolution, max. 10 fps\nat 1280x1024 resolution, max. 8 fps\n2. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate.\n\n"]
["ACTi","ACTi ACM-5001","Camera ","V3.12.13-AC","1","1","+","+",{"$nulls":3},"640x480",{"$nulls":7},"-"]
["ACTi","ACTi ACM-5601","Camera ","A1D-220--V3.12.13-AC","1",null,"+","+",{"$nulls":3},"1280x1024",null,null,"+","-",null,"+","+","-","1. У самой камеры есть ограничение на fps:\n-при размершении 1280х720 максимально 10 fps\n-при размершении 1280x1024 максимально 8 fps\n2. для MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n3. при включении настройки Flickless Mode=50Hz в веб-интерфейсе возможно \"проседание\" fps до 7-8, но это особенность самой камеры.","1. The camera itself has frame rate limits:\nat 1280x720 resolution, max. 10 fps\nat 1280x1024 resolution, max. 8 fps\n2. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate.\n3. When the Flickerless Mode=50Hz setting is on in the web interface, the frame rate may drop to 7–8 fps, but this is a limitation of the camera itself. "]
["ACTi","ACTi ACM-5611","Camera ","A1D-220-V3.13.06-AC","1",null,"+","+",{"$nulls":3},"1280x1024",null,null,"+","-",null,"+","+","-","1. У самой камеры есть ограничение на fps:\n-при размершении 1280х720 максимально 10 fps\n-при размершении 1280x1024 максимально 8 fps\n2. для MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n","1. The camera itself has frame rate limits:\nat 1280x720 resolution, max. 10 fps\nat 1280x1024 resolution, max. 8 fps\n2. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate.\n"]
["ACTi","ACTi ACM-5711","Camera ","A1D-220-V3.12.13-AC","1",null,"+","+",{"$nulls":3},"720x576",null,null,"+","-",null,"+","+","-","1. при MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n \nкамера с прошивкой A1D-V3.11.13 не работает в Intellect 4.7.8","1. in MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate.\n \nIn Intellect 4.7.8, the camera does not work with the A1D-V3.11.13 firmware. "]
["ACTi","ACTi ACM-7411","Camera ","A1D-220-V3.12.15-AC","1","1","+","+",{"$nulls":3},"1280x1024",{"$nulls":7},"-"]
["ACTi","ACTi ACM-7511","Camera ","A1D-220-V3.12.13-AC","1","1","+","+",{"$nulls":3},"720x576",{"$nulls":7},"-"]
["ACTi","ACTi ACM-8211","Camera ","V3.11.13-AV","1","1","+","+",{"$nulls":3},"1280x1024",null,null,"+","-","+","+","+","-","1. У самой камеры есть ограничение на fps:\n-при размершении 1280х720 максимально 10 fps\n-при размершении 1280x1024 максимально 8 fps\n2. для MPEG-4 ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n","1. The camera itself has frame rate limits:\nat 1280x720 resolution, max. 10 fps\nat 1280x1024 resolution, max. 8 fps\n2. In MPEG-4 mode, in Intellect, you may use the Quality slider to adjust the video stream bit rate.\n"]
["ACTi","ACTi ACM-8511","Camera ","v3.12.15-AC ","1","1","+","+",{"$nulls":3},"720x576","+",{"$nulls":3},"+",{"$nulls":3},"1. при подключении к камере следует следить, чтобы значение настройки \"ТВ-стандарт\" в ПО ITV соответствовало типу камеры (PAL или NTSC).","1. When connecting to the camera, be sure to set the TV standard in the AxxonSoft software to the right camera type (PAL or NTSC). "]
["ACTi","ACTi CAM-6600","Camera ","A1D-M2N-V2.09.11-AC","1",null,"+","+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)",{"$nulls":4},"+",null,null,"-","1. За неимением на самом устройства настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.","1. The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the MPEG-4 video stream."]
["ACTi","ACTi CAM-6610","Camera ","A1D-M2N-V2.09.11-AC","1",null,"+","+",{"$nulls":3},"720x576(PAL)/720x480(NTSC)",{"$nulls":4},"+.",{"$nulls":3},"Для корректной работы самого устройства с прошивкой A1D-M2N-V2.09.11-AC рекомендуется выставлять только PAL","If the device has the A1D-M2N-V2.09.11-AC firmware, to ensure that the device works smoothly, set PAL."]
["ACTi","ACTi CAM-6630","Camera ","A1D-M2N-V2.09.11-AC","1","1","+","+",{"$nulls":3},"720x576(PAL)/720x480(NTSC)",{"$nulls":4},"+",{"$nulls":3},"Для корректной работы самого устройства с прошивкой A1D-M2N-V2.09.11-AC рекомендуется выставлять только NTSC","If the device has the A1D-M2N-V2.09.11-AC firmware, to ensure that the device works smoothly, set NTSC."]
["ACTi","ACTi D11 / D21 / D31 / D41 / D51 / D54 / D61 / D64 / D71 / D81 / E21 / E31 / E41 / E45 / E51 / E52 / E61 / E64 / E66 / E71 / E81 / E85 / E91 / E94 ","Camera ","6.01.06","1","2","+",null,"+",null,null,"1280x720","+",{"$nulls":6},"motion detection","1. Для изменения частоты опорных кадров через Интеллект необходимо выбирать следующие значения: \"1 Second\" - 10, \"2 Second\" - 20,..., \"5 Second\" - 50. Особенность устройства.","1. To change the keyframe rate in Intellect, please select one out of the range: \"1 Second\" - 10, \"2 Second\" - 20,..., \"5 Second\" - 50. This is a limitation of the device itself."]
["ACTi","ACTi D12 / D32 / D42 / D52 / D55 / D65 / D72 / D82 / E24 / E32 / E34 / E42 / E46 / E53 / E62 / E65 / E72 / E74 / E82 / E86 / E92","Camera ","V6.03.17","1","2","+",null,"+",null,null,"2048x1536","+",{"$nulls":6},"motion detection","1. Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность текущей прошивки.\n2. Частота опорных кадров задается в секундах и может принимать значения от 1 до 5. ","1. To work with MJPEG correctly, please select low resolution, quality and FPS. This is a limitation of the current firmware. 2. The keyframe rate is set in seconds and can range from 1 to 5."]
["ACTi","ACTi D22 / E22 / E33 / E43 / E43A / E54 / E63 / E73 / E83","Camera ","V6.04.15","1","2","+",null,"+",null,null,"2592x1944 ","+",{"$nulls":6},"motion detection","1. Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность текущей прошивки.\n2. Частота опорных кадров задается в секундах и может принимать значения от 1 до 5. ","1. To work with MJPEG correctly, please select low resolution, quality and FPS. This is a limitation of the current firmware. 2. The keyframe rate is set in seconds and can range from 1 to 5."]
["ACTi","ACTi E11 ","Camera ","V6.02.03","1","2","+",null,"+",null,null,"1280x720 ","+",null,"-","-","-","-","-","-","1. Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность текущей прошивки. 2. В ПО Axxon аудио-кодек и для микрофона и для динамика устройства устанавливается в настройках объекта Микрофон.","1. To work with MJPEG correctly, please select low resolution, quality and FPS. This is a limitation of the current firmware. 2. In AxxonSoft software, you can set the codecs for mics and speakers in the Microphone object settings."]
["ACTi","ACTi E12 ","Camera ","V6.03.17 ","1","2","+",null,"+",null,null,"2048x1536 ","+",null,"+",{"$nulls":4},"motion detection","1. Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность текущей прошивки. 2. На камере есть два режима отображения Auto / 4:3, которые переключаются в веб-интерфейсе. ","1. To work with MJPEG correctly, please select low resolution, quality and FPS. This is a limitation of the current firmware. 2. The camera has two display modes, Auto/4:3, which can be toggled in the web interface. "]
["ACTi","ACTi E13","Camera ","V6.03.17 ","1","2","+",null,"+",null,null,"2592x1944 ","+",null,"+",{"$nulls":4},"motion detection","Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность текущей прошивки. ","1. To work with MJPEG correctly, please select low resolution, quality and FPS. This is a limitation of the current firmware."]
["ACTi","ACTi E23 / E44 / D62 / E67 / E84 / E95 ","Camera ","V6.03.17 ","1","2","+",null,"+",null,null,"1920x1080 ","+",{"$nulls":6},"motion detection","Для корректной работы кодека MJPEG в ПО ITV/Axxon следует в его настройках выбирать низкие значения разрешения, качества и частоты кадров. Это особенность текущей прошивки. ","1. To work with MJPEG correctly, please select low resolution, quality and FPS. This is a limitation of the current firmware."]
["ACTi","ACTi KCM-3911 / KCM-7911","Camera ","5.07.05","1","10","+","+","+",null,null,"1920x1072","+",null,"+","-",null,"+","+","motion detection","1. Разрешение в Интеллект нужно настраивать через вэб-интерфейс","1. You can configure resolution in Intellect via web interface."]
["ACTi","ACTi KCM-5111","Camera ","5.07.05","1","7","+","+","+",null,null,"2032x1920","+",null,"+.","-",null,"+","+","motion detection","1. Устройство поддерживает 3 режима видео (в Axxon Next выбирается соответствующей настройкой в группе \"Другое\"): \n 1)Однопоточный. Используется поток 0. Максимально доступная частота кадров зависит от выбранного кодека и разрешения.\n2) Двухпоточный. Используются потоки 1 и 2. \nДоступность разрешений и значений частоты кадров в одном потоке зависит от текущей конфигурации другого потока. \nВ режиме \"Двойной поток\" доступны комбинации кодеков:\nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) Четырёхпоточный. Используются потоки 3,4,5 и 6. Каждый поток показывает выбранную часть картинки от всего изображения, получаемого камерой. Координаты каждого фрагмента в Axxon Next задаются в группе настроек \"Другое\".","1. The device supports 3 video modes (in AN, you select a video mode in the Other group of settings): \n 1) 1 stream. Stream 0 is used. The maximum available frame rate depends on which codec and resolution are selected.\n2) 2 streams. Streams 1 and 2 are used. Which resolutions and frame rates are available for one stream depends on the current settings of the other. In *2 streams* mode, the following codec combinations are available: \nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) 4 streams. Streams 3, 4, 5, and 6 are used. Each stream shows a part of the image received from the camera. In AN, the coordinates of each part are set in the Other group of settings."]
["ACTi","ACTi KCM-5211(E)","Camera ","5.03.02","1","7","+","+","+",null,null,"2032х1920","+",null,"+","-","+.","+","+","-","1. Устройство поддерживает 3 режима видео (в Axxon Next выбирается соответствующей настройкой в группе \"Другое\"): \n 1)Однопоточный. Используется поток 0. Максимально доступная частота кадров зависит от выбранного кодека и разрешения.\n2) Двухпоточный. Используются потоки 1 и 2. \nДоступность разрешений и значений частоты кадров в одном потоке зависит от текущей конфигурации другого потока. \nВ режиме \"Двойной поток\" доступны комбинации кодеков:\nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) Четырёхпоточный. Используются потоки 3,4,5 и 6. Каждый поток показывает выбранную часть картинки от всего изображения, получаемого камерой. Координаты каждого фрагмента в Axxon Next задаются в группе настроек \"Другое\".","1. The device supports 3 video modes (in AN, you select a video mode in the Other group of settings): \n 1) 1 stream. Stream 0 is used. The maximum available frame rate depends on which codec and resolution are selected.\n2) 2 streams. Streams 1 and 2 are used. Which resolutions and frame rates are available for one stream depends on the current settings of the other. In *2 streams* mode, the following codec combinations are available: \nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) 4 streams. Streams 3, 4, 5, and 6 are used. Each stream shows a part of the image received from the camera. In AN, the coordinates of each part are set in the Other group of settings."]
["ACTi","ACTi KCM-5311 / KCM-5311E","Camera ","5.03.02","1","3","+","+","+",null,null,"1920x1080","+",null,"+","-","+.","+","+","-","1. Устройство поддерживает 3 режима видео (в Axxon Next выбирается соответствующей настройкой в группе \"Другое\"): \n 1)Однопоточный. Используется поток 0. Максимально доступная частота кадров зависит от выбранного кодека и разрешения.\n2) Двухпоточный. Используются потоки 1 и 2. Доступность разрешений и значений частоты кадров в одном потоке зависит от текущей конфигурации другого потока. В режиме \"Двойной поток\" доступны комбинации кодеков:\nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n2. Камера не поворотная, но есть встроенный трансфокатор.","1. The device supports 3 video modes (in Axxon Next, select the right video mode in the Other group of settings): \n1) Single Stream. Stream 0 is used. The maximum available frame rate depends on which codec and resolution are selected. \n2) Double Stream. Streams 1 and 2 are used. The availability of resolutions and frame rates for one stream depends on the current settings of the other. In Dual Stream mode, the following codec combinations are available: mjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n\n2. This is not a PTZ camera, but it has a built-in zoom lens. "]
["ACTi","ACTi KCM-5511","Camera","V5.11.17","1","3","+","+","+","-","-","1920х1072","+",null,"-","-","-","-","-","motion detection"]
["ACTi","ACTi KCM-7111","Camera ","5.03.02","1","7","+","+","+",null,null,"2032х1920","+",null,"+","-",null,"+","+","-","1. Устройство поддерживает 3 режима видео (в Axxon Next выбирается соответствующей настройкой в группе \"Другое\"): \n 1)Однопоточный. Используется поток 0. Максимально доступная частота кадров зависит от выбранного кодека и разрешения.\n2) Двухпоточный. Используются потоки 1 и 2. Доступность разрешений и значений частоты кадров в одном потоке зависит от текущей конфигурации другого потока. В режиме \"Двойной поток\" доступны комбинации кодеков:\nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) Четырёхпоточный. Используются потоки 3,4,5 и 6. Каждый поток показывает выбранную часть картинки от всего изображения, получаемого камерой. Координаты каждого фрагмента в Axxon Next задаются в группе настроек \"Другое\".","1. The device supports 3 video modes (in Axxon Next, select the right video mode in the Other group of settings): \n1) Single Stream. Stream 0 is used. The maximum available frame rate depends on which codec and resolution are selected. \n2) Double Stream. Streams 1 and 2 are used. The availability of resolutions and frame rates for one stream depends on the current settings of the other. In Dual Stream mode, the following codec combinations are available: mjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) 4-stream. Streams 3, 4, 5, and 6 are used. Each stream shows a part of the image received from the camera. In Axxon Next, the coordinates of each part are set in the Other group of settings. "]
["ACTi","ACTi KCM-7211","Camera ","5.03.02","1","7","+","+","+",null,null,"2032x1920","+",null,"+","-","+.","+","+","-","1. Устройство поддерживает 3 режима видео (в Axxon Next выбирается соответствующей настройкой в группе \"Другое\"): \n 1)Однопоточный. Используется поток 0. Максимально доступная частота кадров зависит от выбранного кодека и разрешения.\n2) Двухпоточный. Используются потоки 1 и 2. Доступность разрешений и значений частоты кадров в одном потоке зависит от текущей конфигурации другого потока. В режиме \"Двойной поток\" доступны комбинации кодеков:\nmjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) Четырёхпоточный. Используются потоки 3,4,5 и 6. Каждый поток показывает выбранную часть картинки от всего изображения, получаемого камерой. Координаты каждого фрагмента в Axxon Next задаются в группе настроек \"Другое\".\n2. Камера не поворотная, но есть встроенный трансфокатор.","1. The device supports 3 video modes (in Axxon Next, select the right video mode in the Other group of settings): \n1) Single Stream. Stream 0 is used. The maximum available frame rate depends on which codec and resolution are selected. \n2) Double Stream. Streams 1 and 2 are used. The availability of resolutions and frame rates for one stream depends on the current settings of the other. In Dual Stream mode, the following codec combinations are available: mjpeg +mjpeg/mpeg4/h264; \nmpeg4 +mjpeg/mpeg4; \nh264 +mjpeg/h264.\n3) 4-stream. Streams 3, 4, 5, and 6 are used. Each stream shows a part of the image received from the camera. In Axxon Next, the coordinates of each part are set in the Other group of settings. \n2. This is not a PTZ camera, but it has a built-in zoom lens. "]
["ACTi","ACTi KCM-7311 ","Camera ","5.08.06","1","6","+","+","+",null,null," 2032x1920 ","+",{"$nulls":3},"+",null,null,"motion detection"]
["ACTi","ACTi KCM-8211","Camera ","V5.09.12","1","2","+","+","+",null,null,"1280x720","+",{"$nulls":3},"+",null,null,"motion detection","Между потоками камеры есть следующая зависимость:\nесли на одном потоке выставить MPEG4, то на другом будут доступны только кодеки MJPEG и MPEG4\nесли на одном потоке выставить MJPEG, то на другом будут доступны все кодеки\nесли на одном потоке выставить H.264, то на другом будут доступны только кодеки H.264 и MJPEG\nПри выборе в по Axxon Next двухпоточного режима рекомендуется для настройки \"режим передачи видеоизображения\" выставить значение \"2 видеопотока\". Также необходимо для настройки \"режим передачи видеоизображения\" выставить значение \"2 видеопотока\", если в режиме однопоточности необходимо получать видео со второго потока\nДля того чтобы настройка фокуса работала в продукте, необходимо в веб-интерфейсе камеры режим управления фокусом выставить в ручной режим.\nДетектор движения работает только с кодеками H.264 и MPEG4","There is a following relationship between camera's streams:\nif one stream MPEG4, then on the other stream will be available codecs MJPEG and MPEG4;\nif one stream MJPEG, then on the other one will be available all codecs;\nif one stream H.264, then on the other one will be accessed only codecs H.264 and MJPEG;\nWhen selecting dualstream mode in Axxon Next is recommended for setting \"video transmission mode\" set to \"2 video stream\". Also need to adjust the \"transmission mode video\" set to \"2 video\" if you need to receive multistreaming mode with second video stream.\nTo adjust the focus setting in AxxonSoft products, it is necessary using camera's web interface, the camera focus control mode set to manual mode.\nMotion detector works only with codecs H.264 and MPEG4."]
["ACTi","ACTi TCD-2100 encoder","Encoder ","V4.07.15-AC","1",null,"+","+","+",null,null,"720x480"]
["ACTi","ACTi TCD-2500 encoder","Encoder ","A1D-310-V4.06.08-AC","1",null,"+","+","+",null,null,"720x576",null,null,"+","-","+","+","+","-"]
["ACTi","ACTi TCM-1231","Camera ","V4.12.09-AC","1","2","+","+","+",null,null,"1280x1024","+",null,"+","-",null,"+","+","motion detection.","Между потоками камеры есть следующая зависимость:\n если на одном потоке выставить MPEG4, то на другом будут доступны только кодеки MJPEG и MPEG4\n если на одном потоке выставить MJPEG, то на другом будут доступны все кодеки\n если на одном потоке выставить H.264, то на другом будут доступны только кодеки H.264 и MJPEG\nДля получения видео по Axxon Next с двух потоков или со второго потока необходимо для настройки \"режим передачи видеоизображения\" выставить значение \"2 видеопотока\".\nДетектор движения на камере доступен только если на первом потоке стоят кодеки H.264 и MPEG4.\nЕсли режим экспозиции выставить в ручной режим, то для настройки баланс белого становится недоступным значение \"авто\"\nДиапазон значений fps зависит от значения разрешения.","Streams of the camera depend on below behavior:\nif at one stream select MPEG4, at other one will be available MJPEG and MPEG4\nif at one stream select MJPEG, then, at second one will ba available all codecs\nif at one stream select H.264, at other one will be available only H.264 and MJPEG.\nTo get video from two or second stream(s) in Axxon Next Для need to select \"video transmit mode\" in value \"2 streams\".\nMotion detection is available only if at first stream schoosen codecs H.264 or MPEG4.\nIf you select exposition mode in manual mode, for white balance setting will be not available value \"auto\".\nFPS range depends on from resolution."]
["ACTi","ACTi TCM-1511","Camera ","V4.07.15-AC","1",null,"+","+","+",null,null,"1280x1024",{"$nulls":8},"Для H.264 и MPEG-4 качество регулируется через Bit Rate. Для корректной работы качества необходимо, что бы значение поля Video Bit Rate Mode было Constant Bit Rate.\n","For H.264 and MPEG-4, the quality is adjusted with Bit Rate. For the quality to work smoothly, be sure to set the Video Bit Rate Mode field to Constant Bit Rate.\n"]
["ACTi","ACTi TCM-3001","Camera ","V4.07.15-AC","1",null,"+","+","+",null,null,"640x480",{"$nulls":7},"-","Для H.264 и MPEG-4 качество регулируется через Bit Rate. Для корректной работы качества необходимо, что бы значение поля Video Bit Rate Mode было Constant Bit Rate.","For H.264 and MPEG-4, the quality is adjusted with Bit Rate. For the quality to work smoothly, be sure to set the Video Bit Rate Mode field to Constant Bit Rate."]
["ACTi","ACTi TCM-3011","Camera ","4.08.05","1","2","+","+","+",null,null,"640x480"]
["ACTi","ACTi TCM-3401 / TCM-3411","Camera ","A1D-310-V4.07.15-AC ","1",null,"+","+","+",null,null,"1280x1024",{"$nulls":7},"-","При удаленном тестировании не невозможно было проверить: ip-wizard, audio in / out, лучи / реле","During the remote testing, we were not able to check the following: IP Wizard, audio in / out, sensors / relays. "]
["ACTi","ACTi TCM-3511","Camera ","4.07.15-AC","1",null,"+","+","+",null,null,"1280x1024"]
["ACTi","ACTi TCM-4001","Camera ","V4.07.15-AC","1",null,"+","+","+",null,null,"640x480"]
["ACTi","ACTi TCM-4201","Camera ","V4.07.15-AC","1","2","+","+","+",null,null,"1280x1024",null,null,"+",{"$nulls":4},"-"]
["ACTi","ACTi TCM-4301","Camera ","A1D-310-V4.06.09-AC","1",null,"+","+","+",null,null,"1024x768","+",null,"+","-",{"$nulls":3},"-"]
["ACTi","ACTi TCM-4511","Camera ","v4.12.09","1","2","+","+","+",null,null,"1280x1024","+",{"$nulls":7},"1. Детектор движения работает только при H.264 или MPEG4 на 1-ом потоке","1. VMD works only if H.264 or MPEG4 is enabled for stream 1."]
["ACTi","ACTi TCM-5001","Camera ","V4.07.15-AC","1","2","+","+","+",null,null,"640x480"]
["ACTi","ACTi TCM-5111","Camera ","v4.12.09","2","3","+","+","+",null,null,"1280x1024","+",{"$nulls":7},"1. Детектор движения работает только при H.264 или MPEG4 на 1-ом потоке","1. VMD works only if H.264 or MPEG4 is enabled for stream 1."]
["ACTi","ACTi TCM-5311","Camera ","A1D-310-V4.06.09-AC","1",null,"+","+","+",null,null,"1280x960",null,null,"+","-",null,"+","+","-","1. Поддержка двух стримингов (т.е. двух независимых видеоканалов в Intellect пока отсутствует)\n2. в разрешении 1280х960  сама камера выдает максимально 15 fps\n ","1. Dual streaming (i.e., two independent video channels ) is not yet supported by Intellect.\n2. At 1280x960 resolution, the camera itself is capable of running at 15 fps max. \n "]
["ACTi","ACTi TCM-5601","Camera ","V4.07.15-AC","1","2","+","+","+",null,null,"1280x1024"]
["ACTi","ACTi TCM-5611","Camera ","V4.07.15-AC","1","2","+","+","+",null,null,"1280x1024"]
["ACTi","ACTi TCM-7011","Camera ","V4.07.15-AC","1","2","+","+","+",null,null,"640x480",{"$nulls":7},"-"]
["ACTi","ACTi TCM-7411","Camera ","V4.07.15-AC","1",null,"+","+","+",null,null,"1280x1024"]
["ACTi","ACTi TCM-7811","Camera ","V4.08.05-AC","1",null,"+","+","+",null,null,"1280x960"]
["Acumen","Acumen AiP-U53K","Camera ","1.1.010(Ai)","1","3","+",null,"+",null,null,"1920x1080","+"]
["Acumen","Acumen AiP-B34N 05Y2B","Camera ","1.0.506k(Ai)","1","4","+",null,"+",null,null,"1920x1080(MJPEG) / 2048x1536(H264)","+",null,"+",{"$nulls":5},"На камере есть настройка Profile, от которой зависят не только разрешение и кодеки на стримингах, но и количество этих самых стримингов. В настройках камеры в ПО ITV/AxxonSoft необходимо выбирать тот же кодек, который установлен в веб-интерфейсе камеры для соответствующего потока.\nНастраивать потоки необходимо исходя из зависимостей в веб-интерфейсе.\nПри смене профиля камера перезагружается в течение полутора минут.\nНастройка RTSP-порта не изменяет текущее значение порта на камере, её необходимо выставлять согласно вебу.","The camera has Profile setting, this setting influences to resolution, codecs available on streams, and to number of streams. In SW AxxonSoft you need to select the same codec as in camera's web-interface for corresponding stream. \nYou need to tune streams in accordance with dependences in web-interface.\nAfter profile changing camera will be rebooted during 90 seconds.\nRTSP port setting doesn't change current value at camera's port. You need to tune it in accordance with web-interface."]
["Acumen","Acumen AiP-L24N-66Y2B","Camera","1.0.504(Ai)","1","4","+",null,"+",null,null,"1920x1080","+",null,"-","-","-","-","-","audio detection","Значение настройки RTSP порт должно соответствовать значению аналогичной настройки, выставленному в веб-интерфейсе на странице Network → HTTP/RTSP Service. Особенность прошивки камеры не позволяет провести полноценную интеграцию настроек видео без необходимости совершения дополнительных действий в веб-интерфейсе камеры. Для корректной работы настроек в ПО ITV/Axxon необходимо, настройки \"Видеокодек\" и \"Разрешение\" в ПО ITV/Axxon соответствовали аналогичным настройкам в веб-интерфейсе камеры, где они зависят от значения параметра Profile (Settings → Video / Audio).","The value of RTSP port setting is to correspond to the value of the similar setting set in the web interface on the Network → HTTP/RTSP Service page. Camera firmware does not allow integrating video settings without other actions in the camera web interface. For proper operation of settings in Axxon software, the Video codec and Resolution settings in Axxon software are to correspond to the similar settings in the camera web interface where they depend on the Profile (Settings → Video / Audio) parameter. ","new"]
["Acumen","Acumen AIP-M53K(ONVIF)","Camera ","1.1.006(Ai)","1","1","+",{"$nulls":4},"720x480","+"]
["Acumen","Acumen AiP-P53N-45Y2B","Camera","1.1.006.2(Ai) ","1","3","+",null,"+",null,null,"1920x1080","+",null,"-","-",null,"-","-","-","Значение настройки RTSP порт должно соответствовать значению аналогичной настройки, выставленному в веб-интерфейсе на странице Network → HTTP/RTSP Service.Особенность прошивки камеры не позволяет провести полноценную интеграцию настроек видео без необходимости совершения дополнительных действий в веб-интерфейсе камеры. Для корректной работы настроек в ПО ITV/Axxon необходимо, настройки \"Видеокодек\" и \"Разрешение\" в ПО ITV/Axxon соответствовали аналогичным настройкам в веб-интерфейсе камеры, где они зависят от значения параметра Profile (Settings → Video / Audio). ","The value of RTSP port setting is to correspond to the value of the similar setting set in the web interface on the Network → HTTP/RTSP Service page. Camera firmware does not allow integrating video settings without other actions in the camera web interface. For proper operation of settings in Axxon software, the Video codec and Resolution settings in Axxon software are to correspond to the similar settings in the camera web interface where they depend on the Profile (Settings → Video / Audio) parameter. ","new"]
["Acumen","Acumen AiP-R53K-05Y1B","Camera","1.1.010(Ai)","1","3","+",null,"+",null,null,"1920x1080","+",null,"-","-",{"$nulls":3},"-","Значение настройки RTSP порт должно соответствовать значению аналогичной настройки, выставленному в веб-интерфейсе на странице Network → HTTP/RTSP Service. Особенность прошивки камеры не позволяет провести полноценную интеграцию настроек видео без необходимости совершения дополнительных действий в веб-интерфейсе камеры. Для корректной работы настроек в ПО ITV/Axxon необходимо, настройки \"Видеокодек\" и \"Разрешение\" в ПО ITV/Axxon соответствовали аналогичным настройкам в веб-интерфейсе камеры, где они зависят от значения параметра Profile (Settings → Video / Audio).","The value of RTSP port setting is to correspond to the value of the similar setting set in the web interface on the Network → HTTP/RTSP Service page. Camera firmware does not allow integrating video settings without other actions in the camera web interface. For proper operation of settings in Axxon software, the Video codec and Resolution settings in Axxon software are to correspond to the similar settings in the camera web interface where they depend on the Profile (Settings → Video / Audio) parameter. ","new"]
["Adino","Adino TC-NC6453S2-2MP","Camera","NVSSv3.0.1_20120619","1","1","+","-","+","-","-","1600x1200","+","-","-","-","-","-","-","-","Диапазон значений битрейта на камере динамичен и зависит от текущего значения разрешения.","Camera bitrate range is dynamic and depends on the current resolution."]
["Alinking","Alinking ALC-9122P","Camera ","V1.32 STD-1","1","2","+","+",{"$nulls":3},"1280x960","+",null,"-","-","-","-","-","-","1. Настройка PAL / NTSC в ПО Intellect переключается режимы Partial / Full Scan\n2. Разрешение 1280х960 доступно только в MJPEG и только в режиме Full Scan (максимальный fps в данном режиме = 12)\n3. При смене разрешения на одном стримминге разрешение автоматически изменится и на втором. Особенность интеграции.","1. In Intellect, the PAL / NTSC setting switches between Partial mode and Full Scan mode.\n2. 1280х960 is available only in MJPEG and only in Full Scan mode (in this mode, max. frame rate is 12 fps).\n3. When you change the resolution of one stream, the resolution of the other one changes automatically. This is for integration. "]
["Alinking","Alinking ALC-9171P","Camera ","V1.04 STD-1","1","3","+",null,"+",null,null,"1280x720 / 1600x1200","+",null,"-","-","-","-","-","-","1. Фактический fps видеопотока очень сильно зависит от разрешения, качества и фокусировки картинки.\n2. Настройка яркости не работает на самом устройстве\n3. Настройка PAL/NTSC в ПО ITV/Axxon переключает режимы UXGA / WXGA (различаются набором разрешений).","1. The actual frame rate very much depends on the image resolution, quality, and focus. \n2. The brightness setting does not work on the device itself. In the AxxonSoft software, the PAL/NTSC setting switches between the UXGA and WXGA modes (the modes offer different sets of resolutions). "]
["AMG","AMG-Panogenics PanoCam360","Camera ","01.04.03","1","14","+","+","+",null,null,"2144x1944","+",{"$nulls":3},"-","+.","+",null,"1. Видео кодек устанавливается на все потоки\n2. Настройка \"bitrateControl\" также устанавливается на все потоки","1. Video codec is applied to all streams.\n2. BitrateControl is applied to all streams either."]
["A-MTK ","A-MTK AM2030D / AM2290D / AM2530D / AM2560D / AM2570D / AM2630D / AM2730D ","Camera ","6.D.2.9659","1","20","+","+","+",null,null,"1920x1080","+"]
["Arecont Vision","Arecont Vision AV10005/-DN","Camera ","65201","1","2","+",null,"+",null,null,"3648x2752","+",{"$nulls":4},"+","+","+","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Камера имеет ограничение по FPS:\n - 6fps @ 3648x2752\n - 25fps @ 1824x1376\nДатчик должен быть под напряжением","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. The camera has frame rate limits:\n - 6 fps at 3648x2752\n - 25 fps at 1824x1376. \nClose the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV10115/-DN/-AI","Camera ",65218,"1","2","+",null,"+",null,null,"3648x2752","+",{"$nulls":4},"+","+","motion detection","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Камера имеет ограничение по FPS:\n - 7fps @ 3648x2752\n - 27fps @ 1824x1376\nДатчик должен быть под напряжением","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. The camera has frame rate limits:\n - 7 fps at 3648x2752\n - 27 fps at 1824x1376. \nClose the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV1115/-DN/-AI","Camera ","65200","1","2","+",null,"+",null,null,"1280x1024","+",{"$nulls":4},"+","+","+","1. Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.\n2. Производитель заявляет о частоте кадров в 40 fps (2 x 20 fps в двухпотоковом режиме). Камера достигает заявленных fps только при работе через протокол TFTP. При работе через протокол HTTP максимальная частота кадров - 25 fps (2 x 12 fps в двухпотоковом режиме).\n3. Прошивка 65200: при использовании встроенного детектора частота кадров падает до 5 fps.\n4.Луч должен быть под напряжением.","1. The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. \n2. The vendor states that the frame rate is 40 fps (2 x 20 fps in dual-stream mode). The camera reaches this frame rate only when using the TFTP protocol. When using the HTTP protocol, the max. frame rate is 25 fps (2 x 12 fps in dual-stream mode). \n3. 65200 firmware: when the embedded detection tool is used, the frame rate drops to 5 fps. \n4. Close the alarm input when it is energized."]
["Arecont Vision","Arecont Vision AV1125/-DN/-IR","Camera ","65201 / 65202","1","2","+",null,"+",null,null,"1280x1024","+",{"$nulls":4},"+",null,"+","AV1125 - прошивка 65201\nAV1125-DN/-IR - прошивка 65202\nПараметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет. \nЛуч должен быть под напряжением.","\"AV1125 - firmware v.65201 \nAV1125-DN/-IR - firmware v .65202\nThe Auto Iris and Shutter Speed parameters are integrated as telemetry settings - but the camera does not have the telemetry functionality. \nThe sensor must be energized.\n"]
["Arecont Vision","Arecont Vision AV12186DN","Camera ","65184","4","2","+",null,"+",null,null,"2048x1536","+",{"$nulls":5},"+","motion detection","Работа данной камеры по протоколу TFTP не поддерживается.","Work through RFTP protocol with this device is not supported."]
["Arecont Vision","Arecont Vision AV1300/-DN/-AI","Camera ","64116","1",null,"+",{"$nulls":4},"1280x1024",{"$nulls":5},"-","+","+","1. при мегапиксельном разрешении макимально доступны fps ~20\n2. Лучи не могут быть интегрированы. ","1. With megapixel resolutions, the max. resolution is 20 fps.\n2. The sensor cannot be integrated. "]
["Arecont Vision","Arecont Vision AV1305/-DN/-AI","Camera ","65143 / 65144","1","2","+",null,"+",null,null,"1280x1024","+",{"$nulls":5},"+","+","1. AV1305/-Ai - прошивка 65143\n AV1305DN - прошивка 65144\n 2. Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.\n\n","1. AV1305/-Ai - firmware 65143\n AV1305DN - firmware 65144\n2. The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. Close the sensor when it is energized"]
["Arecont Vision","Arecont Vision AV1310/-DN","Camera ","65143 / 65144","1","1","+",{"$nulls":4},"1280x1024",{"$nulls":5},"+","+",null,"1) аналог камеры Arecont AV1300\nотличие - AV1310 имеет более компактный корпус , улучшена работы настройки насыщенности цвета \n2) AV1310 - прошивка 65143\n AV1310DN - прошивка 65144 \n3) Лучи замыкаются под напряжением. ","1. This camera is very similar to the Arecont AV1300.\nDifferences: the AV1310 is smaller, the saturation setting works better. 2) AV1310 - fw 65143\n AV1310DN - fw 65144 \n3) Close the sensor when it is energized. "]
["Arecont Vision","Arecont Vision AV1315/-DN / AV1325/-DN/-IR","Camera ","65201","1","2","+",null,"+",null,null,"1280x1024","+",{"$nulls":4},"+","+","+","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.При просмотре видео через HTTP наблюдается падение FPS в AxxonNext/Next (MJPEG, H264) и Интеллект (H264) примерно до 6-10 кадров в секунду. По TFTP частота кадров нормальная.Датчик должен быть под напряжением","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. When the video is viewed via HTTP, the frame rate drops to 6–10 fps in AN (MJPEG and H.264) and in Intellect (H.264). When TFTP is used, the frame rate is normal. Close the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV1355/-DN/-HK/-DN-HK","Camera ","65139","1","2","+",null,"+.",null,null,"1280x1024",{"$nulls":4},"+","-","+","+","1. На прошивке 65139 H264-поток с камеры идет с искажениями. Искажения видны и в ПО ITV, и в ПО производителя камеры.\n","1. With the 65139 firmware, the H.264 stream becomes distorted. You can see the distortions both in the AxxonSoft software and in the vendor software. \n"]
["Arecont Vision","Arecont Vision AV20185DN / AV20365DN","Camera ","65170","4","2","+",null,"+",null,null,"2560x1920","+",{"$nulls":4},"+","+","+","Устройство представляет собой панорамную 4-объективную камеру.Модели 20185 и 20365 отличаются суммарным углом обзора: 180 и 360 градусов соответственно.Конструкция камеры имеет особенность: сенсор 2 и 4 перевернуты относительно сенсора 1 и 3 на 180 градусов. Поэтому изображение с них идет в нашем ПО перевернутым. Для коррекции в AxxonNext/Next нужно использовать специальный параметр, в Интеллекте - через веб-интерфейс.В ПО ITV интегрировано как видеосервер с 4-мя независимыми каналами видео, которые можно включать/отключать.Изменение некоторых настроек применяется ко всем каналам одновременно.Разрешения (см. выше) указаны для отдельного канала.Чем больше каналов одновременно используется, тем ниже частота кадров для каждого канала.Наивысшей частоты кадров камера достигает при работе по протоколу TFTP.Луч должен быть под напряжением.","This is a 4-lens panoramic camera. The 20185 and 20365 models have different total angles of view: 180 and 360 degrees, respectively. The camera's design has one peculiarity: sensors 2 and 4 are rotated by 180 degrees with respect to sensors 1 and 3. For this reason, for those rotated sensors, our software shows an upside-down image. To correct this, you must use a special parameter (in AN) or use the web interface (in Intellect). In the AxxonSoft software, the camera is integrated as a video encoder with 4 independent video channels, which can be switched on and off. Changes to some settings are applied to all the channels at once. The above resolutions are for a single channel. The more channels are used at the same time, the lower the frame rate is for each channel. The camera reaches the maximum frame rate when using the TFTP protocol. Close the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV2100/-DN/-AI","Camera ","64327 / 64328","1",null,"+",{"$nulls":4},"1600x1200",{"$nulls":5},"-","+","+","1) AV2100/-Ai - прошивка 64327\n AV2100DN - прошивка 64328\n2_ Ограничение по fps: 800x600 - 15 fps, 1600x1200 -14 fps \n\n","1. AV2100/-Ai - firmware 64327\n AV2100DN - firmware 64328\n2. Frame rate limits:\n- 800x600: 15 fps\n- 1600x1200: 14 fps\nyou may find the right balance between quality and speed (by manually setting a value between 1 and 10 ms)"]
["Arecont Vision","Arecont Vision AV2105/-DN/-AI","Camera ","65009","1",null,"+",null,"+.",null,null,"1600x1184",{"$nulls":5},"-","+","+","1) проблемы с H.264 - с CUDA искажается живое видео, в архиве искажение ещё сильнее\n2) если отключить CUDA , то искажений почти нет, но при это в компоненте \"web-сервер\" - видео нет, изредка мигает - скорее всего проблема с h.264\n3)в Slave и УРМА искажение видео усиливаются\n ","1) Problems related to H.264: With CUDA on, live video is distorted and video in the archive is distorted even more.\n2) If you switch CUDA off, there is almost no distortion, but at the same time, there is almost no video in the web server component (occasional flickering) then most likely this is an H.264 problem,\n3) In Slave and URMA, the video is even more distorted.\n "]
["Arecont Vision","Arecont Vision AV2110/-DN","Camera ","65143 / 65144","1","1","+",{"$nulls":4},"1600x1200",{"$nulls":5},"+","+","+","1. AV2110 - прошивка 65143\nAV2110DN - прошивка 65144 \n2. Реальный fps сильно зависит от настроек камеры и может быть от 9 fps (при полном разрешении и макс. качестве) до 25 fps (при средних настройках)","1. AV2110 - firmware 65143\nAV2110DN - firmware 65144 \n2. The actual frame rate very much depends on the camera's settings: it ranges from 9 fps (at full resolution and maximum quality) to 25 fps (with medium settings). "]
["Arecont Vision","Arecont Vision AV2115/-DN/-AI","Camera ","65201","1","2","+",null,"+",null,null,"MJPEG: 1920x1072 H264: 1920x1056","+",{"$nulls":4},"+","+","+","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Датчик должен быть под напряжением","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. Close the sensor when it is energized"]
["Arecont Vision","Arecont Vision AV2115v1 / AV2115DNAIv1 / AV2115DNv1 / AV2145-3310-D(-LG) / AV2145-3310-W / AV2145-04-D(-LG) / AV2145-04-W / AV2145DN-3310-D(-LG) / AV2145DN-3310-W / AV2145DN-04-D(-LG) / AV2145DN-04-W ","Camera ","65218 ","1","2","+",null,"+",null,null,"1920x1056","+",{"$nulls":4},"+","+","motion detection","Камеры AV2145-3310-D(-LG) / AV2145-3310-W / AV2145-04-D(-LG) / AV2145-04-W / AV2145DN-3310-D(-LG) / AV2145DN-3310-W / AV2145DN-04-D(-LG) / AV2145DN-04-W определяются как AV2145. ","AV2145-3310-D(-LG) / AV2145-3310-W / AV2145-04-D(-LG) / AV2145-04-W / AV2145DN-3310-D(-LG) / AV2145DN-3310-W / AV2145DN-04-D(-LG) / AV2145DN-04-W cameras are identified as AV2145."]
["Arecont Vision","Arecont Vision AV2116DNv1 / AV2146DN-3310-D(-LG) / AV2146DN-3310-W / AV2146DN-04-D(-LG) / AV2146DN-04-W ","Camera ","65219 ","1","2","+",null,"+",null,null,"1920x1072 ","+",{"$nulls":4},"+","+","motion detection","Модели AV2146DN-3310-D(-LG), AV2146DN-3310-W, AV2146DN-04-D(-LG), AV2146DN-04-W определяются, как AV2146\n","AV2146DN-3310-D(-LG), AV2146DN-3310-W, AV2146DN-04-D(-LG), AV2146DN-04-W cameras are identified as AV2146.\n"]
["Arecont Vision","Arecont Vision AV2125/-DN/-IR","Camera ","65201 / 65202","1","2","+",null,"+",null,null,"MJPEG: 1920x1072 | H264: 1920x1056","+",{"$nulls":4},"+",null,"+","1. AV2125 - прошивка 65201\nAV2125-DN/-IR - прошивка 65202\n2. Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.\n3. Луч должен быть под напряжением.\n4. Устройство выдает 64 fps при половинчатом разрешении","1. AV2125 - firmware v.65201\nAV2125-DN/-IR - firmware v .65202\n2. The Auto Iris and Shutter Speed parameters are integrated as telemetry settings - but the camera does not have the telemetry functionality.\n3. The sensor must be energized.\n4. The device allows 64 fps at half the resolution.\"\n"]
["Arecont Vision","Arecont Vision AV2155/-DN/-HK/-DN-HK","Camera ","65143 / 65144 ","1","2",null,null,"+.",null,null,"1600 x 1184",{"$nulls":5},"+","+","+","1.AV2155/-HK - прошивка 65143\nAV2155DN/-DN-HK - прошивка 65144 \n2. При выборе протокола TFTP камера фактически не работает. \n3. Прошивка 65139, 65143: H264-поток с камеры идет с искажениями (картинка рассыпается, смазывается). Искажения видны и в ПО ITV, и в ПО производителя.","1.AV2155/-HK - firmware 65143\nAV2155DN/-DN-HK - firmware 65144 \n2. If you select the TFTP protocol, the camera practically stops working. \n3. 65139 and 65143 firmware: The H.264 stream becomes distorted (the image is pixelated and/or blurred). You can see the distortions both in the AxxonSoft software and in the vendor software."]
["Arecont Vision","Arecont Vision AV2255AM(IR)/-A/-H/-AH","Camera","65221","1","2","+","-","+","-","-","1920х1072","+","-","-","-","+","+","+","motion detection"]
["Arecont Vision","Arecont Vision AV2256PM-IR","Camera ","65221","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":3},"+","+","+","motion detection."]
["Arecont Vision","Arecont Vision AV2456DN-F","Camera","65221","1","2","+","-","+","-","-","1920x1080","+","-","-","-","-","+","-","motion detection"]
["Arecont Vision","Arecont Vision AV2805/-DN","Camera ","65197","1","2",null,null,"+",null,null,"1920x1080 (MJPEG) / 1920x1056(H264)",{"$nulls":4},"-","+","+","+","Луч должен быть под напряжениемСтабильный видеопоток с 30 fps с камеры возможно получить только по протоколу TFTP","Close the sensor when it is energized. The camera produces a stable video stream at 30 fps only when the TFTP protocol is used."]
["Arecont Vision","Arecont Vision AV2815/-DN / AV2825/-DN/-IR","Camera ","65201","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":4},"+","+","+","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Максимальная частота кадров значительно ниже заявленной и зависит от множества дополнительных условий (~15 fps).Прошивка 65197: при использовании встроенного детектора частота кадров падает до 5 fps.Луч должен быть под напряжением.","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have the telemetry functionality. The maximum frame rate is much lower than stated in the documentation; it also depends on many additional factors (around 15 fps). 65200 firmware: when the embedded detection tool is used, the frame rate drops to 5 fps. Close the sensor when it is energized"]
["Arecont Vision","Arecont Vision AV3100/-DN/-AI","Camera ","64327 / 64328","1",null,"+",{"$nulls":4},"2048x1536",{"$nulls":6},"+","+","1. AV3100/-Ai - прошивка 64327\nAV3100DN - прошивка 64328 \n2. При мегапиксельном разрешении ограничение по fps равны 6,5 -10 fps (в зависимости от качества)\n\n \n\n ","1. AV3100/-Ai - firmware 64327\nAV3100DN - firmware 64328 \n2. With megapixel resolutions, the frame rate is limited to 6.5 –10 fps (depending on the quality)\n\n \n\n "]
["Arecont Vision","Arecont Vision AV3105/-DN/-AI","Camera ","65151 / 65152","1",null,"+",null,"+",null,null,"2048x1536",{"$nulls":5},"+","+","motion detection.","1. AV3105/-Ai - прошивка 65151\nAV3105DN - прошивка 65152 \n2. max значение fps у камеры 14\n2. лучи не интегрировались\n3. fps можно регулировать в настройке Low Light Mode\n4. при включении режима поддержки CUDA в ПО ITV видео в формате H.264 не будет. Это ограничение самой технологии CUDA. Поддержка CUDA отключается через утилиту tweaki.exe (tweaki.exe - вкладка Video Subsystem) ","1. AV3105/-Ai - firmware 65151\nAV3105DN - firmware 65152 \n2. The max. frame rate is 14 fps.\n3. Sensors are not integrated.\n4. You can adjust the frame rate by using the Low Light Mode setting.\n5. When CUDA support mode is on, the AxxonSoft software does not show video in H.264 format. This has to do with the limitations of the CUDA technology itself. You may switch CUDA off by using the tweaki.exe tool (tweaki.exe, Video Subsystem tab)."]
["Arecont Vision","Arecont Vision AV3110/-DN","Camera ","65143 / 65144","1","1",{"$nulls":5},"1920x1072",{"$nulls":5},"+","+","+","1. AV3110 - прошивка 65143\n AV3110DN - прошивка 65144 ","1. AV3110 - firmware 65143\n AV3110DN - firmware 65144 "]
["Arecont Vision","Arecont Vision AV3115/-DN/-AI","Camera ","65201","1","2","+",null,"+",null,null,"2048x1536","+",{"$nulls":4},"+","+","+","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Датчик должен быть под напряжением","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. Close the sensor when it is energized"]
["Arecont Vision","Arecont Vision AV3115v1 / AV3115DNAIv1 / AV3115DNv1 / AV3145-3310-D(-LG) / AV3145-3310-W / AV3145-04-D(-LG) / AV3145-04-W / AV3145DN-3310-D(-LG) / AV3145DN-3310-W / AV3145DN-04-D(-LG) / AV3145DN-04-W","Camera ","65218 ","1","2","+",null,"+",null,null,"2048x1536 ","+",{"$nulls":4},"+","+","motion detection","1. Модели AV3145-3310-D(-LG), AV3145-3310-W, AV3145-04-D(-LG), AV3145-04-W, AV3145DN-3310-D(-LG), AV3145DN-3310-W, AV3145DN-04-D(-LG), AV3145DN-04-W определяются, как AV3145\n2. C кодеком MJPEG при включенном детекторе движение Частота кадров падает до 5-7 fps\n\n","1. AV3145-3310-D(-LG), AV3145-3310-W, AV3145-04-D(-LG), AV3145-04-W, AV3145DN-3310-D(-LG), AV3145DN-3310-W, AV3145DN-04-D(-LG), AV3145DN-04-W cameras are identified as AV3145.\n2. With the motion detection tool enabled, the frame rate for MJPEG falls to 5–7 fps.\n\n"]
["Arecont Vision","Arecont Vision AV3116DNv1 / AV3146DN-3310-D(-LG) / AV3146DN-3310-W / AV3146DN-04-D(-LG) / AV3146DN-04-W","Camera ","65219 ","1","2","+",null,"+",null,null,"2048x1536","+",{"$nulls":4},"+","+","motion detection.","Камеры AAV3146DN-3310-D(-LG) / AV3146DN-3310-W / AV3146DN-04-D(-LG) / AV3146DN-04-W определяются в ПО ITV/Axxon как AV3146. ","AV3146DN-3310-D(-LG) / AV3146DN-3310-W / AV3146DN-04-D(-LG) / AV3146DN-04-W cameras are identified as AV3146. "]
["Arecont Vision","Arecont Vision AV3125/-DN/-IR ","Camera ","65201 ","1","2","+",null,"+",null,null,"2048x1536","+",{"$nulls":4},"+","+","+","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Луч должен быть под напряжением.","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. Close the sensor when it is energized"]
["Arecont Vision","Arecont Vision AV3130/-DN","Camera ","64329","1","1","+",{"$nulls":4},"2048х1536(day)/1280х1024(night)","+",{"$nulls":4},"-","-",null,"Сама камера выдает не более 14 fps.Прошивка 64329: камера не поддерживает работу лучей и реле.","The camera itself allows max. 14 fps. 64329 firmware: the camera does not support sensors or relays. "]
["Arecont Vision","Arecont Vision AV3135","Camera ","65153","1","2","+",null,"+",null,null,"2048x1536 (Day) / 1280x1024 (Night)","+",{"$nulls":4},"+","+","+","Луч должен быть под напряжением","Close the sensor when it is energized. "]
["Arecont Vision","Arecont Vision AV3155/-DN/-HK/-DN-HK","Camera ","65143 / 65144","1","2",null,null,"+",null,null,"2048x1536","+",{"$nulls":4},"+","+","+","1. AV3155/-HK - прошивка 65143\nAV3155DN/-DN-HK - прошивка 65144 \n2. Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.","1. AV3155/-HK - firmware 65143\nAV3155DN/-DN-HK - firmware 65144 \n2. The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality."]
["Arecont Vision","Arecont Vision AV3255AM/-HK / AV3255AMIR","Camera ","65218 ","1","2","+",null,"+",null,null,"2048x1536","+",{"$nulls":3},"+","+","+","motion detection"]
["Arecont Vision","Arecont Vision AV3256PMIR","Camera ","65221","1","2","+",null,"+",null,null,"2048x1536","+",{"$nulls":3},"+","+","+","motion detection."]
["Arecont Vision","Arecont Vision AV5100/-DN/-AI","Camera ","64327 / 64328","1",null,"+",{"$nulls":4},"2560x1600",{"$nulls":6},"+","+","1. AV5100/-AI - прошивка 64327\nAV5100DN - прошивка 64328 \n2. Ограничение по fps:\n2560x1600(SDK) 8-10 fps \n2560x1600(WEB) 10 fps\n1280x800(SDK)  10 fps \n1280x800(WEB)  10 fps\n\n\n\n ","1. AV5100/-AI - firmware 64327\nAV5100DN - firmware 64328 \n2. Frame rate limits: \n2560x1600(SDK) 8–10 fps \n2560x1600(WEB) 10 fps\n1280x800(SDK)  10 fps \n1280x800(WEB)  10 fps\n\n\n\n "]
["Arecont Vision","Arecont Vision AV5105/-DN/-AI","Camera ","65151 / 65152 ","1","2","+",null,"+",null,null,"2560x1600","+",{"$nulls":4},"+","+","motion detection"," AV5105/-AI - прошивка 65151\n AV5105DN - прошивка 65152 "," AV5105/-AI - fw 65151\n AV5105DN - fw 65152 "]
["Arecont Vision","Arecont Vision AV5110/-DN","Camera ","65143 / 65144","1","1","+",{"$nulls":4},"2592x1944","+",{"$nulls":4},"+","+","-","AV5110 - прошивка 65143\nAV5110-DN - прошивка 65144\nКамера имеет ограничение по fps:\n - 9fps @ 2592x1936\n - 12fps @ 1296x9686\nДатчик должен быть под напряжением","AV5110 - firmware v.65142\nAV5110 - firmware v.65144\nThe camera has frame rate limits:\n - 9fps @ 2592x1936 \n - 12fps @ 1296x9686\nThe sensor must be energized.\n"]
["Arecont Vision","Arecont Vision AV5115/-DN/-AI","Camera ","65201","1","2","+",null,"+",null,null,"2592x1936 (MJPEG) / 2560x1920 (H264)","+",{"$nulls":4},"+","+","+","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Луч должен быть под напряжением.","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. Close the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV5115v1 / AV5115DNAIv1 / AV5115DNv1 / AV5145-3310-D(-LG) / AV5145-3310-W / AV5145-04-D(-LG) / AV5145-04-W / AV5145DN-3310-D(-LG) / AV5145DN-3310-W / AV5145DN-04-D(-LG) / AV5145DN-04-W ","Camera ","65218 ","1","2","+",null,"+",null,null,"2560x1920(H264) / 2592x1936(MJPEG) ","+",{"$nulls":4},"+","+","motion detection","Модели AV5145-3310-D(-LG), AV5145-3310-W, AV5145-04-D(-LG), AV5145-04-W, AV5145DN-3310-D(-LG), AV5145DN-3310-W, AV5145DN-04-D(-LG), AV5145DN-04-W будут определяться как AV5145 ","AV5145-3310-D(-LG), AV5145-3310-W, AV5145-04-D(-LG), AV5145-04-W, AV5145DN-3310-D(-LG), AV5145DN-3310-W, AV5145DN-04-D(-LG), AV5145DN-04-W cameras are identified as AV5145 "]
["Arecont Vision","Arecont Vision AV5125/-DN/-IR","Camera ","65201","1","2","+",null,"+",null,null,"2592x1936 (MJPEG) / 2560x1920 (H264)","+",{"$nulls":4},"+",null,"+","Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.Луч должен быть под напряжением.","The Auto Iris and Shutter Speed parameters are integrated as telemetry settings, but the camera itself does not have telemetry functionality. Close the sensor when it is energized."]
["Arecont Vision","Arecont Vision AV5155/-DN/-HK","Camera ","65151 / 65152","1","2","+",null,"+",null,null,"2560x1920","+",{"$nulls":4},"+","+","+","1. AV5155/-HK - прошивка 65151\nAV5155DN - прошивка 65152\n2. Параметры \"Автодиафрагма\" и \"Скорость затвора\" интегрированы как настройки телеметрии - но сама камера функционала телеметрии не имеет.\n3. Камера имеет ограничение по FPS:\n - 9fps @ 2592x1944\n - 12fps @ 2560x1600\n - 15fps @ 2048x1536\n - 24fpsfps @ 1600x1200\n - 30fps @ 1280x1024\n4. Датчик должен быть под напряжением ","1. AV5155/-HK - firmware 65151\nAV5155DN - firmware 65152\n2. The Auto Iris and Shutter Speed parameters are integrated as telemetry settings - but the camera itself does not have the telemetry functionality.\n3. The camera has the following frame rate / resolution limits:\n - 9fps @ 2592x1944\n - 12fps @ 2560x1600\n - 15fps @ 2048x1536\n - 24fpsfps @ 1600x1200\n - 30fps @ 1280x1024\n4. The sensor must be energized. "]
["Arecont Vision","Arecont Vision AV5255AM/-HK","Camera ","65218 ","1","2","+",null,"+",null,null,"2592x1944 ","+",{"$nulls":3},"+","+","+","motion detection"]
["Arecont Vision","Arecont Vision AV8180/AV8360","Camera ","65010","4","1","+",{"$nulls":4},"1600x1200",{"$nulls":7},"+","1. Сама камера имеет ограничение по fps:\n800x600 10-13fps в зависимости от качества\n1600x1200 7-8fps в зависимости от качества","1. The camera itself has frame rate limits:\n800x600 10–13 fps (depending on quality)\n1600x1200 7–8 fps (depending on quality)"]
["Arecont Vision","Arecont Vision AV8185DN","Camera ","65166","4","2","+",null,"+",null,null,"1600x1200","+",{"$nulls":4},"-","-","+","Панорамные AV8185 и AV8365 отличаются только углом обзора: 180 и 360 градусов соответственно.Максимальная частота кадров: ~10 fps в разрешении \"800х600\" и ~5 fps в разрешении \"1600х1200\" в зависимости от качества.На всех 4х каналах устройства должен стоять один и тот же видеокодек. Луч должен быть под напряжениемПри выборе протокола TFTP камера фактически не работает.C текущей прошивкой 65166 интегрировать лучи и реле нет возможности.","The only difference between the panoramic AV8185 and AV8365 models is the total angle of view: 180 and 360 degrees, respectively. Max. frame rate: around 10 fps at 800х600 resolution and around 5 fps at 1600х1200 resolution, depending on the quality. All of the camera's 4 channels must have the same video codec. Close the sensor when it is energized. If you select the TFTP protocol, the camera practically stops working. With the current firmware (65166), sensors and relays cannot be integrated."]
["Arecont Vision","Arecont Vision AV8365DN","Camera ","65166","4","2","+",null,"+",null,null,"1600x1200","+",{"$nulls":4},"-","-","+","Панорамные AV8185 и AV8365 отличаются только углом обзора: 180 и 360 градусов соответственно.Максимальная частота кадров: ~10 fps в разрешении \"800х600\" и ~5 fps в разрешении \"1600х1200\" в зависимости от качества.На всех 4х каналах устройства должен стоять один и тот же видеокодек. Луч должен быть под напряжениемПри выборе протокола TFTP камера фактически не работаетС текущей прошивкой 65166 интегрировать лучи и реле нет возможности.","The only difference between the panoramic AV8185 and AV8365 models is the total angle of view: 180 and 360 degrees, respectively. Around 10 fps at 800х600 resolution and around 5 fps at 1600х1200 resolution, depending on the quality. All of the camera's 4 channels must have the same video codec. Close the sensor when it is energized. If you select the TFTP protocol, the camera practically stops working. With the current firmware (65166), sensors and relays cannot be integrated."]
["ARH","ARH ParkIT","Camera ","1.11.1.0","1","1","+",{"$nulls":4},"752x480","+",{"$nulls":3},"+.","-","-","-","Камера не поворотная, но есть встроенный трансфокатор.","This is not a PTZ camera, but it has a built-in zoom lens."]
["Arlotto","Arlotto AR1500(H/T)","Camera ","2.60.27","1","3","+","+","+",null,null,"2592x1920","+",null,"+","-",null,"+","+","motion detection","1. С камеры можно получать от одного до трех видеопотоков, на камере есть три режима работы: Single, Dual и Tri-Stream. Существует зависимость между параметрами поток-кодек-разрешение, т.к. набор разрешений для потока зависит от того, сколько потоков сейчас включено. При настройке камеры в ПО Axxon необходимо об этом помнить и выставлять на камере только совместимые настройки.\n2. Лучи необходимо замыкать под напряжением\n3. В ПО Intellect максимальное разрешение 1280х720\n4. В кодеке H264 в разрешении 5MP частота кадров недоступна для изменения.\n5. Прошивка 2.60.17: Встроенный детектор в Axxon Next начинает работать только после изменения любых параметров видео. 6. Поиск находит камеру как неподдерживаемое устройство.","1. From the camera, you can receive from one to three video streams. The camera has three operation modes: Single, Dual, and Tri-Stream. The Stream, Codec, and Resolution parameters are interrelated, because the set of available resolutions for a stream depends on how many streams are currently on. When you configure the camera in the AxxonSoft software, remember this and use compatible values for the camera's settings. \n2. Close the sensors when they are energized.\n3. In Intellect, the max. resolution is 1280x720.\n4. At 5MP resolution, the H.264 codec does not allow you to change the frame rate. \n5. 2.60.17 firmware: In Axxon Next, the embedded detection tool starts working only after a video setting is changed. \n6. Search detects the camera as an unsupported device. "]
["Arlotto","Arlotto AR2200(H/T)","Camera ","2.60.18","1","3","+","+","+",null,null,"1920x1080","+",null,null,"-",{"$nulls":3},"+","Камера поддерживает до трех потоков, при этом параметры \"Кодек\" и \"Разрешение\" на разных потоках взаимосвязаны.","The camera supports up to three streams; the Codec and Resolution parameters for different streams are interdependent. "]
["Arlotto","Arlotto AR2500(H/T)","Camera ","2.60.18","1","3","+","+","+",null,null,"H.264, MJPEG: 2592x1920, MPEG4: 1920x1080","+",null,null,"-",{"$nulls":3},"+","Камера поддерживает до трех потоков, при этом параметры \"Кодек\" и \"Разрешение\" на разных потоках взаимосвязаны. ","The camera supports up to three streams; the Codec and Resolution parameters for different streams are interdependent. "]
["Arlotto","Arlotto AR2510/AR2520","Camera ","2.60.18","1","3","+","+","+",null,null,"2592x1920 (h264, mjpeg) / 1920x1080 (mpeg4)","+",null,null,"-",{"$nulls":3},"motion detection.","С камеры можно получать от одного до трех видеопотоков, на камере есть три режима работы: Single, Dual и Tri-Stream. Параметры \"кодек\" и \"разрешение\" разных потоков зависят друг от друга. При настройке камеры в ПО Axxon необходимо об этом помнить и выставлять на камере только совместимые настройки.В первом потоке в кодеке mpeg4 не доступны разрешения выше 1920х1080, а в кодеке mjpeg не доступны разрешения ниже 1600x1200.Прошивка 2.60.18: поиск обнаруживает устройство как AR1500.Максимальная частота кадров в разрешении 5MP - 10fps.Прошивка 2.60.18: камера в целом ведет себя достаточно нестабильно - иногда зависает, перестает передавать видео.Максимальное значение битрейта для первого потока - 7000, а для второго - 800. В стандартном разрешении Интеллект подключается ко второму потоку для всех кодеков, поэтому качество картинки на стандартном разрешении значительно уступает качеству на высоком и полном разрешениях.","From the camera, you can receive from one to three video streams. The camera has three operation modes: Single, Dual, and Tri-Stream. The Codec and Resolution parameters for different streams are interdependent. When you configure the camera in the AxxonSoft software, remember this and use compatible values for the camera's settings. In the first stream, the mpeg4 codec does not allow resolutions higher than 1920x1080 and the mjpeg codec does not allow resolutions lower than 1600x1200. 2.60.18 firmware: Search detects the device as AR1500.With 5PM resolution, the maximum frame rate is 10 fps. 2.60.18 firmware: in general, the camera is pretty unstable – sometimes it freezes and stops sending video. The max. bit rate is 7,000 for the first stream and 800 for the second stream. At standard resolution, Intellect connects to the second stream for all codecs; for this reason, at standard resolution, the image quality is much lower than the quality at high and full resolutions. "]
["Arlotto","Arlotto AR3210","Camera ","2.60.18.r1","1","3","+","+","+",null,null,"1920x1080","+",null,null,"-",{"$nulls":3},"+","Камера поддерживает до трех потоков, при этом параметры \"Кодек\" и \"Разрешение\" на разных потоках взаимосвязаны.","The camera supports up to three streams; the Codec and Resolution parameters for different streams are interdependent."]
["Arlotto","Arlotto AR3510","Camera ","2.60.18.r1","1","3","+","+","+",null,null,"H.264, MJPEG: 2595x1920, MPEG4: 1920x1080","+",null,null,"-",{"$nulls":3},"+","Камера поддерживает до трех потоков, при этом параметры \"Кодек\" и \"Разрешение\" на разных потоках взаимосвязаны.","The camera supports up to three streams; the Codec and Resolution parameters for different streams are interdependent."]
["Arlotto","Arlotto AR4200(H/T)","Camera ","2.60.18","1","3","+","+","+",null,null,"1920x1080","+",null,null,"-",{"$nulls":3},"+","С камеры можно получать от одного до трех видеопотоков, на камере есть три режима работы: Single, Dual и Tri-Stream. Параметры \"кодек\" и \"разрешение\" разных потоков зависят друг от друга. При настройке камеры в ПО Axxon необходимо об этом помнить и выставлять на камере только совместимые настройки.","From the camera, you can receive from one to three video streams. The camera has three operation modes: Single, Dual, and Tri-Stream. The Codec and Resolution parameters for different streams are interdependent. When you configure the camera in the AxxonSoft software, remember this and use compatible values for the camera's settings."]
["Arlotto","Arlotto AR4500(H/T)","Camera ","2.60.18","1","3","+","+","+",null,null,"2592x1960 (h264, mjpeg) / 1920x1080 (mpeg4)","+",null,null,"-",{"$nulls":3},"+","С камеры можно получать от одного до трех видеопотоков, на камере есть три режима работы: Single, Dual и Tri-Stream. Параметры \"кодек\" и \"разрешение\" разных потоков зависят друг от друга. При настройке камеры в ПО Axxon необходимо об этом помнить и выставлять на камере только совместимые настройки.","From the camera, you can receive from one to three video streams. The camera has three operation modes: Single, Dual, and Tri-Stream. The Codec and Resolution parameters for different streams are interdependent. When you configure the camera in the AxxonSoft software, remember this and use compatible values for the camera's settings."]
["Asoni","Asoni CAM439P","Camera ","V3.2.66_As.1","1","2","+","+",{"$nulls":3},"1280x1024","+",null,"-","-",{"$nulls":3},"+","В максимальном разрешении (1280x1024) максимальная частота кадров - 10 fpsПри одновременном использовании нескольких видеопотоков суммарная частота кадров должна быть 25 fps. Причем после изменения частоты кадров на значение A на одном из потоков частота кадров на другом потоке автоматически становится равной 25 - A.","At the maximum resolution (1280x1024), the max. frame rate is 10 fps. When multiple video streams are used simultaneously, the total frame rate must be 25 fps. After the frame rate for a stream is changed by A fps, the frame rate for the other stream automatically becomes (25-A) fps. "]
["Asoni","Asoni CAM636MVP / CAM613","Camera ","V1.0.14_As.1","1","2","+",null,"+",null,null,"1600x1200","+",null,"+","+",null,"+","+","+","На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В Axxon Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.Тревога по замыканию луча срабатывает при условии соблюдения заданного временного интервала (мин. 10 сек) между замыканиями. Интервал настраивается в веб-интерфейсе. Особенность камеры.В Интеллект поиск находит камеру как FineCCTV IP-Cam.","The camera has the Video Parameters option (the max. resolution and max. frame rate). In Axxon Next, you must make sure that there is no conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value. Closing the sensor makes the alarm go off, but only if the time between two consecutive closures is a minimum of 10 seconds. You must set the interval using the web interface. This is a limitation of the camera itself. In Intellect, search detects the camera as FineCCTV IP-Cam."]
["Asoni","Asoni SVR610-PoE","Camera ","V1.0.8_As.1","1","2","+",null,"+",null,null,"720x576","+",null,"+","-","+","+","+","+","Тревога по замыканию луча срабатывает при условии соблюдения заданного временного интервала (мин. 10 сек) между замыканиями. Интервал настраивается в веб-интерфейсе. Особенность камеры.Правильный ТВ-стандарт (PAL/NTSC) нужно выставить в зависимости от подключенной аналоговой камеры.В Интеллект поиск находит камеру как FineCCTV IP-Cam.","Closing the sensor makes the alarm go off, but only if the time between two consecutive closures is a minimum of 10 seconds. You must set the interval using the web interface. This is a peculiarity of the camera itself. You must set the right TV standard (PAL/NTSC), depending on what analog camera is connected. In Intellect, search detects the camera as FineCCTV IP-Cam."]
["Aver","Aver FD2000","Camera ","0.1.28 ","1","3","+",null,"+",null,null,"1920x1080","+",null,"+",{"$nulls":5},"Значение настройки ТВ-стандарт в ПО ITV/Axxon следует выставлять в соответствии со значением ТВ-стандарта в веб-интерфейсе.","TV-standard value in ITV | AxxonSoft should be put in line with the value of TV-standard in the web-interface."]
["Aver","Aver SF1311H-C","Camera ","5.a.2.7766 ","1","2","+","+","+",null,null,"1280x1024","+",null,null,"-",{"$nulls":3},"-"]
["Aver","Aver SF2121H-BHR","Camera ","1.1.1.38","1","3","+","+","+",null,null,"1920x1080","+",null,"+",null,"+",{"$nulls":3},"Камера передает видео только в Full HD (1920x1080). При выборе меньших разрешений изображение обрезается до нужного размера. Область отображения настраивается через веб-интерфейс.","The camera transmits video only in Full HD (1920x1080). When you select the image resolution less that Full HD, image will be cut to the desired size. The display area chould be configured via web-interface."]
["Avigilon","Avigilon 2.0W-H3PTZ-DP20 (ONVIF)","Camera","2.4.4.38","1","1","+",null,"+",null,null,"1920x1080","+",null,"-","-","+","-","-","-"]
["Avigilon","Avigilon 3.0W-H3-D2 (ONVIF)","Camera","2.4.2.8","1","1","+",null,"+",null,null,"2048x1536","+",null,"+","-","+.","-","-","-"]
["AVTech","AVTech AVM504","Camera","1038-1021-1024-1012-A3","1","4","+","-","+","-","-","from WEB","+","-","-","-","+","-","-","-","При смене значения настройки антимерцания камера перезагружается.","When the anti blink setting is changed, the camera reboots."]
["Axis","Axis 210A","Camera ","4.47","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","+",null,"+","+","-"]
["Axis","Axis 211","Camera ","4.40","1",null,"+","+",{"$nulls":3},"640x480",{"$nulls":5},"+","+","-"]
["Axis","Axis 211W","Camera ","4.40.1","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","+",null,"+","+","-"]
["Axis","Axis 212PTZ","Camera ","4.40","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","+","+","+","+","-"]
["Axis","Axis 214PTZ","Camera ","4.40","1","1","+","+",{"$nulls":3},"704x576",null,null,"+","+","+","+","+","-"]
["Axis","Axis 215PTZ","Camera ","4.40","1",null,"+","+",{"$nulls":3},"704x576",null,null,"+","+","+","+","+","-"]
["Axis","Axis 216FD","Camera ","4.47","1",null,"+","+",{"$nulls":3},"640x480",null,"+","+","-",null,"+","+","-","1. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","1. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 216MFD","Camera ","4.47.1","1",null,"+","+",{"$nulls":3},"1280x1024",null,null,"+","+",null,"+","+","-","1. Ограничения fps самой камеры:\n- 1280х1024 - max. 12 fps для MJPEG и 8 fps для MPEG-4\n- 1024x768 - max. 20 fps для MJPEG и 13 fps для MPEG-4\n ","1. The camera itself has frame rate limits: \n- 1280х1024 – max. 12 fps for MJPEG and 8 fps for MPEG-4\n- 1024x768 – max. 20 fps for MPEG and 13 fps for MPEG-4\n "]
["Axis","Axis 221","Camera ","4.45.1","1",null,"+","+",{"$nulls":3},"640x480",null,"+",{"$nulls":3},"+","+","-","максимальное значение fps = 49 1. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","The max. frame rate is 49 fps. 1. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 223М","Camera ","4.47","1",null,"+","+",{"$nulls":3},"1600x1200(MJPEG) / 640x480(MPEG-4)",null,null,"+","+",null,"+","+","-","У камеры два режима. «Normal resolutions (NR)» и «Widescreen resolutions (WR)». Соответственно набор разрешений для этих режимов разный, fps также разный. Для NR max fps=9, для WR max fps=12. Это ограничение самой камеры.","The camera has two modes: Normal Resolutions (NR) and Widescreen Resolutions (WR). The two modes differ in the set of resolutions and in frame rate. For NR, the max. frame rate is 9 fps; for WR, the max. frame rate is 12 fps. This is a limitation of the camera itself. "]
["Axis","Axis 232D+","Camera ","4.47","1",null,"+","+",{"$nulls":3},"704x576",null,"+",null,null,"+.","-","+","-","1. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","1. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 233D","Camera ","4.48","1",null,"+","+",{"$nulls":3},"704x576",null,null,"+","-","+.","+","+","-"]
["Axis","Axis 240Q encoder","Encoder ","4.40","4",null,"+",{"$nulls":4},"704x576",{"$nulls":4},"+","+","+","-"]
["Axis","Axis 241Q encoder","Encoder ","4.47","4",null,"+","+",{"$nulls":3},"704x576",null,"+",null,null,"+","+","+","-","1. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","1. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 241QA encoder","Encoder ","4.47","4",null,"+","+",{"$nulls":3},"704x576",null,null,"+","+","+","+","+","-"]
["Axis","Axis 241S encoder","Encoder ","4.47","1",null,"+","+",{"$nulls":3},"704x576",{"$nulls":4},"+","+","+","-"]
["Axis","Axis 243Q blade encoder","Encoder ","4.41","4",null,"+","+",{"$nulls":3},"704x576",null,"+",null,null,"+","+","+","-","ВАЖНО!\n1. данный сервер - устройство для подключения 4 аналоговых камер, но при этом каждый канал сервера имеет свой собственный ip-адрес. Поэтому в ПО ITV чтобы задействовать все 4 канала необходимо создавать 4 Граббера (на каждый канал свой граббер). Поэтому и ключ нужно иметь соответствующий.\n2.лучи/реле - по одному на каждый вход т.е. нельзя для одной камеры создать несколько лучей/реле на разные каналы 3. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","THIS IS IMPORTANT!\n1. This encoder is a single device that allows you to connect 4 analog cameras; however, each channel of the encoder has its own IP address. For this reason, in AxxonSoft software, if you want to use all the 4 channels, you must create 4 Grabber objects (one grabber per channel). \n2. Sensors/relays, one for each port (i.e., only one sensor/relay per camera)."]
["Axis","Axis 243SA encoder","Encoder ","4.45","1",null,"+","+",{"$nulls":3},"704x576",null,"+","+","+","+","+","+","-","1. Для включения мультикаста в Интеллекте необходимо в реестре ключей по адресу(HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols) добавить строковый параметр Axis со значением multicast ","1. In Intellect, to enable Multicasting, you should create a string parameter in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\Video\\TransportProtocols registry folder and assign it the value of \"mulitcast\". "]
["Axis","Axis 247S encoder","Encoder ","4.42","1",null,"+","+",{"$nulls":3},"704x576",null,null,"+",null,null,"+","+","-"]
["Axis","Axis M1011","Camera ","5.00","1",null,"+","+","+.",null,null,"640x480",{"$nulls":7},"-","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n\n ","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution). \n\n "]
["Axis","Axis M1011-W","Camera ","5.00","1",null,"+","+","+.",null,null,"640x480",{"$nulls":7},"-","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n\n","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution).\n\n"]
["Axis","Axis M1013","Camera ","5.40.5.2","1","5","+",null,"+",null,null,"800x600","+",{"$nulls":3},"+",null,null,"motion detection","1. Через AxxonNext настраивается только первый поток, остальные - через web-интерфейс;\n2. При включенной настройке \"цифровая ptz телеметрия\" не применяются некоторые настройки, в частности - видеопотока.\n3. Для подключения камеры как ONVIF device необходимо произвести дополнительные настройки через web-интерфейс: синхронизировать время с локальным сервером, добавить пользователя ONVIF; снять галку Enable replay attack protection по пути: System Options -> Advanced -> Plain Config -> Select Group -> Web-service","1. In AxxonNext, you can configure only stream 1, while other stream are set up in the camera's web interface;\n2. With Digital PTZ enabled, the video stream settings, among others, become unavailable.\n3. To connect the camera via ONVIF, use following settings in the camera's web interface: Sync time with the local Server, Add ONVIF User, deselect the checkbox for Enable replay attack protection. You can do this here: System Options -> Advanced -> Plain Config -> Select Group -> Web-service"]
["Axis","Axis M1014 ","Camera ","5.40.5.1","1","5","+",null,"+",null,null,"1280x800","+",{"$nulls":3},"+",null,null,"motion detection, tampering detection","1. Чтобы работала цифровая телеметрия, необходимо включить соответствующую настройку на камере. \n2. Для работы в ПО ITV/Axxon RTSP порт должен быть стандартным - 554 ","1. To use digital PTZ, it must be on in camera web interface. \n2. To work in Axxonsoft SW RTSP port should be staddard - 554."]
["Axis","Axis M1031-W","Camera ","5.20.3","1","5","+","+.","+.",null,null,"640x480",null,null,"+","+.",{"$nulls":3},"+"]
["Axis","Axis M1034-W","Camera","5.40.5.4","1","1","+","-","+",null,"-","1280x800","+",null,"+","+","+","-","-","motion detection; audio detection; hacking detection"]
["Axis","Axis M1054","Camera ","5.15.1","1",{"$nulls":3},"+.",null,null,"1280x800",null,null,"+",null,"+",null,null,"-","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном веб-интерфейсе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect. \n3. Preset 1 is reserved for Home Position."]
["Axis","Axis M1103","Camera ","5.08.1","1",{"$nulls":3},"+.",null,null,"800x600",{"$nulls":4},"+",null,null,"-","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position\n","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Preset 1 is reserved for Home Position.\n"]
["Axis","Axis M1104","Camera ","5.09","1",{"$nulls":3},"+.",null,null,"1280x800",{"$nulls":4},"+",null,null,"-","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position\n","1. This is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Preset 1 is reserved for Home Position.\n"]
["Axis","Axis M1113","Camera ","5.09","1",{"$nulls":3},"+",null,null,"800x600",{"$nulls":4},"+",null,null,"-","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position\n","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Preset 1 is reserved for Home Position.\n"]
["Axis","Axis M1114","Camera ","5.08","1",{"$nulls":3},"+.",null,null,"1280x800",{"$nulls":7},"-","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position\n","1. This is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Preset 1 is reserved for Home Position.\n"]
["Axis","Axis M1144-L","Camera ","5.40.10.6","1","5","+",null,"+",null,null,"1280x800","+",{"$nulls":3},"+","+","+","motion detection, tampering detection","На устройстве для кодека MJPEG недоступны следующие разрешения:\n\n 480x300\n 480x270\n 800x500\n 800x450 ","Unavailable resolution for MJPEG is the folowing:\n\n 480x300\n 480x270\n 800x500\n 800x450 "]
["Axis","AXIS M3004-V","Camera ","5.40.5","1","5","+",null,"+",null,null,"1280x800","+",{"$nulls":3},"+"]
["Axis","Axis M3005-V ","Camera ","5.40.5.5","1","5","+",null,"+",null,null,"1920x1080 ","+",{"$nulls":3},"+",null,null,"motion detection, tampering detection"]
["Axis","Axis M3006-V","Camera ","5.40.13.2","1","5","+",null,"+",null,null,"2048x1536","+",{"$nulls":3},"+",null,null,"motion detection, tampering detection","Чтобы работала цифровая телеметрия, необходимо включить соответствующую настройку. ","To use digital PTZ, it must be on in camera web interface."]
["Axis","Axis M3007-P/-PV","Fisheye Camera","5.40.13.1","1","5","+","-","+","-","-","2592x1944","+","-","-","-","-","-","-","motion detection","\nКамера имеет две степени свободы поворотного крепления. Если открыть кожух, то камеру можно наклонять вверх-вниз, а так же вращать вокруг оси линзы. Для корректной работы настройки \"Поворот видеоизображения\" необходимо в устанавливать поворотное крепление в правильное положение.","Camera rotary fastening has 2 degrees of freedom. If you open the camera casing, then you can tilt the camera up and down and rotate it around the lens axis. For proper operation of the Video rotation setting, you are to place the rotary fastening into the correct position."]
["Axis","Axis M3011","Camera ","5.01","1",null,"+","+","+.",null,null,"640x480",{"$nulls":7},"-","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n\n","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution).\n\n"]
["Axis","Axis M3014","Camera ","5.05","1",null,"+",null,"+.",null,null,"1280x800",{"$nulls":4},"+",null,null,"-","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\", результаты работы телеметрии будут видны при достаточном зумировании картинки.\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Для корректной работы H.264-видеопотока следует настройку \"Качество\" выставить в среднее положение","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box. You will see the result of PTZ after you zoom enough. \n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. To make the H.264 video stream work correctly, set the Quality setting at a medium position. "]
["Axis","Axis M3024-LVE","Camera","5.40.5","1","2","+",null,"+",null,null,"1280x800","+",{"$nulls":3},"-","-","-","motion detection",null,null,"new"]
["Axis","Axis M3113-R","Camera ","5.12","1",{"$nulls":3},"+",null,null,"800x600",{"$nulls":4},"+",null,null,"-","у камеры Digital PTZ (цифровая телеметрия)","The camera has Digital PTZ (digital telemetry). "]
["Axis","Axis M3114-R","Camera ","5.12","1","5",null,null,"+.",null,null,"1280x800",{"$nulls":4},"+",{"$nulls":3},"1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellecte необходимо поставить галочку в родном вебе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellecte будет игнорироваться.\n","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n"]
["Axis","Axis M3203","Camera ","5.11","1",{"$nulls":3},"+.",null,null,"800x600",{"$nulls":4},"+",null,null,"-","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Preset 1 is reserved for Home Position."]
["Axis","Axis M3204","Camera ","5.40","1","5","+",null,"+",null,null,"1280x800","+",{"$nulls":3},"+",null,null,"+","1. Камера не поворотная, но есть цифровая телеметрия. Чтобы заработало в Intellecte необходимо включить настройки в веб-интерфейсе enable PTZ\n2. При включенной цифровой телеметрии разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии в веб-интрфейсе. В этом случае переключатель разрешений в Intellecte будет игнорироваться \n3. Пресет №1 зарезервирован за Home position\n4. В Axxon Next потоки со 2 по 5 (Авто) отвечают Stream Profiles веб-интерфейса и задаются только от туда ","1. This is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ checkbox.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution set in the device's own web interface, in the telemetry settings. In this case, switching resolution in Intellect will have no effect. \n3. Preset 1 is reserved for Home Position\n4. In AN, streams 2 to 5 (Auto) are configured via web interface in Stream Profiles.\n"]
["Axis","Axis M5014/-V","Camera ","5.40.11.2","1","5","+",null,"+",null,null,"1280x720","+",{"$nulls":6},"motion detection; audio detection"]
["Axis","Axis M5013","Camera ","5.25.2 ","1","5","+",null,"+",null,null,"800x600","+",null,"+",null,"+",null,null,"motion detection.","На камере предусмотрены 5 видеопотоков:0. Получение видео H264/MJPEG и применение настроек.1. Соответствует профилю \"Quality\" в веб-интерфейсе камеры. Получение видео без настроек.2. Соответствует профилю \"Balanced\" в веб-интерфейсе камеры. Получение видео без настроек.3. Соответствует профилю \"Bandwith\" в веб-интерфейсе камеры. Получение видео без настроек.4. Соответствует профилю \"Mobile\" в веб-интерфейсе камеры. Получение видео без настроек.При использовании потоков 1-4 после изменения настроек (через веб-интерфейсе) необходимо перезапускать поток или объект \"камера\".Встроенная аналитика работает:В 0-м потоке в любом кодеке.В любом другом потоке, но только в H264.Камера поворотная, но зум у нее только цифровой.Через Onvif не работают настройки изображения - проблема устройства.Работа камеры проверялась только по протоколу TCP - из-за особенностей удаленного доступа.","The camera allows 5 video streams: 0. Receiving video in H.264/MJPEG with settings applied. 1. Corresponds to the Quality profile in the camera's web interface. Receiving video without settings applied. 2. Corresponds to the Balanced profile in the camera's web interface. Receiving video without settings applied. 3. Corresponds to the Bandwidth profile in the camera's web interface. Receiving video without settings applied. 4. Corresponds to the Mobile profile in the camera's web interface. Receiving video without settings applied. When you use a stream between 1 and 4, you must restart the stream or the Camera object after you change settings in the web interface .Embedded video analytics work in stream 0 with any codec. In any other stream, they work only with H.264. This is a PTZ camera, but it has only digital zoom. The image settings do not work via the ONVIF protocol; this is a problem of the device itself. When checking how the camera works, we checked only the TCP protocol. This is a limitation of remote access."]
["Axis","Axis M7001 encoder","Encoder ","5.02","1",null,"+",null,"+.",null,null,"720x576",{"$nulls":4},"+",null,null,"+","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution)."]
["Axis","Axis M7014 encoder","Encoder ","5.40.7.1","4","5","+",null,"+",null,null,"720x576","+",{"$nulls":3},"+",null,null,"motion detection.; tampering detection."]
["Axis","Axis P1311","Camera ","5.01.1","1",null,"+","+","+.",null,null,"640x480",null,null,"+","+",null,"+","+","-","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution)."]
["Axis","Axis P1343","Camera ","5.06","1",{"$nulls":3},"+",null,null,"800x600",null,null,"+","+","+","+","+","-","1) данная камера является аналогом камеры Axis P1344, от которой отличается другим набором разрешений видеопотока.\n2) камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\"\n3) при включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии. В этом случае переключатель разрешений в Intellect будет игнорироваться.","1. This camera is very similar to the Axis P1344 camera; the cameras differ in the set of available resolutions.\n2. This is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own web interface and select the Enable PTZ check box.\n3. When digital PTZ telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the telemetry settings. In this case, Intellect's resolution switch has no effect."]
["Axis","Axis P1346","Camera","5.40.9.5","1","5","+","-","+","-","-","2048x1536","+",null,"+","+","+","+","+","motion detection; audio detection; tampering detection","\n1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellecte необходимо поставить галочку в родном вебе \"enable PTZ\", в режиме View Areas\n \n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии. В этом случае переключатель разрешений в Intellecte будет игнорироваться.\n \n3. Пресет №1 зарезервирован за Home position\n \n4. максимальное разрешение зависит от режима Capture mode, включенного на камере\n \n5. при Capture mode HDTV или 2MP видео в Полном разрешении в Intellecte не отображается. Чтобы видео появилось, необходимо в веб-интерфейсе сменить разрешение на 1920х1080 или 1600х1200 соответсвенно. Разрешения Высокое и Стандартное доступны при любых режимах Capture mode ","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box in View Areas mode. 2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the device's own web interface, in the telemetry settings. In this case, Intellect's resolution switch has no effect. 3. Preset 1 is for Home position 4.The highest resolution depends on the Capture mode enabled on the camera. 5. HDTV or 2MP video is not displayed with High resolution in Intellect when Capture mode is enabled. In web interface change the resolution for 1920х1080 or 1600х1200 correspondingly to display video. Full and Standard resolutions are available in any state of Capture mode.","improved"]
["Axis","Axis P1347","Camera ","5.11","1",{"$nulls":3},"+.",null,null,"2560x1920 / 2048x1536 / 1920x1080 / 1600x1200",null,null,"+","+","+","+","+","-","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\", в режиме View Areas\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. Пресет №1 зарезервирован за Home position\n4. максимальное разрешение зависит от режима Capture mode, включенного на камере\n5. при Capture mode HDTV, 2MP или 3MP видео в Полном разрешении в Intellect не отображается. Чтобы видео появилось, необходимо в веб-интерфейсе сменить разрешение на 1920х1080 или 1600х1200 bили 2048х1536 соответсвенно. Разрешения Высокое и Стандартное доступны при любых режимах Capture mode \n","1. This is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box, in View Areas mode\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Preset 1 is reserved for Home Position.\n4. The max. resolution depends on which Capture mode, is on for the camera.\n5. When Capture mode is HDTV, 2MP, or 3MP and with full resolution, Intellect does not show video. To fix this, go to the web interface and change the resolution to 1920x1080 (for HDTV), 1600x1200 (for 2MP), or 2048x1536 (for 3MP). High and Standard resolutions are available in any Capture mode. \n"]
["Axis","Axis P1353/-Е ","Camera ","5.40.19","1","5","+",null,"+",null,null,"800x600","+",null,"+","+","+","+","+","motion detection, tampering detection, audio detection"]
["Axis","Axis P1354/-E","Camera","5.40.18 ","1","5","+","-","+","-","-","1280x960","+","-","+","+","+","+","-","motion detection; audio detection; tampering detection","Встроенные детекторы работают только с кодеком MJPEGКамера имеет две степени свободы поворотного крепления. Если открыть кожух, то камеру можно наклонять вверх-вниз, а так же вращать вокруг оси линзы. Для корректной работы настройки \"Поворот видеоизображения\" необходимо в устанавливать поворотное крепление в правильное положение.","On-board detection tools work only with MJPEG codec.  Camera rotary fastening has 2 degrees of freedom. If you open the camera casing, then you can tilt the camera up and down and rotate it around the lens axis. For proper operation of the Video rotation setting, you are to place the rotary fastening into the correct position."]
["Axis","Axis P1355/-E","Camera","5.40.19","1","5","+","-","+","-","-","1920x1080","+","-","-","-","+","-","-","motion detection","Для того, чтобы на камере заработала цифровая телеметрия, нужно включить соответствующую настройку.Камера имеет две степени свободы поворотного крепления. Если открыть кожух, то камеру можно наклонять вверх-вниз, а так же вращать вокруг оси линзы. Для корректной работы настройки \"Поворот видеоизображения\" необходимо в устанавливать поворотное крепление в правильное положение.","To use digital PTZ, enable the appropriate setting. Camera rotary fastening has 2 degrees of freedom. If you open the camera casing, then you can tilt the camera up and down and rotate it around the lens axis. For proper operation of the Video rotation setting, you are to place the rotary fastening into the correct position."]
["Axis","AXIS P1357/-Е","Camera ","5.40.19.1","1","5","+",null,"+",null,null,"2592x1944","+",null,"+","+","+","+","+","motion detection, tampering detection, audio detection","Максимальное разрешение в Интеллекте зависит от настройки \"Capture mode\" в веб-интерфейсе камеры","Max resolution depends on \"Capture mode\" setting in camera web interface."]
["Axis","Axis P3301/-V","Camera ","5.11","1",{"$nulls":3},"+.",null,null,"640x480",null,null,"+","+",null,"+","+","-","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n\n","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution).\n\n"]
["Axis","Axis P3304/-V","Camera","5.40.9.2","1","4","+",null,"+",null,null,"1280x800","+",null,"+","+","+","+","+","audio detection","\n\n При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.Диапазон значений настроек Максимальное время экспозиции и минимальное время экспозиции зависят от значения настройки режим экспозиции\n\n","In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution). Range of values of the Max.exposure and min.exposure parameters depends on the values of the exposure mode setting. \n","improved"]
["Axis","Axis P3343","Camera ","5.20.1","1",null,"+",null,"+.",null,null,"800x600",null,null,"+","+","+","+","+","-","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\", выставить разрешение не больше чем ограниение на странице телеметрии и сделать увеличение.\n2. помимо \"цифровой\" телеметрии у камеры есть оптические зум и фокус, но они не интегрированы. Настраиваются из родного веба.\n3. пресет №1 = home position\n4. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n5. В настройках микрофона при выборе кодека AAC и частоты дискретизации 8 КГц необходимо выбирать битрейт <= 32 Кбит/с","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box. Then set the resolution to the limit on the telemetry web page, or lower, and zoom in. \n2. Apart from digital telemetry, the camera has optical zoom and focus, but they are not integrated. Must be configured from the device's own web interface. \n3. Preset 1 = home position.\n4. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution).\n5. In the microphone settings, when selecting the AAC codec and the 8 kHz sampling rate, set the bit rate to equal to or less than 32 kbps. "]
["Axis","Axis P3344","Camera ","5.06","1",{"$nulls":3},"+.",null,null,"1280x800",null,null,"+","+","+","+","+","-","1. камера не поворотная, но есть \"цифровая телеметрия\". Чтобы заработало в Intellect необходимо поставить галочку в родном вебе \"enable PTZ\", результаты работы телеметрии будут видны при достаточном зумировании картинки.\n2. При включенной \"цифровой телеметрии\" разрешение видеопотока будет ограничено разрешением, выставленным в настройках телеметрии. В этом случае переключатель разрешений в Intellect будет игнорироваться.\n3. помимо \"цифровой\" телеметрии у камеры есть оптические зум и фокус, но они не интегрированы. Настраиваются из родного веба. \n4. Preset №1 зарезервирован за Home Position\n \n","1. It is not a PTZ camera, but it has digital telemetry. To make it work in Intellect, go to the device's own interface and select the Enable PTZ check box. You will see the result of PTZ after you zoom enough.\n2. When digital telemetry is on, the resolution of the video stream is bounded by the resolution that is set in the telemetry settings. In this case, Intellect's resolution switch has no effect.\n3. Apart from digital telemetry, the camera has optical zoom and focus, but they are not integrated. Must be configured from the device's own web interface. \n4. Preset 1 is reserved for Home Position.\n \n"]
["Axis","Axis P3346/P3346-V/P3346-VE","Camera ","5.40.9.3","1","5","+",null,"+",null,null,"2048x1536","+",null,"+","+","+","+","+","+","На камере предусмотрены 5 видеопотоков:0. Получение видео H264/MJPEG и применение настроек.1. Соответствует профилю \"Quality\" в веб-интерфейсе камеры. Получение видео без настроек.2. Соответствует профилю \"Balanced\" в веб-интерфейсе камеры. Получение видео без настроек.3. Соответствует профилю \"Bandwith\" в веб-интерфейсе камеры. Получение видео без настроек.4. Соответствует профилю \"Mobile\" в веб-интерфейсе камеры. Получение видео без настроек.При использовании потоков 1-4 после изменения настроек (через веб-интерфейсе) необходимо перезапускать поток или объект \"камера\".Встроенная аналитика работает:В 0-м потоке в любом кодеке.В любом другом потоке, но только в H264.В максимальном разрешении при максимальном качестве во время съемки быстро движущихся объектов возможны замедления и искажения видео.","The camera allows 5 video streams: 0. Receiving video in H.264/MJPEG with settings applied. 1. Corresponds to the Quality profile in the camera's web interface. Receiving video without settings applied. 2. Corresponds to the Balanced profile in the camera's web interface. Receiving video without settings applied. 3. Corresponds to the Bandwidth profile in the camera's web interface. Receiving video without settings applied. 4. Corresponds to the Mobile profile in the camera's web interface. Receiving video without settings applied. When you use a stream 1 to 4, you must restart the stream or the Camera object after you change settings in the web interface .The embedded video analytics work in stream 0 with any codec. In any other stream, they work only with H.264. At max. resolution and max. quality, fast-moving objects may cause the video to slow down or become distorted. "]
["Axis","Axis P3353","Camera ","5.40.10.2","1","5","+",null,"+",null,null,"800x600","+",{"$nulls":3},"+.",null,null,"motion detection","1. Для того, чтобы заработала телеметрия, необходимо включить настройку \"Цифровая PTZ телеметрия\". \n2. При включенной опции не работают настройки видеопотока.","1. To enable PTZ, select the Digital PTZ checkbox. \n2. With this option enabled, the video stream settings become unavailable."]
["Axis","Axis P3354","Camera","5.40.17","1","5","+","-","+",null,"-","1280x960","+",null,"-","-","+","-","-","motion detection; hacking detection","Для того, чтобы работала телеметрия, необходимо включить соответствующую настройку в свойствах камеры.При включенной опции \"Цифровая PTZ телеметрия\" не работают настройки видеопотока.","To make PTZ works, you need to turn on appropriate setting in device's properties. If you select \"Digital PTZ telemetry\", videostream settings will not be active."]
["Axis","Axis P3363-V/VE","Camera ","5.40.10.2","1","5","+",null,"+",null,null,"800x600","+",{"$nulls":3},"+",{"$nulls":3},"1. В AxxonNext/Next/Next потоки со 2 по 5 (Авто) отвечают Stream Profiles веб-интерфейса и задаются только от туда\n2. Чтобы заработала телеметрия, нужно включить в веб-интерфейсе Enable View Areas ","1. In AxxonNext/AxxonNext, streams 2 to 5 correspond to the relevant Stream profiles in the camera's web interface and can be configured from there\n2. To enable PTZ, select Enable View Areas in the camera's web interface. "]
["Axis","Axis P3364-V/VE","Camera ","5.40.10.2","1","5","+",null,"+",null,null,"1280x960","+",null,"+","+","+.","+","+","motion detection; audio detection; tampering detection","1. На камере предусмотрены 5 видеопотоков:\n0 Получение видео H264/MJPEG и применение настроек\n1-4 Соответствует профилям \"Quality\", \"Balanced\", \"Bandwith\" и \"Mobile\" в веб-интерфейсе камеры. Получение видео без настроек.\n2. При включенной опции \"Цифровая PTZ телеметрия\" не работают настройки видеопотока.","1. The camera allows 5 video streams:\n0 Receiving H264/MJPEG video and applying the settings Corresponds to the Quality, Balanced, Bandwidth and Mobile profiles in the camera's web interface.\n1-4 Corresponds to the Quality, Balanced, Bandwidth and Mobile profiles in the camera's web interface. Receiving video without settings.\n2. With Digital PTZ enabled, the video stream settings become unavailable."]
["Axis","Axis P3367-V/VE","Camera ","5.40.3.2","1","5","+",null,"+",null,null,"2592x1944","+",null,"+","+","+","+","+","+","В AxxonNext/Next потоки со 2 по 5 (Авто) отвечают Stream Profiles веб-интерфейса и задаются только от туда\nЧтобы заработала телеметрия, нужно включить в веб-интерфейсе Enable View Areas ","In AxxonSmar streams from 2 to 5 (Auto) respond Stream Profiles of the web interface and are set only from there\nThat the telemetry earned, it is necessary to include in web interface the Enable View Areas "]
["Axis","Axis P5512","Camera ","5.25","1","5","+",null,"+",null,null,"704x576","+",{"$nulls":3},"+",null,null,"motion detection.","На камере предусмотрены 5 видеопотоков:0. Получение видео H264/MJPEG и применение настроек.1. Соответствует профилю \"Quality\" в веб-интерфейсе камеры. Получение видео без настроек.2. Соответствует профилю \"Balanced\" в веб-интерфейсе камеры. Получение видео без настроек.3. Соответствует профилю \"Bandwith\" в веб-интерфейсе камеры. Получение видео без настроек.4. Соответствует профилю \"Mobile\" в веб-интерфейсе камеры. Получение видео без настроек.При использовании потоков 1-4 после изменения настроек (через веб-интерфейсе) необходимо перезапускать поток или объект \"камера\".Встроенная аналитика работает:В 0-м потоке в любом кодеке.В любом другом потоке, но только в H264.Через Onvif не работают настройки изображения - проблема устройства.Работа камеры проверялась только по протоколу TCP - из-за особенностей удаленного доступа.","The camera allows 5 video streams: 0. Receiving video in H264/MJPEG and applying settings. 1. Corresponds to the Quality profile in the camera's web interface. Receiving video without settings. 2. Corresponds to the Balanced profile in the camera's web interface. Receiving video without settings. 3. Corresponds to the Bandwidth profile in the camera's web interface. Receiving video without settings. 4. Corresponds to the Mobile profile in the camera's web interface. Receiving video without settings. When you use a stream 1 to 4, you must restart the stream or the Camera object after you change settings in the web interface. The embedded video analytics work in stream 0 with any codec; in any other stream, they work only with H264. The image settings do not work via the ONVIF protocol. This is a problem of the device itself. When checking how the camera works, we checked only the TCP protocol; this is a limitation of remote access."]
["Axis","Axis P5522 ","Camera ","5.50.2 ","1","5","+",null,"+",null,null,"720x576 ","+",null,"+","+","+.","+","+","motion detection; audio detection","На камере есть 4 программируемых луча/реле, настройка происходит в меню камеры System Options > Port & Devices > Port Status","There's 4 alarm In/Out on camera. To set up it, please use System Options > Port & Devices > Port Status in camera menu."]
["Axis","Axis P5522-E ","Camera ","5.50.2 ","1","5","+",null,"+",null,null,"720x576 ","+",{"$nulls":3},"+.",null,null,"motion detection"]
["Axis","Axis P5532","Camera ","5.41.2 ","1","5","+",null,"+",null,null,"720x576",{"$nulls":4},"+",null,null,"motion detection","1. Звук, лучи и реле остались непроверенными по причине отстуствия необходимого оборудования","1. Audio, sensors, and relays were not tested, because we did not have the necessary equipment. "]
["Axis","Axis P5534","Camera ","5.40.9.3","1",null,"+",null,"+",null,null,"1280x720","+",null,"+","-","+","-","-","motion detection","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution)."]
["Axis","Axis P7210 / P7214","Encoder ","5.40.7.1","16 / 4","1","+",null,"+",null,null,"720x576","+",null,"+","+","+","+","+","motion detection; audio detection; tampering detection","P7210 представляет из себя 4 4-х канальных одинаковых модуля в одном корпусе, каждый из которых имеет собственный сетевой интерфейс и интегрирован в ПО ITV как отдельное устройство. Назначение контактов лучей/реле нужно настраивать в веб-интерфейсе устройства, в ПО ITV они будут работать соответственно.\nДля того, чтобы в Интеллекте корректно работала привязка микрофонов к видео-каналам, рекомендуется либо использовать транспортный протокол HTTP (используется по умолчанию), либо осуществлять аналогичную настройку в веб-интерфейсе.","P7210 is 4 of the 4th channel identical the module in one casing, each of which has own network interface and is integrated into ITV software as the separate device. Pin assignment of Alarm I/O needs to be set up in the device web interface, in ITV | AxxonSoft software they will work respectively.\nIn order that in Intellect the binding of microphones to video channels correctly worked, the transport protocol HTTP (it is used by default) is recommended or to use, or to realize similar setup in the web interface."]
["Axis","Axis P8221","I/O Module","5.10","8",{"$nulls":6},"-",null,null,"+","-","-","+","+",null,"1. Устройство не имеет видео-канала; только лучи, реле, аудио и телеметрию.","1. No video channel on the device. Only sensors, relays, audio channels and PTZ. "]
["Axis","Axis Q1602/-E","Camera","5.40.3.3","1","5","+","-","+","-","-","768x576","+","-","+","+","-","+","+","+","В ASIP потоки со 2 по 5 (Авто) отвечают Stream Profiles веб-интерфейса и задаются только от тудаКамера имеет две степени свободы поворотного крепления. Если открыть кожух, то камеру можно наклонять вверх-вниз, а так же вращать вокруг оси линзы. Для корректной работы настройки \"Поворот видеоизображения\" необходимо в устанавливать поворотное крепление в правильное положение.","In ASIP, streams 2 to 5 (Auto) are configured via web interface in Stream Profiles. Camera rotary fastening has 2 degrees of freedom. If you open the camera casing, then you can tilt the camera up and down and rotate it around the lens axis. For proper operation of the Video rotation setting, you are to place the rotary fastening into the correct position."]
["Axis","Axis Q1604/-E","Camera ","5.40.3.2","1","5","+",null,"+",null,null,"1280x960","+",null,"+","+",null,"+","+","+","В AxxonNext/Next потоки со 2 по 5 (Авто) отвечают Stream Profiles веб-интерфейса и задаются только от туда","In AxxonNext streams from 2 to 5 (Auto) respond Stream Profiles of the web interface and are set only from there"]
["Axis","Axis Q1755/-E","Camera","5.02","1",null,"+",null,"+",null,null,"1920x1080","-",null,"+","+","+","+","+","-","\n1. в режиме Capture mode=1080i при выставленном разрешении 1920х1080 реально видео будет идти в разрешении 1440х1080. Это особенность самой камеры.\n \n2. у камеры 2 порта I\\O, каждый из которых можно настроить и как Луч и как Реле. Если в Intellecte создать и Луч и Реле проассоциированные с одним и тем же портом, то может наблюдаться картина, когда при замыкании Реле автоматически будет срабатывать и Луч. Особенность интеграции.\n 3. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n ","1. When Capture mode=1080i and you select the 1920x1080 resolution, the actual video resolution is only 1440x1080. This is a limitation of the camera itself.\n2. The camera has 2 I/O ports; each port may be configured as a Sensor and as a Relay at the same time. In Intellect, if you associate a Sensor and a Relay with the same port, then sometimes when the Relay is closed, the Sensor goes off as well. This is how integration has been done.\n3. In H.264 mode and with max. settings, the video may shutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution).","improved"]
["Axis","Axis Q1910","Thermal Imaging Camera ","5.08","1",null,"+",null,"+",null,null,"720x576",null,null,"+","+","-","+.","+","-","1. Камера не обычная, а термальная. Воспринимает тепловое излучение и конвертирует его в цветную картинку.\n2. Максимально доступны 8 fps, это ограничение самой камеры.\n3. Сама камера не PTZ, но позволяет подключать сторонее поворотное устроййство и управлять им.","1. This is a thermal camera, not an ordinary one. It \"sees\" thermal radiation and converts it to a color image. \n2. The max. frame rate is 8 fps; this is a limitation of the camera itself.\n3. The camera itself is not a PTZ camera, but you may attach a third-party pan/tilt drive and control it. "]
["Axis","Axis Q1921/-E","Thermal Imaging Camera","5.50.2","1","5","+","-","+","-","-","768x576","+","-","+","+","+","+","+","motion detection; audio detection; tampering detection","\n1. Камера не обычная, а термальная. Воспринимает тепловое излучение и конвертирует его в цветную картинку.\n3. Сама камера не PTZ, но позволяет подключать стороннее поворотное устройство и управлять им.\n","1. This is a thermal imaging camera. It \"sees\" thermal radiation and converts it to a color image. 3. The camera itself is not a PTZ one, but you may attach a third-party pan/tilt drive and control it."]
["Axis","Axis Q6032/Q6032-E","Camera ","5.41.1.2 ","1","5","+",null,"+",null,null,"704x576",{"$nulls":4},"+",null,null,"motion detection","При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.Для управление функцией автоматического слежения необходимо:Axxon Next:Создать предустановки с номерами 20 и 21Переход на предустановку #20 включает автоматическое слежениеПереход на предустановку #21 выключает автоматическое слежениеИнтеллект:Переход на предустановку #21 включает автоматическое слежениеПереход на предустановку #22 выключает автоматическое слежение","In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution). To manage the auto-tracking functionality: In Axxon Next: Create presets numbered 20 and 21. By switching to preset 20, you switch auto-tracking on. By switching to preset 21, you switch auto-tracking off. In Intellect: By switching to preset 21, you switch auto-tracking on. By switching to preset 22, you switch auto-tracking off."]
["Axis","Axis Q6034","Camera ","5.15","1",{"$nulls":3},"+",null,null,"1280x720",null,null,"+",null,"+",null,null,"-"]
["Axis","Axis Q6034-E","Camera ","5.20.2","1",{"$nulls":3},"+",null,null,"1280x720",{"$nulls":4},"+",null,null,"-"]
["Axis","Axis Q6035 / Q6035-E","Camera ","5.25","1","5","+",null,"+",null,null,"1920x1080","+",{"$nulls":3},"+.",null,null,"motion detection."]
["Axis","Axis Q7401 encoder","Encoder ","5.01","1",{"$nulls":3},"+.",null,null,"768x576 / 720x576",null,null,"+","+.","+","+","+","-","1. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.","1. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times, the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution)."]
["Axis","Axis Q7404 encoder","Encoder ","5.02","4",{"$nulls":3},"+.",null,null,"720x576 (PAL) / 720x480 (NTSC) или 768x576 (PAL) / 640x480 (NTSC)",null,null,"+","+.","+","+.","+","-","1. Максимальное разрешение зависит от настройки \"Aspect ratio correction\"\n2. Каждый канал как отдельное устройство, имеет свой веб-интерфейс. Поэтому в нашем ПО надо создавать 4 граббера (и ключ иметь соответствующий)\n3. Звук есть только на первом \"канале\". IP-wizard будет создавать \"Звуковые платы\" на всех 4-х \"каналах\", но работать будет только звук с 1-го \"канала\"\n4. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.","1. The max. resolution depends on how Aspect Ratio Correction is configured. \n2. Each channel is like a separate device and has its own web interface. For this reason, in our software, you must create 4 grabbers\n3. You have audio only on the first channel. The IP Wizard creates an Audio Card for each channel, but only the first channel has audio.\n4. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution)."]
["Axis","Axis Q7406 encoder","Encoder ","5.01","6",{"$nulls":3},"+.",null,null,"720x576 (PAL) / 720x480 (NTSC) или 768x576 (PAL) / 640x480 (NTSC)",{"$nulls":4},"+","+","+","-","аналог Axis 7404\nисполнено в виде платы\nособенности - 6 каналов, каждый из которых имеет свой IP, т.е. в нашем ПО нужно создавать 6 плат видеоввода\n1. Каждый канал как отдельное устройство, имеет свой веб-интерфейс. Поэтому в нашем ПО надо создавать 6 грабберов \n2. При просмотре H.264 видео с максимальными настройками возможно возникновение эффекта отображения видео в \"рваном\" ритме (видеопоток идет рывками, частота отображения кадров \"плавает\"). Для устранения этого эффекта необходимо изменить настройки (качество, а также частота кадров и разрешение) в сторону уменьшения.\n3. Максимальное разрешение зависит от настройки \"Aspect ratio correction\" ","Very similar to Axis 7404\nCard form factor.\nUnique features: 6 channels and each channel has its own IP address, so in our software you must create 6 grabbers.\n1. Each channel is like a separate device and has its own web interface. For this reason, in our software, you must create 6 grabbers. \n2. In H.264 mode and with max. settings, the video may stutter (the video stream freezes at times and the frame rate goes up and down). To fix this, you must lower the settings (quality + frame rate and resolution).\n3. The max. resolution depends on how Aspect Ratio Correction is configured. "]
["Axis","Axis Q7414","Encoder ","5.25.1","4","5","+",null,"+",null,null,"720x576","+",{"$nulls":7},"Устройство 4-канальное, но каждый канал имеет собственный IP-адрес и интегрирован в ПО ITV/Axxon как отдельное устройство. ","It's 4-channel device, however every channel has its own ip address and integrated in Axxonsoft SW as separate device. "]
["Basler","Basler BIP-1000c/c-dn","Camera ","1.5-0","1","3","+","+","+",null,null,"1024x768",{"$nulls":5},"+","+","-","1. Ограничение по fps:\n-MJPEG:\n1024x768 - 20 fps\n720x576 - 30 fps\n-MPEG-4:\n1024x768 - 12 fps\n720x576 - 30 fps\n-H.264:\n1024x768 - 7 fps\n720x576 - 18 fps\n2. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.","1. Frame rate limits:\n-MJPEG:\n1024x768 – 20 fps\n720x576 – 30 fps\n-MPEG-4:\n1024x768 – 12 fps\n720x576 – 30 fps\n-H.264:\n1024x768 – 7 fps\n720x576 – 18 fps\n2. Intellect supports for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry."]
["Basler","Basler BIP-1300c/c-dn","Camera ","1.6-1","1","3","+","+","+",null,null,"1280x960",{"$nulls":5},"+","+","-","1. Ограничение fps на самой камере при разрешении 1280х960:\n-MJPEG   11 fps\n-MPEG-4  9 fps\n-H.264     7 fps\n2. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.","1. At 1280x960 resolution, the camera has the following frame rate limits: \n-MJPEG – 11 fps\n-MPEG-4 – 9 fps\n-H.264 – 7 fps\n2. Intellect supports for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry."]
["Basler","Basler BIP-1600c/c-dn","Camera ","1.6-1","1","3","+","+","+",null,null,"1600x1200",{"$nulls":5},"+","+","-","1. Ограничение fps на самой камере при разрешении 1600х1200:\n-MJPEG   8 fps\n-MPEG-4  5 fps\n-H.264     4 fps\n2. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.","1. At 1600x1200 resolution, the camera has the following frame rate limits:\n-MJPEG – 8 fps\n-MPEG-4 – 5 fps\n-H.264 – 4 fps\n2. Intellect supports for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry."]
["Basler","Basler BIP2-1000c-dn","Camera ","BIP2-3.0.1","1","3","+","+","+",null,null,"1024x768",{"$nulls":7},"-","1. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.\n\n","1. Intellect implements support for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry.\n\n"]
["Basler","Basler BIP2-1300c/с-dn","Camera ","3.5.1","1","3","+","+","+",null,null,"1280x960",{"$nulls":5},"+","+","+","Разрешения 800х600 и 480х360 недоступны в кодеке H264\nВ Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.Встроенная аналитика будет работать только при активных кодеках MJPEG/H264.","With the H.264 codec, you cannot get the 800x600 and 480x360 resolutions. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 in the Windows Registry. The embedded video analytics woks only when the MJPEG/H264 codecs are active."]
["Basler","Basler BIP2-1600c-dn ","Camera ","BIP2-3.0.1","1","3","+","+","+",null,null,"1600x1200",{"$nulls":7},"-","1. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.","1. Intellect supports for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry."]
["Basler","Basler BIP2-1600-25c-dn","Camera ","3.11.1","1","3","+","+","+",null,null,"1600x1200","+"]
["Basler","Basler BIP2-1920c-dn","Camera ","3.4.0","1","2","+","+","+",null,null,"1920x1080","+",{"$nulls":4},"+","+","-","Для поддержки многопоточности в Интеллекте камера интегрирована как двухканальный ip-сервер, где каждому каналу соответствует отдельный поток.Для получения видео с потоков в разных кодеках в Интеллекте нужно создать дополнительную плату видеоввода и переместить на нее одну из камер с соответствующим потоку номером канала. После этого кодек выбирается в свойствах платы видеоввода.В Интеллекте частота кадров и настройки изображения применяются для обоих потоков сразу при изменении их на любом из каналов.Для получения потоков с различной частотой кадров нужно:Создать дополнительную плату видеоввода и переместить на нее одну из камер с соответствующим потоку номером канала.Включить в реестре UseConfigureByWeb = 1.Перезапустить Интеллект и настраивать частоту кадров через веб-интерфейс.","To support multistreaming, Intellect integrates the cameras as a dual-channel IP server, where each channel corresponds to a stream. To receive video from streams with different codecs in Intellect, create an additional grabber and associate it with one of the cameras, so that the channel number corresponds to the required stream. After that, go to the grabber's properties and select a codec. In Intellect, when you change the frame rate and image settings for one of the channels, the changes are applied to both streams. To get streams with different frame rates: Create an additional grabber and associate it with one of the cameras, so that the channel number corresponds to the required stream. Set UseConfigureByWeb = 1 in the Windows Registry. Restart Intellect and set the frame rate in the web interface."]
["Basler","Basler BIP2-640c-dn ","Camera ","BIP2-3.0.1","1","3","+","+","+",null,null,"640x480",{"$nulls":7},"-","1. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.\n\n","1. Intellect supports for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry.\n\n"]
["Basler","Basler BIP2-D1920c-dn","Camera ","3.4.0 ","1","2","+","+","+",null,null,"1920x1080","+",null,"-","-",null,"+","+","-","Для поддержки многопоточности в Интеллекте камера интегрирована как двухканальный ip-сервер, где каждому каналу соответствует отдельный поток.Для получения видео с потоков в разных кодеках в Интеллекте нужно создать дополнительную плату видеоввода и переместить на нее одну из камер с соответствующим потоку номером канала. После этого кодек выбирается в свойствах платы видеоввода.В Интеллекте частота кадров и настройки изображения применяются для обоих потоков сразу при изменении их на любом из каналов.Для получения потоков с различной частотой кадров нужно:Создать дополнительную плату видеоввода и переместить на нее одну из камер с соответствующим потоку номером канала.Включить в реестре UseConfigureByWeb = 1.Перезапустить Интеллект и настраивать частоту кадров через веб-интерфейс.","To support multistreaming, Intellect integrates the cameras as a dual-channel IP server, where each channel corresponds to a stream. To receive video from streams with different codecs in Intellect, create an additional grabber and associate it with one of the cameras, so that the channel number corresponds to the required stream. After that, go to the grabber's properties and select a codec. In Intellect, when you change the frame rate and image settings for one of the channels, the changes are applied to both streams. To get streams with different frame rates: Create an additional grabber and associate it with one of the cameras, so that the channel number corresponds to the required stream. Set UseConfigureByWeb = 1 in the Windows Registry. Restart Intellect and set the frame rate in the web interface."]
["Basler","Basler BIP2-2500c-dn","Camera ","3.11.1","1","2","+",null,"+",null,null,"from WEB","+"]
["Basler","Basler BIP-640c/c-dn","Camera ","1.6-1","1","3","+","+","+",null,null,"640x480",{"$nulls":5},"+","+","-","1. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.","1. Intellect supports streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry."]
["Basler","Basler BIP-D1300c-dn","Camera ","1.6-1","1","3","+","+","+",null,null,"1280x960",{"$nulls":4},"-","+","+","-","1. Ограничение fps на самой камере при разрешении 1280х960:\n-MJPEG   11 fps\n-MPEG-4  9 fps\n-H.264     7 fps\n \n2. В Intellect реализована поддержка стриммингов. Для этого необходимо в конфигурации настроить 3 Граббера (можно с разными кодеками) на одну и ту же камеру. Единственно fps по каждому стриммингу необходимо настраивать через веб-интерфейс с флагом UseConfigureByWeb в реестре.","1. At 1280x960 resolution, the camera has the following frame rate limits:\n-MJPEG: 11 fps\n-MPEG-4: 9 fps\n-H.264: 7 fps\n \n2. Intellect supports for streams. For this, configure 3 Grabbers (possibly with different codecs) for the same camera. Important: For each stream, you must set the frame rate in the web interface and you must have the option UseConfigureByWeb=1 set in the Windows Registry."]
["Beward","Beward B-1014","Camera ","2.2.1.5()","4",null,"+",null,"+",null,null,"704x576",null,null,"+","-","+","-","+","-","1. При подключении к камере следует указвать порт 5000 \n\n ","1. To connect to the camera, enter port 5000. \n\n "]
["Beward","Beward B-1070","Camera ","2.2.1.5(reove-iris)","1",null,"+",null,"+",null,null,"704x576",null,null,"+",null,null,"-","+","-","1. При подключении к камере следует указвать порт 5000 \n2. лучи не работают даже в веб-интерфейсе камеры\n","1. To connect to the camera, enter port 5000. \n2. Sensors do not work in the camera's web interface. \n"]
["Beward","Beward B-2.920","Camera ","2.0.2.2(1000103)","1",null,"-",null,"+",null,null,"1600x1200",null,null,"+","-",null,"-","+","-","1. Порт по-умолчанию на камере 5000, а в Intellect 80. \n2. Ограничение fps:\n1280x720 - 25 fps при H.264 и 15 fps при MJPEG\n1280x960 - 21 fps при H.264 и 7 fps при MJPEG\n1600х1200 - 15 fps при H.264 и 5 fps при MJPEG\n3. чтобы в Intellect Луч работал правильно, нужно чтобы в вебе в разделе Sensor стояло NO, если будет стоять NC, то луч в Intellece,  будет работать наоборот.\n4. При изменении одновременно нескольких настроек, некоторые настройки могут не применяться. Т.е. при изменении допустим разрешения, сама камера перезагружается и в течении 20-30 секунд она недоступна, если в это время (пока камера недоступна) изменить еще и fps, например, то эта настройка (fps) может не примениться. Особенность самой камеры.\n\n\n\n ","1. The default port is 5000; in Intellect, we have 80 as the default port. \n2. Frame rate limits:\n1280x720: 25 fps with H.264 and 15 fps with MJPEG\n1280x960: 21 fps with H.264 and 7 fps with MJPEG\n1600х1200: 15 fps with H.264 and 5 fps with MJPEG\n3. In Intellect, to make Sensor work correctly, set NO in the Sensor section; if you set NC, Sensor works in the opposite way in Intellect. \n4. If you change multiple settings at the same time, some of the settings may not be applied. For example, after you change the resolution, the camera reboots and remains unavailable for 20–30 seconds; if during that time (when the camera is unavailable) you change the frame rate as well, then the changed frame rate may not be applied. This is a limitation of the camera itself.\n\n\n\n "]
["Beward","Beward B85-5-IP","Camera ","6.0.5.7","1",{"$nulls":3},"+",null,null,"704x576",null,null,"+","-","+","+","+","-","1. При подключении к камере следует указвать порт 5000 \n2. чтобы в Intellect Луч работал правильно, нужно чтобы в вебе в разделе Sensor стояло NO, если будет стоять NC, то луч в Intellece,  будет работать наоборот \n3. Звук, лучи, реле подключаются внутри ящика к ip-камере без объектива.\n 4. При изменении одновременно нескольких настроек, некоторые настройки могут не применяться. Т.е. при изменении допустим разрешения, сама камера перезагружается и в течении 20-30 секунд она недоступна, если в это время (пока камера недоступна) изменить еще и fps, например, то эта настройка (fps) может не примениться. Особенность самой камеры.","1. To connect to the camera, enter port 5000. \n2. In Intellect, to make Sensor work correctly, set NO in the Sensor section; if you set NC, Sensor works in the opposite way in Intellect. \n3. To connect audio, sensors, or relays to the IP camera, you have to remove its lens and get inside the case. \n4. If you change multiple settings at the same time, some of the settings may not be applied. For example, after you change the resolution, the camera reboots and remains unavailable for 20–30 seconds; if during that time (when the camera is unavailable) you change the frame rate as well, then the changed frame rate may not be applied. This is a limitation of the camera itself."]
["Beward","Beward B-920WF","Camera ","2.2.1.5","1",null,"+",null,"+",null,null,"1600x1200",null,null,"+","-",null,"-","+","-","1. при подключении к камере необходимо указывать порт 5000 (по-умолчанию он стоит 80)\n2. лучи неработоспособны - заявлено производителем ","1. To connect the camera, enter port 5000 (it is 80 by default).\n2. The sensors do not work (as stated by the manufacturer). "]
["Bosch","Bosch NBC-255-P","Camera ","4.53 (09500453)","1","3",null,null,"+",null,null,"640x480",null,null,"+","+",null,"+","+","motion detection.","1. Лучи/Реле работают только если подключаться к камере с логином «service»","1. To use Sensors/Relays, connect to the camera with the user name \"service\" . "]
["Bosch","Bosch NBC-455-12P","Camera ","4.53","1","2",null,null,"+",null,null,"704x576",null,null,"+","-",null,"+.","+.","motion detection.","Разрешение в MJPEG совпадает с выбранным разрешением в H264 и отдельно не настраивается.Поиск в Axxon Next возвращает модель камеры \"NBC-455-P-IVA series\"Перед работой с лучами/реле необходимо настроить их на режим \"N.O.\" в веб-интерфейсеДля работы с лучами/реле к устройству следует подключаться с логином service","The resolution with MPEG is the same as with H.264 (cannot be set separately). In Axxon Next, the camera is detected as the NBC-455-P-IVA series. Before using sensors/relays, go to the web interface and switch them to NO mode. To use Sensors/Relays, connect to the camera with the user name \"service\". "]
["Bosch","Bosch NBN-498-12P","Camera ","4.10 (46500410)","1","3","+",null,"+",null,null,"704x576",null,null,"+",null,"-","-","+","motion detection.","1. Телеметрия реализована только в ПО Intellect\n2. Лучи/Реле работают только если подключаться к камере с логином «service»","1. Telemetry is implemented only in Intellect\n2. To use Sensors/Relays, connect to the camera with the user name \"service\"."]
["Bosch","Bosch NBN-733V-IP","Camera ","73500580","1","3","+","-","+",null,null,"from WEB(H.264) / 1280x720(mjpeg)","+",{"$nulls":7},"Разрешение настраивается в веб-интерфейсе камеры. В продукте настройка разрешения доступна только для потока в MJPEG.\nВcтроенный детектор IVA4 (intelligent video analytics).\n","You need to set resolution in web-interface of the camera. Only for MLPEG codec accessible to set resolution via ITV | AxxonSoft products. Analytics on-board: intelligent video analytics."]
["Bosch","Bosch NBN-932V-IP","Camera ","73500580","1","3","+",null,"+",null,null,"from WEB(H.264) / 1920x1080(mjpeg)","+",{"$nulls":7},"Разрешение настраивается в веб-интерфейсе камеры. В продукте настройка разрешения доступна только для потока в MJPEG.\nВcтроенный детектор IVA4 (intelligent video analytics).\n","You need to set resolution in web-interface of the camera. Only for MLPEG codec accessible to set resolution via ITV | AxxonSoft products. Analytics on-board: intelligent video analytics."]
["Bosch","Bosch NDC-265-P","Camera ","5.51","1","3","+",null,"+",null,null,"1280x720","+",null,"+","+.",null,"+","+","motion detection.","1. На устройстве две группы разрешений выставляемые в вебе (\"свойство\") - HD и стандартные. На первом канале работает только HD, второй канал можно дублировать с первого, тогда доступно одно разрешение HD или выставить \"h264 BP+\", тогда можно переключаться между двумя малыми разрешениями. Если выбрать свойство \"h264 BP+ с ограничением скорости\", то из продукта можно регулировать ещё и FPS.","1. In web interface, you can select resolutions from 2 types in Properties - HD and standard. Stream 1 work with HD only, stream 2 can be set up to inherit settings from stream 1 and work with HD only or, if you select h264 BP+, then you can switch between two resolutions. If you select \"h264 BP+ with max.fps limit\", then you can also adjust fps on the device.\n"]
["Bosch","Bosch NDC-274-PT (ONVIF)","Camera ","5.80.0032","1","1","+",null,"+",null,null,"1920x1080","+"]
["Bosch","Bosch NDC-455V09-12PS","Camera ","5.51","1","3","+",null,"+",null,null,"704x576","+",null,"+","+",null,"+","+","motion detection.","1. На устройстве две группы разрешений выставляемые в вебе (\"свойство\") - HD и стандартные. На первом канале работает только HD, второй канал можно дублировать с первого, тогда доступно одно разрешение HD или выставить \"h264 BP+\", тогда можно переключаться между двумя разрешениями. если выбрать свойство \"h264 BP+ с ограничением скорости\", то из продукта можно регулировать ещё и FPS.","1. In web interface, you can select resolutions from 2 types in Properties - HD and standard. Stream 1 work with HD only, stream 2 can be set up to inherit settings from stream 1 and work with HD only or, if you select h264 BP+, then you can switch between two resolutions. If you select \"h264 BP+ with max.fps limit\", then you can also adjust fps on the device.\n"]
["Bosch","Bosch NDN-832V03-P","Camera ","5.01","1","3","+",null,"+",null,null,"H.264: 1280x720; MJPEG: 704x480","+",{"$nulls":6},"motion detection."]
["Bosch","Bosch NIN-832-V03P","Camera","5.85 build 16","1","3","+","-","-",null,"-","1920x1080","+",{"$nulls":3},"-",null,"-",null,"Разрешение настраивается в веб-интерфейсе камеры. В продукте настройка разрешения доступна только для потока в MJPEGВcтроенный детектор IVA4 (intelligent video analytics)","You need to adjust resolution in web-interface. In AxxonSoft products resolution is setting available only for MJPEG stream IVA4 (intelligent video analytics)."]
["Bosch","Bosch NWC-0455-10P","Camera ","4.10","1","3","+.","+.",{"$nulls":3},"look at note",{"$nulls":5},"+","+","other detectors; onboard tracker","1. SDK производителя не позволяет провести полноценную интеграцию камеры.  Все настройки (разрешение, битрейт и проч.) необходимо выставлять в веб-интерфейсе камеры, и в Intellect видео будет менятся.\n2. Лучи/Реле работают только если подключаться к камере с логином «service»\n","1. The vendor's SDK does not allow us to fully integrate the camera.   In Intellect, you cannot change any setting (resolution, bit rate, color, etc.). To make the video change in Intellect, you must go to the camera's web interface and configure all the settings there. \n2. To use Sensors/Relays, connect to the camera with the user name \"service\" .\n"]
["Bosch","Bosch NWC-0495-10P","Camera ","4.10(19500410)","1","2","-","+.",{"$nulls":3},"from WEB",{"$nulls":5},"+.","+","-","1. SDK производителя не позволяет провести полноценную интеграцию камеры.  Все настройки (разрешение, битрейт и проч.) необходимо выставлять в вебе, и в Intellect видео будет менятся.\n2. Лучи/Реле работают только если подключаться к камере с логином «service»\n3. Камера поддерживает встроенную аналитику IVA.\n","1. The vendor's SDK does not allow us to fully integrate the camera.  You cannot change any settings in Intellect (resolution, bit rate, color, etc.). To make the video change in Intellect, you must go to the camera's web interface and configure all the settings there.\n2. To use Sensors/Relays, connect to the camera with the user name \"service\".\n3. Onboard analytics IVA\n"]
["Bosch","Bosch NWD-495V03-10P","Camera ","4.00","1","1","-","+.",{"$nulls":3},"704x576",{"$nulls":7},"-","1. SDK производителя не позволяет провести полноценную интеграцию камеры.  Все настройки (разрешение, битрейт, цветность и проч.) необходимо делать в веб-интерфейсе камеры, и в Intellect видео будет менятся.\n2. Камера работает через ONVIF, но только в режиме совместимости","1. The vendor's SDK does not allow us to fully integrate the camera.  To make the video change in Intellect, you must go to the camera's web interface and set all the settings (resolution, bit rate, color, etc.) there.\n2. The camera works via the ONVIF protocol, but only in compatibility mode."]
["Bosch","Bosch VG4-3xx series","Camera","Hardware version F0000E41 / Firmware version 01500415 / Major version number 4.15 / Build number 01","1","3","+","+","-",null,"-","look into notes","-",null,null,"-","-","+.","+.","other detectors; onboard tracker.","SDK производителя не позволяет провести полноценную интеграцию камеры.  Все настройки (разрешение, битрейт и проч.) необходимо выставлять в вебе, и в Intellectе видео будет изменяться.Для полноценной работы телеметрии в ПО ITV рекомендуется  выбирать \"протокол\" телеметрии \"Bosch-Autodome\". Назначение пресетов осуществляется с подтверждением (нажатие кнопки \"Фокус +\" на панели телеметрии).Прошивка 30500410: для того, чтобы получить в ПО ITV видео в формате h263, в веб-интерфейсе устройства необходимо выбрать кодек mpeg4 HS++. Камера поддерживает встроенную аналитику IVA.","Manufacture's SDK doesn't allow to do full integration. You need to adjust all device settings (resolution, bitrate, etc.) in web-interface, then settings will be changed in Axxon Intellect. In AxxonSoft products for complete works of PTZ is recommended to select Bosch-Autodome PTZ-protocol. To adjust presets you need to approve it by pressure \"Focus +\" in telemetry panel. Firmware 30500410: to get video in h263 codec in AxxonSoft products you need to select MPEG4 HS++ codec in web-interface. Camera supports inbuilt analitics IVA."]
["Bosch","Bosch VG5 AutoDome 700 Series","Camera ","5.52","1","3","+",null,"+",null,null,"704x576","+",{"$nulls":3},"-",null,null,"-","1. Перечень встроенных детекторов: \nIVA 5.5 \nОбъект в поле\nПересечение линии\nПраздношатание\nИзменение условий\nСледование по маршруту\nНесанкционированный доступ\nУдаленный объект\nБездействующий объект\nВход в поле\nВыход из поля\nПоиск сходства\nСчетчик\nСчетчик BEVIVA 5.5 Flow\nНесанкционированный доступ\nОбнаружение скоплений\nПоток в поле\nПротивопоток в поле\n2. Для корректного отображения и записи видео в формате H264 для настройки частоты опорных кадров не следует выбирать значение 0.\n3. Для работы функций Zoom и Focus в ПО Интеллект нужно в реестре Wondows в папке HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\TELEMETRY\\ создать строковый параметр UseBoschOSRD40 со значением 1.","1. Embedded IVA 5.5 detection allows you to: \nDetect objects entering, leaving, or just being within an area (detection field)Detect multiple line crossing from single line up to three lines combined in a logical row Detect loitering in an area related to radius and time Detect condition change properties such as size, speed, direction, and aspect ratio change within a specified time span (for example something falling down)Detect trajectories/routes of objects, passing in the scene, displayed with tracking lines Detect Camera Tampering (alarms on camera hooding/masking, blinding, defocusing, and repositioning).Detect removed objects within a configurable time span Detect idle objects within a configurable time span Count objects crossing a virtual line or entering a certain area (Counter)Detect a certain crowd level in a predefined field Detect flow of constantly moving objects Detect object that moves against a flow of objects\n2. H264 video is displayed correctly only if you set the key frame frequency value other than 0.\n3. In Intellect, to enable Zoom and Focus, you should create a string parameter UseBoschOSRD40 in the HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\TELEMETRY\\ folder and assign it the value of 1."]
["Bosch","Bosch VG5 AutoDome 800 Series  ","Camera","5.52","1","3","+",null,"+",null,null,"H.264: 1920x1084; MJPEG: 1920x1072","+",null,"-","-","-","-","-","-","Что бы настройки изменялись на втором потоке нужно выставить определенные настройки в веб-интерфейсе:Max. frame rate - \"25/30 ips (up to 1920x1080)\"Property на Stream 1 - \"H.264 MP 7200p25/30 fixed\"Property на Stream 2 - \"H.264 BP+bit-rate-limited\" или \"H.264 MP SD\" В ПО Интеллект версии 4.8 и ниже для работы функций Zoom и Focus в ПО Интеллект нужно в реестре Wondows в папке HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\TELEMETRY\\ создать строковый параметр UseBoschOSRD40 со значением 1","To change the settings of the second stream, the settings in the web interface are to be: Max. frame rate - \"25/30 fps (up to 1920x1080)\"Property for Stream 1 - \"H.264 MP 7200p25/30 fixed\"Property for Stream 2 - \"H.264 BP+bit-rate-limited\" or \"H.264 MP SD\". In Intellect software (version 4.8 or older) to enable Zoom and Focus features, create 'UseBoschOSRD40' string parameter with '1' value in HKEY_LOCAL_MACHINE\\SOFTWARE\\ITV\\INTELLECT\\TELEMETRY\\ folder of Windows registry.","improved"]
["Bosch","Bosch VIP X1 encoder","Encoder ","2.53(05500253)","1","1","-","+.",{"$nulls":3},"from WEB",{"$nulls":4},"-","+","+","other detectors; onboard tracker.","1. SDK производителя не позволяет провести полноценную интеграцию камеры.  Все настройки (разрешение, битрейт и проч.) необходимо выставлять в вебе, и в Intellect видео будет изменяться.\n2. Лучи/Реле работают только если подключаться к камере с логином «service»\n3. Телеметрия работает только в ПО Intellect и только через \"явный\" протокол (напр. Pelco-D)\n4. Камера поддерживает встроенную аналитику IVA.","1. The vendor's SDK does not allow us to fully integrate the camera.  You cannot change any settings in Intellect (resolution, bit rate, color, etc.). To make the video change in Intellect, you must go to the camera's web interface and configure all the settings there.\n2. To use Sensors/Relays, connect to the camera with the user name \"service\". \n3. Telemetry works only in Intellect and only via an \"explicit\" protocol (for example, Pelco-D). )\n4. Onboard analytics IVA"]
["Bosch","Bosch VIP X1 XF encoder","Encoder ","4.53 (09500453)","1","3",null,null,"+.",null,null,"704x576",null,null,"+","+","-","+","+","motion detection.","1. Телеметрия реализована только в ПО Intellect\n2. Лучи/Реле работают только если подключаться к камере с логином «service»\n","1. Telemetry is implemented only in Intellect.\n2. To use Sensors/Relays, connect to the camera with the user name \"service\" .\n"]
["Bosch","Bosch VIP X16 XF E","Encoder","28500570","16","3","+",null,"+",null,null,"704x576","+",null,"+","-","-","+","+","motion detection","Настройки контроллера телеметрии в Интеллекте должны совпадать с настройками на вкладке COM1 в веб-интерфейсе камеры.","In Intellect setting of PTZ controller are to be the same as the setting in COM1 tab in the camera web interface.","new"]
["Bosch","Bosch VIP X1600 encoder","Encoder ","3.53","16",null,"-","+.",{"$nulls":3},"704x576 (from web)",{"$nulls":4},"-","+","+","-","1. Интеграция выполнена через SDK, поэтому не важно какой порт, логин и пароль указывать при подключении.\n2. Сам сервер – это 4 отдельных сетевых устройства (модуля)  в одном корпусе. Каждый модуль настраивается в Intellect как отдельный 4-х канальный граббер. На это нужно обратить внимание при покупке/создании ключа для ПО\n3. MJPEG видео - вспомогательный видеопоток. В Intellect его не интегрируем.\n4. Все настройки (разрешение/цветность/яркость и проч.) через Intellect менять нельзя, необходимо настраивать через веб-интерфейс камеры, а в Intellect настройки будут применяться и видео изменяться.","1. The camera is integrated using the SDK; therefore, it does not matter which port, user name, or password is used to connect. \n2. The encoder itself consists of 4 separate network devices (units) in the same case. In Intellect, configure each unit as a separate 4-channel grabber. Have this in mind when buying/creating a key for the software.\n3. MJPEG is an auxiliary video stream. We cannot integrate it with Intellect. \n4. You cannot change any settings in Intellect (resolution, bit rate, color, etc.). To make the video change in Intellect, you must go to the camera's web interface and configure all the settings there."]
["Bosch","Bosch VIP X1600 M4SA","Encoder ","4.10","4","3","+","+",{"$nulls":3},"from WEB","+",null,"+",null,"-","+","+","motion detection.","Сам сервер – это 4 отдельных сетевых устройства (модуля) в одном корпусе. Каждый модуль настраивается в Intellect как отдельный 4-х канальный граббер. На это нужно обратить внимание при покупке\\создании ключа для ПО","The server consists of 4 separate network devices (units) in the same case. In Intellect, configure each unit as a separate 4-channel grabber. Have this in mind when buying/creating a license key for the software."]
["Bosch","Bosch VIP-X1600 XFM4","Encoder ","4.21","4","3","+",null,"+",null,null,"480x576","+",null,"+","+","-","+","+","motion detection.","Сам сервер – это 4 отдельных сетевых устройства (модуля) в одном корпусе. Каждый модуль настраивается в Intellect как отдельный 4-х канальный граббер. На это нужно обратить внимание при покупке\\создании ключа для ПО","The server consists of 4 separate network devices (units) in the same case. In Intellect, configure each unit as a separate 4-channel grabber. Have this in mind when buying/creating a license key for the software."]
["Bosch","Bosch VJR-F801-IxxV","Camera ","4.53","1","3","+",null,"+",null,null,"1280x720","+",{"$nulls":3},"-",null,null,"motion detection.","В драйвере прописан только один набор для значений Частоты кадров для 50Hz. Если активирован режим 60 Гц, то устройство само ставит ближайшее подходящее значение","Only one set of values of fps for 50Hz is registered in the driver. If the mode of 60 Hz is activated, the device itself puts the next suitable value."]
["Bosch","Bosch VOT-320V060L","Thermal Imaging Camera ","4.51(05500451)","1","3","+",null,"+",null,null,"320x240",{"$nulls":4},"-","+","+","motion detection.","1. Камера не обычная, а термальная. Воспринимает тепловое излучение и конвертирует его в цветную картинку.\n2. Cамо устройство выдает только 8 fps максимум\n3. Cамо устройство выдает видео в разрешении 320х240 максимум \n4. Управление телеметрией возможно реализовать только в ПО Intellect\n5. Само устройство с прошивкой 4.51 при подключении по ONVIF не может выдавать MJPEG-видео, только H.264","1. This is a thermal camera, not an ordinary one. It \"sees\" thermal radiation and converts it to a color image.\n2. Frame rate: the device itself allows max. 8 fps.\n3. Resolution: the device itself allows max. 320x240. \n4. Telemetry is implemented only in Intellect.\n5. With the 4.51 firmware and when you connect via the ONVIF protocol, the device itself allows only H.264 video; no MJPEG support. "]
["Brickcom","Brickcom (W)CB-100Ae-08","Camera ","3.0.6.12","1","2","+","+",{"$nulls":3},"1280x800","-",null,"+",{"$nulls":4},"-","1. В ПО ITV/Axxon камеры определяются как CB-100Ae и WCB-100Ae. 2. С прошивкой 3.0.6.12 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу не будет. \n3. AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","1. In ITV/Axxon software cameras are identified as CB-100Ae and WCB-100Ae. 2. With the 3.0.6.12 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. \n3. ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W)CB-100Ae-08(VGA)","Camera ","3.0.6.12","1","2","+","+","+",null,null,"640x480","-",null,"+",{"$nulls":4},"-","В ПО ITV/Axxon камеры определяются как CB-100Ae-VGA и WCB-100Ae-VGA. Прошивка v3.0.6.12: камера обнаруживается поиском как Onvif, но работать по этому протоколу не будет.AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество","In ITV/Axxon software cameras are identified as CB-100Ae-VGA and WCB-100Ae-VGA. 3.0.6.12 firmware: Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W)CB-100Ap","Camera ","3.0.6.12","1","2","+","+","+",null,null,"1280x800",null,null,"+","+",{"$nulls":3},"-","С прошивкой 3.0.6.12 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет.В кодеке MPEG4 в сочетании с максимальным разрешением 1280x800 видео поступает с максимальной частотой кадров, равной 15 fps. (Ограничение самого устройства)Axxon Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the 3.0.6.12 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. With the MPEG4 codec and the max. frame rate (1280x800), video comes at 15 fps max (this is a limitation of the device itself). Axxon Next: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W)CB-100Ap-0c ","Camera ","3.0.6.12","1","2","+","+","+",null,null,"1280x800","-",null,"+","+",{"$nulls":3},"-","С прошивкой 3.0.6.12 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет.В кодеке MPEG4 в сочетании с максимальным разрешением 1280x800 видео поступает с максимальной частотой кадров, равной 15 fps. (Ограничение самого устройства)Axxon Smart: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the 3.0.6.12 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. With the MPEG4 codec and the max. frame rate (1280x800), video comes at 15 fps max (this is a limitation of the device itself). Axxon Smart: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W)FB-100Ap-31","Camera ","3.0.6.12","1","2","+","+","+",null,null,"1280x800",null,null,"+","+",null,"+","+","-","С прошивкой 3.0.6.12 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет.В кодеке MPEG4 в сочетании с максимальным разрешением 1280x800 видео поступает с максимальной частотой кадров, равной 15 fps. (Ограничение самого устройства)Axxon Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the 3.0.6.12 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. With the MPEG4 codec and the max. frame rate (1280x800), video comes at 15 fps max (this is a limitation of the device itself). Axxon Next: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W)FB-130Np","Camera ","3.0.6.25 ","1","2","+","+","+",null,null,"1280x1024","+",null,"+","+",null,"+","+","-","1. Под ТВ-стандартами PAL / NTSC в ПО Intellect подразумеваются форматы отображения 4:3 и 16:9 соответственно\n\n","1. In Intellect, TV standard means aspect ratio (PAL for 4:3 and NTSC for 16:9). \n\n"]
["Brickcom","Brickcom (W)OB-100Ae","Camera ","3.1.0.6C15","1","2","+","+","+",null,null,"1280x800","+",null,"+","+",null,"+","+","+","Максимальный FPS для H264 составляет 15 кадров в секунду.Аудио на камере не работает, если выбран кодек MJPEG.Детектор движения не работает, если выбран кодек MJPEG.","With H.264, the max. frame rate is 15 fps. If you select the MJPEG codec, audio does not work on the camera and the motion detection tool does not work."]
["Brickcom","Brickcom (W)OB-100Ap-73","Camera ","3.0.6.27","1","2","+","+","+",null,null,"1280x800","-",null,"+","+","-","+","+","-","В ПО ITV/Axxon камеры определяются как OB-100Ap, GOB-100Ap и WOB-100Ap. В кодеке MPEG4 при максимальном разрешении 1280x800 есть ограничение на максимальную частоту кадров - 15 fpsВ кодеке MJPEG при увеличении качества падает частота кадров.Прошивка 3.0.6.14: Через Onvif работает только получение видео (без настроек) и поискПрошивка 3.0.6.14: Управление фокусом не всегда работает. Такое же поведение и в веб-интерфейсе - проблема самой камеры.AxxonSmart/Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","In ITV/Axxon software cameras are identified as OB-100Ap, GOB-100Ap and WOB-100Ap. With the MPEG4 codec and the max. frame rate (1280x800), the max. frame rate is 15 fps. With the MJPEG codec, the frame rate drops when you increase the quality. 3.0.6.14 firmware: Via the ONVIF protocol, you can only search and receive video (the settings do not work). 3.0.6.14 firmware: Sometimes focus control does not work. The same is true in the web interface; this is a problem of the device itself. ASIP: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W)VS-01Ap","Camera ","3.1.0.3","1","1","+","+","+",null,null,"720x576","+",null,"+","+","+","+","+","-","1. С прошивкой 3.0.6.18 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет. \n2. Axxon Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","1. With the 3.0.6.18 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. \n2. Axxon Next: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality. "]
["Brickcom","Brickcom (W/G)OB/FD/VD-300Np ","Camera ","3.2.1.3","1","3","+","+","+",null,null,"2032x1536","+",{"$nulls":3},"+",null,null,"motion detection","Чтобы было видео на 2-ом потоке, нужно чтобы TV-out был выключен и разрешение на 1-ом потоке было ниже, чем 2032х1536.","To receive video with stream 2, you should make sure that TV-out is disabled and the resolution for stream 1 is lower than 2032х1536."]
["Brickcom","Brickcom (W/G)OB/FD/VD-302Np / FB-300Np","Camera ","3.2.1.3","1","3","+","+","+",null,null,"2032x1536","+",{"$nulls":3},"+",null,null,"motion detection","Чтобы было видео на 2-ом потоке, нужно чтобы TV-out был выключен и разрешение на 1-ом потоке было ниже, чем 2032х1536.","To receive video with stream 2, you should make sure that TV-out is disabled and the resolution for stream 1 is lower than 2032х1536."]
["Brickcom","Brickcom (W/G)OB-100Ap-73","Camera ","3.0.6.14","1","2","+","+","+",null,null,"1280x800","-",null,"+","+","-","+","+","-","В кодеке MPEG4 при максимальном разрешении 1280x800 есть ограничение на максимальную частоту кадров - 15 fpsВ кодеке MJPEG при увеличении качества падает частота кадров.Прошивка 3.0.6.14: Через Onvif работает только получение видео (без настроек) и поискПрошивка 3.0.6.14: Управление фокусом не всегда работает. Такое же поведение и в веб-интерфейсе - проблема самой камеры.Axxon Smart: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the MPEG4 codec and the max. frame rate (1280x800), the max. frame rate is 15 fps. With the MJPEG codec, the frame rate drops when you increase the quality. 3.0.6.14 firmware: Via the ONVIF protocol, you can only search and receive video (the settings do not work). 3.0.6.14 firmware: Sometimes focus control does not work. The same is true in the web interface; this is a problem of the device itself. Axxon Smart: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom (W/G)OB-130Np / (F/V)D-130Np ","Camera ","3.1.0.9","1","2","+","+","+",null,null,"1280x1024","+",{"$nulls":3},"+",null,null,"-","Камера не поворотная, но имеет встроенный трансфокатор.Максимальная частота кадров в кодеке mjpeg в максимальном разрешении - 15 fps.Переключение соотношения сторон реализовано через параметр \"ТВ-стандарт\" по следующей схеме: PAL = 5:4, NTSC = 4:3, 16:9 = 16:9. Данный параметр меняется для обоих потоках сразу.","This is not a PTZ camera, but it has a built-in zoom lens. With the MJPEG codec, the maximum frame rate is 15 fps. The aspect ratio is changed by changing the value of the TV standard parameter: PAL = 5:4, NTSC = 4:3, 16:9 = 16:9. A change to this parameter applies to both streams at the same time. "]
["Brickcom","Brickcom CB-100Ae-08","Camera ","2.3.7.8","1","2","+","+","-",null,null,"1280x800","-",null,"+",{"$nulls":4},"-","Пока не интегрированы h.264 и аналитикаПрошивка 2.3.7.8: при поиске устройство возвращает неверную прошивку \"100\" - проблема самой камеры.Axxon Smart: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","H.264 and the embedded video analytics are not yet integrated. 2.3.7.8 firmware: the search returns the wrong firmware, 100, for the device; this is the problem of the device itself. Axxon Smart: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom CB-100Ae-08(VGA)","Camera ","v3.0.4.0","1","2","+","+","+",null,null,"640x480","-",null,"+",{"$nulls":4},"-","Axxon Smart: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество","Axxon Smart: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality. "]
["Brickcom","Brickcom FB-100Ae-21","Camera ","2.3.7.8","1","2","+","+",{"$nulls":3},"1280x800","-",null,"+.","+",null,"+","+","-","1. С прошивкой 2.3.7.8 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет. \n2. Axxon Smart: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","1. With the 2.3.7.8 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. \n2. Axxon Smart: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom FB-100Ap","Camera ","v3.0.6.12","1","2","+","+","+",null,null,"1280x800","-",null,"+.","+",null,"+","+","-","В кодеке MPEG4 при максимальном разрешении 1280x800 есть ограничение на максимальную частоту кадров - 15 fpsВ кодеке MJPEG при увеличении качества падает частота кадров. При максимальном качестве видео может не поступать вообще - особенность камеры.Прошивка 3.0.6.12: Камера обнаруживается поиском как устройство, поддерживающее ONVIF, но через ONVIF не работает.Axxon Smart: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the MPEG4 codec and the max. frame rate (1280x800), the max. frame rate is 15 fps. With the MJPEG codec, when you increase the quality, the frame rate drops. At max. quality, video does not come from the camera at all. This is a problem of the camera. The 3.0.6.12 firmware: Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. Axxon Smart: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom FB-200Np","Camera","3.2.2.7.1","1","3","+","+","+",null,null,"1920x1080","+",null,"-","-",null,"-","-","-",null,null,"new"]
["Brickcom","Brickcom FD-100Ae-73","Camera ","2.3.7.8","1","2","+","+",{"$nulls":3},"1280x800",null,null,"+","+",null,"+","+","-","Прошивка 2.3.7.8: при поиске устройство возвращает неверную прошивку \"100\" - проблема самой камеры.Прошивка 2.3.7.8: Реле камеры по умолчанию находится в состоянии замкнуто (хотя в настройках камеры стоит \"нормально разомкнуто\"). Следует сделать пробное замыкание-размыкание его через ПО Axxon/ITV, тогда дальнейшая работа с реле проходит корректно.Прошивка 2.3.7.8: Возможно, что при первичном подключении камера не заработает. Нужно перезапустить камеру.В кодеке MPEG4 видео поступает с максимальной частотой кадров, равной 15 fps. (Ограничение самого устройства)Axxon Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","2.3.7.8 firmware: Search returns the wrong firmware, 100, for the device; this is a problem of the device itself. 2.3.7.8 firmware: By default, the camera's relay is closed (though the camera's settings are set to \"normally open\"). To make the relay work correctly, test it: open/close the relay in the AxxonSoft software. 2.3.7.8 firmware: Sometimes, the camera does not work at the first connection. Restart the camera. With the MPEG4 codec, video comes at 15 fps max (this is a limitation of the device itself). Axxon Next: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom FD-100Ap-73","Camera ","3.0.6.13","1","2","+","+","+",null,null,"1280x800","-",null,"+.","+",null,"+","+","-","1. Камера определяется поиском как onvif, но с данной прошивкой 3.0.6.13 через ONVIF не работает. \n2. Axxon Smart: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"\n","1. With the 3.0.6.13 firmware, Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. \n2. Axxon Smart: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality.\n"]
["Brickcom","Brickcom FD-130Ap-73","Camera ","3.0.6.13","1","2","+","+","+",null,null,"1280x1024",null,null,"+","+",null,"+","+","-","С прошивкой 3.0.6.13 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет.Axxon Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the 3.0.6.13 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. Axxon Next: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom FD-300Ap","Camera ","3.1.0.8","1","2","+","+","+",null,null,"2032x1536","+",null,"+.","+",null,"+","+","+","1. Для мегапиксельных разрешений максимальный FPS = 8.\n2. Разрешение на втором потоке всегда такое же, как на первом. ","1. With megapixel resolution, max. FPS is 8. \n2. Resolution for the 2nd video stream is the same as for the 1st video stream."]
["Brickcom","Brickcom MB-130Ap / WMB-130Ap","Camera","v3.2.2.8","1","3","+","+","+","-","-","1280x1024","+","-","-","-","-","-","-","-"]
["Brickcom","Brickcom MB-300A_series","Camera ","v3.2.1.3","1","3","+","+","+",null,null,"H.264/MPEG4: 2032x1536; MJPEG: 2048x1536","+"]
["Brickcom","Brickcom MD-100Ae","Camera ","3.0.6.12","1","2","+","+",{"$nulls":3},"1280x800","-",{"$nulls":6},"-","1. С прошивкой 3.0.6.12 устройство обнаруживается автопоиском как поддерживающее протокол ONVIF. Но работать по этому протоколу оно не будет. \n2. Axxon Smart: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","1. With the 3.0.6.12 firmware, search detects the device as supporting the ONVIF protocol. But the device does not work via this protocol. \n2. Axxon Smart: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom MD-100Ap","Camera ","v3.1.0.8","1","2","+","+","+",null,null,"PAL: 640x480; NTSC: 1280x720; 16:10: 1280x800","+"]
["Brickcom","Brickcom MD-130Ap","Camera","v3.2.2.8","1","3","+","+","+","-","-","1280x1024","+","-","-","-","-","-","-","-"]
["Brickcom","Brickcom MD-300Ap-360 / MD-300Np-360 / VD-300Af-360 ","Fisheye Camera","3.2.2.6","1","3","+","+","+",null,null,"2032x1536","+"]
["Brickcom","Brickcom MD-300Np","Camera ","3.2.1.3","1","3","+","+","+",null,null,"2032x1536","+",{"$nulls":3},"+",null,null,"motion detection","1. Чтобы было видео на 2-ом потоке, нужно чтобы TV-out был выключен и разрешение на 1-ом потоке было ниже, чем 2032х1536.","1. To receive video with stream 2, you should make sure that TV-out is disabled and the resolution for stream 1 is lower than 2032х1536."]
["Brickcom","Brickcom MD-300Np-360P","Camera","v3.2.2.8","1","3","+","+","+",null,"-","2032x1536(H264) / 2048x1536","+",null,null,"-","-",null,"-"]
["Brickcom","Brickcom MD-500Ap-360","Fisheye Camera","v3.2.2.7","1","3","+","+","+",null,"-","2032x1936(H264/MPEG4) / 2592x1944(MJPEG)","+",null,null,"-","-","-","-"]
["Brickcom","Brickcom OB-100Ap-73","Camera ","v3.0.6.27","1","2","+","+","+",null,null,"1280x800","-",null,"+","+","-","+","+","-","В кодеке MPEG4 при максимальном разрешении 1280x800 есть ограничение на максимальную частоту кадров - 15 fpsВ кодеке MJPEG при увеличении качества падает частота кадров.Прошивка 3.0.6.27: Камера обнаруживается поиском как устройство, поддерживающее Onvif, но не работает.Прошивка 3.0.6.27: Управление фокусом не всегда работает. Такое же поведение и в веб-интерфейсе - проблема самой камеры.Axxon Smart: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the MPEG4 codec and the max. frame rate (1280x800), the max. frame rate is 15 fps. With the MJPEG codec, the frame rate drops when you increase the quality. 3.0.6.27 firmware: Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. 3.0.6.27 firmware: Sometimes focus control does not work. The same is true in the web interface; this is a problem of the device itself. Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","BrickCom OSD-040-D/-E","Camera","v3.1.1.3","1","2","+","+","+",null,"-","720x480","+",{"$nulls":3},"+",null,"-","motion detection"]
["Brickcom","Brickcom OSD-200A","Camera","gk20121228NSA","1","2","+","-","+",null,"-","1920x1080","+",{"$nulls":3},"+",null,"-"]
["Brickcom","Brickcom 50xA_series","Camera ","v3.2.2.3 ","1","3","+","+","+",null,null," H.264/MPEG4: 2032x1936; MJPEG: 2592х1944","+",null,"+.","-",null,"+","+","+","В высоких разрешениях частота кадров ограничена до 15-20 fps\nПри выборе высоких разрешений в первом потоке второй и третий потоки становятся ограниченно доступны:2592x1944 в 1-м потоке: 2-й и 3-й недоступны2032x1936, 2032x1536 в 1-м потоке: 2-й недоступен, в 3-м доступно только разрешение 336х240\nВстроенный детектор движения не работает с кодеком mjpeg.Встроенный детектор движения присылает уведомление об окончании тревоги спустя 3-5 секунд после окончания движения.\nfw 3.2.0.2, 3.2.0.6: Аудио-выход не работает на самом устройстве. Возможно, проблема в конкретном экземпляре, т.к. производители уверяют, что на этих же прошивках у них аудио-выход работает.","At high resolutions, the max. frame rate is 15–20 fps. When you select a high resolution for the first stream, the second and third streams are not always available. 2592x1944 for the 1st stream: the 2nd and 3rd streams are not available; 2092x1936 or 2032x1536 for the 1st stream: the 2nd stream is not available; for the third stream, only 336x240 resolution is available. With the MJPEG codec, the embedded motion detection tool does not work. The embedded motion detection tool notifies about the end of an alarm only 3–5 seconds after the motion stops."]
["Brickcom","Brickcom PZ-040D/E","Camera ","3.1.0.8","1","2","+","+","+",null,null,"720x480 / 720x576","+",{"$nulls":3},"+",null,null,"-"]
["Brickcom","Brickcom VD-100Ap-73","Camera ","3.0.6.12","1","2","+","+","+",null,null,"1280x800",null,null,"+","+",null,"+","+","-","1. Камера обнаруживается поиском как устройство, поддерживающее Onvif, но не работает. \n2. Axxon Next: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","1. Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. \n2. Axxon Next: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom VD-130Ap-73","Camera ","3.0.6.13","1","2","+","+","+",null,null,"1280x1024","-",null,"+","+",null,"+","+","-","В кодеке MJPEG при увеличении качества падает частота кадров.Прошивка 3.0.6.13: Устройство обнаруживается поиском как поддерживающее Onvif, но не работает.Axxon Smart: Перед переключением кодека на MJPEG параметр \"Режим компресии\" должен иметь значение \"Постоянное качество\"","With the MJPEG codec, when you increase the quality, the frame rate drops. 3.0.6.13 firmware: Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. Axxon Smart: Before switching the codec to MJPEG, set the Compression Control parameter to Constant Quality."]
["Brickcom","Brickcom VD-200Np ","Fisheye Camera","v3.2.2.7","1","3","+","+","+",null,"-","1920x1080","+",{"$nulls":3},"-",null,"-"]
["Canon","Canon VB-H610 / VB-H610D / VB-H610VE","Camera","Ver. 1.2.0","1","1","+","-","+",null,"-","1920x1080","+",null,"-","-","+.","+","+","-"]
["Canon","Canon VB-H710F","Camera","Ver. 1.2.0 3015","1","1","+","-","+","-","-","1920x1080","+","-","-","-","-","+","+","-"]
["Canon","Canon VB-M40","Camera","Ver. 1.1.0","1","1","+","-","+",null,"-","1280x960","+",null,"-","-","+.","+.","+","-"]
["Canon","Canon VB-S900F","Camera","Ver. 1.1.0","1","2","+",null,"+",null,null,"1920x1080","+",null,"-",null,null,"+","+",{"$nulls":3},"improved"]
["Certis","Certis NBV-3800RFH","Camera ","ce20130424NSA","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":7},"При смене режима ТВ-стандарта камера перезагружается","After changing TV-standart, the camera will be rebooted."]
["Certis","Certis NDF-3100FH","Camera ","ce20120202ANS","1","2","+",null,"+",null,null,"1920x1080","+",null,null,"-",{"$nulls":4},"1. Разрешения 1280х1024 и 1920х1080 во втором потоке доступны только для кодека MJPEG.\n2. Использование максимальных разрешений (1280х1024 и 1920х1080) доступно только в однопоточном режиме","1. 1280х1024 and 1920х1080 resolution for the 2nd video stream is available just for MJPEG. \n2. 1280х1024 and 1920х1080 using is available just for a single stream mode."]
["Certis","Certis NDF-3100FH-E","Camera ","ce20120615NSA","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":7},"1. Разрешения 1280х1024 и 1920х1080 во втором потоке доступны только для кодека MJPEG\n2. Использование максимальных разрешений (1280х1024 и 1920х1080) доступно только в однопоточном режиме","1. 1280х1024 and 1920х1080 resolution for the 2nd video stream is available just for MJPEG. \n2. 1280х1024 and 1920х1080 using is available just for a single stream mode."]
["Certis","Certis NDV-3300RFH","Camera ","ce20120202ANS","1","2","+",null,"+",null,null,"1920x1080","+",null,null,"-",{"$nulls":4},"1. Частота кадров меняется для обоих потоков одновременно\n2. Максимальные разрешения 1280х1024 и 1920х1080 доступны только в однопоточном режиме\n3. Во втором потоке разрешения 1280х720, 1280х1024 и 1920х1080 доступны только для кодека MJPEG","1.The frame rate is changed for both streams simultaneously. \n2. 1280х1024 and 1920х1080 resolutions are available only for a single stream mode. \n3.1280х720, 1280х1024 and 1920х1080 resolutions for the 2nd video stream are available only for MJPEG."]
["Certis","Certis NDV-3300RFH-E","Camera ","ce20120615NSA","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":7},"1. Разрешения 1280х1024 и 1920х1080 во втором потоке доступны только для кодека MJPEG\n2. Использование максимальных разрешений (1280х1024 и 1920х1080) доступно только в однопоточном режиме\n3. Настройки аудио-кодека и битрейта для динамика и микрофона переключаются одновременно (одна настройка в веб-интерфейсе) ","1. 1280х1024 and 1920х1080 resolution for the 2nd video stream is available just for MJPEG. \n2. 1280х1024 and 1920х1080 using is available just for a single stream mode."]
["Certis","Certis NDV-4100HD","Camera ","ce20120202NS","1","2","+","+","+",null,null,"1280x960","+",null,null,"-",{"$nulls":4},"1. Максимальная частота кадров в разрешении 1280х960 - 12.5 fps.\n Во втором потоке разрешение 1280х960 доступно только для кодека MJPEG.\n При использовании комбинации кодеков h264+h264 разрешение 1280х720 во втором потоке доступно только при выборе 1280х720 на первом потоке. При этом максимальная частота кадров составляет 12.5 fps.","The max. frame rate for 1280х960 resolution is 12.5 fps. \n1280х960 resolution for the 2nd video stream is available only for MJPEG. \nFor combination of h264+h264 codecs, 1280х720 resolution for the 2nd stream is available, when 1280х720 resolution is for the 1st stream, and its max. frame rate is 12.5 fps.\n"]
["Certis","Certis NSD-6036H / NSD-6030H / NSD-6018H / NSD-6018PI-X","Camera ","ce20121228NSA ","1","2","+",null,"+",null,null,"720x576 ","+",{"$nulls":3},"+"]
["Certis","Certis NSD-7018FH / NSD-7020FH","Camera ","ce20120413NSA","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":3},"+",null,null,"+","Поворот изображения на 90 градусов по/против часовой стрелки работают только при разрешениях начиная с 640x480.","Image turn on / counter-clockwise on 90 degrees is possible only in case of resolution since 640x480."]
["CNB","CNB IDC 4050F","Camera ","XNET.M1-1.01.10.1021","1","2",null,null,"+",null,null,"640x480 (MJPEG) / 1920x1080 (H264)",null,null,"+","-",null,"-",null,"+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.Набор доступных разрешений во втором потоке зависит от выбранного кодека во втором потоке и текущего разрешения в первом потоке: Разр-е в 1м потоке Кодек в 2-м потоке Доступные разр-я в 2-м потоке 352x288 h264 352x288 mjpeg 352x288 640x480 h264 320x240 mjpeg 320x240,640x480 720x576 h264 352x288 mjpeg 352x288, 720x576 1280x720 h264 352x288 mjpeg 352x288, 720x576 1280x1960 --- --- 1920x1080 --- --- Перед сменой потока на \"1.MJPEG/H264\" (в Axxon Next) или кодека на \"MJPEG\" (в Интеллекте) необходимо выбрать в потоке \"0.H264\" (в Axxon Next) или в кодеке \"H264\" (в Интеллекте) приемлемое разрешение (см. таблицу выше)В Интеллекте в кодеке MJPEG \"полное\" разрешение недоступно","According to the vendor, currently it is not possible to integrate sensors. Which resolutions are available for the second stream depends on the codec selected for the second stream and the current resolution for the first stream: Resolution (1st stream) Codec (2nd stream) Resolutions available (2nd stream) 352x288 h264 352x288 mjpeg 352x288 640x480 h264 320x240 mjpeg 320x240,640x480 720x576 h264 352x288 mjpeg 352x288, 720x576 1280x720 h264 352x288 mjpeg 352x288, 720x576 1280x1960 --- --- 1920x1080 --- --- Before changing the stream to 1.MJPEG/H264 (in Axxon Next) or the codec to MJPEG (in Intellect), select the acceptable resolution for the 0.H264 stream (in Axxon Next) or H264 codec (in Intellect) (see the table above). In Intellect, \"full\" resolution is not available for the MJPEG codec."]
["CNB","CNB IDC 4050IR","Camera ","XNET.A2-1.01.10.0827","1","2",null,null,"+",null,null,"640x480 (MJPEG) / 1920x1080 (H264)",null,null,"+","-",null,"-",null,"+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.Набор доступных разрешений во втором потоке зависит от выбранного кодека во втором потоке и текущего разрешения в первом потоке: Разр-е в 1м потоке Кодек в 2-м потоке Доступные разр-я в 2-м потоке 352x288 h264 352x288 mjpeg 352x288 640x480 h264 320x240 mjpeg 320x240,640x480 720x576 h264 352x288 mjpeg 352x288, 720x576 1280x720 h264 352x288 mjpeg 352x288, 720x576 1280x1960 --- --- 1920x1080 --- --- Перед сменой потока на \"1.MJPEG/H264\" (в Axxon Next) или кодека на \"MJPEG\" (в Интеллекте) необходимо выбрать в потоке \"0.H264\" (в Axxon Next) или в кодеке \"H264\" (в Интеллекте) приемлемое разрешение (см. таблицу выше)В Интеллекте в кодеке MJPEG \"полное\" разрешение недоступноПрошивка XNET.A2-1.01.10.0827: значение \"25 fps\" параметра \"частота кадров\" не работает на самой камере.","According to the vendor, currently it is not possible to integrate sensors. Which resolutions are available for the second stream depends on the codec selected for the second stream and the current resolution for the first stream: Resolution (1st stream) Codec (2nd stream) Resolutions available (2nd stream) 352x288 h264 352x288 mjpeg 352x288 640x480 h264 320x240 mjpeg 320x240,640x480 720x576 h264 352x288 mjpeg 352x288, 720x576 1280x720 h264 352x288 mjpeg 352x288, 720x576 1280x1960 --- --- 1920x1080 --- --- Before changing the stream to 1.MJPEG/H264 (in Axxon Next) or the codec to MJPEG (in Intellect), select the acceptable resolution for the 0.H264 stream (in Axxon Next) or H264 codec (in Intellect) (see the table above). In Intellect, the \"full\" resolution is not available for the MJPEG codec. XNET.A2-1.01.10.0827 firmware: the value of 25 fps for the Frame Rate parameter does not work on the camera itself. "]
["CNB","CNB IDC 4050VR","Camera ","XNET.M1-3.00.13.0204","1","2","+",null,"+",null,null,"1920x1080 (H264) / 720x576 (MJPEG)",null,null,"+",{"$nulls":5},"1. Настройка битрейта / качества на камере имеет динамический диапазон значений (зависит от выбранного разрешения). В ПО ITV/Axxon такую зависимость реализовать невозможно, поэтому интегрирован весь диапазон возможных значений.\n2. Набор разрешений на потоках взаимозависим:\n(1-ый поток) 1920x1080, 1280x1024, 1280x960 <=> (2-й поток) недоступен вообще\n(1-ый поток) 1280x720, 720x576 <=> (2-й поток) 720x576, 352x288\n(1-ый поток) 640x480 <=> (2-й поток) 640x480, 320x240\n(1-ый поток) 352x288 <=> (2-й поток) 352x288","1. Bitrate / quality on camera has dynamic value range (it depends on selected resolution). It can't be implemented in Axxosoft SW, that's why the whole range of possible value has been integrated. \n2. The list of resolution for the streams is interdependent:\n(1st stream) 1920x1080, 1280x1024, 1280x960 <=> (2nd stream) not available;\n(1st stream) 1280x720, 720x576 <=> (2nd stream) 720x576, 352x288;\n(1st stream) 640x480 <=> (2nd stream) 640x480, 320x240;\n(1st stream) 352x288 <=> (2nd stream) 352x288"]
["CNB","CNB IDP 4000VD","Camera ","XNET.A1-1.1.10.0630","1","1","+","+","+",null,null,"640x480",null,null,"+","-",null,"-","+","+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной. ","According to the vendor, currently it is not possible to integrate sensors. "]
["CNB","CNB IDP 4000VR","Camera ","XPDN.A1-1.1.10.126","1","2","+","+","+",null,null,"640x480",{"$nulls":3},"-",null,"-",null,"+"]
["CNB","CNB IDP 4030VR","Camera ","XNET.A1-1.1.11.0325","1","2","+","+","+",null,null,"H264/MPEG4: 640x480; MJPEG: 1280x960",null,null,"+","-",null,"-","+","+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.Прошивка XNET.A1-1.01.10.0630: Камера присылает неправильные метки времени - время идет ускоренно, поэтому архив не будет работать правильно.Прямое переключение потоков \"2.MJPEG\" -> \"1.MJPEG\" не работает. Нужно выполнять переключение по схеме \"2.MJPEG\" -> \"0.MPEG4/H264\" -> \"1.MJPEG\".","According to the vendor, currently it is not possible to integrate sensors. XNET.A1-1.01.10.0630 firmware: The camera sends wrong timestamps: the archive does not work correctly, because time \"moves\" faster than it should. You cannot switch from the 2.MJPEG stream to the 1.MJPEG stream directly. You must switch from 2.MJPEG first to 0.MPEG4/H264 and then to 1.MJPEG. "]
["CNB","CNB IGP 1030","Camera ","XNET.A1-1.01.10.634","1","2","+","+","+",null,null,"1280x960(MJPEG) / 640x480(MPEG-4) / 640x480(H.264)",null,null,"+","-","+","-","+","+","1. По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной. \n2. Из цифровой телеметрии доступно только перемещение изображения. Реализация увеличения и предустановок невозможна по утверждению производителя. ","1. According to the vendor, currently it is not possible to integrate sensors. \n2. Of the digital telemetry functions, only image movement is available. According to the vendor, zoom and presets cannot be implemented. "]
["CNB","CNB INS 2000 encoder","Encoder ","XNET.x1-1.1.10.304","1","2","+","+","+",null,null,"704x576(PAL) / 704x480 (NTSC)",null,null,"+","-","+","-","+","+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.","According to the vendor, currently it is not possible to integrate sensors. "]
["CNB","CNB IPM 3063 N(P)","Camera ","XPDN.A1-1.1.10.126","1",null,"+","+","+",null,null,"704x576",null,null,"+","-","+","-","+","+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.","According to the vendor, currently it is not possible to integrate sensors. "]
["CNB","CNB ISMC 1063N","Camera ","XPDN.A1-1.1.10.126","1","2","+","+","+",null,null,"704x480",{"$nulls":3},"-","+","-",null,"+"]
["CNB","CNB IVC 4000T","Camera ","XNET.T1-1.0.10.1222","1","2","+","+",{"$nulls":3},"640x480",null,null,"-","-",null,"-","+","-","1. Разрешение меняется сразу для обоих стриммингов одновременно. Это особенность самой камеры.\n2. По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.","1. The resolution is adjusted for both streams at the same time. This is a limitation of the camera itself. \n2. According to the vendor, currently it is not possible to integrate sensors. "]
["CNB","CNB IVP 4030VR","Camera ","XNET.A1-1.1.11.0325","1","2","+","+","+",null,null,"1280x960(MJPEG) 640x480(MPEG-4) 640x480(H.264)",null,null,"+","-",null,"-","+","+","По утверждению производителя, в настоящий момент интеграция лучей не представляется возможной.Прошивка XNET.A1-1.01.10.0630: Камера присылает неправильные метки времени - время идет ускоренно, поэтому архив не будет работать правильно.","According to the vendor, currently it is not possible to integrate sensors. XNET.A1-1.01.10.0630 firmware: The camera sends wrong timestamps and the archive does not work correctly, because time \"moves\" faster than it should. "]
["ComOnyx","ComOnyx CO-i03MY1","Camera ","V1.0.32_Y ","1","2","+","-","+",null,null,"640x480","+",null,"+","+",{"$nulls":3},"+","Камера определяется как Yudor CO-i03MY1 (YUC-HS94)","In the AxxonSoft products, the camera is identified as Yudor CO-i03MY1 (YUC-HS94)"]
["ComOnyx","ComOnyx CO-i04DY2","Camera ","V1.0.32_Y","1","2","+","-","+",null,null,"720x576","+",null,"+","+",null,"+","+","+","1. Между переходами луча в состояние \"замкнуто\" должен соблюдаться временной интервал, настраиваемый через веб-интерфейс. Минимальное значение - 10 секунд.\n2. Через Onvif камера работает только в режиме совместимости. Видео и звук идут, но никакие настройки не применяются.\n3. В Интеллект поиск находит камеру как FineCCTV.\n4. Камера определяется как Yudor CO-i04DY2(3.7-12) (YUC-HM93-312)","1. You can configure the delay before a sensor closes in the camera's web interface. Min 10 seconds.\n2. Via the ONVIF protocol, the camera works only in the compatibility mode. Video and audio streams are there but changes can't be applied.\n3. In AxxonSoft Intellect, the camera is identified as FineCCTV IP-Cam.\n4. In the AxxonSoft products, the camera is identified as CO-i04DY2(3.7-12) (YUC-HM93-312)"]
["ComOnyx","ComOnyx CO-i10SY2IRP ","Camera ","VB1.0.34","1","2","+","+","+",null,null,"1280x800 ","+",{"$nulls":4},"+","+"]
["ComOnyx","ComOnyx CO-i13MY1","Camera ","V1.0.32_Y","1","2","+","-","+",null,null,"1280x1024","+",null,"+","+",{"$nulls":3},"+","1. На камере есть ограничение FPS в зависимости от разрешения:\n Для разрешений не больше 640x480 ограничение составляет 30 fps, для больших разрешений - 15. Ограничение включается для всех потоков, если разрешение >640x480 установлено хотя бы на одном из двух потоков. \n2. Камера определяется как Yudor CO-i13MY1 (CO-YUC-HS95)","1. The camera has frame rate limits (depending on the resolution):\n For resolutions lower than 640x480 the max fps is 30, fro greater resolutions it is 15. This limitation applies to all streams if a resolution greater than 640x480 is set for any of the 2 streams. \n2. In the AxxonSoft products, the camera is identified as Yudor CO-i13MY1 (CO-YUC-HS95)."]
["ComOnyx","ComOnyx CO-i20DY2(P)","Camera ","V1.0.32_Y","1","2","+","-","+",null,null,"1600x1200","+",null,"+","+",null,"+","+","+","1. Поиск в AN не определяет прошивку: ее нужно выбрать самостоятельно.\n2. Между переходами луча в состояние \"замкнуто\" должен соблюдаться временной интервал, настраиваемый через веб-интерфейс. Минимальное значение - 10 секунд.\n3. Прошивка V1.0.32_Y: через Onvif камера работает только в режиме совместимости. Видео и звук идут, но никакие настройки не применяются. \n4. В Интеллекте поиск находит камеру как FineCCTV.\n5. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.\n6. Камера определяется как Yudor CO-i20DY2(2,7-9) (CO-YUC-HM96-279)","1. In the AxxonSoft products, the device's firmware version cannot be identified. You must select the firmware version yourself.\n2. You can configure the delay before a sensor closes in the camera's web interface. Min 10 seconds.\n3. The V1.0.32_Y firmware: via the ONVIF protocol, the camera works only in the compatibility mode. Video and audio streams are there but changes can't be applied. \n4. In AxxonSoft Intellect, the camera is identified as FineCCTV.\n5. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, before using the camera, go to the web interface and select the required value.\n6. In the AxxonSoft products, the camera is identified as Yudor CO-i20DY2(2,7-9) (CO-YUC-HM96-279)."]
["ComOnyx","ComOnyx CO-i20DY2IRPV","Camera ","V1.0.32_Y","1","2","+","-","+",null,null,"1600x1200","+",null,"+","+",null,"+","+","+","1. Настройка \"Параметры видео\" определяет ограничение FPS в зависимости от разрешения. Для получения максимального FPS необходимо следить за тем, чтобы разрешение настройки \"Параметры видео\" было не больше, чем выбренное разрешение получаемого видео.\n2. После размыкания датчика реакция на следующее замыкание может произойти не раньше, чем через 10 секунд.\n3. Камера определяется как Yudor CO-i20DY2IRPV (CO-YUC-Hi96RP)","1. The Video Parameters setting is used to limit fps depending on the resolution. To get the maximum frame rate, make sure that the Video Parameters setting has the the same or lower resolution than you selected on the VMS.\n2. After opening, the sensor can close in not earlier than 10 seconds.\n3. In the AxxonSoft products, the camera is identified as Yudor CO-i20DY2IRPV (CO-YUC-Hi96RP)."]
["ComOnyx","ComOnyx CO-i20HY0","Camera ","V1.0.26_Y","1","2",null,null,"+",null,null,"1600x1200",null,null,"+","-","+","+","+","+","1. Поиск в AN не определяет прошивку: ее нужно выбрать самостоятельно.\n2. Прошивка V1.0.26_Y: камера работает по Onvif только в режиме совместимости, поиском как Onvif не находится.\n3. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.\n4. Камера определяется как Yudor CO-YUC-H696","1. In the AxxonSoft products, the device's firmware version cannot be identified. You must select the firmware version yourself.\n2. The V1.0.26_Y firmware: Via the ONVIF protocol, the camera works only in compatibility mode; the search does not find the camera as a device that supports ONVIF.\n3. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, before using the camera, go to the web interface and select the required value.\n4. In the AxxonSoft products, the camera is identified as Yudor CO-YUC-H696."]
["ComOnyx","ComOnyx CO-i20HY0DNP","Camera ","V1.0.26_Y","1","2",null,null,"+",null,null,"1600x1200",null,null,"+","-","+","+","+","+","1. Поиск в AN не определяет прошивку: ее нужно выбрать самостоятельно.\n2. Прошивка V1.0.26_Y: камера работает по Onvif только в режиме совместимости, поиском как Onvif не находится.\n3. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.\n4. Камера определяется как Yudor CO-YUC-H696RP","1. In the AxxonSoft products, the device's firmware version cannot be identified. You must select the firmware version yourself.\n2. The V1.0.26_Y firmware: Via the ONVIF protocol, the camera works only in compatibility mode; the search does not find the camera as a device that supports ONVIF.\n3. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, before using the camera, go to the web interface and select the required value.\n4. n the AxxonSoft products, the camera is identified as Yudor CO-YUC-H696RP."]
["ComOnyx","ComOnyx CO-i20HY0DNW","Camera ","V1.0.20_Y","1","2",null,null,"+",null,null,"1600x1200",null,null,"+","-","+","+","+","+","1. Поиск в AN не определяет прошивку: ее нужно выбрать самостоятельно.\n2. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.\n3. Камера определяется как Yudor CO-YUC-H696RW","1. In the AxxonSoft products, the device's firmware version cannot be identified. You must select the firmware version yourself.\n2. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, before using the camera, go to the web interface and select the required value.\n3. In the AxxonSoft products, the camera is identified as Yudor CO-YUC-H696RW."]
["ComOnyx","ComOnyx CO-i20HY0P","Camera ","V1.0.26._Y","1","2",null,null,"+",null,null,"1600x1200",null,null,"+","-","+","+","+","+","1. Поиск в AN не определяет прошивку: ее нужно выбрать самостоятельно.\n2. Прошивка V1.0.26_Y: камера работает по Onvif только в режиме совместимости, поиском как Onvif не находится.\n3. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.\n4. Камера определяется как Yudor CO-YUC-H696P","1. In the AxxonSoft products, the device's firmware version cannot be identified. You must select the firmware version yourself.\n2. The V1.0.26_Y firmware: Via the ONVIF protocol, the camera works only in compatibility mode; the search does not find the camera as a device that supports ONVIF.\n3. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, before using the camera, go to the web interface and select the required value.\n4. In the AxxonSoft products, the camera is identified as Yudor CO-YUC-H696P."]
["ComOnyx","ComOnyx CO-i20SY2IR(P/W)","Camera ","1.0.38_Y","1","2","+",null,"+",null,null,"1600x1200","+",null,"-","-",null,"+","+","motion detection.","1. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект после добавления камеры необходимо выбрать нужное значение в веб-интерфейсе.\n2. Протокол ONVIF: при переключение кодека с MJPEG на H.264 - нет видео. Проблема устройства. Чтобы получить видео необходимо выставить кодек в веб-интерфейсе и перезапустить продукт\n3. Камера определяется как Yudor YUC-H796R\n","1. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, after adding the camera, go to the web interface and select the required value.\n2. ONVIF: when you switch from MJPEG to H.264, video stream is lost. This is a problem of the camera itself. To make it work, go to the camera's web interface, select a codec and restart the VMS. In the AxxonSoft products, the camera is identified as Yudor YUC-H796R.\n"]
["ComOnyx","ComOnyx CO-i20SY2IRP(HD2)","Camera ","VC1.0.18","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+",null,"+","+","motion detection"]
["Compotrol","Compotrol IP-5130","Camera ","V3.0 110921","1","2","+","+","+",null,null,"2560x1920","+",null,"+","+","+","+","-","motion detection"]
["CP Plus","CP Plus CP-UNC-BP50C","Camera","3.000.AT00.0.R","1","2","+","-","+",null,"-","2560x1920","+",{"$nulls":3},"-",null,"-",null,"Диапазон значений битрейта зависит от значений разрешения и fps.Максимально возможное разрешение определяется текущим значением частоты кадров. При максимальных значениях частоты кадров недоступны большие разрешения. Более подробно зависимость описана в документации производителей.","Range of value ​​depends on the bit rate of the resolution and fps. The highest resolution is determines by current value of frame rate. At maximum frame rate not available high resolution. This dependence described detaily in manufacturer's documentation."]
["CP Plus ","CP Plus CP-UNC-BY20C","Camera ","3.000.AT00.0.R, build : 2013-05-13","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":7},"Диапазон допустимых значений битрейта зависит от текущего значения разрешения и fps.\nНастройку качества для ПО ITV рекомендуется производить в веб-интерфейсе камеры.","Range of available bit rate values ​​depends on current resolution and fps.\nQuality setting for AxxonSOft software recommended to select in camera's web interface."]
["CP Plus ","CP Plus CP-UNC-DP10","Camera ","3.000.AT00.0.R, build : 2013-05-13","1","2","+",null,"+",null,null,"1280x960","+",{"$nulls":7},"Диапазон значений битрейта зависит от значений разрешения и FPS. Если вводимое значение не входит в доступный диапазон, то значение не применяется.\nПри работе с камерой в ПО ITV настройку качества для кодека MJPEG рекомендуется производить в веб-интерфейсе","Range of bit rate values ​​depends on the resolution and FPS. If entered value is not included in available range, the value will not be applied.\nWhen using the camera in AxxonSoft software quality setting for MJPEG codec is recommended to select in camera's web interface."]
["CP Plus","CP Plus CP-UNC-TP10L2C","Camera","3.000.AT00.0.T, build : 2014-01-16","1","2","+",null,"+",null,null,"1280x720","+",{"$nulls":7},"Диапазон значений битрейта зависит от значений разрешения и FPS. Если вводимое значение не входит в доступный диапазон, то значение не применяется.Диапазон значений fps на втором потоке зависит от значения разрешения на первом.","Bit rate value depends on the resolution and fps. If the specified value is not included in available range, the value will not be applied. Range of fps values for the second stream depends on the value of resolution for the first stream.","new"]
["CP Plus","CP Plus CP-UNC-TP13FL2CD","Camera","3.000.AT00.0.R, build : 2013-05-13","1","2","+",null,"+",null,null,"1280x960","+",null,"-","-",null,"-","-","-","Диапазон значений битрейта зависит от значений разрешения и FPS. Если вводимое значение не входит в доступный диапазон, то значение не применяется.","Bit rate value depends on the resolution and fps. If the specified value is not included in available range, the value will not be applied. ","new"]
["CP Plus ","CP Plus CP-UNC-TY10FL5C","Camera ","3.000.AT00.0.R","1","2","+",null,"+",null,null,"1280x960 ","+"]
["CP Plus ","CP Plus CP-UNC-TY20ZL2C","Camera ","3.000.AT00.0.R","1","2","+",null,"+",null,null,"1920x1080","+"]
["CP Plus","CP Plus CP-UNC-VP13FCD / CP-UNC-VP13FL2CD","Camera","3.000.AT00.0.R, build : 2013-05-13","1","2","+",null,"+",null,null,"1280x960","+",null,"-","-",null,"-","-","-","Диапазон значений битрейта зависит от значений разрешения и FPS. Если вводимое значение не входит в доступный диапазон, то значение не применяется.","Bit rate value depends on the resolution and fps. If the specified value is not included in available range, the value will not be applied. ","new"]
["CP Plus","CP Plus CP-UNP-2020L10","Camera","3.000.AT00.0.R","1","2","+","-","+",null,"-","1920x1080","+",{"$nulls":3},"+",null,"-"]
["CP Plus","CP Plus CP-UNP-37","Camera","3.000.AT00.0.R, build 2013-04-18","1","2","+","-","+","-","-","704x576","+","-","-","-","+","-","-"]
["Dahua","Dahua IPC-HDB3200C","Camera","2.211.0000.0.R","1","2","+","-","+",null,"-","1920x1080","+",null,"-","-","-","-","-","-","Максимальное разрешение на первом потоке ограничивает выбор частоты кадров до 18 на двух потоках.Диапазон значений битрейта зависит от значений разрешения и FPS. Если вводимое значение не входит в доступный диапазон, то значение не применяется.При работе с камерой в ПО ITV настройку качества для кодека MJPEG рекомендуется производить в веб-интерфейсеПри разрешении выше 720p не поддерживается настройки зеркального отображения и поворота изображения.Настройка ТВ-стандарт не меняет формат видео. Ее значение следует выбирать в соответствии с версией модели (существуют PAL и NTSC версии).","The max. resolution settings for stream 1 limit fps settings to 18 fps for both streams. The Bit Rate range depends on the stream settings. The lower fps, resolution, key frame rate you have for the stream, the shorter is the bit rate range. In the AxxonSoft products, the bit rate span is set to max. values. With resolutions exceeding 720p, the image rotation and mirroring settings do not work. TV standart setting does not change video format. To need to change the setting in accordance with model version (there are PAL and NTSC versions)."]
["Dahua","Dahua IPC-HDBW3300 / IPC-HF3300 / IPC-HDB3300 / IPC-HFW3300(C)","Camera ","2.210.0000.0.R, build: 2013-01-25","1","2","+",null,"+",null,null,"2048x1536","+",{"$nulls":4},"-","-","-","1. Максимальное разрешение на первом потоке ограничивает выбор частоты кадров до 18 на двух потоках.\n2. Диапазон значений битрейта зависит от настроек потока. Чем меньше значения таких настроек как частота кадров, разрешение, частота опорных кадров, тем меньше диапазон битрейта. В продукте для битрейта задан диапазон от самого маленького значения до самого большого.\n3. При разрешении выше 720p не поддерживается настройки зеркального отображения и поворота изображения.\n4. Для того, чтобы у нас в продукте заработали настройки изображения, нужно в веб-интерфейсе устройства выбрать Профиль \"Day\" (Setup -> Camera -> Conditions -> Config File)\n5. Настройка качества для MJPEG производится в веб-интерфейсе","1. The max. resolution settings for stream 1 limit fps settings to 18 fps for both streams.\n2. The Bit Rate range depends on the stream settings. The lower fps, resolution, key frame rate you have for the stream, the shorter is the bit rate range. In the AxxonSoft products, the bit rate span is set to max. values.\n3. With resolutions exceeding 720p, the image rotation and mirroring settings do not work.\n4. To make video settings work, go to the camera's web interface and select the Day profile in Setup -> Camera -> Conditions -> Config File\n5. You can configure quality settings for MJPEG stream in the camera's web interface."]
["Dahua","Dahua IPC-HFW3101C","Camera ","2.103.0001.0.R","1","2","+",null,"+",null,null,"1280x960","+"]
["Dahua","Dahua IPC-HFW3200C / IPC-HDBW3200","Camera ","2.210.0000.0.R, build : 2013-03-13","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":7},"1. Для работы настроек изображения в ПО ITV | AxxonSoft необходимо в настройках камеры Camera > Conditions > Config file выбрать значение Day\n2. Значения \"поворота на 90 градусов\" настройки Поворот видеоизображения применяются только при разрешении не выше 720р. ","1. To work with image settings in Axxonsoft SW, please select Day in the camera settings (Camera > Conditions > Config file).\n2. The value of \"90 degree rotation\" is applied only if resolution is not higher than 720p. "]
["Dahua","Dahua IPC-HFW3200S","Camera ","2.103.0000.2.R, build : 2013-03-21","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":7},"1. Диапазон допустимых значений битрейта зависит от текущих значений настроек потока (частота кадров, разрешение, частота опорных кадров). В ПО ITV/Axxon интегрирован максимально возможный диапазон значений.\n2. Настройка качества для MJPEG производится в веб-интерфейсе ","1. Valid range of the bit rate depends on the current stream settings (FPS, resolution, keyframe rate). Axxonsoft software supports the maximum possible range of values. 2. To configure quality for MJPEG, please use camera web-interface."]
["Dahua","Dahua SD6582A-HN ","Camera ","2.103.0003.0.R, build : 2012-10-16","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":3},"+",{"$nulls":3},"1. Диапазон допустимых значений битрейта зависит от текущих значений настроек потока (частота кадров, разрешение, частота опорных кадров). В ПО ITV/Axxon интегрирован максимально возможный диапазон значений.\n2. Настройка качества для MJPEG производится в веб-интерфейсе ","1. Valid range of the bit rate depends on the current stream settings (FPS, resolution, keyframe rate). Axxonsoft software supports the maximum possible range of values. 2. To configure quality for MJPEG, please use camera web-interface."]
["Dahua","Dahua SD6982A-HN","Camera","2.212.0000.0.R, build : 2013-09-12","1","2","+","-","+",null,"-","1920x1080","+",{"$nulls":3},"+",null,"-","-","Диапазон допустимых значений битрейта зависит от текущего значения разрешения и fps.Значение разрешения 704x576, для второго потока, недоступно если на первом потоке стоит значение разрешения в 640x480Камера интегрирована под названием SD6XXX-HN","Bitrate value ​​depends on current resolution and fps. Resolution 704x576 for second stream is not available, at first stream adjusted resolution 640x480. Camera is integrated as SD6XXX-HN."]
["Dahua","Dahua SDZ2020B-N","Camera","2.103.0002.0.R, build : 2012-10-31","1","2","+","-","+","-","-","1920x1080","+","-","-","-","+","-","-","-","Диапазон значений битрейта зависит от значений разрешения и частоты кадров в секунду.Минимально допустимое значение частоты опорных кадров соответствует текущему значению FPS, это ограничение камеры.Настройку качества для MJPEG рекомендуется производить в веб-интерфейсе камеры.","Bitrate range depends on resolution and fps. Minimal key frame rate is equal to the current fps- it’s a camera restriction. To set the MJPEG quality, use the camera web interface."]
["Dallmeier","Dallmeier DDF3000IPV (ONVIF)","Camera ","V2.4.4","1",null,"+","+",{"$nulls":3},"720x576",{"$nulls":7},"-","\nработает только через ONVIF\n \n1) в веб-интерфейсе есть вкладки с настройками реле - физически же подключить их некуда\n \n2) настройка звука недоступна на самой камере \n \n3) чтобы камера работала через ONVIF его (т.е. ONVIF) надо активировать\n \n4) поиск через IP-Wizard не реализован - проблемы связаны с самой камерой, а не с ПО ITV\n \n\n5) mpeg2 через ONVIF не реализован","\nWorks only via the ONVIF protocol. \n \n1. The web interface has tabs with relay settings; however, you cannot connect relays physically.\n \n2. The device itself does not allow you to configure audio. \n \n3. To make the camera work via the ONVIF protocol, enable ONVIF.\n \n4. Search through IP Wizard is not implemented, because of a problem with the camera, not with the AxxonSoft software.\n \n\n5. MPEG2 via the ONVIF protocol is not implemented."]
["Dallmeier","Dallmeier MicroStreamer (ONVIF)","Camera ","V2.4.4","1",null,"+","+",{"$nulls":3},"720x576",{"$nulls":8},"\n\n\nработает только через ONVIF\n \n1) в веб-интерфейсе есть вкладки с настройками реле - физически же подключить их некуда\n \n2) настройка звука недоступна в самом устройстве \n \n3) чтобы устройство работало через ONVIF его (т.е. ONVIF) надо активировать\n \n4) поиск через IP-Wizard не реализован- проблемы связаны с самим устройством, а не с ПО ITV\n \n5) mpeg2 через ONVIF не реализован","\n\n\nWorks only via the ONVIF\n protocol.  \n1. The web interface has tabs with relay settings; however, you cannot connect relays physically.\n \n2. The device itself does not allow you to configure audio. \n \n3. To make the device work via the ONVIF protocol, enable ONVIF.\n \n4. Search through IP Wizard is not implemented, because of a problem with the device, not with the AxxonSoft software.\n \n5. MPEG2 via the ONVIF protocol is not implemented."]
["D-Link ","D-Link DCS-932L","Camera ","1.06","1","1","+",{"$nulls":4},"640x480","+",{"$nulls":7}," В ПО ITV устройство обнаруживается поиском как Trendnet DCS-932L ","In Axxonsoft SW camera is detected as Trendnet DCS-932L."]
["D-Link ","D-Link DCS-930L","Camera ","1.08","1","1","+",{"$nulls":4},"640x480","+"]
["Dynacolor","Dynacolor nZH061 -V6A (NV062)","Camera ","d20100630NS ","1","2","+",null,"+",null,null,"1920x1080","+",null,null,"-",{"$nulls":3},"-","1. Камера подключается в продуктах ITV/Axxon под \"именем\" NV062","1. In AxxonSoft products, the camera is connected as NV062"]
["Dynacolor","DynaHawk 801","Camera ","0228-0031-0263","1",null,"+","+",{"$nulls":3},"720x576",null,null,"-","-","+",null,null,"-","1. При смене потока, разрешения, качества, fps (а значит и при старте Intellect, когда все эти настройки применяются) камера на 60 сек. уходит в ребут. И в Intellect и в родном вебе.\n2. При максимальных настройках в MJPEG сама камера способна выдавать только 12 fps\n ","1. After you change the stream, resolution, quality, or frame rate (and on Intellect's startup, when all these settings are applied), the camera restarts for 60 seconds. Both in Intellect and the device's own web interface. \n2. With MJPEG and the max. settings, the camera allows 12 fps max.\n "]
["Dynacolor","DynaHawk 811","Camera ","0167-0010-0232","1",null,"+","+",{"$nulls":3},"720x576",{"$nulls":4},"+",null,null,"-","1. Видео по камере стартует не сразу, а в течении 7-10 секунд. Это связано с тем, что на камере в это время применяются \"интеллектовские\" настройки. ","1. Video does not start immediately, only after 7–10 seconds. This is because it takes time to apply Intellect's settings to the camera. "]
["Dynacolor","DynaHawk NH061","Camera ","d20100310NS","1",null,"+","+","+",null,null,"1280x960",null,null,"+.","-",null,"+","+","-"," Реле камеры по умолчанию работает в режиме \"Нормально замкнуто\". Перед работой можно изменить это через веб-интерфейс камеры.","By default, the camera relay works in Normally Closed mode. Before using the relay, change this in the camera's web interface. "]
["Dynacolor","DynaHawk nZH060","Camera ","d20081226NS","1","2","+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4)",null,null,"+","-",null,"+","+","-","В MJPEG в максимальном разрешении 1280x960 максимальная частота кадров - 15 fps.При одновременном использовании нескольких видеопотоков доступные разрешения в них взаимозависимы. Необходимо вручную контролировать эту зависимость в нашем ПО. Подробнее о взаимосвязи потоков можно узнать в инструкции к камере.","With MJPEG and the max. resolution (1280x960), the max. frame rate is 15 fps. When multiple video streams are used simultaneously, their available resolutions are interrelated. In our software, you must manage this interrelation manually. For more details on how the streams are interrelated, refer to the camera's guide. "]
["EasyN","EasyN F-series","Camera ","4.37.2.38","1","1","+",{"$nulls":4},"640x480","+",null,"-","-","+","+.","+","+","1. Камеры EasyN FM166I, FS-613A-M136 интегрированы как линейка EasyN F-series, весь линейный ряд не тестировался.\n2. Тревога от встроенного детектора длится ровно минуту независимо от фактической продолжительности события - особенность камеры.\n3. Макс fsp: 640x480 - 15 fps | 320x240 - 20 fps | 160x120 - 30 fps ","1. Camera EasyN FM166I has been integrated as , EasyN F-series, although the other models from the range have not been tested yet.\n2. The alarms from embedded detection go off and remain active for 60 seconds sharp, regardless of the actual duration of an alarm event. This is a limitation of the camera.\n3. Max fps: 640x480 - 15 fps | 320x240 - 20 fps | 160x120 - 30 fps "]
["EasyN","EasyN HV10DI","Camera ","V3.4.6.1.1-20111227","1","1",null,null,"+",null,null,"1280x720","+.",null,"+.","-","+","+","-","motion detection.","Поиском камера обнаруживается как \"EasyN ZNY10.22\" ","The device is identified as EasyN ZNY10.22. "]
["Eneo","Eneo GXB-1710M-IR","Camera ","2.07","1","3","+","+","+",null,null,"1920x1080","+",null,null,"-",{"$nulls":4},"Есть проблема с применением разрешений (при переходе к более высокому разрешению видео может не измениться), проблема производителя","There is an issue with higher resolutions. When you set one, video may stay the same. This is a problem of the camera itself."]
["Eneo","Eneo GXB-1720MIR / Eneo GXD-1720MIR","Camera","1.22","1","3","+","+","+",null,null,"from WEB","+",null,"-","-","-","-","-","-",null,null,"new"]
["Eneo","Eneo NLD-1422","Camera ","2.9.5-T1_release","1","2","+","+","+",null,null,"704x576","+",null,null,"-","+"]
["Eneo","Eneo NXC-1403F03 ","Camera ","1.7.0-T5_release","1","3","+","+","+",null,null,"1600x1200","+",null,"-","-","-","-","-","-"]
["Eneo","Eneo NXC-1602M","Camera ","2.2.107","1","4","+",null,"+",null,null,"1920x1080(H264) / 720x576(MJPEG)","+",null,null,"-"]
["Eneo","Eneo PXB-2020M-IR","Camera ","4.17-72-fs","1","2","+",null,"+",null,null,"1280x720","+",{"$nulls":6},"-"]
["Eneo","Eneo PXD-1010F02 / PXD-1020F02 ","Camera ","vr20130122NSA ","1","2","+",null,"+",null,null,"1920x1080 ","+",null,"-","-","-","-","-","motion detection.","1) Разрешение на втором потоке не может быть больше, чем на первом.","The resolution for stream 2 should be lower than or equal to the resolution setting for stream 1."]
["Eneo","Eneo PXD-2018PTZ1080","Camera ","vr20121016NSA ","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":3},"+",null,null,"motion detection."]
["Eneo","Eneo PXD-5360F01IR / PXD-5362F01IR ","Fisheye Camera","vr20130515NSA ","1","2","+",null,"+",null,null,"H.264: 2592x1944; MJPEG: 1920x1080","+",{"$nulls":7},"1. Значения \"Поворот на 90° по часовой стрелки\" и \"Поворот на 90° против часовой стрелки\" настройки Тип отображения не работают при разрешении CIF (352x288)\n2. Значения настроек \"Алгоритм компрессии\", \"Аудиокодек\" и \"Битрейт\" для объектов \"Микрофон\" и \"Динамик\" должны совпадать для корректной работы обоих объектов в ПО Axxon.\n","1. \"90 ° clockwise rotation\"and \"90 ° counter-clockwise rotation\" (Type of mapping) doesn't work for 352x288 resolution. 2. The setting values of \"Compression algorithm \", \" Audio Codec \" and \" Bitrate \" for Microphone and Speaker must be the same for the correct operation of both objects in Axxon software ."]
["Etrovision","Etrovision EV3151A","Camera ","1.9.9","1","2","+","+.","+",null,null,"720x576",null,null,"+","-","-","+","+","-","1. Само устройство с прошивкой 1.9.9 в разрешении 720x576 выдает MPEG-4 видео с \"плавающим\" fps.\n2. Телеметрию можно настроить только в ПО Intellect (протокол телеметрии IPCamera)","1. 1.9.9 firmware: At 720x576 resolution and MPEG-4, the device sends video with a variable frame rate. \n2. Telemetry can be configured only in Intellect (the IPCamera protocol)."]
["Etrovision","Etrovision EV8150A","Camera ","2.0.3 Build 20110513","1","2","+","+","+",null,null,"1280x1024",null,null,"+","-","+","+","+","-","1. Само устройство с прошивкой 1.9.9 в мегапиксельном разрешении ввыдает искаженное H.264 видео\n\n ","1. 1.9.9 firmware: With megapixel resolutions and H.264, the device sends distorted video.\n\n "]
["Etrovision","Etrovision EV8x8xA","Camera ","1.1.2","1","2","+","+","+",null,null,"1280x1024","+",null,"+.","-","-","+","+","+"]
["Etrovision","Etrovision EV8x8xF","Camera ","1.1.2","1","2","+","+","+",null,null,"2592x1920(MJPEG, H.264); 1920x1080(MPEG-4)","+",null,"+.","-","-","+","+","+","1. В ПО Axxon под разрешениями 5МР, 3МР и 1080р в кодеке MPEG-4 подразумевается одно и то же фактическое разрешение 1920х1080.\n2. Максимальный fps зависит от значения настройки \"Max. Resolution\" в веб-интерфейсе ","1. In the AxxonSoft software, with the MPEG-4 codec, the 5MP, 3MP, and 1080p resolutions all mean the same actual resolution of 1920x1080. \n2. The max. resolution depends on Max. Resolution settings in web interface.\n"]
["Etrovision","Etrovision EV8x8xQ","Camera ","1.1.2","1","2","+","+","+",null,null,"2048x1536 (H264/MJPEG) / 1920x1080 (MPEG4)","+",null,"+.","-","-","+","+","+"]
["Etrovision","Etrovision EV8x8xU","Camera ","1.1.2","1","2","+","+","+",null,null,"1920x1080","+",null,"+.","-","-","+","+","+","1. Детектор движения работает только с кодеком h264 и только в 0-м потоке (В Интеллекте нужно выбирать высокое и полное разрешения). Проблема связана с особенностями устройства, подтверждена производителем.\n2. В Интеллекте в стандартном разрешении максимальная частота кадров - 20 fps (PAL) / 25 fps (NTSC)\n3. Применение настроек происходит с задержкой и сопровождается разрывом соединения.\n4. 30 fps в NTSC можно получить с устройства только в однопоточном режиме (в Интеллекте (только с высоким и полным разрешением) для этого нужно отключить второй поток через веб-интерфейс).","1. Motion detector works only with the h264 codec and only in 0 stream (In Intellect it's necessary to choose high and full resolutions). The problem is connected with features of the device, confirmed by the producer.\n2. In Intellect in standard resolution the maximum frame rate is 20 fps (PAL)/25 fps (NTSC)\n3. Application of settings occurs to a delay and is accompanied by a rupture of connection.\n4. 30 fps in NTSC can be received from the device only in one-stream mode (disconnect the second stream via the web interface in Intellect (only with high and full resolution)).\n"]
["Euresys","Euresys Picolo .net HD4 IP Video Encoder (ONVIF)","Encoder ","4.0","4","1","+",null,"+",null,null,"1920x1080"]
["EverFocus","EverFocus EAN3120 (Onvif)","Camera ","1.0.17","1","1","+",null,"+",null,null,"1280x1024 (MJPEG) / 720x576 (H264)","+",null,"+.","-",null,"-","+","motion detection.","Камера интегрирована только по протоколу Onvif.\nЧтобы получать видео в формате H264 с такими же разрешениями, как и MJPEG, нужно в веб-интерфейсе для первого потока выбрать кодек H264.","The camera is integrated only according to the Onvif protocol. \nTo receive video in the H264 format with the same permissions, as well as MJPEG, it is necessary in the web interface for the first flow to select the H264 codec"]
["EverFocus","EverFocus EAN3220 (Onvif)","Camera ","1.0.17","1","1","+",null,"+",null,null,"1920x1080 (MJPEG) / 720x576 (H264)","+",null,"+.","-",null,"-","+","motion detection.","Камера интегрирована только по протоколу Onvif.\nЧтобы получать видео в формате H264 с такими же разрешениями, как и MJPEG, нужно в веб-интерфейсе для первого потока выбрать кодек H264.","The camera is integrated only according to the Onvif protocol. \nTo receive video in the H264 format with the same permissions, as well as MJPEG, it is necessary in the web interface for the first flow to select the H264 codec"]
["EverFocus","EverFocus EAN850A","Camera ","1.2.5","1","4","+","+","+",null,null,"704x560",null,null,"-","-",null,"+","+","-","1. При активации одновременно 3-4 стриммингов видео с камеры может пропадать. Особенность интеграции. Исправляется отключением \"лишних\" стриммингов в веб-интерфейсе камеры","1. If 3–4 streams are enabled at the same time, video may disappear. This is how integration was done. To correct this, go to the camera's web interface and disable \"extra\" streams."]
["EverFocus","EverFocus EDN2245H","Camera ","ev20120220BNS","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+.",null,"+","+","motion detection"]
["EverFocus","EverFocus EDN800","Camera ","1.1.0","1","4","+","+","+",null,null,"704x576",{"$nulls":7},"-"]
["EverFocus","Everfocus EPN4122 / EPN4220 / EPN4220i (PSIA) ","Camera ","1.0.3","1","2","+",null,"+",null,null,"from WEB ","+",null,"+"]
["EverFocus","EverFocus EVS200 encoder","Encoder ","1.0.6","2","2","+","+","+",null,null,"704x576(H.264) / 352x288 (MJPEG) / 352x288 (MPEG-4)","+",null,"-","-","-","+","+","-","1. 2 канала, на каждом по 2 стримминга\n2. телеметрия может быть реализована только в ПО Intellect, и не может быть реализована в ПО Axxon Next. Чтобы она заработала, необходимо в веб-интерфейсе выставить нужный протокол+скорость, затем то же самое установить в Intellect.","1. 2 channels, each has 2 streams.\n2. Telemetry may be used only in Intellect, not in Axxon Next. To make it work, go to the web interface and set the required protocol and baud rate; then go to Intellect and set the same there. "]
["EverFocus","EverFocus EZN3260 (Onvif)","Camera ","1.0.17","1","1","+",null,"+",null,null,"1920x1080 (MJPEG) / 720x576 (H264)","+",null,"+.","-","-","-","+","-","Камера интегрирована только по протоколу Onvif. \nЧтобы получать видео в формате H264 с такими же разрешениями, как и MJPEG, нужно в веб-интерфейсе для первого потока выбрать кодек H264.","The camera is integrated only according to the Onvif protocol. \nTo receive video in the H264 format with the same permissions, as well as MJPEG, it is necessary in the web interface for the first flow to select the H264 codec"]
["EverFocus","Everfocus EZN3260 / EDN3260 / EHN3260 (PSIA)","Camera ","1.0.17","1","2","+",null,"+",null,null,"from WEB ","+",null,"+"]
["eVidence","eVidence Apix - 10ZBox / M1","Camera ","p20101125NS","1","3","+","+","+",null,null,"1280x960","+",null,"+.","-","+","+","+","+","В максимальном разрешении (1280x960) максимальная частота кадров - 12.5 fps.Черезх Onvif работает получение видео с настройками качества и разрешения и звук.Телеметрия: камера не поворотная, но с трансфокальным фокусным объективом. Зум и фокус в нашем ПО поддержаны.Доступны следующие комбинации кодеков и разрешений в потоках:0.MJPEG + 1.MPEG4/H264MJPEG + MPEG4MJPEG + H264При выборе максимального разрешения 1280х960 необходимо выбирать его в обоих потоках.1.MPEG4/H264 + 2.H264-2H264 + H264-2Разрешение 1280х720 в кодеке H264-2 доступно только в том случае, если в кодеке H264 также выбрано разрешение 1280х720.","At maximum resolution (1280x960), the max. frame rate is 12.5 fps. Via the ONVIF protocol, the following work: receiving video, setting the quality and resolution, and receiving audio Telemetry: this is not a PTZ camera, but it has a zoom lens. Our software supports zoom and focus. The available combinations of codecs and resolutions are: 0. MJPEG + 1. MPEG4/H264MJPEG + MPEG4MJPEG + H264. To select the max. resolution (1280x960), you must select it in both streams. 1. MPEG4/H264 + 2. H264-2H264 + H264-2. For the H.264-2 codec, 1280х720 resolution is available only if the same resolution is selected for the H.264 codec."]
["eVidence","eVidence Apix - 12ZDome / D1","Camera ","p20110825NS","1","2","+",null,"+",null,null,"720x576","+",null,"+","-","+","+","+",null,"На камере есть 4 луча и 1 реле. Однако в комплекте с тестовым устройством был кабель, не имеющий тревожных входов/выходов. В инструкции к камере сказано, что кабель с тревожными разъемами идет только в комплекте с \"Outdoor Dome Camera\" - видимо, имеется ввиду модель с индексом \"EXT\". Хотя лучи и реле есть у обеих моделей. Проверка работы тревожных входов и выходов производилась с помощью ручного подключения обычных проводов к нужным разъемам.В Интеллекте не работает изменение частоты кадров в минимальном разрешении 352х288 в кодеке H264 - особенность камеры.В Интеллекте минимальное и среднее значение частоты кадров совпадают - особенность интеграции.","The camera has 4 sensors and 1 relay. However, the trial device came with a cable that had no alarm input/output ports. The camera's guide says that the cable with alarm connectors comes only with the Outdoor Dome Camera: they most likely mean the model whose name contains the string \"EXT\", although both models have sensors and relays. The alarm inputs/outputs were tested by manually connecting ordinary cables to the right connectors. In Intellect, with the min. resolution (352x288) and H.264 codec, frame rate control does not work. This is a limitation of the camera itself. In Intellect, the min. and medium frame rates are the same: this is how the integration was done. "]
["eVidence","eVidence Apix - 18ZBox / M2","Camera ","d20110729NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"-","-","+","-","-","-"]
["eVidence","eVidence Apix - 18ZDome / M2","Camera ","st20120217NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"-","-","+","-","-","-"]
["eVidence","eVidence Apix - 18ZDome / M2-ext","Camera ","st20130924NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","-","+","+","+","motion detection."]
["eVidence","eVidence Apix - 20ZDome / M2-ext","Camera","st20130610NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","-","+","+","+","motion detection",null,null,"new"]
["eVidence","eVidence Apix - 36ZDome / D1 ","Camera ","p20110825NS","1","2","+",null,"+",null,null,"720x576","+",null,"+","-","+","+","+",null,"На камере есть 4 луча и 1 реле. Однако в комплекте с тестовым устройством был кабель, не имеющий тревожных входов/выходов. В инструкции к камере сказано, что кабель с тревожными разъемами идет только в комплекте с \"Outdoor Dome Camera\" - видимо, имеется ввиду модель с индексом \"EXT\". Хотя лучи и реле есть у обеих моделей. Проверка работы тревожных входов и выходов производилась с помощью ручного подключения обычных проводов к нужным разъемам.В Интеллекте не работает изменение частоты кадров в минимальном разрешении 352х288 в кодеке H264 - особенность камеры.В Интеллекте минимальное и среднее значение частоты кадров совпадают - особенность интеграции. ","The camera has 4 sensors and 1 relay. However, the trial device came with a cable that had no alarm input/output ports. The camera's guide says that the cable with alarm connectors comes only with the Outdoor Dome Camera: they most likely mean the model whose name contains the string \"EXT\", although both models have sensors and relays. The alarm inputs/outputs were tested by manually connecting ordinary cables to the right connectors. In Intellect, with the min. resolution (352x288) and H.264 codec, frame rate control does not work. This is a limitation of the camera itself. In Intellect, the min. and medium frame rates are the same: this is how the integration was done. "]
["eVidence","eVidence Apix - Box / M1","Camera ","p20100310NS ","1","2","+","+","+",null,null,"1280x960 (look note)","+",null,"+","-",null,"+","+","-","1. Поиск находит камеру как Dynacolor NH061\n2. Во время получения видео с обоих видеопотоков доступны следующие комбинации кодеков:\nMJPEG + H264\nMJPEG + MPEG4\nH264 + H264-2\n3. Для получения видео с обоих видеопотоков действуют следующие ограничения:\n- Различные разрешения в потоках поддерживаются только при комбинации H264 + H264-2. \n- В остальных комбинациях разрешение будет одинаковым для обоих потоков и задает оно из второго потока.\n- Для кодека H264-2 постоянно недоступно максимальное разрешение 1280х960, а разрешение 1280х720 доступно только в том случае, когда для кодека H264 в этот момент выставлено это же разрешение 1280х720.\n4. Реле камеры по-умолчанию работает в режиме \"нормально-замкнуто\". Особенность устройства, при необходимости можно изменить через web-интерфейс.","1. Search detects the camera as Dynacolor NH061. \n2. When you use both streams, the following codec combinations are available: \nMJPEG + H264\nMJPEG + MPEG4\nH264 + H264-2. \n3. When you use both streams, the following limitations apply: \n- Different resolutions for the streams are supported only for the H264 + H264-2 combination. \n- For all the other combinations, the resolutions will be the same for both streams; to set this common resolution, set the resolution for the second stream. \n- For the H264-2 codec, the max. resolution (1280x960) is never available, and the 1280x720 resolution is available for this codec only when the same resolution (1280x720) is set for the H264 codec. \n4. By default, the camera's relay works in Normally Closed mode. This is a feature of the device; if necessary, you can change it in the web interface. "]
["eVidence","eVidence Apix - Box / M2","Camera ","p20110824BNS","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","-",null,"+","+","+","В максимальном разрешении 1920х1080 максимальная частота кадров 12.5 fpsПри одновременном использовании 2х потоков доступны следующие комбинации:H264 (1280x720) + MJPEG (352x288, 720x576)H264 (1280x720) + H264-2 (352x288, 720x576)","At maximum resolution (1280x1080), the max. frame rate is 12.5 fps. When you use two streams at the same time, the following combinations are available: H264 (1280x720) + MJPEG (352x288, 720x576) H264 (1280x720) + H264-2 (352x288, 720x576)"]
["eVidence","eVidence Apix - Box / M2 Lite","Camera ","st20130924NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"+",null,null,"+","+","motion detection."]
["eVidence","eVidence Apix - Box / M2 WDR","Camera","st20131230NSX","1","2","+","-","+","-","-","1920x1080 (H.264) / 1280x1024 (MJPEG)","+","-","+","+","-","+","+","motion detection","Доступность настроек экспозиции зависит от текущего значения настройки TV System (интегрирована в ПО Axxon как \"ТВ-стандарт\").При изменении TV System настройки видео на камере сбрасываются на дефолтные (особенность камеры). Поэтому для корректной работы камеры после смены ТВ-стандарта требуется через веб-интерфейс привести настройки видео (кодек, разрешение) в соответствие с текущими настройками в ПО Axxon.","Availability of exposure settings depends on the current value of the TV System setting (integrated in Axxon as TV standard). When the TV System setting is changed, settings of camera video become default (camera’s feature). For proper camera operation after changing the TV standard setting, video settings (codec, resolution) are to be in accordance with current settings in Axxon."]
["eVidence","eVidence Apix - Box / M3","Camera ","st20130129NSA","1","2","+",null,"+",null,null,"1920x1080 (MJPEG) / 2048x1536 (H.264)","+",null,"+","+.",null,"+","+","motion detection.","Функционал: лучи, реле, аудиовход, аудиовыход в ПО Интеллект необходимо добавлять вручную.","You need to add ray, reley, audio input and audio output manually in AxxonSoft Software."]
["eVidence","eVidence Apix - Box / M5","Camera ","st20120217NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"-","-",null,"-","-","-"]
["eVidence","eVidence APIX Bullet / E2","Camera","t1.8.1001.67.0.8","1","2","-",null,"+",null,null,"1920x1080","+",null,"+","-",{"$nulls":3},"-","Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.Диапазон битрейта на первом потоке зависит от значения разрешения.","To connect to camera in Axxon software, please specify 30001 port. Bit rate range on the stream 1 depends on the resolution.","new"]
["eVidence","eVidence Apix - Bullet / M2","Camera ","p20120308BNS","1","2","+",null,"+",null,null,"1920x1080","+",null,"-","-",null,"-","-","-","1. В Интеллекте при смене грабера с H.264 на MJPEG (стандартное разрешение, настройка цвет выключено, первое подключение к устройству - черно-белое изображение) - цвет меняться не будет","1. In Intellect, if you change the grabber from H.264 to MJPEG (standard resolution, color off, first connection to device is black and white) - the color will not change."]
["eVidence","eVidence Apix - Bullet / M2 279","Camera ","st20121122NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+",null,"+","+","motion detection"]
["eVidence","eVidence Apix - Bullet / M2 Lite","Camera ","st20130129NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","-",null,"+","+","motion detection"]
["eVidence","eVidence Apix - Bullet / M2 Lite 279","Camera ","st20120713NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+",null,"+","+","motion detection"]
["eVidence","eVidence Apix - Compact / M1","Camera ","VB1.0.26_ST","1","2","+","+","+",null,null,"1280x800","+",null,"+.","+.",null,"+","+","motion detection","1. Картинка на камере периодически замирает на несколько секунд при физическом воздействии (тряска). В веб интерфейсе наблюдается тот же эффект.\n2. В ПО Axxon камера обнаруживается поиском как Apix-Dome/M2 Lite.\n3. В ПО ITV камера обнаруживается поиском как FineCCTV.","1. When you subject the camera to physical impact, i.e. you shake it, video may freeze for a few seconds. The same happens in the web interface.\n2. In the AxxonSoft products, the camera is identified as Apix-Dome/M2 Lite.\n3. In the AxxonSoft products, the camera is identified as FineCCTV."]
["eVidence","eVidence Apix - Dome/ E2 309","Camera","VC1.0.14_ST","1","2","+","-","+","-","-","1920x1080","+","-","+","+","-","+","+","motion detection","Диапазон значений битрейта зависит от значения FPS","Bitrate range depends on FPS."]
["eVidence","eVidence Apix - Dome/ E2 LED 309","Camera","VC1.0.14_ST","1","2","+","-","+","-","-","1920x1080","+","-","+","+","-","+","+","motion detection","Диапазон значений битрейта зависит от значения FPS","Bitrate range depends on FPS."]
["eVidence","eVidence Apix - Dome / M2 LED","Camera ","V1.0.16_ST","1","2","+",null,"+",null,null,"1600x1200","+",null,"+","-",null,"+","+","-","В Интеллекте поиск находит камеру как FineCCTV IPCam.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров) - в веб-интерфейсе называется \"Input resolution\". В Axxon Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе. ","In Intellect, search detects the camera as FineCCTV IPCam. The camera has the Video Parameters option (max. resolution and max. frame rate); in the web interface, this is called Input Resolution. In Axxon Next, you must make sure that there is no conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value. "]
["eVidence","eVidence Apix - Dome / M2 Lite","Camera ","V1.0.26_ST","1","2","+",null,"+",null,null,"1600x1200","+",null,"+","-",null,"+","+","+","В Интеллекте поиск находит камеру как FineCCTV IPCam.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров) - в веб-интерфейсе называется \"Input resolution\". В Axxon Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе","In Intellect, search detects the camera as FineCCTV IPCam. The camera has the Video Parameters option (max. resolution and max. frame rate); in the web interface, this is called Input Resolution. In Axxon Next, you must make sure that there is no conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value."]
["eVidence","eVidence Apix - MiniDome / M143","Camera ","p20110816ANS","1","2","+",null,"+",null,null,"1280x1024","+",null,"+",{"$nulls":4},"+","При одновременном использовании 2х потоков доступны следующие комбинации:H264 (1280x720) + MJPEG (352x288, 720x576)H264 (1280x720) + H264(352x288, 720x576)","When you use two streams at the same time, the following combinations are available: H264 (1280x720) + MJPEG (352x288, 720x576) H264 (1280x720) + H264-2 (352x288, 720x576)"]
["eVidence","eVidence Apix - MiniDome / M2 Lite 40","Camera ","st20120910NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"+",{"$nulls":4},"motion detection","В максимальном разрешении (1920х1080) максимальная частота кадров 12 fpsДоступны следующие комбинации кодеков и разрешений в потоках:0.H264 (1280x720) + 1.MJPEG (320x240...1280x720)0.H264 (1280x720) + 2.H264-2","At maximum resolution (1920x1080), the max. frame rate is 12 fps. The available combinations of codecs and resolutions are: 0. H264 (1280x720) + 1. MJPEG (320x240...1280x720) 0.H264 (1280x720) + 2. H264-2."]
["eVidence","eVidence Apix - VDome / M1","Camera ","p20100310NS","1","2","+","+","+",null,null,"1280x960 (look note)","+",null,"+","-",null,"+","+","-","Поиск находит камеру как InMotion HD-WDRВо время получения видео с обоих видеопотоков доступны следующие комбинации кодеков:MJPEG + H264MJPEG + MPEG4H264 + H264-2Для получения видео с обоих видеопотоков действуют следующие ограничения:Различные разрешения в потоках поддерживаются только при комбинации H264 + H264-2.В остальных комбинациях разрешение будет одинаковым для обоих потоков и задает оно из второго потока.Для кодека H264-2 постоянно недоступно максимальное разрешение 1280х960, а разрешение 1280х720 доступно только в том случае, когда для кодека H264 в этот момент выставлено это же разрешение 1280х720.Реле камеры по-умолчанию работает в режиме \"нормально-замкнуто\". Особенность устройства, при необходимости можно изменить через web-интерфейс.","Search detects the camera as InMotion HD-WDR. When you use both streams, the following codec combinations are available: MJPEG + H264MJPEG + MPEG4H264 + H264-2. When you use both streams, the following limitations apply: Different resolutions for the streams are supported only for the H264 + H264-2 combination. For all the other combinations, the resolutions will be the same for both streams; to set this common resolution, set the resolution for the second stream. For the H264-2 codec, the max. resolution (1280x960) is never available, and the 1280x720 resolution is available for this codec only when the same resolution (1280x720) is set for the H264 codec. By default, the camera's relay works in Normally Closed mode. This is a feature of the device; if necessary, you can change it in the web interface."]
["eVidence","eVidence Apix - VDome / M1 EXT 3312","Camera ","p20110824NS","1","3","+","+","+",null,null,"1280x960","+",null,"+","-",null,"+","+","+","Доступны следующие комбинации кодеков и разрешений в потоках:0.MJPEG + 1.MPEG4/H264MJPEG + MPEG4MJPEG + H264При выборе максимального разрешения 1280х960 необходимо выбирать его в обоих потоках.1.MPEG4/H264 + 2.H264-2H264 + H264-2Разрешение 1280х720 в кодеке H264-2 доступно только в том случае, если в кодеке H264 также выбрано разрешение 1280х720.Ограничение частоты кадров в 12.5 fps:Во всех кодеках в максимальном разрешении1280х960В потоке H264-2 в разрешении 1280х720В потоке H264 в разрешении 1280х720 при использовании одновременно H264+H264-2","The available combinations of codecs and resolutions are: 0. MJPEG + 1. MPEG4/H264MJPEG + MPEG4MJPEG + H264. To select the max. resolution (1280x960), you must select it in both streams. 1. MPEG4/H264 + 2. H264-2H264 + H264-2 For the H.264-2 codec, 1280х720 resolution is available only if the same resolution is selected for the H.264 codec. The frame rate is limited to 12.5 fps for all codecs, at max. resolution (1280х960) For the H.264-2 codec, at 1280x720 resolution For the H.264 codec, at 1280x720 resolution when you use H.264 and H.264-2 at the same time"]
["eVidence","eVidence Apix - VDome / M2 LED","Camera ","p20110121BNS","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","-",null,"+","+","+","В MJPEG в разрешении 1920х1080 максимальная частота кадров ~15 fpsЧерез Onvif работает поиск, видео с настройками и звук.Видеопотоки сильно зависят друг от друга. Правильную комбинацию потоков/кодеков/разрешений нужно выбирать самостоятельно.Таблица комбинаций потоков в Axxon Next: \nКодек в 1-м потоке\nКодек во 2-м потоке\nДоступные разрешения в 1-м потоке\nДоступные разрешения во 2-м потоке\nMJPEG\n-\n320x240...1920x1080\n-\n\nMJPEG\nH.264\n320x240...1280x720\n1280x720\n\nMJPEG\nH.264-2\n-\n-\nH.264\n-\n\n320x240...1920x1080\n-\n\nH.264\nH.264\n-\n-\n\nH.264\nH.264-2\n1280x720\n320x240...720x576\n-\nH.264\n-\n1280x720 - H.264-2 -\n320x240...720x576","With MJPEG and the maximum resolution (1920x1080), the max. frame rate is around 15 fps. Via the ONVIF protocol the following work: search, video (+ settings), and audio. Video streams are very interdependent. You have to select the right combination of streams/codecs/resolutions yourself. The stream combination table for Axxon Next: \nCodec (1st stream)\nCodec (2nd stream)\nResolutions available (1st stream)\nResolutions available (2nd stream)\nMJPEG\n-\n320x240...1920x1080\n-\n\nMJPEG\nH.264\n320x240...1280x720\n1280x720\n\nMJPEG\nH.264-2\n-\n-\nH.264\n-\n\n320x240...1920x1080\n-\n\nH.264\nH.264\n-\n-\n\nH.264\nH.264-2\n1280x720\n320x240...720x576\n-\nH.264\n-\n1280x720 - H.264-2 -\n320x240...720x576"]
["eVidence","eVidence Apix - ViCoder","Encoder ","p20110704NS","1","2","+",null,"+",null,null,"PAL: 720x576 | NTSC: 720x480","+",null,"-","-","-","-","-","-","1. Разрешения и свето-передача зависят от ТВ-стандарта подключенной аналоговой камеры (нужно перезагрузить устройство, чтобы оно переменило ТВ-стандарт).","1. Resolutions and color rendering depend on the TV standard of the analog camera connected. Restart the device to switch the TV standard.\n"]
["EVS","EVS VEC-255-IP / VEN-255-IP","Camera","5.00.00.08.2.1","1","3","+","+","+",null,"-","1600x1200(MJPEG/H264) / 1280x960(MPEG4)","+",null,"-","-","-","-","-",null,"С комбинацией разрешений D1:D1 может не идти видео","With a combination of permissions D1: D1 may not be video"]
["EVS","EVS VEC-355-IP / VEN-355-IP","Camera","5.00.00.08.3.1","1","3","+","+","+",null,"-","2048x1536(MJPEG/H264) / 1280x960(MPEG4)","+",null,"-","-","-","-","-"]
["EVS","EVS VEC-555-IP / VEN-555-IP","Camera","5.00.00.08.5.1","1","3","+","+","+",null,"-","From Web(MJPEG) / 2592x1920(H264) / 1280x960(MPEG4)","+",null,"-","-","-","-","-",null,"Прошивка 5.00.00.08.5.1: передача видео в MJPEG с разрешением 5 MP не поддерживается камерой.С комбинацией разрешений D1:D1 может не идти видео","Firmware 5.00.00.08.5.1: camera with MJPEG codec and resolution 5MP doesn't transmit video. With a combination permits D1: D1 may not be video."]
["FineCCTV","FineCCTV CDV-3V930HU","Camera ","3.2.62","1","1","+","+",{"$nulls":3},"720x576",{"$nulls":5},"-"]
["FineCCTV","FineCCTV CDV-3VM501 ","Camera ","V1.0.40_F","1","2","+",null,"+",null,null,"1600x1200","+",{"$nulls":6},"motion detection"]
["FlexWatch","FlexWatch FW-1178-PE ","Camera ","4.10-06","1","2","+",null,"+",null,null,"720x576",null,null,"-","-","-","-","-","-","1. C текущей прошивкой 4.10-06 Зум и Фокус очень чувствительные на самом устройстве и меняются очень значительно даже при однократном нажатии на кнопки/рычажки органов управления.","1. With the current (4.10-06) firmware, zoom and focus are very sensitive on the device itself: their values change very significantly even if you click the relevant button only once. "]
["FlexWatch","FlexWatch FW-117x-Dx","Camera ","4.18-B1-ds","1","2","+",null,"+",null,null,"720x480","+",null,null,"-","-",null,null,"-"]
["FlexWatch","FlexWatch FW-117x-Fx","Camera","4.18-B1-ds","1","2","+","-","+","-","-","1920x1080","+","-","-","-","-","-","-","-"]
["FlexWatch","FlexWatch FW117x-Mx","Camera ","4.18-B1-ds ","1","2","+",null,"+",null,null,"1280x1024","+",null,null,"-",{"$nulls":3},"-"]
["FlexWatch","FlexWatch FW-3470 (NVR)","NVR","4.06-04","4","1",null,null,"+",null,null,"704x576",{"$nulls":7},"-","Настройки кодека, разрешения, частоты кадров в Axxon Next применяются для всех каналов сразу.","In Axxon Next, the codec, resolution, and frame rate settings are applied for all the channels at once. "]
["FlexWatch","FlexWatch FW-5071 (NVR)","NVR","4.10","16","1","+","+","+",null,null,"auto",null,null,"-",null,"-","-","-",null,"Интегрировано только получение видеоПоиск находит устройство в сети, но правильную прошивку нужно выбрать самостоятельно.","Only video receipt is integrated. Search detects the device on the network, but you have to select the right firmware yourself."]
["FlexWatch","FlexWatch FW-5470C (NVR)","NVR","4.06-04","4",null,"+.","-","+",null,"-","704x576","-",null,"-","-","+","+","+","-","\n1. В ПО ITV реализована только подержка аналоговых камер (4 канала), подключаемых к устройству.\n2. Телеметрия настраивается и работает в ПО ITV через \"протокол\" IPCamera"]
["FlexWatch","FlexWatch FW-5870C (NVR)","NVR","4.07-17","8",{"$nulls":3},"+",null,null,"704x576",null,null,"-","-","+","+","+","-","1. В ПО ITV реализована только подержка аналоговых камер (8 каналов), подключаемых к устройству.\n2. Телеметрия настраивается и работает в ПО ITV через \"протокол\" IPCamera\n3. *использование устройства в Intellect 4.7.8.release не предусмотрено* ","1. The AxxonSoft software implements only support for analog cameras (8 channels) connected to the device. \n2. The telemetry functionality can be configured and used only via the IPCamera \"protocol\".\n3. *in the Intellect 4.7.8 release, the device is not used* "]
["G4S","G4S GIU03-VIR","Camera ","1.0/1.0.0","1","1","-",null,"+",null,null,"from WEB","-",null,"+.","-",{"$nulls":3},"-","Для получения видео в продукте нужно указать порт \"Watch\" из настроек в веб-интерфейсе","Select the Watch port in the camera's web interface."]
["Ganz","Ganz MP2DN","Camera ","65140","1",{"$nulls":3},"+",null,null,"1600x1200",{"$nulls":5},"-","+","-","1. ограничение fps самой камеры:\n MJPEG:\n -при 1600х1200 fps=12-20 (в зависимости от качества)\n -при 800x600 fps =~22\n H.264\n - при любом разрешении fps=~23","1. The camera itself has frame rate limits:\n MJPEG:\n -at 1600х1200, fps=12–20 (depending on quality)\n -at 800x600, fps = around 22\n H.264\n - at any resolution, fps= around 23"]
["Ganz","Ganz ZN-B1MAP","Camera ","ZN2C0.2.1917.32","1","2","+",null,"+",null,null,"1280x1024(H264) / 704x576 (MJPEG)","+",null,"+","+","+","+",null,"motion detection"]
["Ganz","Ganz ZN-D1MTP / ZN-D1MTP-IR / ZN-DT1MTP / ZN-DT1MTP-IR / ZN-B1MTP","Camera","ZN3C0.2.1320.32","1","2","+",null,"+",null,null,"1280x1024","+",null,"+","-","+","+","+","-","Камера не поворотная, но есть встроенный трансфокатор.Разрешения  меняются для обоих потоков одновременно - особенность камеры. В ASIP записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")На камере нельзя выставить на обоих потоках одновременно кодек mjpegВ ПО ITV при добавлении камеры вручную тип граббера следует выбирать Ganz-s","This is not a PTZ camera, but it has a built-in zoom lens. Resolutions are changed for both streams at the same time - the camera feature. In ASIP, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\" : \"resolution, stream 2\"). MJPEG codec can't be selected for both streams at the same time. In Axxon software when you add a camera manually, select the Ganz-s grabber type.","new"]
["Ganz","Ganz ZN-D2MTP / ZN-D2MTP-IR / ZN-DT2MTP / ZN-DT2MTP-IR / ZN-B2MTP","Camera","ZN3C0.2.1320.32","2","2","+",null,"+",null,null,"1920x1080","+",null,"+","-","+","+","+","-","Камера не поворотная, но есть встроенный трансфокатор.Разрешения  меняются для обоих потоков одновременно - особенность камеры. В ASIP записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")На камере нельзя выставить на обоих потоках одновременно кодек mjpegВ ПО ITV при добавлении камеры вручную тип граббера следует выбирать Ganz-s","This is not a PTZ camera, but it has a built-in zoom lens. Resolutions are changed for both streams at the same time - the camera feature. In ASIP, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\" : \"resolution, stream 2\"). MJPEG codec can't be selected for both streams at the same time. In Axxon software when you add a camera manually, select the Ganz-s grabber type.","new"]
["Ganz","Ganz ZN-DT350VPE / ZN-DNT350VPE / ZN-DWNT350VPE / ZN-DNT350VPEL","Camera ","1.8.1","1","2","+","+","+",null,null,"720x576","+",null,"+.","+","+","+","+","+","1. Устройства в продукте определяется как ZN-D350 series\n2. Видеоаналитика VCA:\nДетектор взлома\nДетектор движущихся/неподвижных объектов\nДетектор низкой освещенности\nДетектор оставленных предметов","1. In the AxxonSoft products, the camera is identified as ZN-D350 series\n2. Video Analytics (VCA):\nCamera tampering detection\nVMD/Abandoned object detection\n"]
["Ganz","Ganz ZN-M2AF","Camera ","ZN2C0.2.2046.32","1","2",null,null,"+",null,null,"1920x1080","+",{"$nulls":3},"+"]
["Ganz","Ganz ZN-MD221M / ZN-MD243M / ZN-MD260M ","Camera ","ZN2C0.2.2046.32","1","2",null,null,"+",null,null,"1920x1080","+"]
["Ganz","Ganz ZN-PTZ220M-XT","Camera","51110.2.6056.100","1","2","+","-","+","-","-","1920x1080","+",null,"-","-","+","-","-",null,"Прошивка 51110.2.6056.100: после установки данной прошивки на камеру в ее веб-интерфейсе в разделе информации об устройстве отображается версия встроенного ПО ZN2C0.2.6056.32.Для работы с камерой в ПО ITV необходимо выбирать тип платы GanzZNC.","51110.2.6056.100 firmware: when the firmware is updated on the camera, ZN2C0.2.6056.32 version is displayed in the properties section in the camera web interface. To work with camera in AxxonSoft software, select the GanzZNC board type."]
["Ganz","Ganz ZN-VS801P encoder","Encoder ","V3.2.36_C","1",null,"+","+",{"$nulls":3},"720x576(PAL)/720x480(NTSC)",null,null,"+","-","+","-","-","-","1. В ПО ITV | Axxonsoft следует выбирать граббера Ganz-s(jpeg) и Ganz-s(h264)\n2. у камеры нет монохромного режима, но в Intellect данный функционал реализуется за счтет сброса насыщенности на минимум. В Axxon Next настройки \"Цвет\" не будет.","1. In the AxxonSoft software, select the Ganz-s(jpeg) and Ganz-s(h264) grabbers.\n2. The camera does not have a black-and-white mode, but Intellect implements this functionality by setting the saturation to the minimum. In Axxon Next, the Color setting is not available."]
["Ganz","Ganz ZN-VS804P encoder","Encoder ","v. 1.1.14_i","4",null,"+","+",{"$nulls":3},"688x544(PAL) / 668x448(NTSC)",null,null,"+","-","+","-","-","-","1) Аналог устройства Ganz ZN-VS804P-WL, от которого отличается только отсутствием возможности беспроводного подключения к сети\n2) для работы с устройством в ПО ITV следует выбирать граббера Ganz-s\n3) при Полном и Высоком разрешении максимальный fps =6 (ограничение самого устройства)\n4) при максимальном значении настройки \"насыщенность цвета\" видеоизображение становится черно-белым (ошибка самого устройства)\n5) \"диагональные\" кнопки управления телеметрией на Панели телеметрии не работают (ограничение самого устройства)","1) This device is very similar to the Ganz ZN-VS804P-WL. The only difference is that by contrast to the Ganz ZN-VS804P-WL, this device does not have any wireless network connectivity.\nTo use the device, in the AxxonSoft software, select the Ganz-s grabber.\n3. At full or high resolution, the max. frame rate is 6 fps (this is a limitation of the device itself).\n4. When you set the saturation setting to the maximum, video turns into black and white (this is a problem of the device itself).\n5) On the PTZ Control Panel, the diagonal telemetry control buttons do not work (this is a limitation of the device itself)."]
["Ganz","Ganz ZN-VS804P-WL encoder","Encoder ","v1.1.11_i","4",null,"+","+",{"$nulls":3},"688x544(PAL)/688x448(NTSC)",null,null,"+","-","+","-","-","-","1. В ПО ITV | Axxonsoft следует выбирать граббера Ganz-s(jpeg) и Ganz-s(h264)\n2. при выставлении высокого и полного разрешений fps падают до ~4-5","1. In the AxxonSoft software, select the Ganz-s(jpeg) and Ganz-s(h264) grabbers. \n2. If you set high or full resolution, the frame rate drops to around 4–5 fps. "]
["Ganz","Ganz ZN-Y11VPE / ZN-NH11VPE / ZN-NHW11VPE / ZN-NH11VPEL","Camera ","1.8.1","1","2","+","+","+",null,null,"720x576","+",null,"+.","+","+","+","+","+","1. Устройства в продукте определяется как ZN-CS series\n2. Видеоаналитика VCA:\nДетектор взлома\nДетектор движущихся/неподвижных объектов\nДетектор низкой освещенности\nДетектор оставленных предметов","1. In the AxxonSoft products, the camera is identified as ZN-CS series\n2. Video Analytics (VCA):\nCamera tampering detection\nVMD/Abandoned object detection"]
["Ganz ZNC","Ganz ZN-C1","Camera ","ZN2C0.2.1517.32","1","2",null,null,"+",null,null,"704x576",null,null,"+","-",null,"+","+","motion detection.","1. fps меняется сразу для двух стриммингов одновременно, разрешение второго стримминга зависит от разрешения первого - особенность интеграции в ПО ITV\n2. Луч(Датчик), Реле и Встроенный детектор срабатывает с задержкой в 2-3 секунды, особенность самой камеры","1. The frame rate is adjusted for both streams at once; the resolution of the second stream depends on the resolution of the first stream (this is for integration with AxxonSoft software). \n2. Sensor, Relay, and Embedded Sensor work with a delay (around 2–3 seconds), this is a limitation of the camera itself. "]
["Ganz ZNC","Ganz ZN-C1M","Camera ","ZN2C0.2.1517.32","1","2",null,null,"+",null,null,"704x576 (MJPEG) / 1280x1024 (H.264)",null,null,"+","-",null,"+","+","motion detection."," 0. Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".\n 1. Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В Axxon Next записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\") \n2. Смена настроек видео происходит с задержкой (от 30 сек. до 1 мин. в случае смены видеопотоков)- особенность камеры. \n3. В MJPEG параметр \"качество\" отсутствует на самой камере, в H264 привязан к параметру \"битрейт\"\n4. Луч, реле и встроенный детектор срабатывают с небольшой задержкой (3-4 секунды)"," 0. Before using the camera, go to the web interface and disable the Installation Mode: assign \"Off\" to this parameter. \n 1. The resolution and frame rate are adjusted for both streams at the same time; this is a limitation of the camera. In Axxon Next, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\" : \"resolution, stream 2\") \n2. Changes to the settings are applied with a delay (30–60 seconds for switching to a different video stream); this is a limitation of the camera itself. \n3. With MJPEG, the Quality parameter is missing on the camera itself; in H.264, this parameter depends on the Bit Rate parameter.\n4. Sensor, Relay, and Embedded Sensor work with a short delay (around 3–4 seconds). "]
["Ganz ZNC","Ganz ZN-C2M","Camera ","ZN2C0.2.1517.32","1","2",null,null,"+",null,null,"704x576 (MJPEG) / 1920x1080 (H264)",null,null,"+","-",null,"+","+","motion detection."," Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В Axxon Next записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")При максимальном битрейте в максимальном разрешении падает fps, видео идет с задержками - особенность устройства.Прошивка 51110.2.1499.100 : камера определяется поиском как NCX-2000Смена настроек видео, а также срабатывание лучей и реле происходит с задержкой (от 30 сек. до 1 мин. в случае смены видеопотоков)- особенность камеры.Луч должен быть под напряжением.В MJPEG параметр \"качество\" отсутствует на самой камере, в H264 привязан к параметру \"битрейт\"Луч(Датчик), Реле и Втроенный детектор могут срабатывать с небольшой задержкой (~3 сек)"," Before using the camera, go to the web interface and disable the Installation Mode: assign \"Off\" to this parameter. The resolution and frame rate are adjusted for both streams at the same time; this is a limitation of the camera. In Axxon Next, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\" : \"resolution, stream 2\"). With the max. bit rate, the frame rate drops when you switch to the max. resolution and video comes with delays. This is a limitation of the device itself. 51110.2.1499.100 firmware: Search detects the device as NCX-2000. Changes to the settings are applied with a delay (30–60 seconds for switching to a different video stream). This is a limitation of the camera itself; the same for how sensors and relays work. Close the sensor when it is energized. With MJPEG, the Quality parameter is missing on the camera itself; in H.264 this parameter depends on the Bit Rate parameter. Sensor, Relay, and Embedded Sensor work with a short delay (around 3 seconds)."]
["Grandstream","Grandstream GXV3500","Encoder/Decoder","1.0.1.75","1","2","+",null,"+",null,null,"704x576 (PAL) / 704x480 (NTSC)","+",{"$nulls":3},"+"]
["Grandstream","Grandstream GXV3501","Encoder ","v1.0.4.34","1","2","+",null,"+",null,null,"PAL:704x576, NTSC:704x480","+",null,"+","+",null,"-","+","-","1. Луч должен замыкаться под напряжением.\n2. Разрешения и максимальный fps зависят от ТВ-стандарта подключенной аналоговой камеры. ","1. Alarm in is to be closed being energized.\n2. Resolutions and the maximum fps depend on a TV-standard of the connected analog camera.\n"]
["Grandstream","Grandstream GXV3504","Encoder ","v1.0.4.34","4","2","+",null,"+",null,null,"PAL: 704x576, NTSC:704x480","+",null,"+","+",null,"+","+","-","1. Луч должен замыкаться под напряжением.\n2. Для MJPEG 704x576 максимальный FPS - 15\n3. Разрешения и максимальный fps зависят от ТВ-стандарта подключенной аналоговой камеры. ","1. Alarm in is to be closed being energized.\n2. For 704x576 MJPEG maximum FPS is 15\n3. Resolutions and the maximum fps depend on a TV-standard of the connected analog camera.\n"]
["Grandstream","Grandstream GXV3601 / -LL","Camera ","1.0.4.27","1","2","+",null,"+",null,null,"720x576 (PAL)","+",null,"+","+.",null,"+","+","-","Прошивка 1.0.4.27: видео совместно со звуком идет только по протоколу UDP.Луч должен замыкаться под напряжением.","1.0.4.27 firmware: Video comes together with audio only via the UDP protocol. Close the sensor when it is energized."]
["Grandstream","Grandstream GXV3611_HD","Camera ","1.0.4.42","1","2","+",null,"+",null,null,"1600x1200","+",{"$nulls":5},"+","-","На втором потоке нельзя выставить разрешение большее чем на первом.","At second stream can not be set resolution larger than at first one."]
["Grandstream","Grandstream GXV3611_LL","Camera ","1.0.4.27","1","2","+",null,"+",null,null,"PAL: 720x576 NTSC: 720x480","+",null,"+","+.",null,"+","+","-","Луч должен быть под напряжением.Прошивка 1.0.4.27: видео совместно со звуком идет только по протоколу UDP.","Close the sensor when it is energized. 1.0.4.27 firmware: Video comes together with audio only via the UDP protocol."]
["Grandstream","Grandstream GXV3615/W","Camera ","1.0.4.34","1","2","+",null,"+",null,null,"720x576 (PAL) / 720x480 (NTSC)","+",null,"+","+",{"$nulls":3},"-","Луч должен замыкаться под напряжением.Прошивка 1.0.4.27: видео совместно со звуком идет только по протоколу UDP.","Close the sensor when it is energized.\nThe 1.0.4.27 firmware: Video comes together with audio only via the UDP protocol.\n"]
["Grandstream","Grandstream GXV3615WP_HD","Camera ","1.0.1.69","1","2","+",null,"+",null,null,"1600x1200","+",null,"+","+",{"$nulls":3},"-"]
["Grandstream","Grandstream GXV3651_FHD","Camera ","1.0.1.57","1","2","+",null,"+",null,null,"2048x1536","+",null,"+","+",null,"+","+","-","Прошивка 1.0.1.45: видео совместно со звуком идет только по протоколу UDP.\nМаксимальный FPS зависит от разрешения: 2560x1920 - 10 2048x1536 - 15\nЛуч должен замыкаться под напряжением.","1.0.1.45 firmware: Video comes together with audio only via the UDP protocol. The max. frame rate depends on the resolution: 2560x1920 – 10 fps, 2048x1536 – 15 fps. \nClose Alarm Input when it is energized."]
["Grandstream","Grandstream GXV3662_HD","Camera ","1.0.1.45","1","2","+",null,"+",null,null,"1280x960","+",null,"+.","+.",null,"+","+","-","Луч должен замыкаться под напряжением.Прошивка 1.0.1.45: видео совместно со звуком идет только по протоколу UDP.","Close the sensor when it is energized. 1.0.1.45 firmware: Video comes together with audio only via the UDP protocol."]
["Grundig","Grundig Encoder GEC-D2201AR","Encoder","720130527ANS","1","2","+","-","+","-","-","720x576","+",null,"-","-","-","-","-","-","В ПО Axxon Next, в двухпоточном режиме, настройка fps применяется на оба потока.","In Axxon Next fps setting is applied to both streams in 2-stream mode. "]
["Grundig","Grundig GCI-C0735P","Camera ","720101228NS","1","2","+",null,"+",null,null,"720x576","+",null,"+","-","+","+","+","-","Через Onvif работает:Получение видео со звукомПоиск (с перебоями)","Via the ONVIF protocol the following work: Receiving video (together with audio) Search (most of the time). "]
["Grundig","Grundig GCI-C0745P","Camera ","720110412NS","1","2","+",null,"+",null,null,"720x576","+",null,null,"-","+",null,null,"-","На камере не работает параметр Частота опорных кадров. Значения в Интеллект и в Axxon Next применяются в веб-интерфейсе, но реальная частота опорных кадров не совпадает с установленным значением.","On the camera, the Keyframes Interval parameter does not work. If set a value in Intellect or Axxon Next, the value is applied in the web interface, but the actual keyframes interval does not match the value that is set. "]
["Grundig","Grundig GCI-F0505B","Camera ","gr20121228NSA ","1","2","+",null,"+",null,null,"2048x1536 ","+"]
["Grundig","Grundig GCI-G0509B","Camera ","gr20120613NSA","1","2","+",null,"+",null,null,"2592х1944 (H.264) / 1920x1080 (MJPEG)","+",{"$nulls":6},"motion detection"]
["Grundig","Grundig GCI-H0503B","Camera ","720110422NS","1","3","+","+","+",null,null,"1280x960","+",null,null,"-",{"$nulls":3},"-","Настройки видео (кодек, разрешение, частота кадров) в разных потоках взаимозависимы. Пользователь должен самостоятельно следить за совместимостью выбранной конфигурации.","The video settings (codec, resolution, frame rate) for different streams are interdependent. The user must independently ensure that the selected values are compatible. "]
["Grundig","Grundig GCI-H0522V","Camera ","720120117NS","1","2","+",null,"+",null,null,"1920x1080","+",null,null,"-",{"$nulls":3},"-","В многопотоковом режиме для первого потока доступен только кодек h264 в разрешении 720p.Частота кадров меняется для обоих потоков одновременно.","In multi-stream mode, only the H.264 codec and 720p resolution are available for the first stream. The frame rate is adjusted for both streams at once."]
["Grundig","Grundig GCI-H0602B","Camera ","720110217NS","1","2","+",null,"+",null,null,"1920x1080","+",null,null,"-",{"$nulls":3},"-","Частота кадров меняется для обоих потоков сразу.При совместном использовании 2х потоков в первом доступен только H264 в разрешении 1280х720.","The frame rate is adjusted for both streams at once. When you use two streams at the same time, only H.264 and the 1280x720 resolution are available for the first stream."]
["Grundig","Grundig GCI-H2505B","Camera","gr20130417NSX","1","2","+","-","+","-","-","1280x720","+","-","-","-","-","-","-","-"]
["Grundig","Grundig GCI-K0322V","Camera ","720110413NS","1","2","+",null,"+",null,null,"1920x1080","+",null,null,"-",{"$nulls":3},"-"]
["Grundig","Grundig GCI-K0503B","Camera ","720110413NS","1","2","+",null,"+",null,null,"1920x1080","+",null,null,"-",{"$nulls":3},"-"]
["Grundig","Grundig GCI-K0512W","Camera ","720101228NS","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":6},"-"]
["Grundig","Grundig GCI-K0523T","Camera ","720110413NS","1","2","+",null,"+",null,null,"1920x1080","+",null,null,"-",{"$nulls":3},"-"]
["Grundig","Grundig GCI-K0779P / GCI-K1779P ","Camera ","gr20120522NSA","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":3},"+",null,null,"motion detection"]
["Grundig","Grundig GCI-K1503B(S) / GCI-K1523V(S) / GCI-K1526V(S)","Camera ","gr20130314NSX ","1","2","+",null,"+",null,null,"1920x1080 ","+"]
["Grundig","Grundig GCI-K1526T / GCI-K1526V / GCI-K1586V / GCI-K1503B / GCI-K1585V / GCI-K1812W / GCI-K0589T ","Camera ","gr20121228NSA ","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":6},"motion detection"]
["Grundig","Grundig GCI-K1603B / GCI-K1523V ","Camera ","gr20121228NSA ","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":6},"motion detection"]
["Grundig","Grundig GCI-K1607B","Camera ","gr20130131NSA ","1","2","+",null,"+",null,null,"1920x1080 ","+"]
["Grundig","Grundig GCI-K2505B","Camera ","gr20131101NSX","1","2","+",null,"+",null,null,"1920x1080","+"]
["HikVision","Hikvision DS-2CD2012-I / DS-2CD2112-I","Camera ","V5.0.0 130412","1","2","+",null,"+",null,null,"1280x960 ","+",{"$nulls":6},"motion detection","На втором потоке нельзя выставить значение разрешения большее, чем стоит на первом.\nДетектор движения работает только при заполненной таблице \"Arming Schedule\", в веб-интерфейсе камеры.\n","At second stream can not be set resolution higher than at first one. Motion detection works only with filled table \"Arming Schedule\" from web-interface."]
["HikVision","Hikvision DS-2CD2032-I / DS-2CD2132-I","Camera ","V5.0.0.130412","1","2","+",null,"+",null,null,"2048x1536","+",{"$nulls":6},"motion detection","Детектор движения работает только при заполненной таблице \"Arming Schedule\", в веб-интерфейсе камеры.","Motion detection works only with filled table \"Arming Schedule\" from web-interface."]
["HikVision","Hikvision DS-2CD2432F-I(W)","Camera","V5.1.0 build 131202","1","2","+","-","+","-","-","2048x1536 (H264) / 704x576 (MJPEG)","+","-","+","-","-","-","-","motion detection"]
["HikVision","Hikvision DS-2CD2712F-IS / DS-2CD2612F-IS","Camera ","V5.0.2 130805","1","2","+",null,"+",null,null,"704x576(MJPEG)/1280x960(H264)","+"]
["HikVision","Hikvision DS-2CD2632F-IS","Camera","V5.0.0 130412","1","2","+","-","+",null,"-","2048x1536(H264) / 704x576 (MJPEG)","+",null,"+","+","-","+","-","motion detection"]
["HikVision","Hikvision DS-2CD7133-E","Camera ","V3.0 110516 ","1","2","+","+","+",null,null,"352x288 (MJPEG) / 640x480 (H264/MPEG4)","+",{"$nulls":6},"-","В Axxon Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.В Axxon Next Смена потоков / кодеков требует перезагрузки устройства (~ 1 мин.)В Интеллекте переключение между полным и средним (минимальным) разрешением требует перезагрузки устройства (~ 1 мин).","In Axxon Next, search does not detect the device's firmware. You must yourself select the right version of the camera's software. In Axxon Next, after you switch to a different stream or codec, you must restart the device (around 1 minute). In Axxon Next, after you switch to a different stream or codec, you must restart the device (around 1 minute)."]
["HikVision","Hikvision DS-2CD7153-E","Camera ","V3.0 build 111017","1","2","+","+.","+",null,null,"1600x1200","+",{"$nulls":3},"-",null,null,"+","В разрешении 1600х1200 сама камера выдает только 12 fps максимум.Прошивка 2.0 100423: все настройки видеопотока (разрешение, fps и пр.) меняются только после reboot камеры.Прошивка 2.0 100423: камера не поддерживает ни ONVIF, ни PSIA.Прошивка 3.0 110516: камера работает и по ONVIF и по PSIAПрошивка 2.0 100423 :настройка \"Раскрытие диафрагмы\" работает неправильно на самой камереПрошивка 3.0 110516: настройка \"Раскрытие диафрагмы\"  НЕ работает на самой камере","At 1600x1200 resolution, the camera itself allows 12 fps max. 2.0 100423 firmware: changes to all the settings of a video stream (resolution, frame rate, etc.) are applied only after you restart the camera. 2.0 100423 firmware: the camera does not support ONVIF or PSIA. 3.0 110516 firmware: the camera works via both ONVIF and PSIA. 2.0 100423 firmware: the Iris Adjustment setting does not work correctly on the camera itself. 3.0 110516 firmware: the Iris Adjustment setting DOES NOT work on the camera itself"]
["HikVision","Hikvision DS-2CD7164-E","Camera ","V4.0.3 121010","1","2","+","+","+",null,null,"1280x960(MPEG4/H.264)/704х576(MJPEG)","+"]
["HikVision","Hikvision DS-2CD732F-E","Camera ","V2.0 build 110829","1","2",null,null,"+",null,null,"704x576","+",null,"+.","+","-","+","-","+","Камера поддерживает разрешения видео стандарта NTSC, а передает видео в разрешениях стандарта PAL. Аналогичная ситуация и в веб-интерфейсе камеры. В результате после выбора в нашем ПО, например, разрешения 704х80, видео будет идти в разрешении 704х576. ","The camera seems to support the NTSC resolutions, but sends video with PAL resolutions instead. In the web interface, it is the same. As a result, if you select, for example, 704x80 resolution, video comes at 704x576 resolution. "]
["HikVision","Hikvision DS-2CD733F-E","Camera ","V3.0 110510","1","2",null,null,"+",null,null,"352x288 (MJPEG) / 640x480 (H264)",null,null,"+.","-","-","+","-","-","При высоких настройках (разрешение, битрейт и качество) видеопоток с камеры может поступать нестабильно. Может наблюдаться \"подтормаживание\" видео, \"проседание\" fps и т.д. - проблема самой камеры.Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельноПрошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства. ","With high settings (resolution, bit rate, and quality), the camera's video stream is unstable. Video may be slow and the frame rate may drop, etc. – this is a problem of the camera itself. Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. V3.0 110510 firmware: If you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device. "]
["HikVision","Hikvision DS-2CD752MF-E","Camera ","V2.0 110902","1","2","+",null,"+",null,null,"352x288 (MJPEG) / 1600x1200 (H264)","+",null,"+.","+","-","+","-","+","В Axxon Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.Через Onvif не работает луч и кодек MJPEG.Камера поддерживает одни разрешения, а передает видео в других. Аналогичная ситуация и в веб-интерфейсе камеры.","In Axxon Next, search does not detect the device's firmware. You must select, yourself, the right version of the camera's software. The sensor and MJPEG codec do not work via the ONVIF protocol. The camera seems to support one set of resolutions, but sends video with other resolutions. In the web interface, it is the same."]
["HikVision","Hikvision DS-2CD752MF-FB","Camera ","V2.0 110902","1","2","+",null,"+",null,null,"352x288 (MJPEG) / 1600x1200 (H264)","+",null,"+.","+","-","+","-","+","В Axxon Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.Поиск может находить камеру как Onvif-устройство, однако работать по этому протоколу она не будетКамера поддерживает одни разрешения, а передает видео в других. Аналогичная ситуация и в веб-интерфейсе камеры.","In Axxon Next, search does not detect the device's firmware. You must select, yourself, the right version of the camera's software. Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. The camera seems to support one set of resolutions, but sends video with other resolutions. In the web interface, it is the same."]
["HikVision","Hikvision DS-2CD753F-E","Camera ","V3.0 110510","1","2","+",null,"+",null,null,"352x288 (MJPEG) / 1600x1200 (H264)",null,null,"+.","+","-","+","-","-","Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельноПрошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.","Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. V3.0 110510 firmware: If you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device."]
["HikVision","Hikvision DS-2CD754F-E","Camera ","V3.2 120105","1","2","+","+","+",null,null,"2048x1536 (h264, mpeg4) / 320x240 (mjpeg)","+",null,"+.","+","-","+","-","+","Смена кодека приводит к перезагрузке камеры (~1 минута)Во втором потоке звук с камеры идет с прерываниями. В Интеллекте это воспроизводится в кодеке H264 (в минимальном разрешении) и в кодеке MJPEG.Если на первом потоке выставлен кодек H264, то на втором может быть либо H264, либо MJPEG. Если на первом потоке выставлен кодек MPEG4, то на втором может быть либо MPEG4, либо MJPEG.","If you switch to a different codec, the camera must restart (1 minute). In the second stream, audio is intermittent. In Intellect, this happens with the H.264 codec (at the min. resolution) and with the MJPEG codec. If you set the H.264 codec for the first stream, you must set either H.264 or MJPEG for the second stream. If you set the MPEG4 codec for the first stream, you must set either MPEG4 or MJPEG for the second stream."]
["HikVision","Hikvision DS-2CD754FWD-E","Camera ","V4.1.0","1","2","+","+","+",null,null,"H.264/MPEG4: 1920x1080; MJPEG: 704x576","+",null,"-","-","-","-","-",null,"Чтобы кодек H.264 (MPEG4) был доступен на втором потоке, нужно выставить такой же кодек на первом","To enable H.264 (MPEG4) for stream 2, select the same codec for stream 1."]
["HikVision","Hikvision DS-2CD762MF-FB","Camera ","V2.0 build 110902","1","2","+",null,"+",null,null,"320x240 (MJPEG) / 1280x960 (H264)","+",null,"+.","+","-","+","-","+","В Axxon Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.Поиск может находить камеру как Onvif-устройство, однако работать по этому протоколу она не будетКамера поддерживает одни разрешения, а передает видео в других. Аналогичная ситуация и в веб-интерфейсе камеры. В результате после выбора в нашем ПО, например, разрешения 352х288, видео будет идти в разрешении 320х240.","In Axxon Next, search does not detect the device's firmware. You must select, yourself, the right version of the camera's software. Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol The camera seems to support one set of resolutions, but sends video with other resolutions. In the web interface, it is the same. As a result, if you select, for example, the 352x288 resolution in our software, video comes in 320x240 resolution."]
["HikVision","Hikvision DS-2CD762MF-FBH","Camera ","V2.0 build 110902","1","2","+",null,"+",null,null,"320x240 (MJPEG) / 1280x960 (H264)","+",null,"+.","+","-","+","-","+","В Axxon Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.Поиск может находить камеру как Onvif-устройство, однако работать по этому протоколу она не будетКамера поддерживает одни разрешения, а передает видео в других. Аналогичная ситуация и в веб-интерфейсе камеры. В результате после выбора в нашем ПО, например, разрешения 352х288, видео будет идти в разрешении 320х240.","In Axxon Next, search does not detect the device's firmware. You must select, yourself, the right version of the camera's software. Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol The camera seems to support one set of resolutions, but sends video with other resolutions. In the web interface, it is the same. As a result, if you select, for example, the 352x288 resolution in our software, video comes in 320x240 resolution."]
["HikVision","Hikvision DS-2CD763PF-E","Camera ","V3.0 build 110516 ","1","2","+","+","+",null,null,"352x288 (MJPEG) / 1280x960 (MPEG4) / 1280x960 (H264)","+",null,"+.","+","-","+","-","-","В Axxon Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.В Axxon Next Смена потоков / кодеков требует перезагрузки устройства (~ 1 мин.)В Интеллекте переключение между полным и средним (минимальным) разрешением требует перезагрузки устройства (~ 1 мин).Через Onvif не работают лучи","In Axxon Next, search does not detect the device's firmware. You must yourself select the right version of the camera's software. In Axxon Next, after you switch to a different stream or codec, you must restart the device (around 1 minute). In Intellect, after you switch between the full and medium (average) resolutions, you must restart the device (around 1 min.) Via the ONVIF protocol, the sensors do not work."]
["HikVision","Hikvision DS-2CD764F-E / DS-2CD8264F-E ","Camera ","V4.1.0 130111","1","2","+",null,"+",null,null,"1280х960(H264;Mpeg4); 704x576(MJPEG) ","+",null,"-","-","-","-","-",null,"Для изменения кодека в Интеллекте сначала необходимо выбрать на камере Полное или Высокое разрешение ","To change codecs in Intellect, you should select Full or High resolution in the camera. "]
["HikVision","Hikvision DS-2CD764FWD-E","Camera","V5.0.0 130412","1","2","+","+","+","-","-","1280x960","+",null,"+","+","+","-","-","motion detection","Кодеки на основном и дополнительном потоках взаимозависимы.детектор движения работает только при заполненной таблице \"Arming Schedule\", в веб-интерфейсе камеры.","Codecs on primary and secondary streams are interdependent. From web-interface motion detection tool works only with \"Arming Schedule\" table filled."]
["HikVision","Hikvision DS-2CD783F-E","Camera ","V3.2 120105","1","2","+","+","+",null,null,"H264, MPEG4: 2560x1920, MJPEG: 320x240","+",null,"+.","+","-","+","-","+","Камера имеет ограничение по FPS в зависимости от разрешения: 6.25 к/сек (2560 × 1920), 12.5 к/сек (2048 × 1536), 25 к/сек (1920 × 1080), 25 к/сек (1600 × 1200), 25 к/сек (1280 × 720)Если на первом потоке выставлен кодек H264, то на втором может быть либо H264, либо MJPEG. Если на первом потоке выставлен кодек MPEG4, то на втором может быть либо MPEG4, либо MJPEG. Нужно учитывать эту зависимость при работе в ПО ITV.","The camera has frame rate limits (depending on the resolution): 6.25 fps (2560 × 1920), 12.5 fps (2048 × 1536), 25 fps (1920 × 1080), 25 fps (1600 × 1200), 25 fps (1280 × 720). If you set the H.264 codec for the first stream, you must set either H.264 or MJPEG for the second stream. If you set the MPEG4 codec for the first stream, you must set either MPEG4 or MJPEG for the second stream. Have this in mind when you use the AxxonSoft software. "]
["HikVision","Hikvision DS-2CD792PF-E","Camera ","V2.0 build 110829","1","2",null,null,"+",null,null,"704x576","+",null,"+.","+","-","+","-","+","Камера поддерживает разрешения видео стандарта NTSC, а передает видео в разрешениях стандарта PAL. Аналогичная ситуация и в веб-интерфейсе камеры. В результате после выбора в нашем ПО, например, разрешения 704х480, видео будет идти в разрешении 704х576.Прошивка V2.0 build 110829: камера передает изображение с искажениями (черными полосами, идущими по картинке).","The camera seems to support the NTSC resolutions, but sends video with PAL resolutions instead. In the web interface, it is the same. As a result, if you select, for example, 704x480 resolution, video comes with the 704x576 resolution. The V2.0 build 110829 firmware: the camera sends distorted video (black lines over the image). "]
["HikVision","Hikvision DS-2CD793PF-E ","Camera ","V3.0 110510","1","2","+",null,"+",null,null,"352x288 (MJPEG) / 704x576 (H264)",null,null,"+.","+",null,"+","-","-","Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельноПрошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.Звук с устройства прерывается:Во втором потоке. В Интеллекте это проявляется при выборе кодека mjpeg.В обоих потоках при выборе транспортного протокола TCP.","Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. V3.0 110510 firmware: if you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remain the same; this is a problem of the device itself. Audio is intermittent. In the second stream. In Intellect, this happens if you select the MJPEG codec in both streams if you select the TCP protocol."]
["HikVision","Hikvision DS-2CD793PFWD-E ","Camera ","V3.0 110510","1","2","+",null,"+",null,null,"352x288 (MJPEG) / 704x576 (H264)",null,null,"+.","+","-","+","-","-","Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельно.Прошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.","Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. V3.0 110510 firmware: If you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device."]
["HikVision","Hikvision DS-2CD8133F-E","Camera ","V3.0 110516 ","1","2","+","+","+",null,null,"640x480","+",null,"+.","+",{"$nulls":3},"+","Если на первом потоке выставлен кодек H264, то на втором может быть либо H264, либо MJPEG. Если на первом потоке выставлен кодек MPEG4, то на втором может быть либо MPEG4, либо MJPEG.","If you set the H.264 codec for the first stream, you must set either H.264 or MJPEG for the second stream. If you set the MPEG4 codec for the first stream, you must set either MPEG4 or MJPEG for the second stream."]
["HikVision","Hikvision DS-2CD8153F-E / HikVision DS-2CD8153F-EW","Camera ","V5.0.0 ","1","2","+","+","+",null,null,"1600x1200","+",null,"+","+",{"$nulls":3},"+","1. Камера имеет ограничения по FPS: 12,5к/с (1600 × 1200), 12,5к/с (1600 × 912), 25к/с (1280 x 960), 25к/с (1280 х 720)\n2. Если на первом потоке выставлен кодек H264, то на втором может быть либо H264, либо MJPEG. \n3. Если на первом потоке выставлен кодек MPEG4, то на втором может быть либо MPEG4, либо MJPEG. ","1. The camera has frame rate limits: 12.5 fps (1600 × 1200), 12.5 fps (1600 × 912), 25 fps (1280 x 960), 25 fps (1280 х 720). 2. If you set the H.264 codec for the first stream, you must set either H.264 or MJPEG for the second stream. \n3. If you set the MPEG4 codec for the first stream, you must set either MPEG4 or MJPEG for the second stream. "]
["HikVision","Hikvision DS-2CD8254F-EI","Camera ","V4.1.0","1","2","+","+","+",null,null,"H.264/MPEG4: 2048x1536; MJPEG: 704x576","+"]
["HikVision","Hikvision DS-2CD8254F-EIS","Camera ","V4.0.1 120704","1","2","+","+","+",null,null,"2048x1536","+"]
["HikVision","Hikvision DS-2CD8254FWD-EIS","Camera","V4.1.0 130111","1","2","+","+","+",null,null,"2048x1536 (H.264, MPEG4) / 704x576 (MJPEG)","+",null,"-","-",null,"-","-","-",null,null,"new"]
["HikVision","Hikvision DS-2CD8264FWD-EIS ","Camera ","V4.1.0 130111 ","1","2","+","+","+",null,null,"1280х960(H264;Mpeg4); 704x576(MJPEG) ","+",{"$nulls":7},"Кодеки H264 или MPEG4 на втором потоке камеры доступны в зависимости от выбранного кодека на первом потоке. ","H264 / MPEG4 codecs are available for stream 2 depending the codecs set for stream 1. "]
["HikVision","Hikvision DS-2CD832F-E","Camera ","V2.0 build 110829 ","1","2",null,null,"+",null,null,"704x576","+",null,"+.","+","-","+","-","+","Камера поддерживает разрешения видео стандарта NTSC, а передает видео в разрешениях стандарта PAL. Аналогичная ситуация и в веб-интерфейсе камеры. В результате после выбора в нашем ПО, например, разрешения 704х80, видео будет идти в разрешении 704х576.","The camera seems to support the NTSC resolutions, but sends video with PAL resolutions instead. In the web interface, it is the same. As a result, if you select, for example, 704x80 resolution, video comes at 704x576 resolution."]
["HikVision","Hikvision DS-2CD833F-E","Camera ","V3.0 110510","1","2","+",null,"+",null,null,"352x288 (MJPEG) / 640x480 (H264)",null,null,"+.","+","-","+","-","-","Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельноПрошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.","Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. V3.0 110510 firmware: If you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device."]
["HikVision","Hikvision DS-2CD852MF-E","Camera ","V2.0 110902","1","2","-",null,"+",null,null,"1600x1200 (H264) / 320x240 (MJPEG)",null,null,"+.","+","-","+","-","+","В спецификации камеры заявлен MPEG4, однако фактически камера не поддерживает этот кодек (прошивка V2.0 101426)Прошика V2.0 110117, V2.0 110902: Камера иногда передает видео в неправильном разрешении - проблема устройства.","According to the specification, the camera supports the MPEG4 codec; however, in reality the camera does not support this codec (firmware V2.0 101426). V2.0 110117 and V2.0 110902 firmware: Via the ONVIF protocol, the camera sometimes sends video with the wrong resolution; this is a problem of the device itself. "]
["HikVision","Hikvision DS-2CD853F-E","Camera ","V3.0 110510","1","2","+",null,"+.",null,null,"352x288 (MJPEG) / 1600x1200 (H264)","-",null,"+.","-","-","+","-","-","Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельноПрошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.","Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. V3.0 110510 firmware: If you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device."]
["HikVision","Hikvision DS-2CD854F-E","Camera ","V3.2 120105","1",2,"+","+","+",null,null,"2048x1536 (h264, mpeg4) / 320x240 (mjpeg)","+",null,"+","+","-","+","-","+","Смена кодека приводит к перезагрузке камеры (~1 минута)Во втором потоке звук с камеры идет с прерываниями. В Интеллекте это воспроизводится в кодеке H264 (в минимальном разрешении) и в кодеке MJPEG.При получении видео по протоколу tcp звук также прерывается. Для получения качественного звука нужно переключиться на udp.","If you switch to a different codec, the camera must restart (1 minute). In the second stream, audio is intermittent. In Intellect, this happens with the H.264 codec (at min. resolution) and with the MJPEG codec. When video comes via the TCP, audio is intermittent. To get quality audio, switch to UDP. "]
["HikVision","HikVision DS-2CD854FWD-E","Camera ","V5.0.0 130412","1","2","+","+","+",null,null,"2048x1536(H.264 / MPEG4) / 704x576(PAL MJPEG) / 704x480 (NTSC MJPEG)","+",null,"+","+","+","+",null,"motion detection","Если на первом потоке стоит H.264, то на втором нельзя выставить MPEG4 и наоборот, если на первом потоке стоит MPEG4, то на втором нельзя выставить H.264\nДетектор движения в продукте срабатывает только если в веб-интерфейсе камеры для детектора движения заполнена таблица Arming Schedule\nЛучи в продукте срабатывает только если в веб-интерфейсе камеры для Alarm input заполнена таблица Arming Schedule\nЕсли выбрать максимальное значение разрешения, то уменьшается максимальное значение FPS.","If first stream is in H.264 codec, it is impossible to use at second one MPEG4, and conversely, if the first stream stands in MPEG4, it is impossible to set on second one H.264.\nMotion detector in AxxonSoft products works only if in camera's web interface filled Arming Schedule table.\nRays in AxxonSoft products works only if in camera's web interface filled Arming Schedule table for Alarm input.\nIf you select maximum resolution, maximum FPS will be decreased."]
["HikVision","Hikvision DS-2CD862MF-E","Camera ","V2.0 build 110902","1","2","+",null,"+",null,null,"320x240(MJPEG) / 1280x960 (H264)","+",null,"+.","+","-","+","-","+","В Axxon Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.Через Onvif камера работает только в режиме совместимости.Камера поддерживает одни разрешения, а передает видео в других. Аналогичная ситуация и в веб-интерфейсе камеры","In Axxon Next, search does not detect the device's firmware. You must yourself select the right version of the camera's software. Over ONVIF the camera works only in compatibility mode. The camera seems to support one set of resolutions, but sends video with other resolutions. In the web interface, it is the same."]
["HikVision","Hikvision DS-2Cd863PF-E ","Camera ","V3.0 110510","1","2","+",null,"+",null,null,"352x288 (MJPEG) / 1280x960 (H264)",null,null,"+.","+",null,"+","-","-","Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельноПри подключении ко второму стриммингу камера вещает с частотой ~12 fps. И в Интеллекте, и в Axxon Next. Особенность камеры.Прошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.","Search detects the camera's vendor and model correctly, but you have to select the right firmware yourself. When you connect to the second stream, the camera sends video at around 12 fps. Both in Intellect and Axxon Next. This is a limitation of the camera itself. V3.0 110510 firmware: If you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device."]
["HikVision","Hikvision DS-2CD864FWD-E","Camera ","V3.2 120105","1","2","+","+","+",null,null,"MPEG4, H264: 1280x960; MJPEG: 704x576","+",null,"+","+","-","+","-","+","Если установить FPS = 8, реально приходит примерно один кадр в секунду - проблема камеры. Другие значения работают корректно.","If you set the frame rate to 8 fps, you get only around 1 fps in reality. This is a problem of the camera itself. Other values work fine. "]
["HikVision","Hikvision DS-2CD883F-E","Camera ","V3.0 build 110516 ","1","2","+","+","+",null,null,"320x240 (MJPEG) / 2560x1920 (H264) / 2560x1920 (MPEG4)","+",null,"+","+","-","+","-","-","В Axxon Next поиск не определяет прошивку устройства. Правильную версию ПО камеры необходимо выбрать самостоятельно.В Axxon Next Смена потоков / кодеков требует перезагрузки устройства (~ 1 мин.)В Интеллекте переключение между полным и средним (минимальным) разрешением требует перезагрузки устройства (~ 1 мин).","In Axxon Next, search does not detect the device's firmware. You must yourself select the right version of the camera's software. In Axxon Next. After you switch to a different stream or codec, you must restart the device (around 1 minute). In Intellect, after you switch between the full and medium (average) resolutions, you must restart the device (around 1 minute). "]
["HikVision","Hikvision DS-2CD893PFWD-E / DS-2CD893PF-E","Camera ","V3.0 110510","1","2",null,null,"+",null,null,"352x288 (MJPEG) / 704x576 (H264)",null,null,"+.","+",null,"+","-","-","1. Поиск корректно возвращает производителя и модель камеры, но нужную прошивку необходимо выбрать самостоятельно\n2. Прошивка V3.0 110510: при смене настроек изображения через Onvif они меняются, но визуально картинка остается прежней - проблема устройства.","1. Search detects the camera's manufacturer and model correctly, but you have to select the right firmware yourself. \n2. V3.0 110510 firmware: \nIf you change video settings via the ONVIF protocol, the changes are applied, but the image on the screen remains the same. This is a problem of the device."]
["HikVision","Hikvision DS-2DF1-401H","Camera ","V3.1.0 120107","1","2","+",null,"+",null,null,"704x576","+",null,"+.","+","+","+","-","+","Смена кодека приводит к перезагрузке камеры (~1 минута).Во втором потоке звук с камеры идет с прерываниями.","If you switch to a different codec, the camera must restart (1 minute). In the second stream, audio is intermittent. "]
["HikVision","Hikvision DS-2DF1-402H","Camera ","V3.1.0 110811","1","2","+",null,"+",null,null,"704x576","+",{"$nulls":3},"+"]
["HikVision","Hikvision DS-2DF1-512/514/516/518","Camera ","V3.1.0 120107","1","2","+",null,"+",null,null,"704x576","+",null,"+","+","+","+","-","+","1. Смена кодека приводит к перезагрузке камеры (~1 минута).\n2. Во втором потоке звук с камеры идет с прерываниями.","1. If you switch to a different codec, the camera must restart (1 minute). \n2. In the second stream, audio is intermittent. "]
["HikVision","Hikvision DS-2DF5284-A","Camera ","V5.0.0 build 130518","1","2","+","+","+",null,null,"1920x1080 (H.264 / MPEG4) / 704x576(MJPEG PAL) / 704x480(MJPEG NTSC)","+",null,"+","+","+","+",null,"motion detection","Детектор движения в продукте срабатывает только если в веб-интерфейсе камеры для детектора движения заполнена таблица Arming Schedule\nЛучи в продукте срабатывает только если в веб-интерфейсе камеры для Alarm input заполнена таблица Arming Schedule","Motion detector in AxxonSoft products works only if in camera's web interface filled Arming Schedule table.\nRays in AxxonSoft products works only if in camera's web interface filled Arming Schedule table for Alarm input."]
["HikVision","Hikvision DS-2DF1-572","Camera ","4.0.0 111122","1","2","+",null,"+",null,null,"1280x720","+",null,"+","+","+","+","-","+","Смена кодека приводит к перезагрузке камеры (~1 минута)Во втором потоке звук с камеры идет с прерываниями. В Интеллекте это воспроизводится при выборе минимальных разрешений.","If you switch to a different codec, the camera must restart (1 minute). In the second stream, audio is intermittent. In Intellect, this happens if you select the minimum resolution. "]
["HikVision","Hikvision DS-2DF1-607(H) / 617(H)","Camera ","V3.1.0 110811","1","2","+",null,"+",null,null,"704x576","+",{"$nulls":3},"+"]
["HikVision","Hikvision DS-2DF1-614H","Camera ","V3.1.0 110811","1","2","+",null,"+",null,null,"704x576","+",null,"+.","-","+","+","-","+"]
["HikVision","Hikvision DS-2DF1-714/716/718","Camera ","V3.1.0 120107","1","2","+",null,"+",null,null,"704x576","+",null,"+.","+","+","+","-","+","На камерах физически есть 7 лучей, в нашем ПО они все также интегрированы, но по умолчанию работают только первые 2. Поддержка остальных опциональна. За подробной информацией нужно обращаться к производителю.Камера Hikvision DS-2DF1-714 (прошивка V3.1.0 110811) отличается несколько нестабильным поведением: при изменении разрешения камера очень долго его применяет (3-5 минут). Сначала камера долго думает, затем перезагружается, и после перезагрузки видео начинает идти в установленном разрешении.","Physically, the camera has 7 sensors; in our software, they are all integrated, but only the first 2 work by default. The others are supported optionally. For detailed information, refer to the vendor. The Hikvision DS-2DF1-714 camera (V3.1.0 110811 firmware) is somewhat unstable: when you change the resolution, the camera takes a very long time to apply the change (3–5 min.). The camera first \"thinks\" for a long time, then restarts, and after that video comes at the new resolution. "]
["HikVision","Hikvision DS-2DZ216","Camera ","V3.0 build 111226","1","2","+","-","+",null,null,"H264:1280x960 MJPEG:352x288","+",null,"+.","+","-","+","-","+","Параметр Image Flip (отражение) интегрирован, но на самой камере он не работает. Т.е. при изменении параметра через наш продукт в веб-интерфейсе значение применяется, но реально картинка не отражается.Прошивка V3.0 110408: Устройство обнаруживается поиском только как Onvif.","The Image Flip parameter is integrated, but it does not work on the camera itself. That is, when you change this parameter in our software, the change is applied in the web interface, but in reality the image does not flip. V3.0 110408 firmware: Search detects the device only as a device that supports ONVIF. "]
["HikVision","Hikvision DS-6504HFI","DVR","V1.0.1 build 110104","4","2","-","-","+","-","-","704x576","+","-","-","-","-","-","-","-","В настройках подключения необходимо указывать порт 8000.","Specify port 8000 in the connection settings."]
["HikVision","Hikvision DS-6508HFI","Encoder ","V1.0.1 build 110104","8","2",null,null,"+",null,null,"704x576","+",{"$nulls":3},"-",null,null,"-","Порт должен быть 8000.","Set the port number to 8000."]
["HikVision","Hikvision DS-6516HFI","Encoder ","V1.0.1 build 110104 ","16","2",null,null,"+",null,null,"704x576","+",{"$nulls":3},"+",null,null,"-","Порт должен быть 8000.","Set the port number to 8000."]
["HikVision","Hikvision DS-6701HFI","Encoder/Decoder","V1.1.0 build 130709","1","2","+","+","+","-","-","704x576","+","-","-","-","-","-","-","-"]
["HikVision","Hikvision DS-7204HFI-SH","DVR","V2.2.10 build 130924","4","2",null,null,"+",null,null,"704x576","+"]
["HikVision","Hikvision DS-7216-HWI-SH/A","DVR","V2.2.8 build 130815","16","1",null,null,"+",null,null,"960x576","+",null,"-","-","-","-","-","-",null,null,"new"]
["HikVision","Hikvision DS-7316-HWI-SH","DVR","V2.2.8 build 130815","16","1",null,null,"+",null,null,"960x576","+",null,"-","-","-","-","-","-",null,null,"new"]
["HikVision","HikVision DVR DS-9632NI-ST","DVR","V2.1.0 build 111017","32","2",null,null,"+",null,null,"2048x1536","+",null,"-",null,"-","-",null,"-","Для подключения к устройству используется порт 8000.","To connect the device need to use 8000 port."]
["Honeywell","Honeywell H3D1F1X (ONVIF)","Camera","40.0.6","1","2","+","-","+",null,"-","1280x720 (H264) / 640x368 (MJPEG)","+",null,"+","-","-","-","+","-"]
["Honeywell","Honeywell H4D2F1X (ONVIF)","Camera","V40.0.6","1","2","+","-","+",null,"-","1920x1080 (H264) / 640x368 (MJPEG)","+",null,"+","-","-","-","+","-"]
["Honeywell","Honeywell HCD2FX (ONVIF)","Camera","40.0.6","1","2","+","-","+",null,"-","1280x720","+",null,"+","-","-","-","+","-"]
["Honeywell","Honeywell HDZ20HDEX (ONVIF)","Camera","MW1D-9C2B ","1","2","+","-","+",null,"-","1920x1080","+",null,"+","-","+","-","+.","-"]
["Hunt","Hunt HLV-1FM","Camera ","3.2.44","1",null,"+","+",{"$nulls":3},"1280x1024",null,null,"-","-",null,null,"+","-","1. При мегапиксельном разрешении видео идет с max. 10 fps\n2. У камеры 2 канала (хоть объектив и один). С одного объектива можно получить два видеопотока с разными настройками. В нашем ПО нужно создавать на одном граббере две камеры на 1-ый и 2-ой каналы","1. At megapixel resolutions, the max. resolution is 10 fps \n2. The camera has two channels (though only 1 lens). With the same lens, you can get two video streams with different settings. In our software, you must create two cameras for the same grabber. "]
["Hunt","Hunt HR-HLC-1NCD/P, HR-HLV-1WCD/P","Camera ","VC1.0.18.2","1","2","+",null,"+",null,null,"1920x1080 ","+",null,"+","+",null,"+","+","motion detection"]
["Hunt","Hunt HR-HLC-79CD/W","Camera ","VC1.0.18.2","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+",null,"+","+","motion detection"]
["Hunt","Hunt HR-HLC-84BM/W","Camera ","VB1.0.40","1","2","+","+","+",null,null,"1280x800","+",null,"+","+",null,"+","+","motion detection"]
["Hunt","Hunt HR-HLT-S30/22x/P","Camera ","VB1.0.40.dc","1","2","+","+","+",null,null,"1280x1024","+",null,"+","+","+.","+","+","motion detection"]
["Infinity","Infinity IPB-TDN540SLHP","Camera ","1.6.0-release","1","2","+","+","+",null,null,"704x576","+",null,"-","-",null,"-","-","-"]
["Infinity","Infinity IPS-26ZDN480ED","Camera ","4.1.2-51","1","1",null,"+",{"$nulls":3},"720x576","+",null,"+.","-","+.","+","+","-"]
["Infinova","Infinova V17xxN-M Series ","Camera ","1.05.01.20100730","1","2","+","+",{"$nulls":3},"720x480","+",null,null,"-","+","-","-","-","Прошивка 1.05.01.20100730: значение \"1 fps\" параметра \"Частота кадров\" в кодеке MJPEG не применяется - проблема устройства.","1.05.01.20100730 firmware: with the MJPEG codec, the value of 1 fps for the Frame Rate parameter cannot be applied. This is a problem of the device itself."]
["Infinova","Infinova V17xxN-N Series","Camera ","2.00.01.20111014","1","3","+",null,"+",null,null,"704x480","+",null,null,"-","+","-","-","-"]
["Infinova","Infinova V6201-N0320","Camera ","1.00.00.201108015_onvif ","1","3","+",null,"+",null,null,"2048x1536 (MJPEG) / 1920x1080 (H264)","+",null,"-","-",null,"-","-","-","Через Onvif работает получение видео.","Via the ONVIF protocol, you can receive video. "]
["InMotion","InMotion HD WDR","Camera ","d20100414NS","1",null,"+","+","+",null,null,"1280x960(MJPEG) / 1280x960(MPEG-4) / 640x480(H.264)",null,null,"+.","-","+.","+","+","-","Кнопки упраления Zoom'ом и Focus'ом перепутаны, но это проблема самого устойства, в \"родном\" ПО точно такая же проблема.При разрешении 1280x960 максимальный доступный fps = 12,5Реле камеры по-умолчанию работает в режиме \"нормально-замкнуто\". Особенность устройства, при необходимости можно изменить через web-интерфейс.","The buttons for controlling zoom and focus are mixed up, but this is the problem of the device itself: the device's own software has the same problem. At 1280x960 resolution, the max. frame rate is 12.5 fps. By default, the camera's relay works in Normally Closed mode. This is a feature of the device; if necessary, you can change it in the web interface."]
["InMotion","InMotion L84II","Encoder ","0063-027y-0639-625z","4","1",null,null,"+",null,null,"720x576",{"$nulls":3},"-",{"$nulls":3},"-"]
["InMotion","InMotion L86T","Encoder ","0027-010a-0608-587a","16","1",null,null,"+",null,null,"720x576",{"$nulls":3},"-",{"$nulls":3},"-"]
["InMotion","InMotion L88II","Encoder ","0049-023E-0615-609H","8","1",null,null,"+",null,null,"720x576",null,null,"+.","-","+","+","+","-","Приемлемую частоту кадров можно настроить только через OSD-меню DVR'а.Длительность тревоги после срабатывания луча настраивается в веб-интерфейсе. По умолчанию стоит минимальное значение - 5 секунд.","An acceptable frame rate may be set only using the DVR's OSD menu. To set how long an alarm is \"sounded\" after the sensor goes off, go to the web interface. By default, the minimum value is set (5 minutes). "]
["Intellico ","Intellico IL-IZH72DX ","Camera ","2.3.0.5.56.2 ","1","2","+",null,"+",null,null,"1280x960","+",null,"+.",null,"+",null,"+",null,"Для подключения к камере необходимо в ПО ITV/Axxon указывать порт, настроенный в веб-интерфейсе камеры (Network Settings -> Basic -> Data port). По умолчанию он равен 5000. ","To connect to the camera, please specify in Axxon SW a port that is configured in the web interface of the camera (Network Settings -> Basic -> Data port). The default is 5000."]
["IPS ","IPS IPS-9XX/IPS-Eye-XXX Series ","Camera ","1.8.1.1i_201302211839_DBU","1","1",null,null,"+",null,null,"1600x1200","+",{"$nulls":3},"+",{"$nulls":3},"Прошивка 1.8.1.1i_201302211839_DBU: Для получения видео со второго потока, необходимо чтобы на первом потоке было установлено разрешение 720р. ","Firmware 1.8.1.1i_201302211839_DBU: to get video from the 2nd stream, please specify 720p resolution for the 1st stream. "]
["iPUX","iPUX ICS1330","Camera ","1.1.0","1","2","+","+",{"$nulls":3},"640x480","+",{"$nulls":3},"+.",null,null,"motion detection","Применение настроек видео требует перезагрузки камеры, поэтому на изменение любой настройки уходит около минуты.","Changes are applied after reboot. This is why to change any setting, it takes about 1 minute."]
["iPUX","iPUX ICS203A","Camera ","1.0.0","1","1","+",{"$nulls":4},"640x480","+",{"$nulls":6},"motion detection","Применение настроек видео требует перезагрузки камеры, поэтому на изменение любой настройки уходит около минуты.","Changes are applied after reboot. This is why to change any setting, it takes about 1 minute."]
["iPUX","iPUX ICS2330","Camera ","1.1.0","1","3","+","+","+",null,null,"1280x1024","+",{"$nulls":3},"+.",null,null,"motion detection"]
["iPUX","iPUX ICS7232","Camera ","1.0.0","1","3","+","+","+",null,null,"1280x1024 (H264, MJPEG) / 640x480 (MPEG4)","+",{"$nulls":6},"motion detection","Применение настроек видео требует перезагрузки камеры, поэтому на изменение любой настройки уходит около минуты.","Changes are applied after reboot. This is why to change any setting, it takes about 1 minute."]
["iPUX","iPUX ICS8200 / ICS8220","Camera ","1.0.0","1","2","+","+","+",null,null,"2048x1536 (H264, MJPEG) / 1920x1080 (MPEG4)","+",{"$nulls":6},"motion detection","1. На камере есть зависимость разрешений от кодеков и fps от разрешений.\n2. При разрешениях больше 1280x720 недоступен двухпоточный режим.\n3. Применение настроек видео требует перезагрузки камеры, поэтому на изменение любой настройки уходит около минуты.","1. The camera's resolutions depend on codecs, and fps depend on resolutions. \n2. Dual stream mode is not available with resolutions over 1280x720. \n3. Changes are applied after reboot. This is why to change any setting, it takes about 1 minute."]
["iPUX","iPUX IVS7100","Camera ","1.0.0 build: 122","1","3","+","+","+",null,null,"from WEB","+",{"$nulls":6},"motion detection","1. На камере не применяются разрешения (ошибка прошивки) f.w. 1.0.0 build: 122","1. You can't change resolutions for that camera, due to a bug in firmware. 1.0.0 build: 122"]
["IQinVision","IQeye IQ040S","Camera ","V3.1/8(101026)","1","1","+",{"$nulls":4},"704x480",{"$nulls":7},"-","Можно выставить любое разрешение из диапазона [704x480; 320x240]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [704x480; 320x240] range. To use it in Intellect, set the resolution in the camera's web interface. "]
["IQinVision","IQeye IQ041S","Camera ","V3.1/8(101026)","1","1","+",{"$nulls":4},"1280x1024",{"$nulls":7},"-","Можно выставить любое разрешение из диапазона [1280x1024; 320x240]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1280x1024; 320x240] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ042S","Camera ","V3.1/8(101026)","1","1","+",{"$nulls":4},"1600x1200",{"$nulls":7},"-","в Axxon Next можно задать любое разрешение из диапазона [320*240 ; 1600*1200] - при этом обрезается картинка и отображается только её часть (чем меньше часть, тем больше fps)\nв Intellect разрешение изменить нельзя (можно только через web камеры)","In Axxon Next, you can select any resolution in the [320*240 ; 1600*1200] range; when you do so, the image is cropped and only a part of the image is shown (the smaller the part, the higher the frame rate).\nIn Intellect, you cannot change the resolution (only in the web interface)."]
["IQinVision","IQeye IQ510","Camera ","V2.8/7(090818)","1","1","+",{"$nulls":4},"752x480",{"$nulls":7},"-","Можно выставить любое разрешение из диапазона [752x480; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [752x480; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ511","Camera ","V2.8/7(090818)","1","1","+",{"$nulls":4},"1280x1024",{"$nulls":7},"-","Можно выставить любое разрешение из диапазона [1280x1024; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры. прошивки V2.8/7(090818) в аттаче нет, есть предыдущая V2.8/6(080313)","You can select any resolution from the [1280x1024; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface. The attachment does not contain the V2.8/7(090818) firmware, it contains only the previous version, V2.8/6(080313)."]
["IQinVision","IQeye IQ541S","Camera ","V3.1/7(100810)","1","1","+",{"$nulls":4},"1280x1024",{"$nulls":7},"-","Можно выставить любое разрешение из диапазона [1280x1024; 320x240]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1280x1024; 320x240] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ702","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"1600x1200",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [1600x1200; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1600x1200; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ703","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"2048x1536",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [2048x1536; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [2048x1536; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ705","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"2560x1920",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [2560x1920; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры","You can select any resolution from the [2560x1920; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ711","Camera ","IQeye711 Version V3.0/8","1","1","+",{"$nulls":4},"1280x1024",{"$nulls":5},"-","+","-","1. Для Intellect разрешение выставляется в web-интерфейсе камеры из диапазона [1280x1024; 512x256]","1. You can select any resolution from the [1280x1024; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ732N","Camera ","V3.2/2(101109)","1","6","+",{"$nulls":4},"from WEB",{"$nulls":5},"-",null,"-"]
["IQinVision","IQeye IQ751","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"1280x1024",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [1280x1024; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры","You can select any resolution from the [1280x1024; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ752","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"1600x1200",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [1600x1200; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1600x1200; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ753","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"2048x1536",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [2048x1536; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [2048x1536; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ755","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"2560x1920",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [2560x1920; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры","You can select any resolution from the [2560x1920; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ851","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"1280x1024",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [1280x1024; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1280x1024; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ852","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"1600x1200",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [1600x1200; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1600x1200; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ853","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"2048x1536",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [2048x1536; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [2048x1536; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ855","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"2560x1920",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [2560x1920; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры","You can select any resolution from the [2560x1920; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQ861N","Camera ","V3.4/2(120925)","1","3","+",null,"+",null,null,"1280x720","+",{"$nulls":3},"-"]
["IQinVision","IQeye IQA20S","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"640x480",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [640x480; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [640x480; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQA22S","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"1600x1200",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [1600x1200; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1600x1200; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQA23S","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"2048x1536",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [2048x1536; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [2048x1536; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQA25S","Camera ","V3.0/8(100702)","1","1","+",{"$nulls":4},"2560x1920",{"$nulls":5},"-",null,"-","Можно выставить любое разрешение из диапазона [2560x1920; 512x256]. Для Intellect разрешение выставляется в web-интерфейсе камеры","You can select any resolution from the [2560x1920; 512x256] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQD30S","Camera ","B3.1/609(100329)","1","3",null,null,"+.",null,null,"720x480",null,null,"+","-",{"$nulls":3},"-"]
["IQinVision","IQeye IQD31S","Camera ","B3.1/602(100217","1","3",null,null,"+",null,null,"1280x720",null,null,"+.","-",{"$nulls":3},"-"]
["IQinVision","IQeye IQD32S","Camera ","V3.3/4(120130)","1","7","+",null,"+",null,null,"1920x1080","+",null,"+","-",{"$nulls":3},"-","Продукт может получать видео одновременно только с 1. и 2. ; с 5. и 6. потока","The VMS receives video from streams 1 and 2 or 5 and 6 at the same time. ; с 5. и 6. потока"]
["IQinVision","IQeye IQD40S","Camera ","V3.1/8(101026)","1","1","+",{"$nulls":4},"720x480",{"$nulls":7},"-","Можно выставить любое разрешение из диапазона [720x480; 320x240]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [720x480; 320x240] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQD41S","Camera ","V3.1/8(101026)","1","1","+",{"$nulls":4},"1280x1024",{"$nulls":7},"-","Можно выставить любое разрешение из диапазона [1280x1024; 320x240]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1280x1024; 320x240] range. To use it in Intellect, set the resolution in the camera's web interface."]
["IQinVision","IQeye IQD42S","Camera ","V3.1/8(101026)","1","1","+",{"$nulls":4},"1600x1200",{"$nulls":7},"-","Можно выставить любое разрешение из диапазона [1600x1200; 320x240]. Для Intellect разрешение выставляется в web-интерфейсе камеры.","You can select any resolution from the [1600x1200; 320x240] range. To use it in Intellect, set the resolution in the camera's web interface."]
["ITV","ITV WS-216 (Yuan)","Video Capture Board ","-","16","2",null,null,"+",null,null,"704x576","+",null,"-",null,null,"-","-",null,"1. Поиском устройство обнаруживается как ITV (вендор) TW5864 PCI (модель).\n2. При работе платы возможен выбор двух потоков - первый h264 с возможностью изменения указанных настроек, второй h264 в минимальном разрешении без настроек.\n3. В Axxon Next каждому каналу соответствует отдельное устройство.","1. Board is detected as ITV (vendor) TW5864 PCI (model).\n2. It's possible to use 2 video streams - the first one h264 can change specified settings, the second one h264 can apply with min resolution and without setting changing.\n3. It's configured as each channel is a separate device."]
["iZett","iZett HR-BT2030C(W)","Camera ","VC1.0.18.2","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+","-","+","+","motion detection"]
["iZett","iZett HR-CB1330B(W)","Camera ","VB1.0.40","1","2","+","+","+",null,null,"1280x800","+",null,"+","+","-","+","+","motion detection"]
["iZett","iZett HR-CB6430BP","Camera ","iZett-VB1.0.38_SO-20130823","1","2","+","+","+",null,null,"640x480","+",null,"+","+","-","+","+","motion detection"]
["iZett","iZett HR-FD2030C(P/VP)","Camera ","VC1.0.18.2","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+","-","+","+","motion detection"]
["iZett","iZett HR-SD1330X22","Camera ","VB1.0.40.dc ","1","2","+","+","+",null,null,"1280x1024","+",null,"+","+","+.","+","+","motion detection"]
["J2000IP","J2000IP DWV112-Ir1-PDN / PWH112-Ir4-PDN","Camera ","v1.6_build044014_145","1","3","+",null,"+",null,null,"1920x1080 / 1280x720","+",null,"+",{"$nulls":5},"Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\nЧастота опорных кадров задается в секундах и может принимать значения от 1 до 3.\nДля корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz.\nМаксимально доступное разрешение в ПО ITV/Axxon зависит от значения настройки Source Resolution в веб-интерфейсе камеры","To connect to the camera required in connection settings set port 30001 in AxxonSoft products.\nReference frames frequency specified in seconds and can take values ​​from 1 to 3.\nFor FPS settings correct work in AxxonSoft software, recommended to set 60Hz mode in camera's web interface.\nMaximum available resolution AxxonSoft software depends on Source Resolution setting in camera's web-interface."]
["J2000IP","J2000IP DWV120-Ir1DN / DWV120-Ir1-PDN / DWV120-PDN","Camera ","v1.6_build044012_025","1","4","+",null,"+",null,null,"704x576",null,null,"+"]
["J2000IP","J2000IP DWV311-Ir3-PDN","Camera ","v1.6_build044014_145","1","2","+",null,"+",null,null,"1280x960 / 1280x720",null,null,"+",{"$nulls":5},"1. Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\n2. Набор разрешений в ПО ITV/Axxon зависит от значения настройки Source Resolution в веб-интерфейсе.\n3. При смене разрешений для кодека H.264 меняется диапазон значений битрейта. Если при переходе на новое разрешение текущий битрейт не попадает в новый диапазон, то настройка не применяется.\n4. Для корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz. ","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. The list of resolution in Axxonsoft SW depends on value of Source Resolution in web interface.\n3. When resolution for H.264 is changed, range of bitrate value is also changed. If there's no current bitrate value for new resolution, in this case setting is not applied.\n4. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["J2000IP","J2000IP mDWV112-Ir1-PDN","Camera ","v1.6_build044014_101","1","3","+",null,"+",null,null,"1920x1080",null,null,"+",{"$nulls":5},"1. Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\n2. Для корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz. \n\n","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["J2000IP","J2000IP PWH121-Ir4-PDN","Camera ","v1.6_build044014_136","1","3","+",null,"+",null,null,"1280x720",null,null,"+"]
["J2000IP","J2000IP PWH312-Ir3-PDN / PWH312-Ir4-PDN / PWH312-Ir5-PDN","Camera ","v1.6_build044014_101","1","3","+",null,"+",null,null,"1920x1080",null,null,"+",{"$nulls":5},"1. Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\n2. Частота опорных кадров задается в секундах и может принимать значения от 1 до 3.\n3. Для корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz.\n4. Максимальное разрешение в продукте зависит от настройки максимального разрешение на камере\n","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. The frequency of of keyframes is set in seconds and can be from 1 to 3.\n3. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly.\n4. Max resolution in Axxonsoft SW depends on camera max resolution.\n"]
["J2000IP","J2000IP PWH313-Ir5-PDN / J2000IP-PWVH313-Ir4-PDN","Camera ","v1.6_build044014_145","1","3","+",null,"+",null,null,"2048x1536",null,null,"+",{"$nulls":5},"1. Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\n2. Максимальное разрешение зависит от настройки Source Resolution в веб-интерфейсе\n3. Для корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz. ","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. Max resolution in Axxonsoft SW depends on value of Source Resolution in web interface.\n3. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["J2000IP","J2000IP SDW112-24x20DN","Camera ","v1.6_build044014_101","1","3","+",null,"+",null,null,"1920x1080",null,null,"+",null,"+.",{"$nulls":3},"1. Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\n2. Частота опорных кадров задается в секундах и может принимать значения от 1 до 3.\n3. Для корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz. ","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. The frequency of of keyframes is set in seconds and can be from 1 to 3.\n3. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["J2000IP","J2000IP SDW121-24x18DN","Camera ","v1.6_build044014_145","1","3","+",null,"+",null,null,"1280x720","+",null,"+",null,"+",{"$nulls":3},"1. Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\n2. Для корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz. ","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["Jassun","Jassun JSI-DPV200IR / JSI-XV200IR / JSI-D200IR / JSI-DV200IP / JSI-C200IR","Camera","1.0.5.1.013_20130930","1","3","+","-","+",null,"-","1920x1080","+",null,"+","+","-","+","+"]
["Jassun","Jassun JSI-XV300IR","Camera","1.0.5.1.013","1","2","+","-","+",null,"-","2048x1536","+",{"$nulls":3},"-",null,"-"]
["JVC","JVC VN-H137U","Camera ","3.00.261","1","3","+","+","+",null,null,"1920x1080","+",{"$nulls":3},"+",null,null,"+","1. Телеметрия работает только при выбранном разрешении 640x360 или 640x480. \n2. На разных потоках камера позволяет включать разрешения с одинаковым соотношением сторон: 4:3 (1280x960, 640x480, 320x240) или 16:9 (1920x1080, 1280x720, 640x360).\n3. Максимальная частота кадров в мультипотоковом режим - 15 fps.\n4. В кодеке MPEG4 недоступно разрешение 1920х1080.\n 5. Допустимые комбинации кодеков в мультипотоковом режиме:\n 0/2.h264 + 1.h264\n 0/2.mjpeg + 1.mjpeg\n 0/2.mjpeg + 1.h264\n 0/2.mjpeg (320x240) + 1.mpeg4 (320x240)\n 0/2.mjpeg (640x480) + 1.mpeg4 (640x480)\n 0/2.mjpeg (1280x960) + 1.mpeg4 (320x240)\n 0/2.mjpeg (1280x960) + 1.mpeg4 (640x480) ","1. The telemetry works only with chosen 640x360 or 640x480 resolutions. \n2. For different streams the camera allows enabling resolutions with an identical aspect ratio: 4:3 (1280x960, 640x480, 320x240) or 16:9 (1920x1080, 1280x720, 640x360).\n3. The maximum frame rate in multi-stream mode is 15 fps.\n4. In the MPEG4 codec 1920х1080 resolution is unavailable.\n 5. Admissible combinations of codecs in a multi-stream mode:\n 0/2.h264 + 1.h264\n 0/2.mjpeg + 1.mjpeg\n 0/2.mjpeg + 1.h264\n 0/2.mjpeg (320x240) + 1.mpeg4 (320x240)\n\n 0/2.mjpeg (640x480) + 1.mpeg4 (640x480)\n 0/2.mjpeg (1280x960) + 1.mpeg4 (320x240)\n 0/2.mjpeg (1280x960) + 1.mpeg4 (640x480)\n"]
["JVC","JVC VN-H157WPU","Camera ","4.00.575","1","3","+","+","+",null,null,"1920x1080","+",{"$nulls":3},"+",null,null,"-","1. Телеметрия работает только при выбранном разрешении 640x360 или 640x480. ","1. The telemetry works only with chosen 640x360 or 640x480 resolutions. "]
["JVC","JVC VN-H237U / VN-H237VPU","Camera ","4.00.314","1","3","+","+","+",null,null,"1920x1080","+",{"$nulls":3},"+",null,null,"motion detection","1. Телеметрия работает только при разрешениях 640x480 и 640x360.","1. Telemetry works only for 640x480 and 640x360 resolutions."]
["JVC","JVC VN-H257U / VN-H257VPU","Camera ","4.00.575","1","2","+","+","+",null,null,"1920x1080","+",null,"+","+","+","+","+.","motion detection","1. Цифровая телеметрия работает только при разрешениях 640x480 и 640x360","1. Digital PTZ works only for 640x480 and 640x360 resolutions."]
["JVC","JVC VN-H37U","Camera ","4.00.314","1","3","+","+","+",null,null,"1920x1080","+",{"$nulls":3},"+",null,null,"motion detection","1. Телеметрия работает только при разрешениях 640x480 и 640x360.","1. Telemetry works only for 640x480 and 640x360 resolutions."]
["JVC","JVC VN-H557U","Camera","1.00.524","1","3","+",null,"+",null,null,"1920x1080","+",null,"-","-","+","-","-","-","На втором и третьем потоке нельзя выставить значение разрешения больше чем на первом. ","The second and third streams can’t have resolution higher than the first one.","improved"]
["JVC","JVC VN-H57U","Camera ","4.00.575","1","3","+","+","+",null,null,"1920x1080","+",null,"+","+","+","+","+","motion detection","1. Зум работает только при разрешении 640x480 или 640x360.","1. Zooms works only for 640x480 and 640x360 resolutions."]
["JVC","JVC VN-H657(U) / VN-H657WP(U)","Camera ","2.00.801","1","3","+",null,"+",null,null,"1920x1080","+",{"$nulls":3},"+",{"$nulls":3},"На устройстве есть взаимосвязь между разрешением и минимальным битрейтом.","The camera's settings for resolution and bit rate are interdependent."]
["JVC","JVC VN-T216(VPRU) / VN-T16U","Camera ","j.2.2.1980","1","2","+","+","+",null,null,"MJPEG/MPEG4: 1280х720; H.264: 1920x1080","+",null,null,"-",null,"-","-","-"]
["JVC","JVC VN-V225U","Camera ","1.01","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","-",null,"+","+","-"]
["JVC","JVC VN-V25U","Camera ","2.02","1",null,"+","+",{"$nulls":3},"640x480",{"$nulls":5},"+","+","-"]
["JVC","JVC VN-V26U","Camera ","2.02","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","+",null,"+","+","-"]
["JVC","JVC VN-V685U","Camera ","3.04","1","1","+.","+.",{"$nulls":3},"640x480",{"$nulls":4},"+",null,null,"-"]
["JVC","JVC VN-V686BU","Camera ","3.03","1","1","+.","+.",{"$nulls":3},"640x480",{"$nulls":4},"+",null,null,"-"]
["JVC","JVC VN-V686U","Camera ","1.06","1","1","+","-",{"$nulls":3},"640x480",{"$nulls":4},"+.","+","+","-","1. с прошивкой 1.06 MPEG-4 видео работает с ошибками на самом устройстве","1. With the 1.06 firmware, MPEG-4 video works with errors on the device itself. "]
["JVC","JVC VN-V686WPBU","Camera ","3.05","1","1","+","+",{"$nulls":3},"640x480","+",{"$nulls":3},"+","+","+","motion detection"]
["JVC","JVC VN-X235U","Camera ","1.02","1","2","+","+",{"$nulls":3},"1280x960(MJPEG) / 640x480(MPEG-4)",null,null,"+","+","+","+","+","+","Камера не поворотная, но есть \"цифровая телеметрия\". Начинает работать при достаточном зумировании картинки. В максимальном разрешении 1280x960 недоступна.Поиск в Axxon Next корректно находит камеру, но верную прошивку нужно выбрать самостоятельно.При смене разрешения в одном из видеопотоков, автоматически изменится разрешение и второго потока - особенность камеры. Таким образом, при одновременном использовании обоих видеопотоков, следующие комбинации будут работать:MJPEG: 320x240 - 320x240 MPEG4MJPEG: 640x480 - 640x480 MPEG4MJPEG: 1280x960 - 640x480 MPEG4Для того, чтобы работали все значения параметра \"Скорость затвора\", нужно в веб-интерфейсе присвоить параметру \"Sense Up\" значение \"Off\".Встроенный детектор камеры не всегда работает корректно: иногда он перестает присылать тревоги. Помогает изменение зоны детектирования.","It is not a PTZ camera, but it has digital telemetry. It starts working after you zoom in enough. At max. resolution (1280x960), it is not available. In Axxon Next, search detects the camera correctly, but you have to select the right firmware yourself. If you change the resolution of one of the streams, the resolution of the other stream changes automatically; this is a limitation of the camera itself. For this reason, when you use both streams, the following codec combinations are available: MJPEG: 320x240 – 320x240 MPEG4MJPEG: 640x480 – 640x480 MPEG4MJPEG: 1280x960 – 640x480 MPEG4For the Shutter Speed parameter, to ensure that all the values work, go to the web interface and set the Sense Up parameter to Off. The camera's embedded detection tool does not always work correctly: sometimes it stops sending alarms. It helps to modify the detection zone. "]
["JVC","JVC VN-X235VPU","Camera ","0.02с","1",null,"+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4)",null,null,"+","-","+","+","+","-","1) ограничения fps - 15\n2) камера не поворотная, но есть \"цифровая телеметрия\". Начинает работать при достаточном зумировании картинки. В мегапиксельном разрешении недоступна","1. Frame rate limits: 15 fps. \n2) This is not a PTZ camera, but it has digital PTZ. It starts working after you zoom in enough. At megapixel resolutions, it is not available."]
["JVC","JVC VN-X35U","Camera ","2.01","1",null,"+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4)",null,null,"+","+","+","+","+","-","1) максимально доступный fps = 15, ограничение самой камеры\n2) Камера не поворотная, но есть DigitalPTZ","1. The max. frame rate is 15 fps; this is a limitation of the camera itself.\n2. This is not a PTZ camera, but it has digital PTZ."]
["Legrand","Legrand 430632","Camera","2.103.0000.0.R, build : 2013-02-23","1","2","+","-","+","-","-","1280x960","+","-","-","-","-","-","-","-"]
["Legrand","Legrand 430652","Camera","2.103.0000.0.R, build : 2013-03-06","1","2","+","-","+","-","-","1280x960","+","-","+","+","+","+","+","-"]
["Legrand","Legrand 430661","Camera","2.103.0000.1.R, build : 2013-02-26","1","2","+","-","+","-","-","2040x1536","+","-","+","+","-","+","+","-"]
["LevelOne","LevelOne FCS-3091","Camera","2.3.0326_level1","1","2","+",null,"+",null,null,"1600x1200","+",null,"-","-",null,"-","-","-",null,null,"new"]
["LG","LG LE5016D","DVR","auto ","18","1",null,null,"+",null,null,"from WEB ",{"$nulls":8},"1. В ПО ITV/Axxon нет возможности изменять настройки устройства\n2. Нужно указать порт 9001\n3. Звук проигрывается с того микрофона, который был включен первым. Для проигрывания звука с другого микрофона нужно выключить активный микрофон и включить необходимый\n\n","1. In AxxonSoft software, you cannot change the camera's settings\n2. Specify port 9001\n3. Sound comes from the microphone which was enabled first. To get sound output from another mic, switch off the active mic and switch on the required one."]
["LG","LG LNB3100","Camera ","1826.0.0.1304190","1","2","+",null,"+",null,null,"1280х1024 / 1280х720","+",{"$nulls":7},"Максимальное разрешение в ПО Axxon зависит от значения настройки \"Режим захвата видеоизображения\" ","Max Resolution in Axxon SW depends on \"Video Capture Mode\" setting."]
["LG","LG LNB5100 ","Camera ","1794.0.0.1304190 ","1","2","+",null,"+",null,null,"1280х1024 / 1280х720","+",{"$nulls":7},"Максимальное разрешение в ПО Axxon зависит от значения настройки \"Режим захвата видеоизображения\" ","Max Resolution in Axxon SW depends on \"Video Capture Mode\" setting."]
["LG","LG LND3100 ","Camera ","1828.0.0.1304190","1","2","+",null,"+",null,null,"1280х1024 / 1280х720","+",{"$nulls":7},"Максимальное разрешение в ПО Axxon зависит от значения настройки \"Режим захвата видеоизображения\" ","Max Resolution in Axxon SW depends on \"Video Capture Mode\" setting."]
["LG","LG LND5100","Camera ","1796.0.0.1304190","1","2","+",null,"+",null,null,"1280х1024 / 1280х720","+",{"$nulls":7},"Максимальное разрешение в ПО Axxon зависит от значения настройки \"Режим захвата видеоизображения\" ","Max Resolution in Axxon SW depends on \"Video Capture Mode\" setting."]
["LG","LG LNV5100 ","Camera ","1908.0.0.1304190 ","1","2","+",null,"+",null,null,"1280х1024 / 1280х720","+",{"$nulls":7},"Максимальное разрешение в ПО Axxon зависит от значения настройки \"Режим захвата видеоизображения\" ","Max Resolution in Axxon SW depends on \"Video Capture Mode\" setting."]
["LG","LG LNU5100R","Camera","1954.0.0.1306100","1","2","+","-","+",null,"-","1280x1024","+",{"$nulls":3},"-",null,"-","motion detection.","Детектор движения доступен только для H.264На камера есть встроенная аналитика Smart Analytics","Motion detector is only available for H.264 codec. Onboard Smart Analytics."]
["LG","LG LNU7210R / LNV7210(R) / LND7210(R)","Camera","2219.0.0.1311130","1","2","+",null,"+",null,null,"1920x1080","+",null,"-","-","+","-","-","-","На камере есть детектор лиц.","There is an on-board Face detection tool.","new"]
["LG","LG LRD5080N ","NVR","auto ","8","1",null,null,"+",null,null,"from WEB ",{"$nulls":8},"1. В ПО ITV/Axxon нет возможности изменять настройки устройства\n2. Нужно указать порт 9001\n3. Звук проигрывается с того микрофона, который был включен первым. Для проигрывания звука с другого микрофона нужно выключить активный микрофон и включить необходимый\n\n","1. In AxxonSoft software, you cannot change the camera's settings\n2. Specify port 9001\n3. Sound comes from the microphone which was enabled first. To get sound output from another mic, switch off the active mic and switch on the required one."]
["LG","LG LRD5160N","NVR","auto ","16","1",null,null,"+",null,null,"from WEB ",{"$nulls":8},"1. В ПО ITV/Axxon нет возможности изменять настройки устройства\n2. Нужно указать порт 9001\n3. Звук проигрывается с того микрофона, который был включен первым. Для проигрывания звука с другого микрофона нужно выключить активный микрофон и включить необходимый\n\n","1. In AxxonSoft software, you cannot change the camera's settings\n2. Specify port 9001\n3. Sound comes from the microphone which was enabled first. To get sound output from another mic, switch off the active mic and switch on the required one."]
["LG","LG LRH7080D","DVR","auto ","16","1",null,null,"+",null,null,"from WEB ",{"$nulls":8},"1. В ПО ITV/Axxon нет возможности изменять настройки устройства\n2. Нужно указать порт 9001\n3. Звук проигрывается с того микрофона, который был включен первым. Для проигрывания звука с другого микрофона нужно выключить активный микрофон и включить необходимый\n\n","1. In AxxonSoft software, you cannot change the camera's settings\n2. Specify port 9001\n3. Sound comes from the microphone which was enabled first. To get sound output from another mic, switch off the active mic and switch on the required one."]
["LG","LG LRH7160D","DVR","auto ","24","1",null,null,"+",null,null,"from WEB ",{"$nulls":8},"1. В ПО ITV/Axxon нет возможности изменять настройки устройства\n2. Нужно указать порт 9001\n3. Звук проигрывается с того микрофона, который был включен первым. Для проигрывания звука с другого микрофона нужно выключить активный микрофон и включить необходимый\n\n","1. In AxxonSoft software, you cannot change the camera's settings\n2. Specify port 9001\n3. Sound comes from the microphone which was enabled first. To get sound output from another mic, switch off the active mic and switch on the required one."]
["LG","LG LSW2010F-P","Camera ","258.0.0.1107140","1","2","+",null,"+",null,null,"704x576","+",null,"+","+",null,"+","+","+","Событие об изменении состояния луча приходит с задержкой ~7-10 сек.Встроенный детектор движения работает только с кодеком H264Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства.При наличии нескольких одновременных подключений к камере возможно искажения видео при перезапуске камеры или ПО.Через Onvif работают только видео с настройками, звук и реле.","Notifications on sensor status changes arrive with a delay (around 7 to 10 seconds). The embedded motion detection tool works only with the H.264 codec. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. If you have several connections to the camera at the same time, you may see distorted video after you restart the camera or software. Via the ONVIF protocol only the following works: search, video (+ settings), and audio."]
["LG","LG LSW900P-B","Camera ","2.0.0.1105060","1","2","+",null,"+",null,null,"704x576","+",null,"+.","+","+","+","+","+","Поиск не возвращает прошивку: правильную версию нужно выбрать самостоятельно.Событие об изменении состояния луча приходит с задержкой ~7-10 сек.Встроенный детектор движения работает только с кодеком H264.Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства.При наличии нескольких одновременных подключений к камере возможно искажения видео при перезапуске камеры или ПО.Через Onvif не работают:Датчик (луч)Настройки изображения","Search does not detect the device's firmware: you must yourself select the right version of the camera's software. Notifications on sensor status changes arrive with a delay (around 7 to 10 seconds). The embedded motion detection tool works only with the H.264 codec. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. If you have several connections to the camera at the same time, you may see distorted video after you restart the camera or software. The sensor and video settings do not work over ONVIF."]
["LG","LG LVW700P-B","Camera ","4.0.1.1106150","1","2","+",null,"+",null,null,"704x576","+",null,"+","+",null,"+","+","motion detection.","1. ползунок \"Качество\" работает в ПО Intellect только для MJPEG-потока\n2. Работа встроенной видеоаналитики (motion detection) доступна только при H.264 видеопотоке\n3. Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства. ","1. In Intellect, the Quality slider works only for the MJPEG stream.\n2. The embedded video analytics (motion detection) are available only for the H.264 video stream.\n3. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. "]
["LG","LG LVW901P-B","Camera","4.1.0.1110260","1","2","+",null,"+",null,null,"704x576","+",null,"+","+",null,"+","+","+","Поиск не возвращает прошивку: правильную версию нужно выбрать самостоятельно.Событие об изменении состояния луча приходит с задержкой ~7-10 сек.Встроенный детектор движения работает только с кодеком H264Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства.При наличии нескольких одновременных подключений к камере возможно искажения видео при перезапуске камеры или ПО.Через Onvif не работают:Датчик (луч)Настройки изображения","Search does not detect the device's firmware: you must yourself select the right version of the camera's software. Notifications on sensor status changes arrive with a delay (around 7 to 10 seconds). The embedded motion detection tool works only with the H.264 codec. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. If you have several connections to the camera at the same time, you may see distorted video after you restart the camera or software. The sensor and video settings do not work over ONVIF.","improved"]
["LG","LG LW332","Camera ","1026.0.0.1107060","1","2","+",null,"+",null,null,"1280x1024","+",null,"+","+",null,"+","+","+","В MJPEG в первом потоке максимальная частота кадров - 20 fpsПри наличии нескольких одновременных подключений к камере возможно искажения видео при перезапуске камеры или ПО.Событие об изменении состояния луча приходит с задержкой ~7-10 сек.Встроенный детектор движения работает только с кодеком H264Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства.Прошивка 1026.0.0.1107060: При выборе значений яркости <50 картинка становится почти полностью белой. Проблема устройства.Через Onvif работает видео с настройками и звук","With MJPEG (the first stream), the max. frame rate is 20 fps. If you have multiple connections to the camera at the same time, you may see distorted video after you restart the camera or software. Notifications on sensor status changes arrive with a delay (around 7 to 10 seconds). The embedded motion detection tool works only with the H.264 codec. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. 1026.0.0.1107060 firmware: if you set brightness to <50, the image becomes almost white. This is a limitation of the device itself. Via the ONVIF protocol the following works: video (+ settings), and audio."]
["LG","LG LW345(ONVIF)","Camera ","Package_767.0.0.1105130","1","1","+",null,"+",null,null,"1920x1072","+",null,"+.","-",null,"-","-","motion detection.","1. с прошивкой Package_767.0.0.1104141 реле не работает на самой камере","1) With the Package_767.0.0.1104141 firmware, the relay does not work on the camera itself. "]
["LG","LG LW6324","Camera ","1028.0.0.1107060 ","1","2","+",null,"+",null,null,"1280x1024","+",null,"+","+",null,"+","+","+","В MJPEG в первом потоке максимальная частота кадров - 20 fpsПри наличии нескольких одновременных подключений к камере возможно искажения видео при перезапуске камеры или ПО.Событие об изменении состояния луча приходит с задержкой ~7-10 сек.Встроенный детектор движения работает только с кодеком H264Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства.Прошивка 1028.0.0.1107060: При выборе значений яркости <50 картинка становится почти полностью белой. Проблема устройстваЧерез Onvif работает видео с настройками и звук","With MJPEG (the first stream), the max. frame rate is 20 fps. If you have multiple connections to the camera at the same time, you may see distorted video after you restart the camera or software. Notifications on sensor status changes arrive with a delay (around 7 to 10 seconds). The embedded motion detection tool works only with the H.264 codec. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. 1028.0.1107060 firmware: if you set brightness to <50, the image becomes almost white. This is a limitation of the device itself. Via the ONVIF protocol the following works: video (+ settings), and audio."]
["LG","LG LW6454(ONVIF)","Camera ","Package_767.0.0.1105130","1","1","+",null,"+",null,null,"1920x1072","+",null,"+.","-",null,"-","-","motion detection.","1. с прошивкой Package_767.0.0.1104141 реле не работает на самой камере","1) With the Package_767.0.0.1104141 firmware, the relay does not work on the camera itself."]
["LG","LG LW9228I-AN","Camera ","774.0.0.1107143 ","1","2","+",null,"+",null,null,"704x480","+",null,"+","+","+","+.","+","+","При наличии нескольких одновременных подключений к камере возможно искажения видео при перезапуске камеры или ПО.Событие об изменении состояния луча приходит с задержкой ~7-10 сек.Встроенный детектор движения работает только с кодеком H264Тревоги от встроенного детектора движения приходят в наше ПО значительно реже, чем срабатывает детектор в веб-интерфейсе, и с задержкой в ~5 сек. Особенность устройства.Прошивка 774.0.0.1107143: Предустановки телеметрии не работают - проблема самого устройства.Прошивка 774.0.0.1107143: Из 4-х лучей работает только первый. Проблема устройстваЧерез Onvif работает видео с настройками, звук, телеметрия без предустановок и реле.\n","If you have multiple connections to the camera at the same time, you may see distorted video after you restart the camera or software. Notifications on sensor status changes arrive with a delay (around 7 to 10 seconds). The embedded motion detection tool works only with the H.264 codec. The embedded detection tool sends alarms to our software with delays (around 5 seconds). In the web interface, the detection tool goes off much more often. This is a limitation of the device itself. 774.0.0.1107143 firmware: Telemetry presets do not work. This is a problem of the device itself. 774.0.0.1107143 firmware: of the 4 sensors, only the first sensor works. This is a problem of the device itself. Via the ONVIF protocol the following work: video (+ settings), audio, telemetry (without presets), and the relay.\n"]
["LTV","LTV-ISDNO20-M2 ","Camera ","LTV01.2.1055.42","1","2","+",null,"+",null,null,"1920x1080 ","+",null,"+",null,"+.","+","+"]
["LTV","LTV-ICCM1-B320-F3.8","Camera ","1044-1026-1031-1008","1","3","+","+","+",null,null,"1280x1024","+",null,"+",null,"-","+","+","-","При замыкании луча, камера иногда присылает по очереди, что луч замыкают, размыкают и т.д., это проблема производителей.","When a sensor is closed, the camera signals it is open and closed repeatedly. This is a problem with the camera itself."]
["LTV","LTV-ICDM1-423 / LTV-ICDM1-723-V3.3-12","Camera ","LTV01.2.1913.42","1","2","+",null,"+",null,null,"1280x1024","+",null,"+","+",null,"+","+","+","Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".\nРазрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В ASI записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле.\nПрошивка 51110.2.1784.100: Не работает аудио выход","Before using the camera, go to the web interface and disable the Installation Mode, i.e. assign \"Off\" to this parameter.\nThe resolution and frame rate are adjusted for both streams at the same time - this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\"). The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF.\nThe 51110.2.1784.100 firmware: The audio output doesn't work\n"]
["LTV","LTV-ICDM1-623LH-V3.3-12","Camera ","51110.2.1784.100","1","2","+",null,"+",null,null,"1280x1024","+",null,"+","+","+.","+","+","+","Камера не поворотная, но есть встроенный трансфокатор.Разрешение меняется одновременно для двух потоков. В настройках указано в виде \"Разрешение 1 потока : Разрешение 2 потока\"Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле.","This is not a PTZ camera, but it has a built-in zoom lens. The resolution is adjusted for both streams at the same time. This setting is represented as \"Resolution, stream 1 : resolution, stream 2 The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF."]
["LTV","LTV-ICDM1-623LH-V3-9","Camera ","LTV01.2.1074.42","1","2","+",null,"+",null,null,"1280x1024","+",null,"+","-","+.","+","+","motion detection"]
["LTV","LTV-ICDM1-723(L)-V3-9 / LTV-ICDM1-823LH-V3-9 ","Camera ","LTV01.2.1084.42","1","2","+",null,"+",null,null,"1280x1024","+",null,"+","-","+","+","+","motion detection"]
["LTV","LTV-ICDM1-823H-V3.3-12","Camera ","51110.2.1784.100","1","2","+",null,"+",null,null,"1280x1024","+",null,"+","+","+.","+","+","+","Камера не поворотная, но есть встроенный трансфокатор.Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В ASI записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")Прошивка 51110.2.1784.100: через Onvif не меняется разрешение в кодеке MJPEG - проблема камеры.Прошивка 51110.2.1784.100: через Onvif не меняется частота кадров - проблема камеры.Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле.","This is not a PTZ camera, but it has a built-in zoom lens. Before using the camera, go to the web interface and disable the Installation Mode, i.e. assign Off to this parameter. The resolution and frame rate are adjusted for both streams at the same time - this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\")The 51110.2.1784.100 firmware: Via the ONVIF protocol, you can not change the resolution for the MJPEG codec - this seems to be the problem with the device. The 51110.2.1784.100 firmware: Via the ONVIF protocol, you cannot change the frame rate - this seems to be the problem with the device. The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF."]
["LTV","LTV-ICDM1-B423L-F3.8","Camera ","1044-1026-1031-1008","1","3","+","+","+",null,null,"1280x1024","+",null,"+","+","-","+","+",null,"При замыкании луча, камера иногда присылает по очереди что луч замыкают, размыкают и т.д., это баг на самом устройстве.","When a sensor is closed, the camera signals it is open and closed repeatedly. This is a problem with the camera itself."]
["LTV","LTV-ICDM1-B623L-F3.8","Camera ","1044-1026-1031-1008","1","3","+","+","+",null,null,"1280x1024","+",{"$nulls":3},"-","+","+","-","При замыкании луча, камера иногда присылает по очереди что луч замыкают, размыкают и т.д., это проблема производителей.","When a sensor is closed, the camera signals it is open and closed repeatedly. This is a problem with the camera itself."]
["LTV","LTV-ICDM1-B723L-F3.8","Camera ","1044-1026-1031-1008","1","3","+","+","+",null,null,"1280x1024","+",null,"+","-","-","+","+","-","При замыкании луча, камера иногда присылает по очереди что луч замыкают, размыкают и т.д., это проблема производителей.","When a sensor is closed, the camera signals it is open and closed repeatedly. This is a problem with the camera itself."]
["LTV","LTV-ICDM2-423 / LTV-ICDM2-723-V3.3-12","Camera ","LTV01.2.1913.42","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+",null,"+","+","+"," Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В ASI записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле. \nПрошивка 51110.2.1784.100: Не работает аудио выход","Before using the camera, go to the web interface and disable the Installation Mode, i.e. assign \"Off\" to this parameter. The resolution and frame rate are adjusted for both streams at the same time - this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\")The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF. \nThe 51110.2.1784.100 firmware: The audio output doesn't work\n"]
["LTV","LTV-ICDM2-423-T5","Camera ","LTV01.2.1058.42 ","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":3},"+",null,null,"+","1. В Axxon Next записаны двойные разрешения (\"разрешение для 1-го потока\" : \"разрешение для 2-го потока\")\n2. Режим двухпоточности, при котором на каждом потоке установлен кодек MJPEG, не поддерживается.\n3. Для того, чтобы в ПО ITV видео с кодеком MJPEG шло с корректным разрешением, необходимо сначала выбрать граббер H264, установить требуемое разрешение, а затем изменить тип граббера на MJPEG.\n4. Камера не поворотная, но есть встроенный трансфокатор.","1. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\").\n2. You cannot have MJPEG video for both streams at the same time. \n3. To get video from MJPEG codec wirh correct resolution, firstly you need to select H264 grabber, then select required resolution and before this change grabber type to MJPEG.\n4. The camera is PTZ, but it has onboard zoom lens."]
["LTV","LTV-ICDM2-623L-F.4","Camera ","LTV01.2.1210.42","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":6},"motion detection"]
["LTV","LTV-ICDM2-623LH-V3.3-12","Camera ","51110.2.1784.100 ","1","2","+",null,"+",null,null,"1280x720 (MJPEG) / 1920х1080 (H264)","+",null,"+","+","+.","+","+","+","Камера не поворотная, но есть встроенный трансфокатор.Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В Axxon Next записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")Прошивка 51110.2.1784.100: через Onvif не меняется разрешение в кодеке MJPEG - проблема камеры.Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле.","This is not a PTZ camera, but it has a built-in zoom lens. The resolution and frame rate are adjusted for both streams at the same time - this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\")The 51110.2.1784.100 firmware: Viva the ONVIF protocol, you can not change the resolution for the MJPEG codec - this seems to be the problem with the device. The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF.\n"]
["LTV","LTV-ICDM2-623LH-V3-9","Camera ","LTV01.2.1227.42","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","-","+","+","+","motion detection","Режим двухпоточности, при котором на каждом потоке установлен кодек MJPEG, не поддерживается.\nДля того, чтобы в ПО ITV видео с кодеком MJPEG шло с корректным разрешением, необходимо сначала выбрать граббер H264, установить требуемое разрешение, а затем изменить тип граббера на MJPEG.","Dual-stream mode, where at each stream MJPEG turned on, is not supported.\nTo get video with MJPEG codec and correct resolution in AxxonSoft software, you need firstly to select the grabber H264, set the desired resolution, and then change type of grabber to MJPEG."]
["LTV","LTV-ICDM2-723(L)-V3-9 / LTV-ICDM2-823LH-V3-9 ","Camera ","LTV01.2.1227.42","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","-","+","+","+","motion detection"]
["LTV","LTV-ICDM2-723L-F.4","Camera ","LTV01.2.1210.42","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":6},"motion detection"]
["LTV","LTV-ICDM2-823-F2.1","Camera ","LTV01.2.1058.42","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":6},"+","1. В Axxon Next записаны двойные разрешения (\"разрешение для 1-го потока\" : \"разрешение для 2-го потока\")\n2. Для корректного отображения видео нельзя ставить MJPEG одновременно на двух потоках ","1. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\")\n2. You cannot have MJPEG video for both streams at the same time.\n"]
["LTV","LTV-ICDM2-823H-V3.3-12","Camera ","LTV01.2.1913.42","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+","+.","+","+","+","Камера не поворотная, но есть встроенный трансфокатор. Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В ASI записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")Прошивка 51110.2.1784.100: через Onvif не меняется разрешение в кодеке MJPEG - проблема камеры.Прошивка 51110.2.1784.100: через Onvif не меняется частота кадров - проблема камеры.Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле.","This is not a PTZ camera, but it has a built-in zoom lens. Before using the camera, go to the web interface and disable the Installation Mode, i.e. assign Off to this parameter. The resolution and frame rate are adjusted for both streams at the same time - this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\": \"resolution, stream 2\")The 51110.2.1784.100 firmware: Viva the ONVIF protocol, you can not change the resolution for the MJPEG codec - this seems to be the problem with the device. The 51110.2.1784.100 firmware: Via the ONVIF protocol, you cannot change the frame rate - this seems to be the problem with the device. The 51110.2.1784.100 firmware: The sensors and relays do not work via ONVIF."]
["LTV","LTV-ICDV-423 / LTV-ICDV-723-V3.3-12 / LTV-ICDV-623LH-V3.3-12 / LTV-ICDV-823H-V3.3-12","Camera ","LTV01.2.1913.42","1","2","+",null,"+",null,null,"704x576","+",null,"+","+",null,"+","+","+","1. Перед началом работы с камерой необходимо в веб-интерфейсе выключить режим \"Installation Mode\", т.е. присвоить этому параметру значение \"Off\".\n2. Разрешение и частота кадров меняются для обоих потоков одновременно - особенность камеры. В ASI записаны как двойные разрешения (\"разр-е для 1-го потока\" : \"разр-е для 2-го потока\")\n3. Прошивка 51110.2.1784.100: Через Onvif не работают лучи и реле.","1. Before using the camera, go to the web interface and disable the Installation Mode: assign \"Off\" to this parameter. \n2. The resolution and frame rate are adjusted for both streams at the same time; this is a limitation of the camera. In AN, these resolutions are represented as \"dual\" resolutions (\"resolution, stream 1\" : \"resolution, stream 2\"). 3. 51110.2.1784.100 firmware: the sensor and relay do not work over ONVIF."]
["LTV","LTV LTV-ISDNO20-M2","Camera","LTV01.2.6040.42","1","2","+","-","+","-","-","1920x1080","+",null,"+","-","+","+","+",null,"Значения разрешения применяются для обоих потоков.На камере нельзя выставить MJPEG на обоих потоках.","Resolution values are applied to both streams. You cannot set the MJPEG on the camera for both streams."]
["LTV","LTV-IWCCM1-B320L-F3.8","Camera ","1044-1026-1031-1008","1","3","+","+","+",null,null,"1280x1024","+",null,"+","+","-","+","+","-","При замыкании луча, камера иногда присылает по очереди что луч замыкают, размыкают и т.д., это проблема производителей.","When a sensor is closed, the camera signals it is open and closed repeatedly. This is a problem with the camera itself."]
["Magic Box","Magic Box (ONVIF 2-channel device)","Encoder","v2.1321.5776","2","1","+",null,"+",null,null,"720x576","+",null,"+","+","+","-","+","motion detection.","1. Прошивка 371.2285: MJPEG-видео не работает на самом устройстве.\n2. Прошивка 1055.4380: звук с подключенного микрофона очень тихий.\n3. Прошивка 1055.4380: Лучи инвертированы на самом устройстве\n4. Прошивка 1055.4380: Реле перепутаны на самом устройстве\n5. Прошивка 1055.4380: Видеоканалы перепутаны на самом устройстве\n6. Прошивка 1170.4816: Устройство не поддерживает настройки изображения и фокус (внешняя телеметрия).\n7. Перед работой со встроенной аналитикой в ПО ITV необходимо выполнить предварительную настройку устройства через утилиту ODM:\nУдалить профили axxon0 и axxon1 (если есть)\nНастроить фильтры для аналитики: в разделе Metadata, тип фильтра \"Content ItemFilter\", значение:\nДля первого канала: boolean(//tt:SimpleItem[@Name=\"Source\" and @Value=\"VIDEO_SOURCE_0\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\" and @Value=\"VIDEO_SOURCE_0\"]) or not(boolean(//tt:SimpleItem[@Name=\"Source\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\"]))\nДля второго канала: boolean(//tt:SimpleItem[@Name=\"Source\" and @Value=\"VIDEO_SOURCE_1\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\" and @Value=\"VIDEO_SOURCE_1\"]) or not(boolean(//tt:SimpleItem[@Name=\"Source\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\"]))\n8. С прошивкой v2.1321.5776 не работают лучи","1. The 371.2285 firmware: MJPEG video does not work on the device.\n2. The 1055.4380 firmware: with the external microphone, the sound volume is very low. \n3. The 1055.4380 firmware: The sensors are reversed i.e closed show open and vice versa on the device itself. The 1055.4380 firmware: The relays are reversed on the device itself. The 1055.4380 firmware: The video channels are mixed up on the device itself. The 1055.4380 firmware: The device does not support the video settings and focus (pan/tilt drive). \n7. Before using embedded video analytics in the AxxonSoft software, configure the device using the ODM utility\nDelete the axxon0 and axxon1 profiles (if they exist) \n Set up the video analytics filters: go to the Metadata section, find the Content Item Filter type, and set the following value:\nFor the first channel: boolean(//tt:SimpleItem[@Name=\"Source\" and @Value=\"VIDEO_SOURCE_0\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\" and @Value=\"VIDEO_SOURCE_0\"]) or not(boolean(//tt:SimpleItem[@Name=\"Source\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\"]))\nFor the second channel: boolean(//tt:SimpleItem[@Name=\"Source\" and @Value=\"VIDEO_SOURCE_1\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\" and @Value=\"VIDEO_SOURCE_1\"]) or not(boolean(//tt:SimpleItem[@Name=\"Source\"]) or boolean(//tt:SimpleItem[@Name=\"VideoSourceToken\"]))\n8. In the v2.1321.5776 firmware, the sensors do not work."]
["Mango DSP","Mango Pegasus-M","Encoder ","3.2.7.10","1","3","+","+","+",null,null,"720x576",null,null,"+","-","+","+","+","-","Изменение некоторых параметров требует перезагрузки устройства (~1 мин).При максимальном качестве возможны задержки видеопотока.При минимальном качестве возможна потеря видеопотока. Нужно перезагрузить устройство.Реле устройства по-умолчанию замкнуто. Это проявляется при добавлении устройства, а также при изменении некоторых настроек. После замыкания - размыкания его через наше ПО дальнейшая работа проходит корректно.","For some settings, after you change them, you must restart the device (around 1 minute). At max. quality, the video stream may come with delays or the video stream may stop. Restart the device. By default, the device's relay is closed. This creates problems when adding the device or changing some of the settings. To make the relay work correctly, open/close the relay in the AxxonSoft software."]
["March Networks","VideoSphere MegaPX 720p","Camera ","1.8.5","1",{"$nulls":3},"+",null,null,"1280x720",null,null,"-","-",{"$nulls":3},"-","из-за отсутствия документации  не реализовано:\n1. MJPEG\n2. audio in\n3. audio out","Due to the fact that there is no documentation, the following was not implemented: \n1. MJPEG\n2. Audio in\n3. Audio out"]
["March Networks","VideoSphere MiniDome PTZ","Camera ","2.4.0","1",null,"+","+","-",null,null,"720х288",null,null,"-",null,"+","-","-"]
["MBK","MBK-IP67-CMOS-1.3Mp (ONVIF 1-channel device)","Camera","106.2232","1","1","+",null,"+",null,null,"1280x720",{"$nulls":7},"motion detection.","1. Само устройство выдает только ~15 fps и в MJPEG и в H.264\n2. С прошивкой 106.2232 настройка насыщенности цвета работает наоборот на самом устройстве\n","1. The device itself allows around ~15 fps, both with MJPEG and H.264.  \n2. With the 106.2232 firmware, the saturation control works the other way around on the device itself. \n"]
["Mediatronix","Mediatronix AVSR1","Encoder ","auto","1","1",null,"+.",{"$nulls":3},"352x288","-",{"$nulls":3},"-","-","-",null,"В настройках подключения к устройству нужно указывать порт \"20\"","When configuring the connection to the device, set the port number to 20. "]
["Mediatronix","Mediatronix IPCAM_OVT2715","Camera","F106_009 28A3","1","2","-","-","+",null,"-","1920x1080","-",null,"-","-","-","-","-","-"]
["Merit Lilin","Merit Lilin IPD112ESX","Camera ","0.0.64","1","4","+",null,"+",null,null,"1280x768","+",null,"-","-",null,"-","+","+","Максимальная частота кадров: 20 fps в H264, 10 fps в mjpegИзменение настроек происходит достаточно долго: камера каждый раз перезагружается. Особенность устройства.С прошивками 0.0.60, 0.0.62 и 0.0.64 луч(датчик) не работают на самом устройствеС прошивками 0.0.60 и 0.0.64 настройки изображения (яркость, контраст и т.д) через протокол ONVIF не меняются на самом устройствеДоступность кодеков, разрешений, значений частоты кадров в разных потоках взаимозависима. Пользователю придется самостоятельно следить за совместимостью и при необходимости включать/выключать потоки/профили из веб-интерфейса.","Max. frame rate: 20 fps for H.264, 10 fps for MJPEG. Applying changes to settings takes a lot of time: the camera restarts every time. This is a limitation of the device itself. With the 0.0.60, 0.0.62, and 0.0.64 firmware, the sensor does not work on the device itself. With 0.0.60 and 0.0.64, if you use the ONVIF protocol, the video settings (brightness, contrast, and so on) do not change on the device itself. The availability of codecs, resolutions, and frame rates for one stream depends on the current settings of the other. Users must manually check whether the settings are compatible and use the web interface to enable/disable streams/profiles if needed. "]
["Merit Lilin","Merit Lilin IPD2220ES3 / IPR320ESX3","Camera ","1.0.490","1","4","+",null,"+",null,null,"from WEB","+",null,"-",null,"+",null,null,"-","1. Профили настраиваются вручную в веб-интерфейсе камеры. В ПО ITV/Axxon нужно выбирать соответствующий кодек, чтобы работали настройки.","1. You can configure profiles in the web interface. In the AxxonSoft software, you have to select an appropriate codec to comply with settings."]
["Merit Lilin","Merit Lilin IPD552EX","Camera ","0.3.38","1",{"$nulls":3},"+",null,null,"720x576(H.264) / 352 x 288(MJPEG)",null,null,"-",{"$nulls":4},"-","1) В ПО ITV следует выбирать граббер Merit Lilin\n2) для MJPEG есть только одно разрешение 352*288\n3) для MJPEG максимальное значение fps = 1-2","1. In the AxxonSoft software, select the Merit Lilin grabber.\n2. For MJPEG, you have only one resolution, 352*288.\n3. For MJPEG, the max. frame rate is 1–2 fps."]
["Merit Lilin","Merit Lilin IPR712S","Camera ","0.0.66","1","4","+",null,"+",null,null,"1280x768","+",{"$nulls":6},"+","Изменение настроек видео приводит к перезагрузке камеры (~1 минута)Перед переключением кодека/разрешения нужно убедиться, что в веб-интерфейсе включен соответствующий видео-профиль.Максимальные значения частоты кадров достигаются при отключении неиспользуемых видео-профилей (в веб-интерфейсе).Через Onvif работает только получение видео, смена частоты кадров и транспортного протокола","If you change video settings, the camera must restart (1 minute). Before switching to a certain codec/resolution, go to the web interface and make sure that the relevant video profile is enabled. To reach the max. frame rate, go to the web interface and disable the video profiles that are not in use. Via the ONVIF protocol, you can only receive video, change the frame rate, and change the transport protocol."]
["Merit Lilin","Merit Lilin IPR7428ESX / IPR7424ESX","Camera ","1.0.506","1","4","+",null,"+",null,null,"1920x1080(H264) / 720x480 (MJPEG)","+",null,"-","-","+","-","-","-","1. Профили настраиваются вручную в веб-интерфейсе камеры. В ПО ITV/Axxon нужно выбирать соответствующий кодек, чтобы работали настройки.","1. You can configure profiles in the web interface. In the AxxonSoft software, you have to select an appropriate codec to comply with settings."]
["Merit Lilin","Merit Lilin IPS0258","Camera ","0.3.49a","1",{"$nulls":3},"+",null,null,"352x288(MJPEG) / 720x576(H.264)",{"$nulls":4},"+","+.",null,"-","1) для MJPEG есть только одно разрешение 352*240\n2) для MJPEG максимальное значение fps = 1-2\n3) Реле только как реакция на замыкание Луча, поэтому в ПО ITV не реализовано\n4) Лучи в ПО ITV правильно работают только \"на замыкание\", особенность самой камеры\n5) не работает луч №6 - по заявлению от производителя оборудований данный порт зарезервирован.\n6) после изменения настроек (разрешение, качество, fps) на восстановление видеопотока может потребовать до 50 секунд времени.","1. For MJPEG, you have only one resolution, 352*240\n2. For MJPEG, the max. frame rate is 1-2 fps\n3. The relay works only as a response to a Sensor tripwire; for this reason, it is not implemented in the AxxonSoft software\n4) In the AxxonSoft software, the sensors work properly only as a tripwire, this is a limitation of the camera itself\n5. Sensor 6 does not work - according to the vendor, this port is reserved.\n6. After you change the settings (resolution, quality, frame rate), the video stream may take up to 50 seconds to restart."]
["Merit Lilin","Merit Lilin IPS1354N","Camera ","0.3.41a","1",{"$nulls":3},"+",null,null,"352x240(MJPEG)/720x480(H.264)",{"$nulls":5},"-",null,"-","1) для MJPEG есть только одно разрешение 352*240\n2) для MJPEG максимальное значение fps = 1-2\n3) Реле только как реакция на замыкание Луча, поэтому в ПО ITV не реализовано","1. For MJPEG, you have only one resolution, 352*240.\n2. For MJPEG, the max. frame rate is 1–2 fps.\n3. The relay works only as a response to the Sensor getting closed; for this reason, it is not implemented in the AxxonSoft software."]
["Merit Lilin","Merit Lilin IPS1354N (ONVIF)","Camera ","0.3.41a","1",null,"+",null,"+",null,null,"720x480",{"$nulls":7},"-","1) работает по ONVIF\n2) для MJPEG есть только одно разрешение 352*288\n3) для MJPEG максимальное значение fps = 1-2\n4) Реле только как реакция на замыкание Луча, поэтому в ПО ITV не реализовано\n5) разрешения необходимо переключать через родной веб-интерфейс камеры. Особенность самого устройства","1. Works via the ONVIF protocol.\n2. For MJPEG, you have only one resolution: 352*288.\n3. For MJPEG, the max. frame rate is 1–2 fps.\n4. The relay works only when Sensor is on a closed circuit; for this reason, it is not implemented in the AxxonSoft software.\n5. Resolutions can be switched only in the camera's web interface. This is a limitation of the device itself."]
["Merit Lilin","Merit Lilin IPS1358","Camera ","V0.3.28c","1",null,"+",null,"+",null,null,"352x288(MJPEG)/720x576(H.264)",{"$nulls":4},"+","+.",null,"-","1) В ПО ITV следует выбирать граббер Merit Lilin\n2) для MJPEG есть только одно разрешение 352*288\n3) для MJPEG значение fps = 1-2\n4) Реле только как реакция на замыкание Луча, поэтому в ПО ITV не реализовано\n5) не работает луч №6 - по заявлению от производителй зарезервирован для чего-то","1. In the AxxonSoft software, select the Merit Lilin\n grabber.\n2. For MJPEG, you have only one resolution: 352*288.\n3. For MJPEG, the frame rate is 1–2 fps.\n4. The relay works only as a response to the Sensor getting closed; for this reason, it is not implemented in the AxxonSoft software.\n5. Sensor 6 does not work: according to the vendor, this port is reserved for something else."]
["Merit Lilin","Merit Lilin LR7722EX3.6","Camera","1.1.12","1","3","+",null,"+",null,null,"1920x1080","+",null,"+","-",null,"-","+","motion detection","Значение настройки RTSP порт должно соответствовать значению аналогичной настройки, выставленному в веб-интерфейсе на странице Network → HTTP/RTSP Service.Особенность прошивки камеры не позволяет провести полноценную интеграцию настроек видео без необходимости совершения дополнительных действий в веб-интерфейсе камеры. Для корректной работы настроек в ПО ITV/Axxon необходимо, настройки \"Видеокодек\" и \"Разрешение\" в ПО ITV/Axxon соответствовали аналогичным настройкам в веб-интерфейсе камеры, где они зависят от значения параметра Profile (Settings → Video / Audio).Для того, чтобы в ПО Интеллект работали настройки видео, а также разрешения соответствовали указанным в текущих результатах, необходимо соблюдать следующее соответствие между выбранными параметрами в ПО Интеллект и значением настройки Profile в веб-интерфейсе камеры:Разрешение в ПО ИнтеллектMJPEGH.264СтандартноеProfile 2Profile 1ВысокоеProfile 1Profile 2ПолноеProfile 1Profile 1","The value of RTSP port setting is to correspond to the value of the similar setting set in the web interface on the Network → HTTP/RTSP Service page. Camera firmware does not allow integrating video settings without other actions in the camera web interface. For proper operation of settings in Axxon software, the Video codec and Resolution settings in Axxon software are to correspond to the similar settings in the camera web interface where they depend on the Profile (Settings → Video / Audio) parameter. For video settings to operate and resolutions to correspond to those specified in the results in Intellect, you are to keep the following correspondence of selected parameters in Intellect and Profile setting in the camera web interface: Resolution in Intellect MJPEGH.264 Standard Profile 2 Profile 1 High Profile 1 Profile 2 Full Profile 1 Profile 1","improved"]
["Merit Lilin","Merit Lilin VS012","Camera ","0.3.48","1","2","+",null,"+",null,null,"704x576",null,null,"-",null,"+.","+","+","-","1) для MJPEG есть только одно разрешение 352*288\n2) для MJPEG значение fps = 1-2\n3) после изменения настроек (разрешение, качество, fps) на восстановление видеопотока может потребовать до 50 секунд времени.","1. For MJPEG, you have only one resolution, 352*288.\n2. For MJPEG, the frame rate is 1–2 fps.\n3. After you change the settings (resolution, quality, frame rate), the video stream may take up to 50 seconds to restart."]
["Messoa","Messoa NCB855pro / NCR875pro","Camera ","AP_01-00-59-07_2M_MS03","1","3","+","+","+",null,null,"1920x1080","+",null,"+","+",null,"+","+","+","Прошивка AP_01-00-58_2M_MS03: Настройки на камере применяются довольно долго - после нажатия кнопки Применить камера уходит в ребут и настройки применяются примерно через минуту.Прошивка AP_01-00-59-07_2M_MS03: Чтобы работал втроенный детектор движения необходимо, чтобы на одном из потоков был выбран кодек MJPEG, а на другом - MPEG4 либо H264.Прошивка AP_01-00-59-07_2M_MS03: На камере не работает настройка FPS с кодеками H264 и MPEG4. Независимо от значения параметра реально FPS всегда примерно равен 17.Параметр ТВ-стандарт интегрирован, но на аналогичную настройку в вебе не влияет. Он нужен для работы с камерами -HN5 и -HP5 (они отличаются только ТВ-стандартом, значениями разрешений и FPS). Т.е. при изменении этой настройки в Axxon Next меняется список доступных разрешений и значений FPS и больше ничего.Прошивка AP_01-00-59-07_2M_MS03: Через ONVIF у камеры не работают никакие настройки потока и изображения, кроме смены протокола. Также не работают датчики, реле и встроенная аналитика. Это вина прошивки, а не интеграции.","AP_01-00-58_2M_MS03: The camera takes a lot of time to apply changes to settings: after you click Apply, the camera is restarted, so the changes are applied in around 1 minute. AP_01-00-59-07_2M_MS03 firmware: to make the embedded motion detection tool work, select the MJPEG codec for one of the streams and select MPEG4 or H.264 for the other stream. AP_01-00-59-07_2M_MS03 firmware: With the H.264 or MPEG4 codec, setting the frame rate does not work on the camera itself. No matter what you set, the actual frame rate is always around 17 fps. The TV standard parameter is integrated, but it does not affect the corresponding parameter in the web interface. This parameter is only needed for -HN5 and -HP5 cameras (these models differ only in available TV standards, resolutions, and frame rates). That is, if you change these settings in Axxon Next, you change the list of available resolutions and frame rates, but nothing else. AP_01-00-59-07_2M_MS03 firmware: The camera does not allow changing video or stream settings via the ONVIF protocol, except for switching protocols. The sensors, relays, and embedded video analytics do not work either. The firmware has nothing to do with it; the integration was done incorrectly. "]
["Messoa","Messoa NCB858","Camera ","AP_01-00-61-02_MS05","1","3","+","+","+",null,null,"MJPEG/H.264: 2592x1944; MPEG4: 1920х1080","+",{"$nulls":3},"-",{"$nulls":3},"1. В Интеллекте значению Частоты опорных кадров \"0\" соответствует значение \"1/2\" из веб-интерфейса","1. In Intellect, the keyframe rate of 0 corresponds to that of 1/2 in the camera's web interface."]
["Messoa","Messoa NCR870","Camera ","AP_01-00-60-25_MS00","1","2","+","+","+",null,null,"1920x1080","+",{"$nulls":7},"1. Второй поток не доступен при одновременном выборе кодека MPEG4/H264 и разрешения 1920х1080 в первом потоке\n2. Третий поток не доступен при одновременном выборе кодека MJPEG и разрешения 1920х1080 в первом потоке ","1. If you select the MPEG4/H.264 codec and 1920x1080 resolution for the first stream, the second stream is not available. \n2. If you select the MPEG4 codec and 1920x1080 resolution for the first stream, the third stream is not available. "]
["Messoa","Messoa NDF821 / NDF820 / NDF831 / NDR891 / NCR870","Camera ","AP_01-00-59-07_2M_MS02","1","3","+","+","+",null,null,"1920x1080","+",null,"+","+",null,"+","+","+","Прошивка AP_01-00-55_2M_MS02: Настройки на камере применяются довольно долго - после нажатия кнопки Применить камера уходит в ребут и настройки применяются примерно через минуту.Прошивка AP_01-00-55_2M_MS02: При отключении питания на камере для нее останавливается время. При включении питания на камере установлено время ее отключения.Прошивка AP_01-00-59-07_2M_MS02: Чтобы работал втроенный детектор движения необходимо, чтобы на одном из потоков был выбран кодек MJPEG, а на другом - MPEG4 либо H264.Прошивка AP_01-00-59-07_2M_MS02: На камере не работает настройка FPS с кодеками H264 и MPEG4. Независимо от значения параметра реально FPS всегда примерно равен 17.Параметр ТВ-стандарт интегрирован, но на аналогичную настройку в вебе не влияет. Он нужен для работы с камерами -HN5 и -HP5 (они отличаются только ТВ-стандартом, значениями разрешений и FPS). Т.е. при изменении этой настройки в Axxon Next меняется список доступных разрешений и значений FPS и больше ничего.Прошивка AP_01-00-59-07_2M_MS02: Через ONVIF у камеры не работают никакие настройки потока и изображения, кроме смены протокола. Также не работают датчики, реле и встроенная аналитика. Это вина прошивки, а не интеграции.","AP_01-00-55_2M_MS02 firmware: The camera takes a lot of time to apply changes to settings: after you click Apply, the camera is restarted, so the changes are applied in around 1 minute. AP_01-00-55_2M_MS02 firmware: When you power the camera off, its time freezes. When you power it on again, the camera's time is the time when it was powered off. AP_01-00-59-07_2M_MS02 firmware: To make the embedded motion detection tool work, select the MJPEG codec for one of the streams and select MPEG4 or H.264 for the other stream. AP_01-00-59-07_2M_MS02 firmware: With the H.264 or MPEG4 codec, setting the frame rate does not work on the camera itself. No matter what you set, the actual frame rate is always around 17 fps. The TV standard parameter is integrated, but it does not affect the corresponding parameter in the web interface. This parameter is only needed for -HN5 and -HP5 cameras (these models differ only in available TV standards, resolutions, and frame rates). That is, if you change these settings in Axxon Next, you change the list of available resolutions and frame rates, but nothing else. AP_01-00-59-07_2M_MS02 firmware: The camera does not allow changing video or stream settings via ONVIF, except for switching protocols. The sensors, relays, and embedded video analytics do not work either. The firmware has nothing to do with it; the integration was done incorrectly."]
["Messoa","Messoa NIC830","Camera ","X.2.1.17","1","2","+",{"$nulls":4},"1280x960","+",null,"-","+.",null,"+",null,"-"]
["Messoa","Messoa NIC835","Camera ","X.2.1.17","1","2","+",{"$nulls":4},"1280x960","+",null,"-","+.",null,"+","+","-"]
["Messoa","Messoa NIC836","Camera ","X.2.1.10","1","2","+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4",null,null,"+.","+.",null,"+","+","-","1. при разрешении 1280х960 максимальный fps равен 12-15 fps, ограничение самой камеры\n2. автоматический поиск устройства в сети в ПО ITV  не может быть реализован \n\n","1. At 1280x960 resolution, the max. frame rate is 12–15 fps; this is a limitation of the camera itself.\n2. Automatic detection of the device cannot be implemented in AxxonSoft software. \n\n"]
["Messoa","Messoa NIC990","Camera ","M.0.2.7 ","1","2","+",null,"+",null,null,"1280x720 (MJPEG) / 1920x1080 (H264)","+",null,"-","-","+.",null,null,"-","1. Камера не поддерживает управление зумом/фокусом/диафрагмой с различной скоростью. В Axxon Next это проявляется в том, что нужно отклонять джойстик на максимальный угол.\n2. Прошивка M.0.2.5: видео в кодеке h264 при использовании протокола TCP идет с задержками. Рекомендуется использовать UDP.\n3. В многопоточном режиме настройки потоков зависят друг от друга. Ниже приведена таблица совместимости разрешений:\nH264 / MJPEG:\n1080P / -\n720P / 720P\n720P / CIF\n720P / QVGA\n480P / 480P\nVGA / VGA\nVGA / QVGA\nQVGA / QVGA","1. The camera does not support Zoom/Focus/Iris control at various speeds. In AN, this makes you bend you joystick at a max. angle.\n2. The M.0.2.5 firmware: H.264 video under TCP is lagging. We recommend using UDP.\n3. In Multistreaming mode, the streams' parameters are interdependent. Here below is compatibility table for resolutions:\nH264 / MJPEG:\n1080P / -\n720P / 720P\n720P / CIF\n720P / QVGA\n480P / 480P\nVGA / VGA\nVGA / QVGA\nQVGA / QVGA\n"]
["MicroDigital (MDi)","MicroDigital MDC-i4020C / MDC-i4020CTD / MDC-i7020VTD-30 / MDC-i7020FTD-30 / MDC-i7020F / MDC-i8020V-H / MDC-i8020VTD-30H / MDC-i8020VTD-H","Camera ","4.19-75-ds-Ivgsm","1","2","+",null,"+",null,null,"720x480","+",null,"+",null,null,"+","+"]
["MicroDigital (MDi)","MicroDigital MDC-i4060C / MDC-i4060CTD / MDC-i7060VTD-30 / MDC-i7060FTD-30 / MDC-i7060F / MDC-i8060V-H / MDC-i8060VTD-30H / MDC-i8060VTD-H","Camera ","4.19-75-ds-Ivgsm","1","2","+",null,"+",null,null,"1280x1024","+",null,"+",null,null,"+","+"]
["MicroDigital (MDi)","MicroDigital MDC-i4090C / MDC-i4090CTD / MDC-i7090VTD-30 / MDC-i7090FTD-30 / MDC-i7090F / MDC-i8090V-H / MDC-i8090VTD-30H / MDC-i8090VTD-H","Camera ","4.19-34-ds","1","2","+",null,"+",null,null,"1920x1072","+",null,"+",null,null,"+","+"]
["MicroDigital (MDi)","MicroDigital MDC-i4220CDN","Camera ","4.19-75-ds-Ivgsm","1","2",null,null,"+",null,null,"720x576",null,null,"+","-","+","+","+","-","В NTSC-стандарте видео с камеры поступает только черно-белое - особенность устройства.Значение частоты кадров во втором видеопотоке задается не абсолютно, а относительно частоты кадров в первом потоке при помощи соответствующего параметра.","With NTSC, the camera sends only black-and-white video. This is a problem of the camera. For the second stream, the frame rate is set not as an absolute value, but relative to the frame rate of the first stream; use the relevant parameter."]
["MicroDigital (MDi)","MicroDigital MDC-i4230C","Camera ","4.01-14","1","2","+",null,"+",null,null,"640x480","+",null,"+","-",null,"+","-",null,"1. звук есть только с потоком MJPEG\n2. чтобы настроить работу Луча в ПО ITV. Необходимо после создания объекта \"Луч\" в ПО ITV в веб-интерфейсе камеры переключить состояние Input Type из Normal Open в Normal Close и обратно.\n ","1. Audio works only with the MJPEG stream.\n2. To make a sensor work in the AxxonSoft software, first create a Sensor object in the AxxonSoft software, then go to the camera's web interface, switch Input Type from Normal Open to Normal Close, and then switch it back to Normal Open. \n "]
["MicroDigital (MDi)","MicroDigital MDC-i4240 /-W","Camera ","4.19-75-ds-Ivgsm","1","2",null,null,"+",null,null,"640x480","+",null,"+","-","-","+","+","-"]
["MicroDigital (MDi)","MicroDigital MDC-i4240C","Camera ","4.06","1",{"$nulls":3},"+",null,null,"640x480",null,null,"+","-",null,null,"+","-"]
["MicroDigital (MDi)","MicroDigital MDC-i4250C / MDC-i4250CTD","Camera ","4.11-75md-d1","1","2","+",null,"+",null,null,"1280x720","+",null,"+","-","-","+","+","-","Значение частоты кадров во втором видеопотоке задается не абсолютно, а относительно частоты кадров в первом потоке при помощи соответствующего параметра.","For the second stream, the frame rate is set not as an absolute value, but relative to the frame rate of the first stream; use the relevant parameter."]
["MicroDigital (MDi)","MicroDigital MDC-i4260/C/CTD","Camera ","4.19-75-ds-Ivgsm","1","2","+",null,"+",null,null,"1280x720","+",null,"+","-",null,"+","+","-","1. Прошивка 4.01-14: Чтобы настроить работу луча в ПО ITV. Необходимо после создания объекта \"Луч\" в ПО ITV в веб-интерфейсе камеры переключить состояние Input Type из Normal Open в Normal Close и обратно.\n2. Прошивка 4.11-63: камера интегрирована как MDi4260/C/CTD - именно такой индекс модели имеет устройство и так обнаруживается поиском.\n3. Камера имеет ограничение для мультипотокового режима: с двух потоков нельзя одновременно получать видео в кодеке MJPEG, в H264 - можно.","1. 4.01-14 firmware: To make a sensor work in the AxxonSoft software, first create a Sensor object in the AxxonSoft software, then go to the camera's web interface, switch Input Type from Normal Open to Normal Close, and then switch it back to Normal Open. \n2. 4.11-63 firmware: The camera is integrated as MDi4260/C/CTD: this is the model number of the device and how it is detected by search. \n3. The camera has a limitation on multi-streaming mode: you cannot have MJPEG video for both streams at the same time. There is no such limitation for H.264 video. "]
["MicroDigital (MDi)","MicroDigital MDC-i4270C","Camera ","4.07-06","1","2",null,null,"+",null,null,"720x576",null,null,"+","-","-","+","+","-","Значение частоты кадров во втором видеопотоке задается не абсолютно, а относительно частоты кадров в первом потоке при помощи соответствующего параметра.","For the second stream, the frame rate is set not as an absolute value, but relative to the frame rate of the first stream; use the relevant parameter. "]
["MicroDigital (MDi)","MicroDigital MDC-i6060VTD-24H","Camera ","4.19-75-ds-Ivgsm","1","2","+",null,"+",null,null,"1280x1024 ","+",{"$nulls":7},"Устройство определяется в продукте, как MDi6060VTDd ","Camera is identified as MDi6060VTDd ."]
["MicroDigital (MDi)","MicroDigital MDC-i6090FTD-24H / MDC-i6090VTD-24H","Camera ","4.19-34-ds","1","2","+",null,"+",null,null,"1920x1072","+"]
["MicroDigital (MDi)","MicroDigital MDC-i6261VTD(W)-66H","Camera ","4.19-79m-ds-iv ","1","2","+",null,"+",null,null,"1280x720","+",{"$nulls":6},"-","1. В ПО ITV/Axxon камеры определяются как MDi6261VTDa / MDi6261VTDWa.","1. In the AxxonSoft products, the cameras are identified as MDi6261VTDa / MDi6261VTDWa."]
["MicroDigital (MDi)","Microdigital MDC-i6290VTD-10H","Camera","4.19-96-ds","1","2","+","-","+","-","-","1920x1080","+","-","-","-","-","-","-","-"]
["MicroDigital (MDi)","MicroDigital MDC-i7020FTD-12 / MDC-i6020FTD-24H / MDC-i6020VTD-24H","Camera ","4.19-75-ds-Ivgsm","1","2","+",null,"+",null,null,"720x480","+"]
["MicroDigital (MDi)","MicroDigital MDC-i7060FTD-12 / MDC-i6060FTD-24H / MDC-i6060VTD-24H","Camera ","4.19-75-ds-Ivgsm","1","2","+",null,"+",null,null,"1280x1024","+"]
["MicroDigital (MDi)","MicroDigital MDC-i8250V / MDC-i8250VTD ","Camera ","4.19-75-ds-IVgsm ","1","2","+",null,"+",null,null,"1280x720","+",null,"+","-",null,"+","+","-"]
["MicroDigital (MDi)","MicroDigital MDC-i8270V","Camera ","4.11-14","1","2",null,null,"+",null,null,"960x720",null,null,"+","-","-","+","+","-","Значение частоты кадров во втором видеопотоке задается не абсолютно, а относительно частоты кадров в первом потоке при помощи соответствующего параметра.","For the second stream, the frame rate is set not as an absolute value, but relative to the frame rate of the first stream; use the relevant parameter."]
["MicroDigital (MDi)","MicroDigital MDC-i8270VTD","Camera ","4.11-14","1","2",null,null,"+",null,null,"960x720",null,null,"+","-","-","+","+","-","Значение частоты кадров во втором видеопотоке задается не абсолютно, а относительно частоты кадров в первом потоке при помощи соответствующего параметра. После перезагрузки камера иногда перестает транслировать видео. Нужно повторно перезагрузить камеру.","For the second stream, the frame rate is set not as an absolute value, but relative to the frame rate of the first stream; use the relevant parameter. Sometimes, after the camera restarts, it stops sending video. Restart the camera again."]
["MicroDigital (MDi)","MicroDigital MDS-i101 / MDS-i3621Н / MDS-i3621WН","Camera ","4.19-75-ds-Ivgsm","1","2","+",null,"+",null,null,"720x576","+",null,"+","-","+","+","+"]
["MicroDigital (MDi)","MicroDigital MDS-i1220 / MDS-i1220А / MDS-i1220Н","Camera ","4.19-75-ds-Ivgsm","1","2","+",null,"+",null,null,"720x576","+",null,"+",null,"+"]
["MicroDigital (MDi)","MicroDigital MDS-i301","Camera ","4.19-75-ds-Ivgsm","1","2","+",null,"+",null,null,"720x576","+",null,"+","-","+","+","+","-","Значение частоты кадров во втором видеопотоке задается не абсолютно, а относительно частоты кадров в первом потоке при помощи соответствующего параметра.","For the second stream, the frame rate is set not as an absolute value, but relative to the frame rate of the first stream; use the relevant parameter."]
["Mobotix","Mobotix D12D","Camera ","MX-V3.4.5.18","1",{"$nulls":5},"+.","2048x1536",null,null,"+","-",null,"+","+","-","1. в Intellect 4.7.6 Release поддержки кодека MxPEG нет. В Intellect 4.7.8/4.7.6. SP1 MxPEG поддерживается\n 2. звук с камеры можно получить, только если видео идет в формате MxPEG - особенность самой камеры\n 3. у самой камеры есть ограничение по fps для мегапиксельных разрешений:\n-Полное(2048х1536) - max. fps = 4(для MJPEG) / 7 (для MxPEG)\n-Высокое(1024х768) - max. fps =15 (для MJPEG) / 17 (для MxPEG)","1. Intellect 4.7.6 Release does not support the MxPEG codec. Intellect 4.7.8/4.7.6. SP1 does support MxPEG \n2. The camera sends audio only if video is in the MxPEG format. This is a limitation of the camera itself.\n3. For megapixel resolutions, the camera itself has frame rate limits:\n-Full (2048х1536) – max. fps = 4 (for MJPEG) / 7 (for MxPEG)\n-High (1024х768) – max. fps =15 (for MJPEG) / 17 (for MxPEG)"]
["Mobotix","Mobotix D14D","Camera ","MX-V4.1.4.11","1","1","+",{"$nulls":3},"+","2048x1536","+",null,"+","-","+",null,null,"-"]
["Mobotix","Mobotix D15D / M15D / S15D / V15D","Camera","MX-V4.1.10.28","1","1","+","-","-",null,"+","2048x1536","+",null,"+","-","+",null,"-"]
["Mobotix","Mobotix D22M","Camera ","MX-V3.5.2.23","1",null,"+",{"$nulls":3},"+.","2048x1536",{"$nulls":3},"-",{"$nulls":3},"-","1. в Intellect 4.7.6 Release поддержки кодека MxPEG нет. В Intellect 4.7.8/4.7.6 SP1 MxPEG работает, правда пока с проблемами\n2. для получения звука с данной камеры необходимо подключать сторонний ммикрофон у которого специфичные разьемы. Такого микрофона у нас нет, поэтому проверить звук с данной модели нельзя\n3. у самой камеры есть ограничение по fps для мегапиксельных разрешений:\n-Полное(2048х1536) - max. fps = 4(для MJPEG) / 7 (для MxPEG)\n-Высокое(1024х768) - max. fps =15 (для MJPEG) / 17 (для MxPEG)\n ","1. Intellect 4.7.6 Release does not support the MxPEG codec. In Intellect 4.7.8/4.7.6 SP1,  MxPEG does work, but there are still some problems.\n2. To get audio from this camera, you need to connect a third-party microphone by using special connectors. Because we do not have such a microphone, we cannot test audio for this camera.\n3. For megapixel resolutions, the camera itself has frame rate limits:\n-Full (2048х1536) – max. fps = 4 (for MJPEG) / 7 (for MxPEG)\n-High (1024х768) – max. fps =15 (for MJPEG) / 17 (for MxPEG)\n "]
["Mobotix","Mobotix D24M","Camera ","MX-V4.0.4.28","1","1","+",{"$nulls":3},"+","2048x1536","+",null,null,"-","+.",null,null,"-","Передача аудио доступна с помощью специального расширения.","You can get audio if you use a special plug-in. "]
["Mobotix","Mobotix M12D","Camera ","MX-V3.4.5.18","1",null,"+",{"$nulls":3},"+.","2048x1536",null,null,"+","-",null,"+","+",null,"1. в Intellect 4.7.6 Release поддержки кодека MxPEG нет. В Intellect 4.7.8/4.7.6. SP1 MxPEG работает, правда пока с проблемами\n2. звук с камеры можно получить, только если видео идет в формате MxPEG - особенность самой камеры\n3. у самой камеры есть ограничение по fps для мегапиксельных разрешений:\n-Полное(2048х1536) - max. fps = 4(для MJPEG) / 7 (для MxPEG)\n-Высокое(1024х768) - max. fps =15 (для MJPEG) / 17 (для MxPEG)","1. Intellect 4.7.6 Release does not support the MxPEG codec. In Intellect 4.7.8/4.7.6 SP1, MxPEG does work, but there are still some problems.\n2. The camera sends audio only if video is in the MxPEG format. This is a limitation of the camera itself.\n3. For megapixel resolutions, the camera itself has frame rate limits:\n-Full (2048х1536) – max. fps = 4 (for MJPEG) / 7 (for MxPEG)\n-High (1024х768) – max. fps = 15 (for MJPEG) / 17 (for MxPEG)"]
["Mobotix","Mobotix M22M","Camera ","MX-V3.5.2.23","1",{"$nulls":5},"+.","2048x1536",{"$nulls":3},"-",{"$nulls":3},"-","1. в Intellect 4.7.6 Release поддержки кодека MxPEG нет. В Intellect 4.7.8/4.7.6 SP1 MxPEG работает\n 2. у самой камеры есть ограничение по fps для мегапиксельных разрешений:\n-Полное(2048х1536) - max. fps = 4(для MJPEG) / 7 (для MxPEG)\n-Высокое(1024х768) - max. fps =15 (для MJPEG) / 17 (для MxPEG)","1. Intellect 4.7.6 Release does not support the MxPEG codec. In Intellect 4.7.8/4.7.6 SP1, MxPEG does work\n 2. For megapixel resolutions, the camera itself has frame rate limits:\n-Full (2048х1536) – max. fps = 4 (for MJPEG) / 7 (for MxPEG)\n-High (1024х768) – max. fps = 15 (for MJPEG) / 17 (for MxPEG)"]
["Mobotix","Mobotix M24M","Camera ","MX-V4.0.4.28","1",{"$nulls":5},"+","2048x1536",null,null,"+",null,"+",null,null,"-","1. Звук с камеры есть только если видео идет в формате MxPEG. Это особенность самой камеры.\n2. Камера не PTZ, но у неё есть \"виртуальная\" телеметрия\n3. у самой камеры есть ограничение по fps для мегапиксельных разрешений:\n-Полное(2048х1536) - max. fps = 4(для MJPEG) / 7 (для MxPEG)\n-Высокое(1024х768) - max. fps =15 (для MJPEG) / 17 (для MxPEG)","1. The camera sends audio only if video is in the MxPEG format. This is a limitation of the camera itself.\n2. This is not a PTZ camera, but it has virtual PTZ support.\n3. For megapixel resolutions, the camera itself has frame rate limits:\n-Full (2048х1536) – max. fps = 4 (for MJPEG) / 7 (for MxPEG)\n-High (1024х768) – max. fps = 15 (for MJPEG) / 17 (for MxPEG)"]
["Mobotix","Mobotix Q22M","Camera ","MX-V3.4.5.10 (2009-03-02)","1",null,"+",{"$nulls":3},"+.","2048x1536",null,null,"+",null,"+",null,null,"-","1) максимальное разрешене 2048*1536 или 1456x1088, в зависимости от режима выбранного в камере INTL-7404\n2) Звук с камеры есть только если видео идет в формате MxPEG. Это особенность самой камеры.\n3) Камера не PTZ, но у неё есть \"виртуальная\" телеметрия\n ","1. The max. resolution is 2048*1536 or 1456x1088, depending on which mode you select on the INTL-7404 camera.\n2. The camera sends audio only if video is in the MxPEG format. This is a limitation of the camera itself.\nThis is not a PTZ camera, but it has virtual PTZ. \n "]
["Mobotix","Mobotix Q24M","Camera ","MX-V4.1.4.11 ","1","1","+",{"$nulls":3},"+.","2048x1536","+",null,"+","-","+",null,null,"-","1. Звук с камеры есть только если видео идет в формате MxPEG. Это особенность самой камеры.\n2. Камера не PTZ, но у неё есть \"виртуальная\" телеметрия 3. Частота кадров сильно зависит от разрешения. При максимальном разрешении частота кадров составляет 1-2 кадра в секунду.\n4. При интенсивном движении в поле зрения камеры частота кадров может снижаться почти вдвое. ","1. The camera sends audio only if video is in the MxPEG format. This is a limitation of the camera itself.\n2. This is not a PTZ camera, but it has virtual PTZ. 3. The frame rate very much depends on the resolution settings. If you set the max. resolution, the frame rate drops to around 1-2 fps.\n4. Heavy motion in the FoV causes the frame rate to drop by half. "]
["Mobotix","Mobotix S14D / S14M","Camera ","V4.1.4.11","1","2","+",{"$nulls":3},"+","2048x1536","+",null,"+","-","+",null,null,"-","1. Audio Input работает только, если для видео выбран кодек MxPEG","1. Audio Input works only if video is selected in MxPEG codec "]
["Mobotix","Mobotix T24M","Intercom ","MX-V4.1.1.21","1","1","+",{"$nulls":3},"+","2048x1536","+",null,null,"-","+"]
["MOXA","MOXA Vport 461","Encoder ","3.1 Build 11080216","1","3","+",null,"+",null,null,"720x576","+",null,"+","-","-","+","+","-","В процессе работы с устройством обнаружилась такая особенность: иногда (примерно раз в сутки, может реже) устройство зависает и становится недоступным. Помогает перезагрузка.Телеметрию не удалось заставить работать даже через веб-интерфейс.Чтобы сработал датчик, на его вход необходимо подать напряжение от 13В до 30В (в соответствии с мануалом).","While using the camera, we discovered the following problem: sometimes (approx. once per day, sometimes less often) the device freezes and becomes unavailable. It helps to restart the device. We did not manage to make telemetry work, even in the web interface. To make the sensor go off, energize it (13–30 V, according to the guide)."]
["NexusIP ","NexusIP 1MP-NEX-BOX","Camera ","v1.1.0_20130109","1","3","+","+","+",null,null,"1280x720","+"]
["NexusIP ","NexusIP 1MP-NEX-DOME ","Camera ","v1.1.0_20130109","1","3","+","+","+",null,null,"1280x720","+"]
["NexusIP ","NexusIP 2MP-NEX-BOX","Camera ","v1.1.0_20130109","1","3","+","+","+",null,null,"H.264: 1920x1080; MJPEG / MPEG4: 1280x720","+"]
["NexusIP ","NexusIP 2MP-NEX-DOME","Camera ","v1.1.0_20130109","1","3","+","+","+",null,null,"H.264: 1920x1080; MJPEG / MPEG4: 1280x720","+"]
["Novus","Novus NVIP-2C2011D-P ","Camera ","nv20111011NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"+",{"$nulls":4},"+","Поиск может обнаружить устройство как Onvif-совместимое, но работать через Onvif оно не будет.Доступные кодеки, разрешения и значения частоты кадров в разных потоках зависят друг от друга.","Search detects the camera as an ONVIF-conformant device, but the camera does not work via the ONVIF protocol. The Codec and Resolution parameters for different streams are interdependent."]
["Novus","Novus NVIP-2DN2001D-2P","Camera ","nv20111110NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","-",null,"+","+","+","Доступные кодеки, разрешения и значения частоты кадров в разных потоках зависят друг от друга.Поиск может обнаружить устройство как Onvif-совместимое, но работать через Onvif оно не будет.","The Codec and Resolution parameters for different streams are interdependent. Search detects the camera as an ONVIF-conformant device, but the camera does not work via the ONVIF protocol. "]
["Novus","Novus NVIP-2DN2001D-P/GO","Camera ","NVS01.2.1061.46","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":6},"motion detection"]
["Novus","Novus NVIP-2DN5001С-1P / NVIP-2DN3001H/IR-2P / NVIP-2DN4001V/IRH","Camera ","nv20111110NSA","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","-",null,"+","+","+","Доступные кодеки, разрешения и значения частоты кадров в разных потоках зависят друг от друга.Поиск может обнаружить устройство как Onvif-совместимое, но работать через Onvif оно не будет.","Which codecs, resolutions, and frame rates are available for one stream depends on those for the other stream. Search detects the camera as an Onvif-conformant device, but the camera does not work via the ONVIF protocol "]
["Novus","Novus NVIP-2DN5005CZ-P/GO","Camera ","NVS01.2.1061.46","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":6},"motion detection"]
["Novus","Novus NVIP-2DN5018CZ-2P","Camera ","nv20130115NSA ","1","2","+",null,"+",null,null,"1920x1080 ","+",{"$nulls":3},"+.",{"$nulls":3},"Из функционала телеметрии интегрированы только зум, фокус и пресеты. ","For PTZ (telemetry) only interated zoom, focus, presets."]
["Novus","Novus NVIP-2DN6020SD","Camera ","V1.202R05-T320","1","2","+",null,"+",null,null,"1920x1080(H.264)/720x576(mjpeg)","+",{"$nulls":3},"+","+","+"]
["Novus","Novus NVIP-2DN6020SD-2P","Camera ","nv20130115NSA ","1","2","+",null,"+",null,null,"1920x1080","+",null,"+",null,"+","+","+","motion detection"]
["Novus","Novus NVIP-5DN2021D/IR-2P","Camera ","nv20130115NSA ","1","2","+",null,"+",null,null,"1920x1080(MJPEG) 2592x1944(H264) ","+",null,"+",null,null,"+",null,"motion detection","Разрешение на втором потоке камеры зависит от разрешения на первом потоке, при работе с двумя потоками необходимо проверять в веб интерфейсе существует ли необходимая комбинация разрешений. ","Resolution on the second stream of camera depends on resolution of the first stream. Using two streams, please check in web interface if there's a required combination of resolution."]
["Novus","Novus NVIP-5DN5001C-1P","Camera ","nv20130115NSA","1","2","+",null,"+",null,null,"2592x1944 (H264) / 1920x1080 (MJPEG)","+",null,"+",null,null,"+","+","motion detection"]
["Novus","Novus NVIP-DN6137SD","Camera ","V1.110R02-T322","1","2","+",null,"+",null,null,"720x576","+",null,"+","+","+","-","-","-","Звук с микрофона не идет, если видео получается со второго потока ","If video comes from stream 2, the mic fails to deliver audio. "]
["Novus","Novus NVIP-TDN3401H/IR/MPX2.0","Camera ","v1.0.28_NV","1","2","+",null,"+",null,null,"1600x1200","+",null,"+.",null,null,"+","+","motion detection","1. В ПО Intellect камера обнаруживается поиском как FineCCTV IPCam.","1. In Intellect, the search finds the camera as FineCCTV IPCam."]
["Novus","Novus NVIP-TDN5401C/MPX2.0 ","Camera ","V1.0.42_NV","1","2","+",null,"+",null,null,"1600x1200 ","+",null,"+","+",null,"+","+","motion detection"]
["Oncam Grandeye","Oncam Grandeye EVO-05NCD","Fisheye Camera","1.2.2.S","1","1","+",null,"+",null,null,"2144x1944 ","+",{"$nulls":7},"1. Камера интегрирована в ПО ITV/Axxon как OncamGrandeye Evolution series.\n2. Для корректной работы настройки качества с кодеком H264 необходимо выбрать значение off настройки bitrate control. ","1. Camera is integrated in Axxonsoft SW as OncamGrandeye Evolution series.\n2. Please select value of bitrate control \"off\" to work with quality setting of H.264 correctly."]
["Oncam Grandeye","Oncam Grandeye Halocam IPC","Fisheye Camera","2.1.3","1","14","+",{"$nulls":4},"2144x1944","+",{"$nulls":3},"-","-","-","-",null,null,"new"]
["Optelecom-NKF","Siqura BC24 WDR","Camera ","s20091022NS","1",null,"+","+",{"$nulls":3},"1280x960(MJPEG) / 640x480(MPEG-4)",null,null,"+","-",null,"+","+","-"]
["Optelecom-NKF","Siqura C-60 E-MC encoder","Encoder ","2.5.0","1","3","+","+","+",null,null,"720x576",null,null,"+","-","+","+","+"]
["Optelecom-NKF","Siqura S-54 E encoder","Encoder ","2.5.0","4",null,"+","+",{"$nulls":3},"720x576",{"$nulls":4},"+",null,null,"-","1. fps видеопотока сильно зависит от разрешения и качества видео\n2. видеоформат (MJPEG/MPEG-4) и fps видеопотока в Intellect меняется сразу для всех 4-х каналов.\n ","1. The frame rate very much depends on the video resolution and quality\n2. in Intellect, when you change the codec (MJPEG/MPEG-4) or frame rate, you change it for all 4 channels at once. \n "]
["Optelecom-NKF","Siqura S-64 E encoder","Encoder ","3.0.1","4",{"$nulls":3},"+",null,null,"720x576",{"$nulls":4},"+",null,null,"-"]
["Optelecom-NKF","Siqura V-30 E-MSA encoder","Encoder ","2.5.0","1",null,"+","+",{"$nulls":3},"720x576",{"$nulls":4},"+","+","+","-","1. После смены граббера(MJPEG/MPEG-4) в  ПО ITV, следует то же самое сделать и в веб-интерфейсе самого ip-устройства.","1. After you change the grabber (MJPEG/MPEG-4) in the AxxonSoft software, do the same in the device's web interface."]
["Panasonic (BB/BL)","Panasonic BB-HCM511CE/515CE","Camera ","3.5100R","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","-","+","+","+","-","1) для потока MJPEG нельзя изменить fps, такой настройки нет у самой камеры. Значения такие:\nразрешение 640*480 - 10 fps\nразрешение 320*240 - 29-30 fps\n2) у камеры есть только 3 фиксировыых значения качества - потому некоторые значения на ползунке качество в Intellect не отрабатывают","1) for the MJPEG stream, you cannot change the frame rate, because the camera itself does not have this setting. Frame rate values: \nthe 640*480 resolution - 10 fps\nthe 320*240 resolution - 29-30 fps\n2) the camera itself has 3 positions for quality. For this reason, some of the positions do not work on Intellect's quality slider. "]
["Panasonic (BB/BL)","Panasonic BB-HCM531CE","Camera ","3.60R00","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","-","+","+","+","-","1) для потока MJPEG нельзя изменить fps, такой настройки нет у самой камеры. Значения такие:\nразрешение 640*480 - 10 fps\nразрешение 320*240 - 29-30 fps\n2) у камеры есть только 3 фиксированных значения качества - потому некоторые значения на ползунке качество в Intellect не отрабатывают\n \n ","1) for the MJPEG stream, you cannot change the frame rate, because the camera itself does not have this setting. Frame rate values:\nthe 640*480 resolution - 10 fps\nthe 320*240 resolution - 29-30 fps\n2) the camera itself has 3 positions for quality. For this reason, some of the positions do not work on Intellect's quality slider. \n \n "]
["Panasonic (BB/BL)","Panasonic BB-HCM580CE/581CE","Camera ","3.60R00","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","-","+","+","+","-","1) у камеры есть только 3 фиксированных значения качества при MJPEG - поэтому некоторые значения на ползунке качество в Intellect будут совпадать","1) for MJPEG, the camera itself has 3 positions for quality. For this reason, some of the positions do not work on Intellect's quality slider."]
["Panasonic (BB/BL)","Panasonic BB-HCM715CE","Camera"," 4.31R03","1","2","+","+","+","-","-","1280x960","+","-","+","+","+","+","+","-","Включение/выключение максимального разрешения 1280х960 и применение некоторых других настроек видео требует перезагрузки устройства.В многопоточном режиме смена разрешения на одном из потоков изменяет список доступных разрешений на другом потоке. Нужно самостоятельно исключать конфликты выбранных параметров.Разрешение 192х144 во втором потоке недоступно для кодека H264.Прошивка 4.31R00: Изображение в кодеке H264 искажено.Реле имеет выходное напряжение 10.5-13 В DC","After you switch the max. resolution (1280x960) on/off or apply certain video settings, you have to restart the device. In multistream mode, when you change the resolution for one of the streams, you change the list of resolutions available for another stream. You have to avoid conflicts of selected parameters yourself. For the second stream, the 192x144 resolution is not available with H.264.The 4.31R00 firmware: With H.264, video is distorted. The relay's output voltage is 10.5-13 V DC."]
["Panasonic (BB/BL)","Panasonic BL-C1","Camera ","1.34","1",null,"+",{"$nulls":4},"640x480",{"$nulls":7},"-","1. При Полном разрешении камера способна выдавать только 7-10 fps (в зависимости от качества). Это особенность самой камеры, при Стандартном разрешении - 15 fps\n2. У самой камеры всего 3 положения качества, а в Intellect их 5, поэтому некоторые будут повторяться\n","1. With the Full resolution, the camera allows 7 -10 fps max. (depending on the quality). This is a limitation of the device itself; with the Standard resolution, the camera allows 15 fps. The camera itself has 3 positions for quality. Because Intellect has 5, some of the positions in Intellect mean one and the same quality.\n"]
["Panasonic (BB/BL)","Panasonic BL-C111","Camera ","3.60R00","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+",null,"+",null,null,"-","1. Из мануала на камеру «Частота 30 кадров/сек. невозможна при просмотре изображений MJPEG с разрешением 640 × 480»\n2. У самой камеры всего 3 положения качества, а в Intellect их 5, поэтому некоторые будут повторяться\n\n","1. According to the camera's guide, the 30 fps frame rate is not available when viewing videos with MJPEG and the 640 x 480 resolution\n2. The camera itself has 3 positions for quality. Because Intellect has 5, some of the positions in Intellect mean one and the same quality.\n\n"]
["Panasonic (BB/BL)","Panasonic BL-C131","Camera ","3.60R00","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+",null,"+",null,null,"-","1. Из мануала на камеру «Частота 30 кадров/сек. невозможна при просмотре изображений MJPEG с разрешением 640 × 480»\n2. У самой камеры всего 3 положения качества, а в Intellect их 5, поэтому некоторые будут повторяться","1. According to the camera's guide, the 30 fps frame rate is not available when viewing videos with MJPEG and the 640 x 480 resolution\n2. The camera itself has 3 positions for quality. Because Intellect has 5, some of the positions in Intellect mean one and the same quality."]
["Panasonic (BB/BL)","Panasonic BL-C160","Camera ","3.60R00","1","2","+","+",{"$nulls":3},"640x480","+",{"$nulls":6},"-"]
["Panasonic (BB/BL)","Panasonic BL-C20","Camera ","1.34","1",null,"+",{"$nulls":4},"640x480",{"$nulls":7},"-","1. При Полном разрешении камера способна выдавать только 7-10 fps (в зависимости от качества). Это особенность самой камеры, описана в документации на камеру, при Стандартном разрешении - 15 fps\n2. У самой камеры всего 3 положения качества, а в Intellect их 5, поэтому некоторые будут повторяться","1. With the Full resolution, the camera allows 7 -10 fps max. (depending on the quality). This is a limitation of the device itself (described in the camera's documentation); with the Standard resolution, the camera allows 15 fps.\n2. The camera itself has 3 positions for quality. Because Intellect has 5, some of the positions in Intellect mean one and the same quality."]
["Panasonic i-Pro","Panasonic AW-HE60SN/SE/HN/HE","Camera","V03.06","1","2","+","-","+","-","-","640x480","+","-","-","-","+","-","-",null,"Для получения видео в ПО ITV/Axxon c кодеком H.264 необходимо в web-интерфейсе камеры включить настройки \"H.264 transmission\" и \"Internet mode (over HTTP)\"","To receive video in Axxon software with H.264 codec, enable \"H.264 transmission\" and \"Internet mode (over HTTP)\" settings in the camera web interface."]
["Panasonic i-Pro","Panasonic WJ-GXE500","Encoder ","1.11","4","3","+","+","+",null,null,"640x480 / 640x360 / 720x576","+",null,"+.","-",null,"+","+","+","1. При задействовании на камере H.264 или MPEG-4 на MJPEG-видеопоток накладывается ограничение в 15 fps max\n2. fps для MJPEG потока зависит от количества одновременно задействованных видеоканалов\n3. При выборе других ТВ-стандартов кроме PAL в настройках в ПО Axxon будет доступен MPEG-4, хотя фактически на камере он будет заблокирован\n4. При выборе MPEG-4 в настройках в ПО Axxon будет доступно мегапиксельное разрешение, хотя при MPEG-4 фактически камера его не поддерживает","1. If you enable H.264 or MPEG-4 on the camera, the MJPEG video stream is limited to 15 fps max.\n2. For MJPEG, the frame rate very much depends on how many video channels are used at the same time\n3. If you select any ***TV standard*** other than PAL, the AxxonSoft software shows MPEG-4 as an available option, but the camera itself does not allow this codec. \n4. If you select any MPEG-4, the AxxonSoft software shows a megapixel resolution as an available option, but the camera itself does not allow this resolution for MPEG-4. "]
["Panasonic i-Pro","Panasonic WV-NF284(E)","Camera ","1.60E4","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+",null,null,"+","+","-","1. при включении одновременно MJPEG и MPEG-4, на MJPEG накладывается ограничение по скорости в 5(10) fps - особенность самой камеры, Intellect не причем.\n2. для MPEG-4 ползунок \"Скорость\" регулирует битрейт, поэтому вместе с изменением fps меняется и качество - особенность интеграции в Intellect.\n3. Реле подключается к OUT-GND (срабатывает с задержкой ~5 секунд)","1. when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself, Intellect has nothing to do with it.\n2. for MPEG-4, the ***Rate*** slider changes the bit rate; for this reason, when you adjust the frame rate, you adjust the image quality too - this is how the integration was done in Intellect. \n3. Connect relays to OUT-GND (it works with a delay of around 5 seconds)"]
["Panasonic i-Pro","Panasonic WV-NP240(E)/244(E)","Camera ","1.80E4","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+",null,null,"+","+","-","1. при включении в настройках камеры одновременно MJPEG и MPEG-4 видеопотока, на MJPEG-поток накладывается ограничение по скорости в 5(10) fps - это особенность самой камеры, так камера работает и в \"родном\" софте и в Intellect\n2. для MPEG-4 ползунок \"Скорость\" регулирует битрейт видеопотока, поэтому вместе с изменением fps меняется и качество видеоизображения - так сделано потому что у самой камеры нет настройки \"Скорость\" в чистом виде для MPEG-4 видепотока \n3. У MPEG-4 всего 3 положения кач-ва, а в Intellect их 5, поэтому некотрые будут повторятся - особенность интеграции в Intellect\n4. Реле подключается к OUT-GND","1. when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself, the camera works like this both in its own software and in Intellect. \n2. for MPEG-4, the ***Rate*** slider changes the bit rate of the video stream; for this reason, when you adjust the frame rate, you adjust the image quality too: it was done like this, because for MPEG-4 the camera itself doe not have a \"pure\" Rate setting \n3. For MPEG-4, the camera itself has 3 positions for quality. Because Intellect has 5, some of the positions in Intellect mean one and the same quality - this is how the integration was done.\n4. Connect relays to OUT-GND"]
["Panasonic i-Pro","Panasonic WV-NP502(E)/NW502S(E)","Camera ","1.44","1","3","+","+","+",null,null,"PAL (4:3, 3MP): 2048x1536 (MJPEG) / 1280x960 (H264) / 640x480 (MPEG4) | NTSC (16:9, 3MP): 1920x1080 (MJPEG, H264) / --- (MPEG4)","+","+","+","+",null,"+","+","motion detection.","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.В кодеках MPEG4 и H264 при получении видео по протоколу UDP возможны потери пакетов и рывки видео. В таких случаях рекомендуется использовать протокол RTSP over TCP.Набор разрешений зависит от выбранного режима (1.3 MP, 3MP) и соотношения сторон (4:3, 16:9). В нашем ПО эти настройки реализованы через параметр \"ТВ-стандарт\".Настройки видео (кодек, разрешение, частота кадров) в потоках взаимозависимы. Следить за их совместимостью пользователь должен самостоятельно.Кодеки в потоках 1 и 2 должны совпадать. Одновременно получать с камеры и MPEG4, и H264 нельзя.MPEG4 доступен только в режимах 4:3_3MP и 4:3_1.3MP (PAL)Смена режима 1.3MP - 3MP требует перезагрузки устройства.Для поиска камеры в сети необходимо предварительно настроить постоянную, не ограниченную по времени видимость камеры. Эта настройка осуществляется через веб-интерфейс камеры.Находится в списке неподдерживаемых устройств (общая проблема камер Panasonic). То есть найти устройство можно, но добавить из результатов поиска в конфигурацию нельзя. Добавлять устройство нужно вручную.Из встроенной аналитики в настоящий момент интегрирован детектор лиц, детектор движения не интегрирован.На камере есть 3 программируемых IO-порта. 1й и 3й используются в нашем ПО как лучи, 2й - как реле.","Video transmission (mpeg4/h.264) is implemented via the following protocols: the Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP In Intellect, these protocols correspond to the unicast, tcp, udp, and multicast ***Windows Registry keys***, respectively. For MPEG4 and H.264, when receiving video via the UDP protocol, packets may get lost, video may stop for some time and then continue again. To fix this, use RTSP over TCP. The set of resolutions depends on which mode (1.3 MP, 3MP) and aspect ratio (4:3, 16:9) are selected. Our software implements these settings with the ***TV Standard*** parameter. The video settings (codec, resolution, frame rate) for different streams are interdependent. The user must himself ensure that the settings are compatible. You have to use the same codecs for stream 1 and 2. You cannot get MPEG4 and H.264 streams from the camera at the same time.MPEG4 is available only in 4:3_3MP and 4:3_1.3MP (PAL) modes After you switch resolutions (1.3 MP - 3MP) ), you must restart the device (around 1 minute).To be able to search for the device, set the camera to ***permanent visibility***. Do it in the camera's web interface. This is an unsupported device (a problem shared by Panasonic cameras). That is, the search finds the device, but you cannot add the device directly from the search results. You must add it manually. Of the embedded video analytics, the ***face detector*** is integrated; the motion detector is not integrated. The camera has 3 programmable I/O ports. Our software uses ports 1 and 3 for sensors and port 2 for relays. "]
["Panasonic i-Pro","Panasonic WV-NS202A(E)","Camera ","2.70P7","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","-","+","+","+","-","1. при включении в настройках камеры одновременно MJPEG и MPEG-4 видеопотока, на MJPEG-поток накладывается ограничение по скорости в 5(10) fps - это особенность самой камеры, так камера работает и в \"родном\" софте и в Intellect \n2. Реле подключается к OUT-GND\n","1. when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself, the camera works like this both in its own software and in Intellect. \n2. Connect relays to OUT-GND\n"]
["Panasonic i-Pro","Panasonic WV-NS950(E)/954(E)","Camera ","1.60E3","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+.","-","+","+","+","-","1. при вкл. одновременно MJPEG и MPEG-4, на MJPEG накладывается ограничение по скорости в 5(10) fps - особенность самой камеры\n2. для MPEG-4 ползунок \"Скорость\" регулирует битрейт видеопотока, поэтому вместе с изменением fps меняется и качество видеоизображения - так сделано потому что у самой камеры нет настройки \"Скорость\" в чистом виде для MPEG-4 видепотока\n3. Ползунок \"Качество\" для MPEG-4 видеопотока не работает - особенность интеграции в ПО ITV\n4. Реле подключается к OUT-GND","1. when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself\n2. for MPEG-4, the ***Rate*** slider changes the bit rate of the video stream; for this reason, when you adjust the frame rate, you adjust the image quality too: it was done like this, because for MPEG-4 the camera itself doe not have a \"pure\" Rate setting\n3. For MPEG-4, the Quality slider does not work - this is how the integration was done in the AxxonSoft software\n4. Connect relays to OUT-GND"]
["Panasonic i-Pro","Panasonic WV-NW484S(E)","Camera ","1.60E5","1",null,"+","+",{"$nulls":3},"640x480",{"$nulls":5},"+","+","-","1. при включении в настройках камеры одновременно MJPEG и MPEG-4 видеопотока, на MJPEG-поток накладывается ограничение по скорости в 5(10) fps - это особенность самой камеры, так камера работает и в \"родном\" софте и в Intellect\n2. для MPEG-4 ползунок \"Скорость\" регулирует битрейт видеопотока, поэтому вместе с изменением fps меняется и качество видеоизображения - так сделано потому что у самой камеры нет настройки \"Скорость\" в чистом виде для MPEG-4 видепотока \n3. Реле подключается к OUT-GND","1) when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself, the camera works like this both in its own software and in Intellect. \n2. for MPEG-4, the ***Rate*** slider changes the bit rate of the video stream; for this reason, when you adjust the frame rate, you adjust the image quality too: it was done like this, because for MPEG-4 the camera itself doe not have a \"pure\" Rate setting \n3. Connect relays to OUT-GND"]
["Panasonic i-Pro","Panasonic WV-NW960(E)/964(E)","Camera ","1.60E3","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+.","-","+","+","+","-","1. при вкл. одновременно MJPEG и MPEG-4, на MJPEG накладывается ограничение по скорости в 5(10) fps - особенность самой камеры\n2. для MPEG-4 ползунок \"Скорость\" регулирует битрейт видеопотока, поэтому вместе с изменением fps меняется и качество видеоизображения - так сделано потому что у самой камеры нет настройки \"Скорость\" в чистом виде для MPEG-4 видепотока\n3. Ползунок \"Качество\" для MPEG-4 видеопотока не работает - особенность интеграции в ПО ITV\n4. Реле подключается к OUT-GND","1. when you enable MJPEG и MPEG-4 at the same time, MJPEG is limited to 5(10) fps - this is a limitation of the device itself\n2. for MPEG-4, the ***Rate*** slider changes the bit rate of the video stream; for this reason, when you adjust the frame rate, you adjust the image quality too: it was done like this, because for MPEG-4 the camera itself doe not have a \"pure\" Rate setting\n3. For MPEG-4, the Quality slider does not work - this is how the integration was done in the AxxonSoft software\n4. Connect relays to OUT-GND"]
["Panasonic i-Pro","Panasonic WV-SC385(E)","Camera ","1.05","1","3","+","+","+",null,null,"1280x960","+","+","+.",null,"+","+","+","+","1. При задействовании на камере H.264 или MPEG-4 на MJPEG-видеопоток накладывается ограничение в 15 fps max\n2. Под значениями PAL и NTSC настройки \"ТВ-стандарт\" в ПО ITV/Axxon понимаются форматы видео 4:3 и 16:9 соответственно\n3. При выборе других ТВ-стандартов кроме PAL в настройках в ПО Axxon будет доступен MPEG-4, хотя фактически на камере он будет заблокирован\n4. При выборе MPEG-4 в настройках в ПО Axxon будет доступно мегапиксельное разрешение, хотя при MPEG-4 фактически камера его не поддерживает\n ","1. If you enable H.264 or MPEG-4 on the camera, the MJPEG video stream is limited to 15 fps max.\n2. In the AxxonSoft software, ***TV standard*** means aspect ratio (PAL for 4:3 and NTSC for 16:9).\n3. If you select any ***TV standard*** other than PAL, the AxxonSoft software shows MPEG-4 as an available option, but the camera itself does not allow this codec. \n4. If you select any MPEG-4, the AxxonSoft software shows a megapixel resolution as an available option, but the camera itself does not allow this resolution for MPEG-4.\n "]
["Panasonic i-Pro","Panasonic WV-SC386(E)","Camera","1.81 ","1","3","+","+","+",null,"-","1280x960","+","+",null,null,"+",null,"-",null,"Набор доступных разрешений в ПО ITV зависит от настройки \"Image Capture mode\" в веб-интерфейсе","In AxxonSoft products available permissions depends on \"Image Capture mode\" in camera's web interface."]
["Panasonic i-Pro","Panasonic WV-SC386 (ONVIF) ","Camera ","V.1.61","1","1","+",null,"+",null,null,"1280x960 ","+",{"$nulls":3},"+"]
["Panasonic i-Pro","Panasonic WV-SC588","Camera","1.08","1","3","+",null,"+",null,null,"1920x1080 / 1280x960 / 1280x720","+","+","+","+","+","+","+","-","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.Набор разрешений зависит от выбранного режима (1.3 MP, 2MP) и соотношения сторон (4:3, 16:9). В ПО Axxon эти настройки реализованы через параметр \"ТВ-стандарт\".","Video transmission (mpeg4/h.264) is implemented via the following protocols: the Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. In Intellect, these protocols correspond to the unicast, tcp, udp, and multicast registry keys, respectively. The set of resolutions depends on which mode (1.3 MP, 2MP) and aspect ratio (4:3, 16:9) are selected.  Axxon software implements these settings with the TV Standard parameter.","improved"]
["Panasonic i-Pro","Panasonic WV-SF132(E)","Camera ","1.03","1","3","+",null,"+",null,null,"PAL: 640x480, NTSC: 640x360","+","+",{"$nulls":5},"other detectors","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.Поиск устройств и в Axxon Next и в Интеллект обнаруживает камеру, как неподдерживаемое устройство. Это вина камеры - она присылает некорректные данные.FPS на потоке MJPEG зависит от состояние потоков H264. Если хотя бы один из них включен, FPS с MJPEG не будет превышать 5 кадров в секунду.Чтобы работал встроенный детектор через Onvif необходимо в настройках устройства указать логин и пароль.","Video transmission (mpeg4/h.264) is implemented via the following protocols: the Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP In Intellect, these protocols correspond to the unicast, tcp, udp, and multicast ***Windows Registry keys***, respectively. Both in Axxon Next and Intellect, Search detects the camera as an unsupported device. This is the camera's fault: it sends wrong data. For the MJPEG stream, the frame rate very much depends on the status of the H.264 streams If at least one of them is enabled, MPEG video comes with 5 fps matzo make the embedded detector work via the ONVIF protocol, go to the devices settings and enter the login and password"]
["Panasonic i-Pro","Panasonic WV-SF135(E)","Camera ","1.03","1","3","+",null,"+",null,null,"PAL: 1280x960, NTSC: 640x360","+","+",{"$nulls":5},"motion detection.","Поиск устройств и в Axxon Next и в Интеллект обнаруживает камеру, как неподдерживаемое устройство. Это вина камеры - она присылает некорректные данные.FPS на потоке MJPEG зависит от состояние потоков H264. Если хотя бы один из них включен, FPS с MJPEG не будет превышать 5 кадров в секунду.Чтобы работал встроенный детектор через Onvif необходимо в настройках устройства указать логин и пароль.","Both in Axxon Next and Intellect, Search detects the camera as an unsupported device. This is the camera's fault: it sends wrong data. For the MJPEG stream, the frame rate very much depends on the status of the H.264 streams If at least one of them is enabled, MPEG video comes with 5 fps matzo make the embedded detector work via the ONVIF protocol, go to the devices settings and enter the login and password"]
["Panasonic i-Pro","Panasonic WV-SF332(E)","Camera ","1.03","1","3","+",{"$nulls":4},"640x480 (PAL) / 640x360 (NTSC)",null,"+",{"$nulls":5},"-"]
["Panasonic i-Pro","Panasonic WV-SF335(E) / WV-SF336(E) / WV-SF346","Camera","1.61","1","3","+","+","+",null,null,"PAL: 1280x960 (MJPEG); 640x480 (H264/MPEG4) / NTSC: 1280x720","+","+","+","+","+","+","+","others","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.Кодеки в потоках 1 и 2 должны совпадать. Одновременно получать с камеры и MPEG4, и H264 нельзя.MPEG4 доступен только в режиме PALДля поиска камеры в сети необходимо предварительно настроить постоянную, не ограниченную по времени видимость камеры. Эта настройка осуществляется через веб-интерфейс камеры.Находится в списке неподдерживаемых устройств (общая проблема камер Panasonic). То есть найти устройство можно, но добавить из результатов поиска в конфигурацию нельзя. Добавлять устройство нужно вручную.Из встроенной аналитики интегрирован детектор лиц.","Video transmission (mpeg4/h.264) is implemented via the following protocols: the Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. In Intellect, these protocols correspond to the unicast, tcp, udp, and multicast Windows registry keys, respectively. Codecs for streams 1 and 2 have to be the same. You can not get both MPEG4 and H264 video from this camera at the same time. MPEG4 video is available inly in PAL mode. To be able to discover the device, set the camera to Permanent Visibility. Do it in the camera's web interface. This is an unsupported device (a problem shared by Panasonic cameras). That is, the search finds the device, but you cannot add the device directly from the search results. You must add it manually. Only embedded Facial Recognition has been integrated.","improved"]
["Panasonic i-Pro","Panasonic WV-SF538","Camera","1.31","1","3","+",null,"+",null,null,"2048x1536","+","+","-","-","+","-","-","-","На камере присутствует встроенный детектор лиц. ","There is an on-board Face detection tool.","improved"]
["Panasonic i-Pro","Panasonic WV-SP105(E)","Camera ","1.46","1","3","+",null,"+",null,null,"1280x960 (PAL) / 1280x720 (NTSC)","+","+",{"$nulls":5},"-","Настройки видео (кодек, разрешение, частота кадров) в потоках взаимозависимы. Следить за их совместимостью пользователь должен самостоятельно.\nНаходится в списке неподдерживаемых устройств (общая проблема камер Panasonic). То есть найти устройство можно, но добавить из результатов поиска в конфигурацию нельзя. Добавлять устройство нужно вручную.Для поиска камеры в сети необходимо предварительно настроить постоянную, не ограниченную по времени видимость камеры. Эта настройка осуществляется через веб-интерфейс камеры.","Video settings (codec, resolutions, picture frequency) are interdependent in flows. User shall itself to track their compatibility.\nIt's in the list of unsupported devices (a common problem of the cameras Panasonic). It's possible to find the device but impossible to add it from search results in a configuration. Add the device manually.\nTo find camera on a network it's necessary to set up beforehand the constant which hasn't been restricted on time visibility of the camera. This setup is carried out via the camera web interface."]
["Panasonic i-Pro","Panasonic WV-SP305(E)","Camera ","1.50","1","3","+","+","+",null,null,"1280x960 (PAL) / 1280x720 (NTSC)","+","+","+","+","+","+","+","motion detection.","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.\nВ кодеках MPEG4 и H264 при получении видео по протоколу UDP возможны потери пакетов и рывки видео. В таких случаях рекомендуется использовать протокол RTSP over TCP.\nНастройки видео (кодек, разрешение, частота кадров) в потоках взаимозависимы. Следить за их совместимостью пользователь должен самостоятельно.\nКодеки в потоках 1 и 2 должны совпадать. \nОдновременно получать с камеры и MPEG4, и H264 нельзя.\nНаходится в списке неподдерживаемых устройств (общая проблема камер Panasonic). То есть найти устройство можно, но добавить из результатов поиска в конфигурацию нельзя. Добавлять устройство нужно вручную.Для поиска камеры в сети необходимо предварительно настроить постоянную, не ограниченную по времени видимость камеры. Эта настройка осуществляется через веб-интерфейс камеры.\nИз встроенной аналитики в настоящий момент интегрирован детектор лиц, детектор движения не интегрирован. Детектор движения работает через Onvif.\nЗвук из динамика камеры начинает воспроизводиться с задержкой в несколько секунд. ","In MPEG4 and H264 codecs when obtaining video according to the UDP protocol are possible losses of packets and video breakthroughs. In such cases it is recommended to use the RTSP over TCP protocol.\nVideo settings (the codec, permission, picture frequency) for streams are interdependent. To track their compatibility the user shall independently.\nCodecs in streams 1 and 2 shall match. \nIt is impossible to receive from the camera and MPEG4, and H264 at the same time.\nIs in the list of unsupported devices (a common problem of the cameras Panasonic). It is possible to find the device , but impossible to add from search results in a configuration . To add the device it is necessary manually. For camera search on a network it is necessary to set up beforehand the constant which has not been restricted on time visibility of the camera. This setup is carried out via the camera web interface.\nFrom built-in analytics the face detector is integrated at the moment, motion detector isn't integrated. The motion detector works through Onvif.\nThe sound from the speaker of the camera starts to be reproduced with a time delay in some seconds."]
["Panasonic i-Pro","Panasonic WV-SP306(E)","Camera ","1.04","1","3","+","+","+",null,null,"PAL (4:3): 1280x960 (MJPEG/H264) / 640x480 (MPEG4) | NTSC (16:9): 1280x720 (MJPEG/H264)","+","+","+.","+",null,"+","+","-","В камере 3 стримминга, однако 2 из них - неполноценные, у них один кодек на двоих (MPEG4/H264) . Одновременно получать с камеры и MPEG4, и H264 нельзя.В кодеке H264 возможны задержки и \"рывки\" видео. Для поиска камеры в сети необходимо предварительно настроить постоянную, неограниченную видимость камеры. Эта настройка осуществляется через веб-интерфейс камеры.Поиск обнаруживает камеру как неподдерживаемое устройство - особенность камер Panasonic i-Pro.","The cameras has 3 streams; however, two of them are not full-fledged, they share a codec (MPEG4/H.264). You cannot get MPEG4 and H.264 streams from the camera at the same time. With H.264, sometimes video stops for a while, then starts again. To be able to search for the device, set the camera to ***permanent visibility***. Do it in the camera's web interface. Search detects the camera as unsupported device - this is a limitation of Panasonic i-Pro cameras."]
["Panasonic i-Pro","Panasonic WV-SP509(E) / WV-SF539(E) / WV-SW559(E) / WV-SP508 / WV-SF549 / WV-SF548 / WV-SW558","Camera","1.30","1","3","+",null,"+",null,null,"MJPEG: 2048x1536; H.264: 1920x1080","+","+","+","+","+","+","+","-","Набор доступных разрешений в ПО ITV зависит от настройки \"Image Capture mode\" в веб-интерфейсеНа камере есть 3 программируемых IO-порта. 1й и 3й используются в нашем ПО как лучи, 2й - как реле.Для работы с MJPEG по ONVIF нужно включить в веб-интерфейсе поток H.264, а затем выключить его","In AxxonSoft software, the choice of resolutions depends on Image Capture Mode settings in the camera's web interface. The camera has 3 programmable I/O ports. Our software uses ports 1 and 3 for sensors and port 2 for relays. To work with MJPEG via ONVIF enable H.264 in the camera's web interface and then disable it.","improved"]
["Panasonic i-Pro","Panasonic WV-SW152(E)/-M(E)","Camera ","1.03","1","3","+",null,"+",null,null,"PAL: 800x600, NTSC: 640x360","+","+",{"$nulls":5},"motion detection.","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.Поиск устройств и в Axxon Next и в Интеллект обнаруживает камеру, как неподдерживаемое устройство. Это вина камеры - она присылает некорректные данные.FPS на потоке MJPEG зависит от состояние потоков H264. Если хотя бы один из них включен, FPS с MJPEG не будет превышать 5 кадров в секунду.Чтобы работал встроенный детектор через Onvif, необходимо в настройках устройства указать логин и пароль.","Video transmission (mpeg4/h.264) is implemented via the following protocols: the Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP In Intellect, these protocols correspond to the unicast, tcp, udp, and multicast Both in Axxon Next and Intellect, Search detects the camera as an unsupported device. This is the camera's fault: it sends wrong data. For the MJPEG stream, the frame rate very much depends on the status of the H.264 streams If at least one of them is enabled, MPEG video comes with 5 fps matzo make the embedded detector work via the ONVIF protocol, go to the devices settings and enter the login and password"]
["Panasonic i-Pro","Panasonic WV-SW155(E)/-M(E)","Camera ","1.03","1","3","+",null,"+",null,null,"PAL: 1280x960 NTSC: 1280x720","+","+",{"$nulls":5},"motion detection.","Поиск устройств и в Axxon Next и в Интеллект обнаруживает камеру, как неподдерживаемое устройство. Это вина камеры - она присылает некорректные данные.FPS на потоке MJPEG зависит от состояние потоков H264. Если хотя бы один из них включен, FPS с MJPEG не будет превышать 5 кадров в секунду.Чтобы работал встроенный детектор через Onvif, необходимо в настройках устройства указать логин и пароль.","Both in Axxon Next and Intellect, Search detects the camera as an unsupported device. This is the camera's fault: it sends wrong data. For the MJPEG stream, the frame rate very much depends on the status of the H.264 streams If at least one of them is enabled, MPEG video comes with 5 fps matzo make the embedded detector work via the ONVIF protocol, go to the devices settings and enter the login and password"]
["Panasonic i-Pro","Panasonic WV-SW158 / WV-SF138","Camera","1.05","1","3","+","-","+",null,"-","H264:1280x960 / MJPEG: 2048x1536","+","+","+","-","-","-","-"]
["Panasonic i-Pro","Panasonic WV-SW316(E)/L(E)","Camera ","1.61","1","3","+","-","+",null,null,"1280x720(NTSC)/1280x960(PAL)","+","+","+","+","+","+","+","other detectors","1. Для включения реле через ONVIF необходимо настроить Alarm Terminal 3 в режим AUX output\n2. Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.\n3. Кодеки в потоках 1 и 2 должны совпадать. Одновременно получать с камеры и MPEG4, и H264 нельзя.\n4. MPEG4 доступен только в режиме PAL\n5. Для поиска камеры в сети необходимо предварительно настроить постоянную, не ограниченную по времени видимость камеры. Эта настройка осуществляется через веб-интерфейс камеры.\n6. Находится в списке неопределяемых устройств (общая проблема камер Panasonic). То есть найти устройство можно, но добавить из результатов поиска в конфигурацию нельзя. Добавлять устройство нужно вручную.\n7. Из встроенной аналитики интегрирован детектор лиц.","1. To connect the relay through ONVIF, set up Alarm Terminal 3 to AUX output\n2. Video transmission (mpeg4/h.264) is implemented via the following protocols: the Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP In Intellect, these protocols correspond to the unicast, tcp, udp, and multicast Windows registry keys, respectively.\n3. Codecs for streams 1 and 2 have to be the same. You can not get both MPEG4 and H264 video from this camera at the same time.\n4. MPEG4 video is available inly in PAL mode\n5. To be able to discover the device, set the camera to Permanent Visibility. Do it in the camera's web interface.\n6. This is an unsupported device (a problem shared by Panasonic cameras). That is, the search finds the device, but you cannot add the device directly from the search results. You must add it manually.\n7. Only embedded Facial Recognition has been integrated."]
["Panasonic i-Pro","Panasonic WV-SW316L (ONVIF) ","Camera ","1.66 ","1","1","+",null,"+",null,null,"1280x960","+",null,"+","+",null,null,"+",null,"По ONVIF не работает кодек MPEG4 (особенность устройства).","Via the ONVIF protocol, the MPEG4 codec does not work."]
["Panasonic i-Pro","Panasonic WV-SW355(E)","Camera ","1.49","1","3","+","+","+",null,null,"1280x960 (PAL) / 1280x720 (NTSC)","+","+","+","+","+","+","+","motion detection.","Передача видео (mpeg4/h264) реализована по протоколам Proprietary Unicast UDP, RTSP over TCP, RTSP over UDP, IGMP Multicast UDP. В Интеллекте им соответствуют ключи unicast, tcp, udp, multicast соответственно.\nВ кодеках MPEG4 и H264 при получении видео по протоколу UDP возможны потери пакетов и рывки видео. В таких случаях рекомендуется использовать протокол RTSP over TCP.\nНастройки видео (кодек, разрешение, частота кадров) в потоках взаимозависимы. Следить за их совместимостью пользователь должен самостоятельно.\nКодеки в потоках 1 и 2 должны совпадать. Одновременно получать с камеры и MPEG4, и H264 нельзя.\nНаходится в списке неподдерживаемых устройств (общая проблема камер Panasonic). То есть найти устройство можно, но добавить из результатов поиска в конфигурацию нельзя. Добавлять устройство нужно вручную.\nИз встроенной аналитики в настоящий момент интегрирован детектор лиц, детектор движения не интегрирован. Детектор движения работает через Onvif.\nЗвук из динамика камеры начинает воспроизводиться с задержкой в несколько секунд. ","In MPEG4 and H264 codecs when obtaining video according to the UDP protocol are possible losses of packets and video breakthroughs. In such cases it is recommended to use the RTSP over TCP protocol.\nVideo settings (the codec, permission, picture frequency) for streams are interdependent. To track their compatibility the user shall independently.\nCodecs in streams 1 and 2 shall match. \nIt is impossible to receive from the camera and MPEG4, and H264 at the same time.\nIs in the list of unsupported devices (a common problem of the cameras Panasonic). It is possible to find the device , but impossible to add from search results in a configuration . To add the device it is necessary manually. For camera search on a network it is necessary to set up beforehand the constant which has not been restricted on time visibility of the camera. This setup is carried out via the camera web interface.\nFrom built-in analytics the face detector is integrated at the moment, motion detector isn't integrated. The motion detector works through Onvif.\nThe sound from the speaker of the camera starts to be reproduced with a time delay in some seconds."]
["Panasonic i-Pro","Panasonic WV-SW396(E) / WV-SW395(E) / WV-SW396A / WV-SW395A","Camera","1.44","1","3","+","+","+",null,null,"PAL (4:3, 3MP): 1280x960 (MJPEG, H264) / 640x480 (MPEG4) | NTSC (16:9, 3MP): 1280x720 (MJPEG, H264) / --- (MPEG4)","+","+","+","+","+","+","+","-","Если включен один из потоков H264/MPEG4, на первом потоке (MJPEG) действует ограничение в 5 fps.","If one of the H.264/MPEG4 streams are enabled, the frame rate for the first stream (MJPEG) is 5 fps max. ","improved"]
["Panasonic i-Pro","Panasonic WV-SW458(M) / WV-SF438","Fisheye Camera","1.04","1","3","+","-","+","-","-","2048x1536 (MJPEG) / 1920x1080 (H.264)","+","+","-","-","+","+","+","others","Набор доступных разрешений в ПО ITV зависит от настройки \"Image Capture mode\" в веб-интерфейсеНа камере есть встроенный детектор лиц","In AxxonSoft products available resolutions depend on the Image Capture mode setting in camera web interface. The camera has an on-board Face detection tool."]
["Panasonic i-Pro","Panasonic WV-SW598","Camera ","0.0A","1","3","+",null,"+",null,null,"1920x1080","+","+",null,null,"+",{"$nulls":3},"Набор доступных разрешений в ПО ITV зависит от настройки \"Image Capture mode\" в веб-интерфейсе.","The set of available resolution in Axxon software depends on the \"Image Capture mode\" setting in the web interface."]
["Partizan","Partizan ADF-14S DVR","DVR","1.0.0. build 22","4","1",null,null,"+",null,null,"no test","+"]
["Partizan","Partizan DVR ADH-18V","DVR","1.0.0 build 32","8","2",null,null,"+",null,null,"704x576","+",null,"-","-","-","-","-","-"]
["Pelco","Pelco IDE20DN","Camera ","1.7.8.9111-O3.5288","1","2",null,null,"+",null,null,"1600x1200",null,null,"-","-",null,"+","+","-","Изменение настроек принимается камерой достаточно долго (~1 мин.)Настройки сильно зависят друг от друга. Параметры \"битрейт\", \"интервал включения ключевых кадров\", \"fps\", \"разрешение\" все взаимозависимые: при изменении одного меняются значения всех остальных.В ПО Axxon все настройки установлены от минимального до максимального значения. Поэтому иногда могут возникать несоответствия между настройками в ПО и реальными параметрами видеопотока - особенность интеграции.В Интеллекте в зависимости от выбранных параметров некоторые значения других настроек могут оказаться недоступны. В частности, при максимальной частоте кадров будет недоступна смена разрешений. При необходимости можно настраивать поток в веб-интерфейсе и получать видео в Интеллекте.","The camera takes quite a lot of time to apply changes to video settings (1 minute).The settings depends on each other very much. The Bit Rate, Keyframes Interval, Frame Rate, and Resolution parameters all depends on each other: if you change one of them, all the others change too. In the AxxonSoft software, ***for each parameter, you can set any value, from min. to max [This is how I understand the original sentence, but I am not 100% sure]***. For this reason, sometimes you may get a mismatch between the software's settings and the actual parameters of the video stream - this is how the integration was done. In Intellect, depending on the selected values, some values for some settings are not available. For example, if you select the max. frame rate, then you cannot switch resolutions. If needed, you can configure the stream in the web interface and use Intellect to view video. "]
["Pelco","Pelco IEE20DN","Camera ","1.7.8.8111-03.5288","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":6},"-"]
["Pelco","Pelco IL10","Camera ","1.8.2.4.8310-O3.9119","1","2",null,null,"+",null,null,"1280x720","+"]
["Pelco","Pelco IX10 / ID10 / IE10 / IM10 ","Camera ","1.8.2.11.9080","1","2","+",null,"+",null,null,"1280х1024","+",{"$nulls":6},"-","На камере есть зависимости между разрешением, частотой кадров и битрейтом. Нужно отслеживать зависимости в веб-интерфейсе.","The camera has a few joint settings for resolution, frame rate and bit rate. Check the dependent settings in the web interface."]
["Pelco","Pelco IX30 / ID30 / IE30","Camera ","1.8.2.11.9080","1","2","+",null,"+",null,null,"2048x1536","+",{"$nulls":6},"-"]
["Pelco","Pelco IXE20 / IDE20 / IEE20 ","Camera ","1.8.2.11.9081","1","2","+",null,"+",null,null,"1920x1080","+",null,null,"-",{"$nulls":3},"-","1. Видео в ПО ITV/Axxon можно получать либо только с первого потока, либо одновременно с первого и второго. Получать видео только со второго потока - невозможно, это особенность камеры.\n2. Набор доступных настроек видеопотока (кодек, разрешение, фпс, битрейт) сильно взаимозависим.","1. In the AxxonSoft products, video is available either from stream 1 only, or from stream 1 & 2 at the same time. You cannot get video stream 2 only.\n2. The camera has a few pretty rigid settings for resolution, frame rate, codec and bit rate."]
["Pelco","Pelco Sarix IM10C10","Camera ","1.7.41.9261-O2.6725","1","2","-",null,"+",null,null,"1280x1024","+",{"$nulls":6},"-","1. В ПО ITV нет возможности получать видео только со второго потока. Можно либо только с первого, либо одновременно с обоих потоков.","1. In the AxxonSoft software, you cannot receive video from stream 2 only. Either you get stream 1 or both stream 1 and 2.\n"]
["Pelco","Pelco Sarix IMS0C10-1","Camera ","1.7.8.9260-O2.5288","1","2","+","+","+",null,null,"800x600",null,null,"-","-",{"$nulls":3},"-","Изменение настроек принимается камерой достаточно долго (~1 мин.)Настройки сильно зависят друг от друга. Параметры \"битрейт\", \"интервал включения ключевых кадров\", \"fps\", \"разрешение\" все взаимозависимые: при изменении одного меняются значения всех остальных.  В ПО Axxon все настройки установлены от минимального до максимального значения. Поэтому иногда могут возникать несоответствия между настройками в ПО и реальными параметрами видеопотока - особенность интеграции.","The camera takes quite a lot of time to apply changes to video settings (1 minute).The settings depends on each other very much. The Bit Rate, Keyframes Interval, Frame Rate, and Resolution parameters all depends on each other: if you change one of them, all the others change too.  In the AxxonSoft software, ***for each parameter, you can set any value, from min. to max [This is how I understand the original sentence, but I am not 100% sure]***. For this reason, sometimes you may get a mismatch between the software's settings and the actual parameters of the video stream - this is how the integration was done."]
["Pelco","Pelco Spectra 1080P (S5230)","Camera ","1.9.2.1-20130620-1.9330-A1.9822","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":3},"+",{"$nulls":3},"Параметры \"битрейт\", \"интервал включения опорных кадров\", \"fps\", \"разрешение\" все взаимозависимые: при изменении одного меняется список доступных значений всех остальных. Набор доступных в текущей конфигурации значений этих настроек можно посмотреть в веб-интерфейсе.","Parameters \"bit rate\", \"reference frames range\", \"fps\", \"resolution\" are all interdependent: when you change the list of available values ​​change all the rest. The available values ​​of current configuration can be found in the web interface."]
["Pelco","Pelco Spectra HD 720p (D5118)","Camera ","1.8.2.11-20120623-1.9310-A1.8120","1","2","+",null,"+",null,null,"1280x960","+",{"$nulls":3},"+",{"$nulls":3},"В Интеллекте не применяется максимальное значение FPS. В ПО ITV/Axxon камера интегрирована как D5118 ","1. In AxxonSoft Intellect, you cannot get the max. fps. 2. Camera has been integrated as D5118 in Axxon software."]
["Pelco","Pelco Spectra IV IP (MPEG4)","Camera ","01.00.0015","1",null,"+","+",{"$nulls":3},"704x576",{"$nulls":4},"+",{"$nulls":3},"1. При MJPEG камера поддерживает только 704х576 разрешение. Соответственно в Intellect будет Стандартное\"=\"Высокое\"=\"Полное\"=704 x 576\n\n","1. For MJPEG, the camera support only the 704x576 resolution. For this reason, in Intellect, you have Standard = High = Full= 704 x 576. \n\n"]
["Pelco","Pelco Spectra IV / Exsite IP (TXB-N) ","Camera ","1.8.2.11-20120623-1.2084-O1.8120","1","2","+","+","+",null,null,"704x480","+",null,"+.","-","+","+","-",null,"1. Во втором потоке в разрешении 704x576 частота кадров ограничена: не более 12.5 fps для MJPEG, не более 5 fps для MPEG4/H264.\n2. В ПО ITV нет возможности получать видео только со второго потока. Можно либо только с первого, либо одновременно с обоих потоков. \n3. При добавлении устройства всегда создаются 7 лучей. Все 7 лучей поддерживает модель SD4E35. \nУ модели SD4E23 работает только 1 луч\n4. Настройки видеопотока в продуктах работают только при правильно указанном ТВ-стандарте 5. Для включения/выключения дворника необходимо перейти на пресет №86. Для повторной активации пресета необходимо перейти сначала на любой другой пресет, а затем снова на пресет №86.\n6. Максимальное количество пресетов на камере - 80.","1. For the second stream, if you select the 704x576 resolution, the frame rate is limited: max. 12.5 fps for MJPEG and max. 5 fps for MPEG4/H264.\n2. In the Axxonsoft software, you cannot receive video from stream 2 only. Either you get stream 1 or both stream 1 and 2 at the same time. \n3. When you add the camera, 7 sensors are created. All 7 sensors are supported by SD4E35. \nThe SD4E23 supports only 1 sensor.\n4. Video parameters can be applied only if you select the right TV standard. 5. To turn on/off \"Wash and Wipe\", please go to the preset number 86. To repeat the action, please go to any other preset, and then again to the preset number 86.\n6. The maximum number of presets on the camera is 80."]
["Pelco","Pelco TI3","Thermal Imaging Camera","1.8.2.13-20120816-1.9441-O4.8287","1","2","+",null,"+",null,null,"384x288","+",{"$nulls":6},"-"]
["Pinetron","Pinetron PDR-X7008","DVR","X7K-APP-1.0.3.6","8","1",null,null,"+",null,null,"704x576",null,null,"-","-","-","-","-",null,"Разрешение изменяется только через веб-интерфейс (Установки->Запись)","Resolution changes only via the web interface (Installations-> Record)"]
["Pinetron","Pinetron PDR-XM3104","DVR","XM314-APP-B090910.1880","4","1",null,null,"+.",null,null,"720х288 ","+",null,"-","-","-","-",null,"-","1. Параметры живого потока зависят от настроек потока на запись.\n2. Разрешение изменяется только через веб-интерфейс (Установки->Система) 3. Для корректного отображения видео в ПО ITV необходимо в реестре в папке HKLM/SOFTWARE/ITV/INTELLECT/Video создать ключ MonitorFrameBuffer (строковый параметр) и придать ему значение 5. ","1. Parameters of a live stream depend on settings of a stream for record. \n2. Resolution changes only via the web interface (Installations-> System)"]
["PixEYE","PixEYE MEGA","Camera ","1.4.99","1",null,"+",{"$nulls":4},"1600x1200",{"$nulls":8},"При смене разрешения возможны кратковременные искажения видеопотока - особенность устройства.","When you switch resolutions, video may get distorted for some time - this is a limitation of the device itself. "]
["PixEYE","PixEYE SD1","Camera ","1.4.99","1",null,"+",{"$nulls":4},"720x576",{"$nulls":7},"-","1) данная камера - аналог камеры PixEYE Mega, отличается от неё только отсутствием мегапиксельных разрешений","1) this camera is very similar to the PixEYE Mega camera; the only difference is that this camera does not megapixel resolutions."]
["Probe","Probe PIC-H1300","Camera ","v1.0.0_20110523","1","5","+.","+.","+",null,null,"1280x720",{"$nulls":3},"-",{"$nulls":3},"-"]
["Probe","Probe PIC-H1310T","Camera ","v0.0.1_20110909","1","5","+",null,"+.",null,null,"H264: 1280x720; MJPEG: 720x576","+",null,"+","-",null,"+","+","+","На камере перепутаны микрофон и динамик: микрофон надо подключать к разъему с надписью audio out, а динамик - к audio in.","On the camera the microphone and the loudspeaker are entangled: the microphone is to be connected to the socket with audio out inscription, and the loudspeaker - to audio in."]
["Probe","Probe PIC-H2000T","Camera ","v1.0.4_20120717","1","3","+","+","+",null,null,"H.264: 1920x1080; MJPEG / MPEG4: 1280x720","+",{"$nulls":6},"motion detection"]
["Probe","Probe PID-H1000","Camera ","v1.0.1_20110823","1","5","+","+","+",null,null,"1280x720","+",null,"+","+",null,"+","+","+","1. Для второго потока (MJPEG) при максимальном разрешении (1280x720) максимальный fps составляет 20 кадров в секунду.\n2. \"На размыкание\" луч срабатывает с задержкой в 5-6 секунд - это особенность камеры.","1. The max. fps for stream 2(MJPEG) at max. resolution 1280x720) is 20.\n2. The normally-closed Alarm Input work with a delay (around 5-6 seconds), this is the limitation of the camera.\n"]
["Probe","Probe PIN-H2000","Camera ","1.0.4","1","3","+","+","+",null,null,"1920x1080(H264) / 1280x720(MJPEG/MPEG4)","+"]
["Probe","Probe PMI-400","Camera ","0.10.27_20110819","1","5","+","+","+",null,null,"704x480",{"$nulls":3},"-","+",null,null,"-"]
["Probe","Probe PMI-H2000","Camera ","1.1.0_20130305","1","5","+","+","+",null,null,"1920x1080(H.264) / 1280x720(MJPEG, MPEG-4) ","+",null,"+","+.","+","+","+","motion detection","1. С прошивкой 1.1.0_20130305 камера интегрирована как N1P1-S10H2N_TF01\n2. С разрешением 1920х1080 максимальный fps составляет 15 кадров в секунду\n3. Допустимые диапазоны настроек на том или ином стримминге зависят от текущей конфигурации других стриммингов, зависимость необходимо отслеживать через веб-интерфейс. ","1. With firmware 1.1.0_20130305 camera integrated as N1P1-S10H2N_TF01\n2. Max fps with max resolution 1920x1080 is 15 fps.\n3. Valid ranges of settings for a particular strimming depend on current configuration of other streams, this relationship should be monitored via web-interface."]
["Probe","Probe PTI-503","Camera ","v0.10.15_20110221","1","5","+.","+.","+",null,null,"704x576",{"$nulls":3},"-","+",null,null,"-"]
["QNAP","QNAP VS-12164U-RP Pro / VS-12164U-RP Pro+","NVR","4.0.2","64","2","+","+","+",null,null,"from WEB",null,null,"+",null,"+",{"$nulls":3},"1. Все настройки видеопотока и видеоизображения настраиваются из веб-интерфейса NVR (ограниченный ряд настроек), а также из веб-интерфейса устройств, подключенных к NVR\n2. Через ПО ITV нельзя узнать, что за устройства подключены к NVR\n3. К NVR можно подключить устройства, которые есть у него в списке доступных.","1. All stream settings, however with limitations, are available in the NVR web interface as well as from the web interface of the devices connected to the NVR.\n2. In AxxonSoft software, you can not see what devices are connected to the NVR.\n3. You can connect to the NVR only compatible equipment."]
["QNAP","QNAP VS-xx12Pro / VS-4012U-RP Pro / VS-2112Pro+ / VS-4112Pro+ / VS-4112U-RP Pro+ / VS-6112Pro+ ","NVR","4.0.0","12","2","+","+","+",null,null,"from WEB",null,null,"+.","-","+",null,null,"-","1. Обозначение модели - xx может принимать значения: 20,21,40,41,60,61\n2. Все настройки видеопотока и видеоизображения настраиваются из веб-интерфейса NVR (ограниченный ряд настроек), а также из веб-интерфейса устройств, подключенных к NVR\n3. Через наше ПО нельзя узнать, что за устройства подключены к NVR\n4. К NVR можно подключить устройства, которые есть у него в списке доступных.","1. The model number - xx and currently is: 20,21,40,41,60,61\n2. All stream settings are available in the NVR web interface as well as from the web interface of the devices connected to the NVR.\n3. In the AxxonSoft products, you can not see what devices are connected to the NVR.\n4. You can connect to the NVR only compatible equipment."]
["QNAP","QNAP VS-xx16Pro / VS-4016U-RP Pro / VS-4116Pro+ / VS-4116U-RP Pro+ / VS-6116Pro+ ","NVR","3.6.0","16","2","+","+","+",null,null,"from WEB",null,null,"+.","-","+",null,null,"-","1. Обозначение модели - xx может принимать значения: 40,41,61\n2. Все настройки видеопотока и видеоизображения настраиваются из веб-интерфейса NVR (ограниченный ряд настроек), а также из веб-интерфейса устройств, подключенных к NVR\n3. Через наше ПО нельзя узнать, что за устройства подключены к NVR\n4. К NVR можно подключить устройства, которые есть у него в списке доступных.","1. The model number - xx and currently is: 40,41,61\n2. All stream settings are available in the NVR web interface as well as from the web interface of the devices connected to the NVR.\n3. In the AxxonSoft products, you can not see what devices are connected to the NVR.\n4. You can connect to the NVR only compatible equipment."]
["RIVA","RIVA RC2102HD-5511","Camera ","1.4.0.12","1","2","+",null,"+",null,null,"1920x1080","+"]
["RIVA","RIVA RC3302HD-5344 / RC3702HD-5314","Camera ","1.4.0.12","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":7},"Видеопотоки и встроенные детекторы зависят от ресурсов камеры. В зависимости от конфигурации видеопотока используется определенное количество ресурсов (отображается в вебе, в настройках видеопотока). Включенная VCA аналитика съедает 50% ресурсов. ","Video streams and on-board detection tools depend on camera resources. Different amounts of camera resources are used by different video stream configurations (shown in the camera web interface, in the video stream settings). VCA analytics consume 50% of resources when enabled."]
["RIVA","RIVA RC3502HD-5311 / RC3502HD-5311IR","Camera","1.5.0.12","1","2","+","-","+","-","-","1920x1080","+","-","-","-","-","-","-","-","На камере присутствует видеоаналитика VCAВидеопотоки и встроенные детекторы зависят от ресурсов камеры. В зависимости от конфигурации видеопотока используется определенное количество ресурсов (отображается в вебе, в настройках видеопотока). Включенная VCA аналитика отнимает 50% ресурсов.","Camera has VCA video analytics. Video streams and on-board detection tools depend on camera resources. Different amounts of camera resources are used by different video stream configurations (shown in the camera web interface, in the video stream settings). VCA analytics consume 50% of resources when enabled."]
["RIVA","RIVA RC5500","Camera ","1.06.05","1","2","+","+","+",null,null,"720x576 (PAL) / 720x480 (NTSC)","+",null,"+.","+.","+","+","+",null,"В MJPEG максимальная частота кадров - 5 fps.\nНастройки для аудиовыхода и аудиовхода должны быть одинаковыми.\nЛуч приходит в положение готовности спустя 10-50 секунд после включения в нашем ПО. В дальнейшем замыкание/размыкание луча отрабатывается без задержек.\nАудио-выход камеры воспроизводит звук с задержкой в 5 секунд - проблема камеры.\nЧтобы заработал звук, нужно выставить максимальный уровень громкости на динамике. ","Max frame rate for MJPEG codec is 5 fps.\nSettings for Audio Input and Audio Output should be the same.\nAlarm In comes to a standby position after 10-50 seconds after applying in ITV | AxxonSoft software. Later, closing / opening of Alarm In works without delay.\nAudio Output plays the sound with 5 seconds delay - it's camera's feature.\nTo earn a sound, you must set the maximum volume on the speaker."]
["RIVA","RIVA RC6602HD-5311 ","Camera ","1.4.0.11 ","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":7},"Видеопотоки и встроенные детекторы зависят от ресурсов камеры. В зависимости от конфигурации видеопотока используется определенное количество ресурсов (отображается в вебе, в настройках видеопотока). Включенная VCA аналитика съедает 50% ресурсов.","Video streams and on-board detection tools depend on camera resources. Different amounts of camera resources are used by different video stream configurations (shown in the camera web interface, in the video stream settings). VCA analytics consume 50% of resources when enabled."]
["RIVA","RIVA RC6802HD-6211","Camera","1.5.0.12","1","2","+","-","+","-","-","1920x1080","+","-","-","-","-","-","-","-","На камере присутствует видеоаналитика VCAВидеопотоки и встроенные детекторы зависят от ресурсов камеры. В зависимости от конфигурации видеопотока используется определенное количество ресурсов (отображается в вебе, в настройках видеопотока). Включенная VCA аналитика отнимает 50% ресурсов.","Camera has VCA video analytics. Video streams and on-board detection tools depend on camera resources. Different amounts of camera resources are used by different video stream configurations (shown in the camera web interface, in the video stream settings). VCA analytics consume 50% of resources when enabled."]
["RIVA","RIVA RE1000 / RE110","Encoder ","1.7.0","1","2","+","+","+",null,null,"720x576 (PAL) / 720x480 (NTSC)","+",{"$nulls":3},"+",{"$nulls":3},"Значение параметра \"ТВ-сандарт\" в нашем ПО нужно выбирать в соответствии с реальным ТВ-стандартом видеосигнала, подаваемого на устройство.","In our software, select the value of the ***TV standard*** parameter so that it corresponds to the actual ***TV standard*** of the device's input video signal. "]
["RIVA","RIVA RE4000","Encoder ","1.7.0","4","2","+","+","+",null,null,"720x576 (PAL) / 720x480 (NTSC)","+",{"$nulls":3},"+",{"$nulls":3},"Устройство представляет собой 4-канальный видеосервер. Однако каждый канал имеет отдельный ip-адрес. Поэтому в нашем ПО каждому каналу сервера соответствует независимое ip-устройство. То есть для получения видео со всех 4-х каналов нужно создать 4 устройства \"RIVA RE4000\".При этом управление внешним поворотным устройством поддерживает только первый канал видеосервера.Значение параметра \"ТВ-сандарт\" в нашем ПО нужно выбирать в соответствии с реальным ТВ-стандартом видеосигнала, подаваемого на устройство.","This device is a 4-channel video encoder. However, each channel has its own IP address. For this reason, in our software, each channel corresponds to a separate IP device. That is, to receive video from all 4 channels, you must create 4 RIVA RE4000 devices. Only the first channel supports pan/tilt drives. In our software, select the value of the ***TV standard*** parameter so that it corresponds to the actual ***TV standard*** of the device's input video signal."]
["RVi","RVi-HR16/4","DVR","2.610.0000.0 Build 2013-4-12","16","2",null,null,"+",null,null,"704x576","+",null,"+","-","+.","+","+","-"]
["Samsung electronics","Samsung SNC-B2315","Camera ","2.10_090521","1",null,"+","+",{"$nulls":3},"720x576",null,null,"+","-",null,"+","+","-"]
["Samsung electronics","Samsung SNC-B2331P","Camera ","v1.00-090910","1",null,"+","+","+",null,null,"704x576",{"$nulls":5},"+.","+","-"]
["Samsung electronics","Samsung SNC-B2335P","Camera ","1.10_100129","1",null,"+","+","+",null,null,"704x576",null,null,"+","-",null,"+","+","-","1. Камера может выдавать два независимых видеопотока с различыми настройками. Для этого в ПО ITV создаются два граббера и настраиваются они независимо друг от друга.","1. The camera supports two independent video streams, with different settings. For this, create 2 grabbers in Intellect and configure the grabbers independently. "]
["Samsung electronics","Samsung SNC-B5368P","Camera ","v1.00-090910","1",null,"+","+","+",null,null,"704x576",{"$nulls":5},"+","+","-"]
["Samsung electronics","Samsung SNC-B5395P","Camera ","v2.10_090521","1",null,"+","+",{"$nulls":3},"720x576",null,null,"+","-",null,"+","+","-"]
["Samsung electronics","Samsung SNC-B5399P","Camera ","1.10_100129","1",null,"+","+","+",null,null,"704x576",null,null,"+","-",null,"+","+","-","1. Камера может выдавать два независимых видеопотока с различыми настройками. Для этого в ПО ITV создаются два граббера и настраиваются они независимо друг от друга.","1. The camera supports two independent video streams, with different settings. For this, create 2 grabbers in Intellect and configure the grabbers independently."]
["Samsung electronics","Samsung SNC-C6225P","Camera ","1.01","1",null,"+","+",{"$nulls":3},"720x576",{"$nulls":3},"-","+","+","+","-","Звук остался непроверенным (микрофон подключается через спецразьем, которого у нас нет).Тревога по замкнутому лучу поступает с перебоями.","We did not manage to test audio (the microphone connects via a special connector, which we do not have).When you close the sensor, it does send alarms, but not always."]
["Samsung electronics","Samsung SNC-C7225P","Camera ","1.01","1",null,"+","+",{"$nulls":3},"720x576",{"$nulls":3},"-","+","+","+","-","1. Звук остался непроверенным (микрофон подключается через спецразьем, которого у нас нет)","1. We did not manage to test audio (the microphone connects via a special connector, which we do not have)."]
["Samsung electronics","Samsung SNC-C7478P","Camera ","v1.01_090625","1",null,"+","+",{"$nulls":3},"720x576",null,null,"+","-","+.","+","+","-","1) Рекомендуется в настройках самой камеры отключить режим De-Interlace, иначе при Высоком разрешении видео в Inellecte искажено (эффект ступенек)\n2) Настройки Яркость и Контраст не работают на самой камере","1) In the camera's settings, disable the De-Interlace mode; otherwise, with the Full resolution, video is distorted in Intellect (aliasing)\n2) The Brightness and Contrast settings do not work on the camera itself"]
["Samsung electronics","Samsung SNC-M300P","Camera ","2.10_090521","1",null,"+","+",{"$nulls":3},"2048*1536(MJPEG)/640*480(MPEG-4)",null,null,"+","-",null,"+","+","-","1) в MPEG-4 есть только одно разрешение 640*480\n2) fps в MPEG-4 и MJPEG зависят друг от друга (т.е. что бы получить максимум fps в MJPEG нужно выставить минимум fps в MPEG-4 и наоборот)\n ","1) for MPEG-4, you have only one resolution, 640*480\n2) the frame rates for MPEG-4 and MJPEG depend on each other (that is, to get the max. frame rate for MJPEG, you must set the min. frame rate for MPEG-4, and the other way around)\n "]
["Samsung Techwin","Samsung SNB-1000(P)","Camera ","1.00_100715","1","3","+","+","+",null,null,"640x480",{"$nulls":6},"-","-"]
["Samsung Techwin","Samsung SNB-1001","Camera ","1.00_111226","1","2","+",null,"+",null,null,"640x480","+",null,"+","+",null,"+",null,"+"]
["Samsung Techwin","Samsung SNB-2000(P)","Camera ","1.41","1","2","+","+","+",null,null,"704x576","+",{"$nulls":4},"+","+","+","Прошивка 1.41: камера должна работать через Onvif, но не работает - проблема устройства.","The 1.41 firmware: the camera is supposed to work via the ONVIF protocol, but it does not - this is a problem of the device itself. "]
["Samsung Techwin","Samsung SNB-3000(P)","Camera ","1.41","1","2","+","+","+",null,null,"704x576",null,null,"+","-",null,"+","+","+"]
["Samsung Techwin","Samsung SNB-3002","Camera ","1.00_120114","1","3","+","+","+",null,null,"704x576","+",null,"+","+",null,"+","+","+","ТВ-стандарт интегрирован для поддержки моделей с разными ТВ-стандартами. Сами камеры поддерживают либо только PAL либо только NTSC.","The TV-standard is integrated to support models with different TV-standards. Cameras themselves support either PAL or only NTSC."]
["Samsung Techwin","Samsung SNB-5000","Camera ","1.20_101018","1",null,"+","+","+",null,null,"1280x1024",null,null,"+","-",null,"+","+","-"]
["Samsung Techwin","Samsung SNB-5001 / SND-5011 / SND-5061","Camera","1.00_120521","1","9","+",null,"+",null,null,"1280x1024","+",{"$nulls":4},"+",null,"+",null,null,"improved"]
["Samsung Techwin","Samsung SNB-5004 / SNB-5003 / SNV-5084 / SND-5084 / SND-5083","Camera","1.11_131011","1","2","+","-","+","-","-","1280x1024","+","-","+","+","+","+","+","motion detection; audio detection; tampering detection; others","Диапазон битрейта зависит от значения разрешенияДля настройки профиль нельзя выставить режим базовый если для настройки статическая кодировка стоит режим CAVLCНа камере есть детектор лиц, анализ ситуацииИз двух детекторов: \"детектор ситуации\" и \"анализ ситуации\" одновременно можно создать только один","Bitrate range depends on the resolution. You cannot set the base mode for the Profile setting, if there is CAVLC mode for the static coding. There are Situational Analysis and Face detection tools. You can create only one detection tool: either Situational Analysis or Face detection tool."]
["Samsung Techwin","Samsung SNB-6004 / SNB-6003 / SND-6084 / SND-6083","Camera","1.00_130412","1","9","+",null,"+",null,null,"1920x1080","+",null,"+","+","+","+","+","motion detection; audio detection; tampering detectionothers","Прочие встроенные детекторы:Появление / исчезновение объекта в областиВход / выход объекта из областиПересечение линииДетектор лицПри работе со встроенным детектором \"Анализ ситуации\" нужно иметь в виду, что он позволяет детектировать либо появление/исчезновение объекта в заданной области, либо вход/выход объекта из области. И то и другое одновременно детектировать нельзя, это особенность прошивки.","Other on-board detection tools: Object appearance/disappearance from area, Object entry/exit from area, Line crossing and Face detection tool. When using the on-board Situational Analysis detection tool, remember that it allows detecting either appearance/disappearance of an object in a selected area or the entry/exit of an object from an area. But it is not possible to detect both at the same time, due to firmware limitations.","improved"]
["Samsung Techwin","Samsung SNB-7000","Camera ","1.10_110725","1","2","+",null,"+",null,null,"2048x1536","+",null,"+","+","-","+","+","+","По Onvif работает только в режиме совместимости. Работает только получение H264 видео, звука и релеПосле смены ТВ-стандарта нужно заново настраивать параметры видео, изображения, встроенной аналитикиПри первом использовании аудио-выхода звук камерам начинает воспроизводить звук через ~5 секунд - особенность интеграции.","Via the ONVIF protocol, it works only in compatibility mode. Only the following works: H.264 video, audio, and the relay After you switch ***TV standards***, you have to configure video and embedded video analytics again. When you use the audio output for the first time, you hear audio only after around 5 seconds - this is how the integration was done."]
["Samsung Techwin","Samsung SNB-7001 / SND-7011 / SND-7061 ","Camera","1.00_120622","1","2","+","-","+","-","-","2048x1536","+","-","-","-","-","+","-","+"]
["Samsung Techwin","Samsung SNB-7002 / SND-7082 / SNV-7082 / SNO-7082R","Camera","1.00_121005","1","2","+","-","+","-","-","2048x1536","+","-","+","+","-","+","+","motion detection; tampering detection; others","Встроенные детекторы: Анализ ситуации, Детектор лицКамера не поворотная, но имеет встроенный трансфокатор ","On-board detection tools: Situational Analysis and Face detection tool. This is not a PTZ camera, but it has a built-in zoom lens."]
["Samsung Techwin","Samsung SND-1010(P)","Camera ","1.02_101122","1","3","+","+","+",null,null,"640x480",{"$nulls":6},"-","-"]
["Samsung Techwin","Samsung SND-1011 ","Camera ","1.00_111226 ","1","2","+",null,"+",null,null,"640x480","+",{"$nulls":4},"+",null,"+"]
["Samsung Techwin","Samsung SND-1080 / SNV-1080 / SNV-1080R","Camera ","2.00_121027","1","2","+",null,"+",null,null,"640x480","+",null,"+","+",null,"+",null,"+"]
["Samsung Techwin","Samsung SND-3080C","Camera ","1.41","1","2","+","+","+",null,null,"704x576","+",{"$nulls":4},"+.","+","-"]
["Samsung Techwin","Samsung SND-3080F","Camera ","1.30","1","2","+","+","+",null,null,"704x576",{"$nulls":5},"+","+","-","Прошивка 1.30: устройство обнаруживается поиском как поддерживающее Onvif, но работать через Onvif не будет. Проблема самого устойства.При добавлении устройства с помощью поиска прошивку нужно выбирать вручную: автоматически она не определяется.При максимальных настройках камера передает видео с максимальной частотой кадров ~15-20 fps. Ограничение самого устройства. ","The 1.30 firmware: Search detects the camera as a device that supports ONVIF, but the camera does not work via the ONVIF protocol. This is a problem of the device itself. If you add the device using the search, you must select the firmware manually: it is not detected automatically. With the max. settings, the camera send video at around 15-20 fps.  This is a limitation of the device itself. "]
["Samsung Techwin","Samsung SND-3082 / SNV-3082","Camera ","1.00_111204","1","3","+","+","+",null,null,"704x576","+",null,"+","+",null,"+","+","+","ТВ-стандарт интегрирован для поддержки моделей с разными ТВ-стандартами. Сами камеры поддерживают либо только PAL либо только NTSC.","TV standard is integrated to support models with different TV standards. Cameras support either PAL or NTSC."]
["Samsung Techwin","Samsung SND-5010","Camera ","1.00_120626","1","2","+",null,"+",null,null,"1280x1024","+",{"$nulls":6},"motion detection; tampering detection"]
["Samsung Techwin","Samsung SND-5080","Camera ","1.33_110218","1","3","+","-","-",null,null,"1280x1024",null,null,"+.","-",null,"+","+","-"]
["Samsung Techwin","Samsung SND-6084 / SND-6084R / SNV-6084R / SNO-6084R","Camera","2.21_131008","1","9","+",null,"+",null,null,"1920x1080","+",null,"+","+","-","+","+","motion detection; audio detection; tampering detection; others","Диапазон битрейта зависит от значения разрешенияДля настройки профиль нельзя выставить режим базовый если для настройки статическая кодировка стоит режим CAVLCНа камере присутствует встроенная аналитика:Детектор лицАнализ ситуации ","Bitrate range depends on the resolution. You cannot set the base mode for the Profile setting, if there is CAVLC mode for the static coding. There are Situational Analysis and Face detection tools.","improved"]
["Samsung Techwin","Samsung SND-7080 /SND-7080F / SNO-7080R / SNV-7080R ","Camera ","1.20_111227","1","2","+",null,"+",null,null,"PAL: 2048x1536, NTSC: 1920x1080","+",null,"+","+",null,"+","+","motion detection and others"]
["Samsung Techwin","Samsung SNF-7010(V) ","Fisheye Camera","1.00_130806","1","2","+","-","+",null,"-","2048x1536","+",{"$nulls":3},"-","-","-",null,"Если в ПО, после создания зоны детектирования, менять настройки \"отразить вертикально\" и \"отразить горизонтально\", то созданная на камере зона также отобразиться зеркально/вертикально и перестанет соответствовать зоне, установленной в продукте. ","If in AxxonSoft products, after area zone detection created, you will change the settings \"vertical reflect\" and \"horizontal reflect\", then created area zone will also be changed to mirror/vertical display and will not longer match the zone established in the product."]
["Samsung Techwin","Samsung SNO-1080R","Camera ","1.00_111226","1","2","+",null,"+",null,null,"640x480","+",{"$nulls":4},"+",null,"+"]
["Samsung Techwin","Samsung SNO-5080R","Camera ","0.17_110222","1","3","+","+","+",null,null,"1280x1024","+",{"$nulls":6},"+"]
["Samsung Techwin","Samsung SNO-6011R / SND-6011R","Camera","1.11_131011","1","2","+","-","+","-","-","1920x1080","+","-","-","-","-","-","-","motion detection; tampering detection","Диапазон битрейта зависит от значения разрешенияДля настройки профиль нельзя выставить режим базовый если для настройки статическая кодировка стоит режим CAVLCНа камере есть детектор лиц, анализ ситуации","Bitrate range depends on the resolution. You cannot set the base mode for the Profile setting, if there is CAVLC mode for the static coding. There are Situational Analysis and Face detection tools."]
["Samsung Techwin","Samsung SNP-3120V","Camera ","1.22_110120_1","1","3","+","+","+",null,null,"704x576",{"$nulls":4},"+","+","+","-","Событие о срабатывании лучей приходит с задержкой (~5 сек.) - особенность камеры.","Notifications on a sensor going off arrive with a delay (around 5-10 seconds). This is a limitation of the camera itself."]
["Samsung Techwin","Samsung SNP-3370","Camera ","1.20_101006","1","2","+","+","+",null,null,"704x576",null,null,"+","-","+","+","+","motion detection.","Перед работой с реле необходимо в веб-интерфейсе параметру \"duration\" присвоить значение \"always\"При работе со встроенным детектором зоны детектирования приходится создавать через веб-интерфейс.По утверждению производителя интеграция настроек изображения сейчас невозможна.В видеопотоке \"0. MJPEG\" максимальная частота кадров 10 fps доступна для выбора только в том случае, когда в потоке \"1. MPEG4/H.264 \" выбран кодек MPEG4","Before using the camera, go to the web interface and set the Duration parameter to \"always \"When working with the embedded detector, you have to use the web interface to create detection areas. According to the vendor, currently it is not possible to integrate ***basic video settings*** (?).For the 0. MJPEG stream, you can select the max. frame rate (10 fps) only after you select the MPEG4 codec for the 1.MPEG4/H.264 codec."]
["Samsung Techwin","Samsung SNP-3371(H/TH) / SNP-3302(H)","Camera ","1.01_111121","1","3","+","+","+",null,null,"704x576","+",null,null,"+.","+.","+","+","motion detection.","1. Поиск не возвращает прошивку. Правильную версию нужно выбрать самостоятельно.\n2. Луч срабатывает с задержкой (1 сек).\n3. В мультипотоковом режиме максимальная суммарная частота кадров с обоих потоков - 25 fps.\n4. Через Onvif работает получение видео с некоторыми настройками видео и изображения, телеметрия. На сайте onvif.org камера официально не заявлена как поддерживающая Onvif.","1. Search doesn't restore a firmware. It's necessary to choose the correct version of firmware manually.\n2. Alarm in triggers with a delay (1 second).\n3. In a multi-stream mode the maximum total frame rate from both streams is 25 fps.\n4. Video receiving with some settings of video and the image, telemetry works via Onvif. At www.onvif.org the camera isn't officially declared as Onvif-supporting.\n"]
["Samsung Techwin","Samsung SNP-3430H","Camera ","1.11_111104","1","3","+","+","+",null,null,"704x576","+",{"$nulls":3},"+",null,null,"motion detection."]
["Samsung Techwin","Samsung SNP-5200(H)","Camera ","1.00_110309","1","3","+","+","+",null,null,"1280x1024","+",{"$nulls":3},"+"]
["Samsung Techwin","Samsung SNP-5300/H","Camera ","1.10_130523","1","2","+",null,"+",null,null,"1280x1024","+",null,"+","-","+","+","+","motion detection; audio detection; tampering detection; others","На камере присутствуют детектор лиц и детектор \"анализ ситуации\"","On-board detection tools: Situational Analysis, Face Detection Tool."]
["Samsung Techwin","Samsung SNP-6200 / SNP-6200H","Camera ","1.00_120302","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+.","+.","+","+","motion detection and others","1. Список встроенных детекторов камеры:\nИзменение положения\nВход в область\nВыход из области\nИсчезновение из области\nПоявление в области\nПересечение линии","1. Video analytics embedded in the cameras include:\nTampering\nEnter/Exit\nAppear/Disappear\nVirtual Line\n"]
["Samsung Techwin","Samsung SNP-6200RH","Camera","1.11_131002","1","2","+","-","+",null,"-","1920x1080","+",{"$nulls":3},"+",null,"-"]
["Samsung Techwin","Samsung SNV-3080P","Camera ","1.13","1","2","+","+","+",null,null,"704x576",null,null,"+","+",null,"+","+","+"]
["Samsung Techwin","Samsung SNV-3120P","Camera ","1.20_101123","1","3","+","+","+",null,null,"704x576",null,null,"+","-","+.","+","+","-","Камера не PTZ, телеметрия цифроваяЦифровое увеличение иногда срабатывает с ошибками: сразу в максимум. Проблема устройства.","This is not a PTZ camera, but it has digital telemetry Sometimes digital zoom does not work correctly: it goes to the max. zoom from the start. This is a limitation of the device itself."]
["Samsung Techwin","Samsung SNV-5080R","Camera ","1.00_110421","1","3","+","+","+",null,null,"1280x1024","+",{"$nulls":6},"motion detection."]
["Samsung Techwin","Samsung SNV-6012M","Camera","1.11_131011","1","2","+","-","+",null,"-","1920x1080","+",null,"-","-","-","-","-","motion detection.; hacking detector"]
["Samsung Techwin","Samsung SNV-6084","Camera","1.11_131011","1","2","+","-","+","-","-","1920x1080","+","-","+","+","-","+","+","motion detection; audio detection; tampering detection; others"]
["Samsung Techwin","Samsung SNZ-5200","Camera ","1.00_110218","1","3","+","+","+",null,null,"1280x1024","+"]
["Samsung Techwin","Samsung SPE-100P","Encoder ","1.21_101213","1","3","+","+","+",null,null,"640x480",null,null,"+","-","+","+","+","-"]
["Samsung Techwin","Samsung SPE-101","Encoder ","1.00_110829","1","3","+","+","+",null,null,"704x576","+",{"$nulls":3},"+",null,null,"motion detection.","Настройка ТВ-стандарта сделана для поддержки моделей с разными ТВ-стандартами.","The TV-standard is configured to support models with different TV-standards"]
["Samsung Techwin","Samsung SPE-400","Encoder ","1.00_110114","4","3","+","+","+",null,null,"704x576","+",{"$nulls":6},"motion detection.","1. устройство представляет из себя 4-х канальный ip-видеосервер, причем каждый канал имеет свой ip-адрес, а значит является отдельным граббером в ПО ITV/Axxon\n2. Задать области детектированя встроенной аналитики в ПО Axxon нельзя. Особенность интеграции","1. the device is a 4-channel video encoder; because each channel has its own IP address, it has a separate grabber in the AxxonSoft software.\n2. In AxxonSoft software, you cannot set detection areas for the embedded video analytics. This is how the integration was done."]
["Santec","Santec SNC-637ID","Camera ","3.8.4","1","1","+","+",{"$nulls":3},"720x576","+",{"$nulls":3},"+","+","+","-","Событие о прекращении тревоги по лучу приходит с ~10-секундной задержкой. Особенность камеры.","Notifications on a sensor going off arrive with a delay (around 10 seconds). This is a limitation of the camera itself."]
["Sanyo","Sanyo VCC-HD2100P","Camera ","Main 1.02-02 & Sub 1.01-00 & 2.03-08","1","2",null,null,"+",null,null,"2288x1712(MJPEG) / 1600x1200(H.264)","+",{"$nulls":3},"+","+","+","-","1. ограничение fps самого устройстваMJPEG:\n-Полное 3-5 fps (в завис. от кач-ва)\n-Высокое 10-12 fps (в завис. от кач-ва)\n-Стандартное 25 fps\nH.264:\n-во всех разрешениях при любом качестве 25 fps\n2. Полноценная работа видео реализована только в режиме \"4:3\". В режиме \"16:9\" может быть недоступным максимальное разрешение.\n3. Камера не PTZ, но есть настраиваемый фокус, в ПО ITV работает в телеметрии.\n","1. The camera itself has the following frame rate limits: MJPEG:\n- Full resolution 3-5 fps (depending on the quality)\n- High resolution 10-12 fps (depending on the quality)\n- Standard resolution 25 fps\nH.264:\n25 fps for any resolution and any quality\n2. Full-fledged video is implemented only for 4:3 mode. In 16:9 mode, the max. resolution is not available sometimes. \n3. This is not a PTZ camera, but it has adjustable zoom; in the AxxonSoft software, telemetry works. \n"]
["Sanyo","Sanyo VCC-HD2300P","Camera ","Main 2.03-02 & Sub 1.01-00","1","2","+",null,"+",null,null,"2288x1712(MJPEG) / 1600x1200(H.264)","+",{"$nulls":4},"+","+","-","Ограничение fps самого устройстваMJPEG:Полное 3-5 fps (в завис. от кач-ва)Высокое 10-12 fps (в завис. от кач-ва)Стандартное 25 fpsH.264:Во всех разрешениях при любом качестве 25 fpsПереключение соотношения сторон 4:3 - 16:9 релизовано в Axxon Next (и только в Axxon Next) посредством смены ТВ-стандарта.Камера поддерживает управление фокусом - это интегрировано как частичная телеметрия.","The camera itself has the following frame rate limits: MJPEG:- Full resolution 3-5 fps (depending on the quality)- High resolution 10-12 fps (depending on the quality)- Standard resolution 25 fpsH.264:25 fps for any resolution and any quality Switching aspect ratios (4:3 - 16:9) is implemented in Axxon Next (and only in Axxon Next) as switching ***TV standards***.The camera supports zoom - this is integrated as partial telemetry."]
["Sanyo","Sanyo VCC-HD2500P","Camera ","1.00-08 (100107-02)","1","4","+",null,"+",null,null,"PAL: 2280x1712 (MJPEG), 1600x1200 (H264); PAL16:9: 1920x1080",null,null,"+","-",null,"+","+","-"]
["Sanyo","Sanyo VCC-HD4600P","Camera ","CAM MAIN Ver. 1.02-00 (100604-00) & CAM SUB Ver. 1.01-00 (100528-00)","1",{"$nulls":3},"+",null,null,"2288x1712(MJPEG) / 1600x1200(H.264)",null,null,"+","-","+","+","+","-","1. ограничение fps самого устройстваMJPEG:\n-Полное 3-5 fps (в завис. от кач-ва)\n-Высокое 10-12 fps (в завис. от кач-ва)\n-Стандартное 25 fps\nH.264:\n-во всех разрешениях при любом качестве 25 fps\n2. Полноценная работа видео реализована только в режиме \"4:3\". В режиме \"16:9\" может быть недоступным максимальное разрешение.","1. The camera itself has the following frame rate limits: MJPEG:\n- Full resolution 3-5 fps (depending on the quality)\n- High resolution 10-12 fps (depending on the quality)\n- Standard resolution 25 fps\nH.264:\n25 fps for any resolution and any quality\n2. Full-fledged video is implemented only for 4:3 mode. In 16:9 mode, the max. resolution is not available sometimes. "]
["Sanyo","Sanyo VCC-HD5600P","Camera ","2.03-05","1","2",null,null,"+",null,null,"1600x1200",null,null,"+","-","+","+","+","-","Зум срабатывает с задержкой - особенность камерыВ Интеллекте скорость поворота (телеметрии) нужно устанавливать в диапазоне [1,8] - особенность устройства.В H264 при высоких разрешениях (начиная с 1024х768) набор допустимых значений параметра \"Интервал включения опорных кадров\" сужается до [15, 100]Ограничения частоты кадров при высоких разрешениях:MJPEG:800x600: 12.5 fps1024x768: 12.5 fps1280x960: 10 fps1600x1200: 5 fpsH264: в зависимости от текущего выбранного разрешения в MJPEGначиная с DP 3.2.4.643 в ПО Intellect можно получить одновременно два независимых виодеопотока с камеры, для этого на одном граббере необходимо создать 2 камеры с номерами каналов 1 и 2, но надо помнить что в возмодность открытия очередного видеопотока на самой камере очень сильно зависит от настроек уже существующих видеопотоков, таким образом сама камера не позволяет создать много независимых видеопотоков с максимальными настройками.","Zoom works with a delay - this is a limitation of the camera itself In Intellect, set the PTZ (telemetry) speed to a value between 1 and 8 - this is a limitation of the camera itself. For H.264, for high resolutions (starting from 1024x768), the range of the available values for the Keyframes Interval parameter becomes as narrow as [15, 100]Frame rate limits for high resolutions:MJPEG:800x600: 12.5 fps1024x768: 12.5 fps1280x960: 10 fps1600x1200: 5 fpsH264: depends on the currently selected resolution for MJPEGstarting from DP 3.2.4.643, in Intellect, you can get two independent video streams at the same time; to do this, for the same grabber create 2 cameras and set their channel numbers to 1 and 2; note that whether you can open a new stream on the camera itself depends very much on the settings of the already existing streams; thus, the camera itself does not allow you to create many independent streams with max. settings."]
["Sanyo","Sanyo VDC-HD3100P","Camera ","Main 1.02-02 & Sub 1.01-00","1",{"$nulls":3},"+",null,null,"2288x1712(MJPEG) / 1600x1200(H.264)",{"$nulls":4},"+","+","+","-","1. ограничение fps самого устройстваMJPEG:\n-Полное 3-5 fps (в завис. от кач-ва)\n-Высокое 10-12 fps (в завис. от кач-ва)\n-Стандартное 25 fps\nH.264:\n-во всех разрешениях при любом качестве 25 fps\n2. Полноценная работа видео реализована только в режиме \"4:3\". В режиме \"16:9\" может быть недоступным максимальное разрешение.\n3. Камера не PTZ, но есть настраиваемый фокус, в ПО ITV работает в телеметрии.","1. The camera itself has the following frame rate limits: MJPEG:\n- Full resolution 3-5 fps (depending on the quality)\n- High resolution 10-12 fps (depending on the quality)\n- Standard resolution 25 fps\nH.264:\n25 fps for any resolution and any quality\n2. Full-fledged video is implemented only for 4:3 mode. In 16:9 mode, the max. resolution is not available sometimes. \n3. This is not a PTZ camera, but it has adjustable zoom; in the AxxonSoft software, telemetry works."]
["Sentry360","Sentry360 FS-IP3000","Fisheye Camera","sr20130717NSA","1","2","+",null,"+",null,null,"2048x1536(H.264) / 1920x1080(MJPEG)","+",{"$nulls":7},"После смены режима ТВ-стандарта камера перезагружается.","After TV-standard changing the camera will be rebooted."]
["Sentry360","Sentry360 FS-IP5000","Camera ","442 ","1","2","+",null,"+",null,null,"2560x1920","+",{"$nulls":6},"-","Частота кадров сильно зависит от настроек видео и изображения. Максимальная частота кадров - 15 fps.","The frame rate very much depends on the video settings. The max. frame rate is 15 fps. "]
["Sentry360","Sentry360 IS-DM 220","Camera ","y20120224ANS","1","3","+",null,"+",null,null,"1920x1080","+",null,"+","+",null,"+","+","+","1. В разрешении 1920х1080 максимальный fps на камере равен 12.\n2. Настройки аудио-входа и аудио-выхода должны быть одинаковыми.","1. With the 1920x1080 resolution, the camera allows max. 12 fps. \n2. Settings of an audio input and audio output shall be identical."]
["Sentry360","Sentry360 IS-IP14K-DN","Camera","462","1","2","+","-","+","-","-","4592x3280","+",null,"-","-","-","-","-","-","Максимальное значение FPS зависит от выбранного значения разрешения.Значение разрешения в продукте зависит от значения настройки Size, в веб-интерфейсе камеры.","The max. fps rate depends on the selected resolution. Resolution depends on the Size setting in the camera web interface. "]
["SimpleIP Cam","SimpleIP Cam SPC series","Camera ","06.00.03.02","1","1","+",null,"+",null,null,"704x576","+",null,"+","-",null,"-","+","+","1. Количество реле зависит от конкретной модели подключаемой камеры\n2. Ползунок \"Качество\" в ПО Intellect регулирует битрейт видеопотока","1. The number of relays depends on the model of a particular camera. In Intellect, the Quality slider adjusts the video bit rate. "]
["SimpleIP Cam","SimpleIP Cam SPC series","Camera ","06.00.16.03","1","1","+",null,"+",null,null,"704x576","+",null,"-","-","+",null,null,"-","1. Ползунок \"Качество\" в ПО Intellect регулирует битрейт видеопотока\n","1. In Intellect, the Quality slider adjusts the video bit rate.\n"]
["SimpleIP Cam","SimpleIP Cam SPC series","Camera ","06.00.10.03","1","1","+",null,"+",null,null,"704x576","-",null,"-","-",null,"-","+","-"]
["SimpleIP Cam","SimpleIP Cam SPCHD series","Camera ","1.2.24","1","9","+","+.","+",null,null,"2048x1536(MJPEG) / 1280x960(MPEG-4) / 1920x1072(H.264)",null,null,"+.",null,null,"-","-",null,"Настройки яркость, контраст, резкость, цветность не работают на самой камере с прошивкой 1.2.24В MJPEG при 2048х1536 максимальный fps = 15 (ограничение самой камеры)В H.264 при 1920х1080 максимальный fps = 10 (ограничение самой камеры)Изменение настроек происходит с задержкой (~ 5-10 сек.)Событие о прекращении тревоги по лучу идет достаточно долго (~10 секунд)С прошивкой 1.2.24 аудио не работает на самой камере (шум вместо звука). Проблема устройства.С прошивкой 1.2.24 после перезагрузки камера вместо видео транслирует зеленый экран - проблема самого устройства","With the 1.2.24 firmware, the Brightness, Contrast, Sharpness, and Saturation settings do not work on the camera itself with MJPEG and 2048x1536 resolution, the max. frame rate is 15 fps (this is a limitation of the device itself)with H.264 and 1920x1080 resolution, the max. frame rate is 10 fps (this is a limitation of the device itself)Changes to settings are applied with a delay (around 5-10 seconds).Notifications on sensor alarm terminations arrive with a long delay (around 10 seconds).With the 1.2.24 firmware, audio does not work on the camera itself (noise instead of audio) This is a problem of the device itself. With the 1.2.24 firmware, after you restart the camera, it shows a green screen instead of video - this is a problem of the device itself"]
["SimpleIP Cam","SimpleIP Cam SPCHD series","Camera ","1.2.24","1","9","+.","+.","+",null,null,"2048x1536(MJPEG) / 1920x1072(MPEG-4) / 1920x1072(H.264)",null,null,"+.","-",null,"+","-",null,"1.  настройки яркость, контраст, резкость, цветность не работают на самой камере с прошивкой 1.2.24\n2. в MJPEG при 2048х1536 максимальный fps = 15 (ограничение самой камеры)\n3. в H.264 при 1920х1080 максимальный fps = 10 (ограничение самой камеры)\n4. С прошивкой 1.2.24 аудио не работает на самой камере (шум вместо звука). Проблема устройства.\n5. С прошивкой 1.2.24 после перезагрузки камера вместо видео транслирует зеленый экран - проблема самого устройства ","1.  With the 1.2.24 firmware, the Brightness, Contrast, Sharpness, and Saturation settings do not work on the camera itself\n2. with MJPEG and 2048x1536 resolution, the max. frame rate is 15 fps (this is a limitation of the device itself)\n3. with H.264 and 1920x1080 resolution, the max. frame rate is 10 fps (this is a limitation of the device itself)\n4. With the 1.2.24 firmware, audio does not work on the camera itself (noise instead of audio) This is a problem of the device itself.\n5. With the 1.2.24 firmware, after you restart the camera, it shows a green screen instead of video - this is a problem of the device itself "]
["SimpleIP Cam","SimpleIP SPCHD-200SA","Camera ","1.0.7","1","4","+",null,"+",null,null,"h.264: 1920x1080, mjpeg: 640x352","+",{"$nulls":4},"+.","-","motion detection.","Реле и телеметрия не работает на самой камереЧтобы работал встроенный детектор движения, необходимо выбрать режим Dual или Tri-stream. Из-за этого в Интеллекте детектор не работает - адаптер при любых комбинациях кодека и разрешения выбирает режим Single.При максимальном разрешении и/или качестве fps падает до 2-5 кадров в секундуВстроенный детектор лиц не работает на самой камереМикрофон интегрирован, т.к. он описан в SDK, но фактически на камере нет ни встроенного микрофона, ни аудио-входа.На запросы IP-wizard'a наших продуктов камера вместо имени модели возвращает \"SPCHD series\". Т.к. устройство с таким именем прописано в нашем драйвере совершенно по-другому, в Axxon Next камеру нужно добавлять обязательно только вручную, а в Интеллекте при добавлении обязательно указывать модель \"SPCHD-200SA\".firmware v1.0.7: продолжительность тревоги от встроенного детектора устанавливается в веб-интерфейсе (\"Потеря соединения\" -> \"Последнее событие\").","The relays and telemetry do not work on the camera itself To make the embedded motion detector work, select Dual or Tri-stream mode. For this reason, the detector does not work in Intellect: the adapter selects Single mode for any codec and any resolution. If you set the max. resolution and/or quality, the frame rate drops to around 2-5 fps. The embedded face recognition detector does not work on the camera itself. The microphone is integrated, because it is described in the SDK, but in reality the camera has neither a microphone, nor an audio input. In our software products, IP-wizard's requests return \"SPCHD series\" instead of the model name. A device with this name is supported by our driver in a different way. For this reason, in Axxon Next you must add the camera manually and in Intellect when adding the camera you must specify the model as SPCHD-200SA.The v1.0.7 firmware: You can configure how long an alarm from the embedded detection tools is active in the camera web interface.(\"Connection lost\" -> \"Last event\")"]
["SimpleIP Cam","SimpleIP SPCHD-241VDS","Camera","2.8.1.0O_201309111214_P4P","1","2",null,null,"+",null,null,"1920x1080","+",{"$nulls":6},"-",null,null,"improved"]
["SimpleIP Cam","SimpleIP SPCHD-260VO.IRS / SPCHD-231VBIRS / SPCHD-221VDIRS","Camera","2.8.2.0O_201309111214_P2P","1","2",null,null,"+",null,null,"1280x720","+",{"$nulls":6},"-",null,null,"improved"]
["Sinkross","Sinkross UID-01","Camera ","v.01","1","1","+",{"$nulls":4},"800x600","-",{"$nulls":6},"motion detection; other detectors","На камере два сетевых интерфейса. При подключении нужно указывать порт 1100.\nНа камере есть детектор огня, движения и дыма\nНастройки камеры и детекторов необходимо производить в вебе.","There are two network interfaces. For connection required to set port 1100. The camera has fire, motion and smoke detection. Camera's settings and detection should be performed using web-interface."]
["SNR","SNR SNR-CI-DW3.0I","Camera","2.211.0000.0.T, build : 2013-10-15","1","2","+","-","+","-","-","2048x1536","+","-","-","-","-","-","-","-"]
["Smartec","Smartec STC-IP2571A/1","Camera ","A1D-M2N-V2.09.11-NB","1","1",null,"+",{"$nulls":3},"720x576(PAL)/720x480(NTSC)","+","+","+","-",null,"+","+",null,"1. За неимением на самом устройства настройки качества видеоизображения, ползунок \"Качество\" в Intellecte регулирует bit rate видеопотока.\n2. Если выбрать неверный тип цветопередачи (ТВ-стандарт), возможна потеря части изображения.","1. The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream.\n2. If you select an incorrect color rendering (TV standard), parts of the image may be lost. \n"]
["Smartec","Smartec STC-IP3975A/2","Camera ","A1D-M2N-V2.09.11-NB","1",null,"+","+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)",null,null,"+","-","+","-","-","-","1. Для работы телеметрии в настройках самой камеры необходимо проставить протокол-Pelco D,скорость-2400, адрес-001\n2. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока\n","1) When configuring telemetry devices in Intellect, choose the protocol Pelco D, Baud Rate -2400, adress -001\n2) The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream.\n"]
["Smartec","Smartec STC-IP3985A/2","Camera ","A1D-M2N-V2.09.11-NB","1",null,"+","+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)",null,null,"+","-","+","-","-","-","1. Для работы телеметрии при выборе протокола \"Ip camera\" будет работать по протоколу Pelco-D с адресом 1 и baud rate'ом 2400\nПри выборе протокола \"Pelco-D\" или \"Dynacolor\" будет работать по выбранному протоколу с выбраным baud rate'ом и адресом\n2. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока\n","1) When configuring telemetry devices in Intellect, choose the protocol \"Ip camera\", telemetry will be work by protocol Pelco D, Baud Rate -2400, adress-001\n2) The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream.\n"]
["Smartec","Smartec STC-IPM2090A","Camera ","A1D-220-V3.08.08-NB","1",null,"+","+",{"$nulls":3},"1280x1024",null,null,"+","-",null,"+","+","-","1. При \"Полном\" разрешении (1280х1024) камера способна выдавать максимум 8 fps\n2. При MPEG-4 за неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока","1) With the Full resolution (1280х1024), the camera allows 8 fps max. \n2. For MPEG-4, the device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream."]
["Smartec","Smartec STC-IPM3077A / STC-IPM3578A / STC-IPM3577A","Camera ","BgWT8130035N04 V24 1211052A","1","10","+","+","+",null,null,"1280x1024","+"]
["Smartec","Smartec STC-IPM3086A, STC-IPM3186A, STC-IPM3586A","Camera ","BgWT8202715N03 V23 1208153A","1","9","+","+","+",null,null,"1920x1072","+",null,"+","-","-","+","+.","motion detection"]
["Smartec","Smartec STC-IPM3090A","Camera ","A1D-220-V3.09.14-NB","1",null,"+","+",{"$nulls":3},"1280x1024",null,null,"+","-",null,"+","+.","-","Интегрировано в Intellect 4.7.6.125 и старше. Т.е. в Intellect 4.7.6 Release камера работать не будет.","Already integrated in Intellect 4.7.6.125 and above. i.e. this camera is not going to work in Intellect 4.7.6."]
["Smartec","Smartec STC-IPMX3593A/1","Camera ","1.3.0","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+",null,"+.","+","motion detection and others","1. Список детекторов встроенной аналитики: Presence Enter Exit Appear Disappear Stopped Dwell Direction filter Speed Filter Tailgating","1. List of detectors of built-in analytics: Presence Enter Exit Appear Disappear Stopped Dwell Direction filter Speed Filter Tailgating"]
["Smartec","Smartec STC-IPMX3693A","Camera ","1.4.0.12","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+",null,"+","+","motion detection.; tampering detection; other detectors.","Список детекторов встроенной аналитики:\nPresence\nEnter\nExit\nAppear\nDisappear\nStopped\nDwell\nDirection filter\nSpeed Filter\nTailgating","Onboard detectors:\nPresence\nEnter\nExit\nAppear\nDisappear\nStopped\nDwell\nDirection filter\nSpeed Filter\nTailgating"]
["Smartec","Smartec STC-IPX3630A / STC-IPX3561A ","Camera ","1.6.7","1","2","+","+","+",null,null,"720x576 ","+",null,"+","+.",{"$nulls":4},"1. Для корректной работы динамика и микрофона в ПО ITV/Axxon необходимо, чтобы их настройки совпадали.\n2. Кодек G.711 работает только с частотой дискретизации 8 КГц, частота 16 кГц не поддерживается. ","1. To work with the speaker and the microphone in Axxon SW correctly, their settings must be the same.\n2. G.711 codec works only with a sampling rate of 8 kHz. 16 kHz is not supported."]
["Smartec","Smartec STS-IPT180 encoder","Encoder ","A1D-M2N-V2.09.11-NB","1",null,null,"+",{"$nulls":3},"720х576(PAL)/720x480(NTSC)",null,null,"+","-","+","+.","+.","-","1. При настройке телеметрии в настройках Intellecta протокол следует выбирать не \"IPCamera\", а тот, по-которому работает подключенная поворотная камера (Pelco-D, DynaColor, Panasonic-850 проч.). Также необходимо указывать настройку \"Скорость\" (Boud Rate)\n2. За неимением на самом устройстве настройки качества видеоизображения, ползунок \"Качество\" в Intellect регулирует bit rate видеопотока.\n","1) When configuring telemetry devices in Intellect, choose the protocol that the newly plugged camera (Pelco-D, DynaColor, Panasonic-850 etc.) supports. Do not choose the \"IPCamera\" protocol. Then specify the Baud Rate. 2 The device itself does not have a way to adjust the video image quality. For this reason, in Intellect, you may use the Quality slider to adjust the bit rate of the video stream.\n"]
["Smartec_G2","Smartec STC-IPM3095A/3","Camera ","X.2.1.8","1",null,"+","+",{"$nulls":3},"1280x960",null,null,"+.","+.",null,"+","+","-","1. при разрешении 1280х960 максимальный fps равен 12-15 fps, ограничение самой камеры\n2. автоматический поиск устройства в сети в ПО ITV  не может быть реализован ","1) With the 1280x960 resolution, the max. frame rate is 12-15 fps; this is a limitation of the camera itself in the AxxonSoft software, the automatic search for the device cannot be implemented. "]
["Smartec_G2","Smartec STC-IPM3096A/3","Camera ","X.2.1.10","1","2","+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4)",null,null,"+.","-",null,"+","+","-","1. при разрешении 1280х960 максимальный fps равен 12-15 fps, ограничение самой камеры","1. With the 1280x960 resolution, the max. frame rate is12-15 fps; this is a limitation of the camera itself"]
["Smartec_G2","Smartec STC-IPM3097A / STC-IPM3597A","Camera ","gWT8300036NO0001 V21 1202024F","1","10","+","+","+",null,null,"2048x1536 (MJPEG, H264) / 1920x1072 (MPEG4)","+",null,"-",null,"-","-","-","-","Получать несколько независимых потоков с камеры нельзя. Потоки в Axxon Next по сути представляют собой различные профили получения видео.Настройки видео применяются с небольшой задержкой (~ 5-10 секунд)Максимальная частота кадров в MJPEG - 15 fps в минимальном разрешении и 5-8 fps в высоких разрешениях.Устройство находится поиском как Onvif, но работать через Onvif не будет.Прошивка gWT8300036NO0001 V21 1202024F: в потоках 5 и 6 в кодеках mpeg4.1 и h264.1 в разрешении QVGA видео идет в 320х240.","No multistreaming for that camera. Video streams in Axxon Next are basically different profiles for video. Video settings are applied with a delay of 5 to 10 sec. Max frame rate in MJPEG is 15 fps under min. resolution and 5 to 8 fps with high resolution. Device discovery mistakenly shows this device as ONVIF ready. Firmware gWT8300036NO0001 V21 1202024F: video is streamed at 320 [240 when via channels 5 and 6 and coded in MPEG4 and H264 with the QVGA resolution."]
["Sony","Sony SNC-CH110 / SNC-DH110(T)","Camera ","1.78.00","1","2","+","+","+",null,null,"1280x960","+","+",null,null,"+","+",null,"motion detection.","1. При максимальных разрешениях и качестве камера имеет ограничения, накладываемые на частоту кадров (см. инструкцию к камере)\n2. Во втором потоке камера имеет ограничения на частоту кадров и набор разрешений в зависимости от текущих настроек первого потока (см. инструкцию к камере)\n3. При изменении \"ТВ-стандарта\" происходит сброс на значения по умолчанию настроек видео, встроенного детектора \"Интеллектуальное обнаружение\", предустановок телеметрии.\n4. Изменение \"ТВ-стандарта\" происходит с задержкой (~1 минута) - камера перезагружается.\n5. Цифровая PTZ-телеметрия камеры работает только при выбранном \"ТВ-стандарте\" \"PAL, 4:3\"\n6. Встроенный детектор \"Интеллектуальное обнаружение\" будет работать при использовании только нулевого видеопотока и только при выключенной \"Цифровой PTZ-телеметрии\"\nПри включенной \"Цифровой PTZ-телеметрии\" максимальное разрешение - \"768x576\"\n7. При включении двух стриммингов и выборе для обоих кодека MJPEG камера перестает присылать видео по второму стриммингу. Проблема самой камеры с текущей прошивкой 1.27.02","1. For max. resolutions and video quality settings the camera is limited in fps. (see the camera manual).\n For stream 2 the camera fps and resolution limitation depend on stream 1 settings. (see the camera manual). \n3. When you change the TV standard, video parameters, telemetry presets and Next Detection settings are reset to the default values.\n4. Changes to TV standard are applied with a delay (around 1 min) while the camera is rebooted.\n5. Digital PTZ-works only with PAL 4:3\n6. Embedded Next Detection works only with stream 0 and when Digital PTZ is disabled \nIf the Digital PTZ is enabled, then the max resolution is \"768x576\"\n7. If you choose MJPEG for both streams In the dual stream mode, the camera fails to feed stream 2. This is a bug of the camera's current firmware 1.27.02"]
["Sony","Sony SNC-CH140 / SNC-CH180","Camera ","1.77.00","1","2","+","+","+",null,null,"1280x1024","+","+","+.","+","+","+","+","motion detection","1. При изменение настроек встроенного детектора устанавливается максимальное разрешение","1. If you change the embedded detection settings, then the max. resolution is applied."]
["Sony","Sony SNC-CH120 / SNC-CH160","Camera ","1.78.00","1","2","+","+","+",null,null,"1280x1024","+","+",null,null,"+","+","+","motion detection; onboard tracker","1. Камера не поворотная, но есть цифровая телеметрия (solidPTZ)\n2. При включении телеметрии на камеру накладывается ограничение по разрешению (макс. разрешение - 768х576). Для включения мультикаста в Интеллекте необходимо открыть редактор реестра, перейти по пути \\HKEY_LOCAL_MACHINE\\SOFTWARE\\Wow6432Node\\ITV\\INTELLECT\\Video\\ создать там каталог TransportProtocols и в этом каталоге создать строковый параметр SonyIpela со значением multicast ","1. The camera is not swivel, but there is a digital telemetry (solidPTZ)\n2. When you turn on the camera telemetry is constrained resolution (max. resolution - 768x576). To turn Multicast in Intellect Enterprice necessary to open Registry Editor, follow to the path \\ HKEY_LOCAL_MACHINE \\ SOFTWARE \\ Wow6432Node \\ ITV \\ INTELLECT \\ Video \\ directory and create there TransportProtocols directory, in this directory create a string parameter SonyIpela with a value \"multicast'."]
["Sony","Sony SNC-CH210 / SNC-DH210(T)","Camera ","1.78.00","1","2","+","+","+",null,null,"MJPEG: 2048x1536; H.264/MPEG4: 1600х1200","+","+",null,null,"+",null,null,"motion detection; onboard tracker","1. При максимальных разрешениях и качестве камера имеет ограничения, накладываемые на частоту кадров (см. инструкцию к камере)\n2. Во втором потоке камера имеет ограничения на частоту кадров и набор разрешений в зависимости от текущих настроек первого потока (см. инструкцию к камере)\n3. При изменении \"ТВ-стандарта\" происходит сброс на значения по умолчанию настроек видео, встроенного детектора \"Интеллектуальное обнаружение\", предустановок телеметрии.\n4. Изменение \"ТВ-стандарта\" происходит с задержкой (~1 минута) - камера перезагружается.\n5. Цифровая PTZ-телеметрия камеры работает только при выбранном \"ТВ-стандарте\" \"PAL, 4:3\"\nВстроенный детектор \"Интеллектуальное обнаружение\" будет работать при использовании только нулевого видеопотока и только при выключенной \"Цифровой PTZ-телеметрии\"\nПри включенной \"Цифровой PTZ-телеметрии\" максимальное разрешение - \"768x576\"","1. For max. resolutions and video quality settings the camera is limited in fps. (see the camera manual). For stream 2 the camera fps and resolution limitation depend on stream 1 settings. (see the camera manual). \n3. When you change the TV standard, video parameters, telemetry presets and Next Detection settings are reset to the default values.\n4. Changes to TV standard are applied with a delay (around 1 min) while the camera is rebooted.\n5. Digital PTZ works only with PAL 4:3 \nEmbedded Next Detection works only with stream 0 and when Digital PTZ is disabled.\nIf the Digital PTZ is enabled, then the max resolution is \"768x576\""]
["Sony","Sony SNC-CH220 / SNC-CH260","Camera","1.80.00","1","2","+","+","+",null,"-","1920x1440 / 1920x1080","+","+","-","-","+",null,"-","motion detection; onboard tracker","Максимально доступное разершение (1920x1080 / 1920x1440) зависит от значения настройки Maximum image size в веб-интерфейсеПри максимальных разрешениях и качестве камера имеет ограничения, накладываемые на частоту кадров (см. инструкцию к камере)Во втором потоке камера имеет ограничения на частоту кадров и набор разрешений в зависимости от текущих настроек первого потока (см. инструкцию к камере)Изменение \"ТВ-стандарта\" происходит с задержкой (~1 минута) - камера перезагружается.Цифровая PTZ-телеметрия камеры работает только при выбранном \"ТВ-стандарте\" \"PAL, макс разрешение 1920х1440\"Встроенный детектор \"Интеллектуальное обнаружение\" будет работать при использовании только нулевого видеопотока и только при выключенной \"Цифровой PTZ-телеметрии\" ","Maximum available resolution (1920x1080 / 1920x1440) depends on from Maximum image size setting in web interface of device. With maximum resolution and quality value of camera, frame rate setting has limitations (look into camera's instructions). At second stream, it is limitations of frame rate and permissions sets, it depends on from current settings of first stream (look into instructions).  \"TV standard\" changing is delayed (about 1 minute) - the camera is rebooting. Digital PTZ: camera's telemetry works only when selected TV standard is PAL and resolution 1920x1440 resolution .\" Built-in detector \"Intelligent detection\" will work only with selected zero stream of video and switched off \" Digital PTZ- telemetry \"."]
["Sony","Sony SNC-CH240 / SNC-CH280","Camera","1.77.00","1","2","+","+","+",null,null,"1920x1440","+","+","-","-","+","-","-","motion detection; inbult tracker","1. У камеры цифровая телеметрия - ePTZ \n2. Для того, чтобы на камере были доступны разрешения больше 1920*1080, нужно в веб-интерфейсе на вкладке Installation выбрать max image size 1920*1440\n","1. The camera offers digital telemetry (ePTZ) 2. To make camera resolutions over 1920x1080 available, select max image size 1920x1440 on the Installation tab  in the camera web interface. ","improved"]
["Sony","Sony SNC-CM120","Camera ","1.10","1",null,"+","+",{"$nulls":3},"1280x960(MJPEG)/640x480(MPEG-4)",null,null,"+","-",null,"+","+","motion detection; onboard tracker","1.  реле требуют предварительного включения в web-интерфейсе камеры\n2. у камеры есть функция Light Funnel\n - при включенной функции, значения fps в Intellect максимум 30, но нельзя выставить мегапиксельное разрешение в потоке MJPEG\n - при выключеной функции значения fps в Intellect максимум 10, но можно выставить мегапиксельное разрешение в потоке MJPEG\n","1. Enable the relay in the camera web interface \n2. The camera offers the Light Funnel function. If you enable it, the max. fps in Intellect will be 30, and no mega pixel resolutions in MJPEG. If you disable it, the max fps will be 10, but you can set the mega pixel resolution in MJPEG.\n"]
["Sony","Sony SNC-CS10Р/11P","Camera ","1.06","1","1","+","+",{"$nulls":3},"640x480",null,null,"+.","+.",null,"+","+","-"]
["Sony","Sony SNC-CS20","Camera ","1.10","1","2","+","+",{"$nulls":3},"640x480",null,null,"+","-",null,"+","+","motion detection; onboard tracker"]
["Sony","Sony SNC-CS50P","Camera ","2.32","1",null,"+","+","+",null,null,"640x480",null,null,"+","-",null,"+","+","motion detection; onboard tracker","1. У самой камеры в родном вебе есть настройка Image mode и три положения для неё (Field, Frame и Auto). Frame – для неподвижных изображений, Field – для движущейся картинки, Auto –камера сама распознает режим .  Поэтому если в Intellect вы увидите эффект похожий на интерлейсинг (лесенка) – это не баг скорее всего, просто проверьте параметр Image mode в родном вебе\n ","1) The camera's web interface offers 3 settings (Field, Frame and Auto) in the Image mode. Frame - is for still images, Filed - is for video and Auto is when the camera switches to the appropriate mode itself.  For that reason if you see saw-tooth / interlacing artifacts, check the Image mode settings.\n "]
["Sony","Sony SNC-CX600(W)","Camera","1.9.2","1","3","+",null,"+",null,null,"1280x720","+",null,"+","-","+",null,null,"motion detection; inbult tracker","На камере есть встроенный детектор лиц.","There is an on-board Face detection tool.","improved"]
["Sony","Sony SNC-DF80P","Camera ","1.22","1",null,"+","+","+",null,null,"640x480",{"$nulls":7},"motion detection; onboard tracker","1. Ползунок \"Качество\" для MPEG и H.264 регулирует bit rate видеопотока\n2. Звук, Лучи и Реле не проверены, т.к. нет необходимых для этого разъемов.\n3. При H.264 сама камера выдает только 8-12 fps","1. For MPEG-4 and H.264 use the Quality slider to adjust the video stream bit rate. \n2. Sound, Sensors and Relays haven't been checked so far since there are no suitable connectors at the moment.\n3. With H.264, the camera is capable of running at -12 fps max."]
["Sony","Sony SNC-DF85P","Camera ","1.20","1",null,"+","+","+",null,null,"640x480",{"$nulls":3},"-",{"$nulls":3},"motion detection; onboard tracker","ауди, лучи и реле не проверены т.к. с камерой не предоставили нужных переходников","Sound, Sensors and Relays haven't been checked so far since there are no no adapters for that camera in the test kit."]
["Sony","Sony SNC-DH120(T) / SNC-DH160 ","Camera","1.80.00","1","2","+","+","+",null,"-","1280x1024","+","+","-","-","+",null,"-","motion detection; onboard tracker","Разрешение на втором потоке должно быть меньше, чем на первомДля включения мультикаста в Интеллекте необходимо открыть редактор реестра, перейти по пути \\HKEY_LOCAL_MACHINE\\SOFTWARE\\Wow6432Node\\ITV\\INTELLECT\\Video\\ создать там каталог TransportProtocols и в этом каталоге создать строковый параметр SonyIpela со значением multicast","The resolution for stream 2 should be lower than or equal to one for stream. To use the camera in Axxon Intellect with multicast you need to launch registry editor, move to \\HKEY_LOCAL_MACHINE\\SOFTWARE\\Wow6432Node\\ITV\\INTELLECT\\Video\\, create directory TransportProtocols and create there link parameter SonyIpela with value multicast "]
["Sony","Sony SNC-DH140(T) / SNC-DH180","Camera ","1.73.01","1","2","+","+","+",null,null,"1280x1024","+","+","+","+","+",null,null,"motion detection; onboard tracker"," 1. Максимальное разрешение в Intellect зависит от настройки Maximum image size"," 1. The max. resolution in AxxonSoft Intellect depends on the Maximum Image Size setting."]
["Sony","Sony SNC-DH240(T) / SNC-DH280","Camera ","1.73.01","1","2","+","+","+",null,null,"1920x1440","+","+",null,null,"+",null,null,"motion detection; onboard tracker","1. У камеры цифровая телеметрия - ePTZ\n2. Для того, чтобы на камере были доступны разрешения больше 1920*1080, нужно в вебе на вкладке Installation выбрать max image size 1920*1440\n3. Видео в ПО Intellect с \"Полным\" разрешением будет только если в веб-интерфейсе на вкладке Installation выбрать max image size 1920*1440","1. The camera offers digital telemetry (ePTZ)\n2. To make camera resolutions over 1920x1080 available, select max image size 1920x1440 on the Installation tab in the camera web interface. 3. Intellect offers the Full resolution video only if you select max image size 1920x1440 on the Installation tab in the camera web interface."]
["Sony","Sony SNC-DM110","Camera ","1.10","1","2","+","+",{"$nulls":3},"1280x960(MJPEG) / 640x480(MPEG-4)",null,null,"+","-","+","+","+","motion detection.","1. У камеры есть функция Light Funnel:\n - при включенной функции, значения fps в Intellect максимум 30, но нельзя выставить мегапиксельное разрешение в потоке MJPEG\n - при выключеной функции значения fps в Intellect максимум 15, но можно выставить мегапиксельное разрешение в потоке MJPEG\n2. При включении функции Light Funnel нельзя менять разрешение MJPEG-видео через Intellect\n3. Реле требуют предварительного включения в web-интерфейсе камеры\n4. Камера не поворотная, но есть solidPTZ","1. The camera has the Light Funnel function:\n If you enable it, the max. fps in Intellect will be 30, and no mega pixel resolutions in MJPEG. \nIf you disable it, the max fps will be 15, but you can set the mega pixel resolution in MJPEG. \n2. If enabled, Light Funnel makes it impossible to change MJPEG resolution via Intellect. \n3. Enable the relay in the camera web interface \n4. This is not a PTZ camera, but it has digital telemetry (solidPTZ)."]
["Sony","Sony SNC-DM160","Camera ","1.11","1",null,"+","+",{"$nulls":3},"1280x960(MJPEG) / 640x480(MPEG-4)",{"$nulls":7},"motion detection; onboard tracker","1. У камеры есть функция Light Funnel:\n- при включении функции нельзя менять разрешение MJPEG-видео через Intellect\n- при включенной функции значения fps в Intellect максимум 30, но нельзя выставить мегапиксельное разрешение в потоке MJPEG\n- при выключеной функции значения fps в Intellect максимум 15, но можно выставить мегапиксельное разрешение в потоке MJPEG \n2. При включении функции Light Funnel нельзя менять разрешение MJPEG-видео через Intellect","1. The camera has the Light Funnel function:\nIf you enable it, the max. fps in Intellect will be 30, and no mega pixel resolutions in MJPEG. \nIf you disable it, the max fps will be 15, but you can set the mega pixel resolution in MJPEG. \n2. If enabled, Light Funnel makes it impossible to change MJPEG resolution via Intellect. "]
["Sony","Sony SNC-EB520 / SNC-EM521","Camera ","1.78.00","1","2","+","+","+",null,null,"800x600","+","+",null,null,"+","+","+.","motion detection.; tampering detection","1. Чтобы работала цифровая телеметрия, нужно включить соответствующую настройку объекта камеры.\n2. Разрешение на втором потоке не может быть больше, чем на первом.","1. To make digital PTZ work, enable the relevant setting for the camera object.\n2. The resolution for stream 2 should be lower than or equal to one for stream 1."]
["Sony","Sony SNC-EB600(B) / SNC-EM600 / SNC-EM601 / SNC-EM602R","Camera","1.9.2","1","2","+",null,"+",null,null,"1280x1024","+",{"$nulls":3},"+",null,null,"-","Настройка \"Поворот видеоизображения\" актуальна только для камеры SNC-EM600","Video rotation setting is relevant only for SNC-EM600 camera.","improved"]
["Sony","Sony SNC-EM520","Camera ","1.78.00","1","2","+","+","+",null,null,"800x600","+","+",null,null,"+",{"$nulls":3},"1. Чтобы работала цифровая телеметрия, нужно включить соответствующую настройку объекта камеры.\n2. Разрешение на втором потоке не может быть больше, чем на первом.","1. To make digital PTZ work, enable the relevant setting for the camera object.\n2. The resolution for stream 2 should be lower than or equal to one for stream 1."]
["Sony","Sony SNC-EP520, SNC-EP521, SNC-ER520, SNC-ER521","Camera ","1.78.00","1","2","+","+","+",null,null,"720x576","+","+","+.","+","+","+","+","motion detection; tampering detection","1. Разрешение на втором потоке не может быть больше, чем разрешение на первом потоке.\n2. При изменение настроек встроенного детектора устанавливается максимальное разрешение","1. The resolution for stream 2 should be lower than or equal to one for stream 1.\n2. If you change the embedded detection settings, then the max. resolution is applied."]
["Sony","Sony SNC-EP550 / SNC-ER550 / SNC-ZR550 / SNC-ZP550","Camera ","v1.70.00","1","2","+","+","+",null,null,"1280x720","+","+",null,null,"+",null,null,"onboard tracker"]
["Sony","Sony SNC-ER580 / SNC-EP580 / SNC-ER585 / SNC-ER585H ","Camera ","1.78.00","1","2","+","+","+",null,null,"1920x1080","+","+",null,null,"+",null,null,"motion detection; onboard tracker","1. Чтобы заработал встроенный детектор движений нужно отключить 2 поток, Letterbox и Cropping в веб-интерфейсе\n2. При изменение настроек встроенного детектора устанавливается максимальное разрешение","1. To enable embedded motion detection, you should disable stream 2, Letterbox and Cropping in the web interface.\n2. If you change the embedded detection settings, then the max. resolution is applied."]
["Sony","Sony SNC-P1","Camera ","1.30","1","1","+","+",{"$nulls":3},"640x480",null,null,"+.","+.",null,"+","+","-","При разрешении 640х480 максимально 15-18 fps","With the 640x480 resolution, the camera allows 15-18 fps max."]
["Sony","Sony SNC-RH124 / SNC-RH164","Camera ","1.73.00","1","2","+","+","+",null,null,"1280x720","+","+",null,null,"+",null,null,"motion detection; onboard tracker"]
["Sony","Sony SNC-RS44N/P, SNC-RS46N/P, SNC-RS84N/P, SNC-RS86N/P","Camera ","1.73.00","1","3","+","+","+",null,null,"720x576 (PAL) / 720x480 (NTSC)","+","+",null,null,"+",null,null,"motion detection; onboard tracker","1. SNC-RS44/46/84/86N и SNC-RS44/46/84/86P отличаются друг от друга ТВ-стандартом.","1. SNC-RS44/46/84/86N differs from SNC-RS44/46/84/86P by the TV standard they use."]
["Sony","Sony SNC-RX530N/P","Camera ","3.01","1","2","+","+","+",null,null,"640x480",{"$nulls":4},"+.",null,null,"motion detection; onboard tracker"]
["Sony","Sony SNC-RX550P","Camera ","3.10","1",null,"+","+","+",null,null,"640x480",null,null,"+",null,"+","+","+","motion detection; onboard tracker","1. Реле требуют предварительного включения в web-интерфейсе камеры \n2. добавилось новое разрешение 704x576 ( после прошивки на 3.10, если прошивка ниже, то максимальное (полное) разрешение 640*480) - ждем его добавления и выбора в качестве полного разрешения\n3. Настройка качества видео есть только для потока MJPEG (в web-интерфейсе камеры так же)","1. Enable the relay in the camera web interface. \n2. New 704x576 resolution is available now after firmware update to 3.10. For older versions the max. resolution is 640x480. We are expecting it to be added and being available for the Full resolution choice. \n3. You can configure video quality only for MJPEG streams (same in camera interface)"]
["Sony","Sony SNC-RX570P","Camera ","3.10","1",null,"+","+","+",null,null,"640x480",null,null,"+","-","+","+","+","motion detection; onboard tracker","1) Видео в формате H.264 может отображаеться с максимальной частотой 8-15 fps (в зависимости от Bit rate видеопотока). Ограничение самой камеры.\n2) Чтобы можно было управлять настройкой фокуса, необходимо в веб-интерфейсе камеры выставить Focus mode=Manual","H.264 video is available only with the 8-15 fps max. depending on the bit rate. This is a limitation of the camera itself.\n2) To be able to adjust the focal length, select Manual in the Focus mode in the camera web interface."]
["Sony","Sony SNC-RZ25P","Camera ","1.40","1","1","+","+",{"$nulls":3},"640x480",null,null,"+.","+.","+","+","+","-","1. При разрешении 640х480 достижимы максимально 15-18 fps","1) With the 640x480 resolution, the camera allows 15-18 fps max."]
["Sony","Sony SNC-RZ50P","Camera ","2.42","1",null,"+","+","+",null,null,"640x480",null,null,"+","-","+","+","+","motion detection; onboard tracker","1. Ползунок \"Качество\" для MPEG и H.264 регулирует bit rate видеопотока\n2. При H.264 сама камера выдает только 8-12 fps","1. For MPEG-4 and H.264 use the Quality slider to adjust the video stream bit rate. 2. With H.264, the camera is capable of running at 8-12 fps max."]
["Sony","Sony SNC-VB600 / SNC-VM600 / SNC-VM601 / SNC-VM602R","Camera","1.12.0","1","3","+","-","+","-","-","1280x1024","+","-","+","+","+","+","+","motion detection; tampering detection; others; on-board tracker","Значение 60 FPS для Интеллект применяется через веб, а в AN включением настройки \"режим высокой частоты кадров\"Прочие встроенные детекторы:Детектор лиц","You can set 60 fps for Intellect in the camera's web interface, while in Axxon Next you have to enable high frame rate mode to get 60 fps. Other on-board detection tools: Face detection tool."]
["Sony","Sony SNC-VB600B / SNC-VM600B / SNC-VM601B","Camera","1.12.0","1","3","+","-","+","-","-","1280x1024","+","-","+","+","+","+","+","motion detection; tampering detection; others; on-board tracker","Прочие встроенные детекторы:Детектор лиц","Other on-board detection tools: Face detection tool"]
["Sony","Sony SNC-VB630 / SNC-VB635 / SNC-VM630 / SNC-VM631 / SNC-VM632R","Camera","1.9.2","1","3","+",null,"+",null,null,"1920x1080","+",null,"+",null,"+","+","-","motion detection; tampering detection; others; inbult tracker","Значение 60 FPS для Интеллект применяется через веб, а в AN включением настройки \"режим высокой частоты кадров\"Прочие встроенные детекторы:Детектор лиц","You can set 60 fps for Intellect in the camera's web interface, while in Axxon Next you have to enable high frame rate mode to get 60 fps. Other on-board detection tools: Face detection tool.","improved"]
["Sony","Sony SNT-EX154","Encoder ","1.77.03 ","1","2","+","+","+",null,null,"704x576","+","+",{"$nulls":5},"onboard tracker","1. Устройство представляет из себя 4-канальный сервер, но у каждого из каналов - свой сетевой адрес.","1. This is a 4 channel server, where each channel has its own IP address."]
["ST","ST ST-170 IP","Camera","H18C01-B.771","1","1",null,null,"+",null,null,"1280x720","+",{"$nulls":6},"-","В продукте, для подключения камеры, необходимо ввести номер порта 9000 (значение по-умолчанию для камеры)","To connect a camera, specify 9000 port (default value for the camera).","improved"]
["ST","ST ST-171 IP / ST-172 IP / ST-181 IP / ST-182 IP","Camera","H18C01-C.889","1","1",null,null,"+",null,null,"1920x1080","+",{"$nulls":6},"-","В продукте, для подключения камеры, необходимо ввести номер порта 9000 (значение по-умолчанию для камеры)","To connect a camera, specify 9000 port (default value for the camera).","improved"]
["ST","ST ST-180 IP","Camera","H18C01-B.774","1","1",null,null,"+",null,null,"1280x960","+",{"$nulls":6},"-","В продукте, для подключения камеры, необходимо ввести номер порта 9000 (значение по-умолчанию для камеры)","To connect a camera, specify 9000 port (default value for the camera).","improved"]
["StarDot","NetCam SC 1.3 MP IR","Camera ","1.1.66","1","1","+",{"$nulls":4},"1296x960",{"$nulls":5},"-","-","-","1. Fps при максимальном разрешении очень сильно зависит от размера фрейма, а размер фрейма в свою очередь зависит от качества,  движения в кадре, освещенности и т.д. У меня fps был от 4 до 12.","1) Frame rate at max. resolution depends heavily on the frame size, which in turn is a function of video quality, motion in the scene and lighting conditions etc. We experienced fps from 4 to 12."]
["StarDot","StarDot SDH300VN / SDH300BN ","Camera ","1.1.78","1","2","+",null,"+",null,null,"2048x1536","+",{"$nulls":7},"1. В ПО ITV/Axxon камеры интегрированы как серия \"3MP\"\n2. Для корректной работы двухпоточности в ПО Axxon в настройках обоих потоков должно быть установлено одно и то же значение разрешения ","1. Cameras has been integrated as the series \"3MP\" in Axxon SW.\n2. To work correctly with dual-stream in the Axxon, the same resolution should be set in the settings of both streams."]
["Stream Labs","WaveCam MX","Camera ","Ubicom 2.1.0.0; PNX Bios 2.4.0.0; PNX Main 2.6.1.0","1","1",{"$nulls":3},"+",null,"768х576(PAL)/640х480(NTSC)"]
["Stream Labs","WaveCam MX-A","Camera ","Ubicom 2.1.0.0; PNX Bios 2.4.0.0; PNX Main 2.6.1.0","1","1",{"$nulls":3},"+",null,"768х576(PAL)/640х480(NTSC)",null,null,"+","+."]
["Stream Labs","WaveCam MXE","Camera ","Ubicom 2.1.0.0; PNX Bios 2.4.0.0; PNX Main 2.6.1.0","1","1",{"$nulls":3},"+",null,"768х576(PAL)/640х480(NTSC)",{"$nulls":4},"-"]
["Stream Labs","WaveCam MX-M","Camera ","Ubicom 2.1.0.0; PNX Bios 2.4.0.0; PNX Main 2.6.1.0","1","1",{"$nulls":3},"+",null,"768х576(PAL)/640х480(NTSC)",{"$nulls":8},"Для корректной работы устройства в ПО ITV рекомендуется в настройках камеры поле декомпрессор оставлять пустым, либо указывать декомпрессор Wavelet 2. При выборе других декомпрессоров корректная работа ПО не гарантируется. ","For correct works between the device and ITV | AxxonSoft software is recommended to leave fiend decompressor blank in camera settings, or specify the decompressor \"Wavelet\" 2. When choosing other decompressors correct work of Software is not guaranteed."]
["Stream Labs","WaveCam QX","Camera ","Ubicom 1.8.1.0\\PNX Bios 1.6.2.0\\PNX Main 1.8.3.0","1",{"$nulls":4},"+",null,"768х576(PAL)/640х480(NTSC)",null,null,"+","-","-","+","+",null,"1. Лучи необходимо замыкать под напряжением\n2. Камера сама по себе не поворотная, но имеет RS-485 порт для подключения сторонней поворотной платформы.\n3. Камера не поворотная, но у неё есть оптический зум и фокус, но работает этот фунционал только со спец. объективом","1. Close the sensors when they are energized\n2. This is not a PTZ camera, but it has a RS-485 port to connect a third-party pan/tilt drive.\n3. This is not a PTZ camera, but it has optical zoom and focus. However, this functionality requires a special lens. "]
["Stream Labs","WaveServer 1501A encoder","Encoder ","Ubicom 2.0.0.0; PNX Bios 2.0.3.0; PNX Main 2.3.0.0","1","1",{"$nulls":3},"+",null,"768х576(PAL)/640х480(NTSC)",null,null,"+","+.","-","+","+",null,"Для того, чтобы в Интеллект заработал аудио-выход, нужно присвоить параметру \"Частота дискретизации\" значение \"16000\". Для корректной работы устройства в ПО ITV рекомендуется в настройках камеры поле декомпрессор оставлять пустым, либо указывать декомпрессор Wavelet 2. При выборе других декомпрессоров корректная работа ПО не гарантируется. ","To activate the audio output in Intellect, set Sampling Rate at 16000. For correct works between the device and ITV | AxxonSoft software is recommended to leave fiend decompressor blank in camera settings, or specify the decompressor \"Wavelet\". When choosing other decompressors correct work of Software is not guaranteed."]
["Stream Labs","WaveServer 1504R encoder","Encoder ","Ubicom 0.8.0.0; PNX BIOS 0.8.1.0; PNX Main 1.4.0.0","4","1",{"$nulls":3},"+",null,"768x576(PAL) / 640x480(NTSC)",null,null,"+",{"$nulls":5},"1. Если настроен один канал, то у него 25 fps. Если задействован мультиплекс(т.е. два или более каналов), то 16 fps на все каналы - это значит, если два канала, то на каждый приходится 16/2=8 fps, если четыре канала, то на каждый приходится 16/4=4 fps","1. If only one channel is enabled, its max. frame rate is 25 fps. If multiplex is enabled (that is, two channels or more), you have 16 fps for all the channels - this mean: if you have two channels, each gets 16/2=8 fps, if you have four channels, each gets 16/4=4 fps"]
["Stream Labs","WaveServer 1554 encoder","Encoder ","Ubicom 2.0.0.0 \\ PNX Bios 2.0.3.0 \\ PNX Main 2.3.0.0","4","1",{"$nulls":3},"+",null,"768x576(PAL) / 640x480(NTSC)",null,null,"+","+.","-","+","+",null,"1. Если настроен один канал, то у него 25 fps. Если задействован мультиплекс(т.е. два или более каналов), то 16 fps на все каналы - это значит, если два канала, то на каждый приходится 16/2=8 fps, если четыре канала, то на каждый приходится 16/4=4 fps\n2. Телеметрия в ПО Axxon не реализована. Для корректной работы устройства в ПО ITV рекомендуется в настройках камеры поле декомпрессор оставлять пустым, либо указывать декомпрессор Wavelet 2. При выборе других декомпрессоров корректная работа ПО не гарантируется. \n \n2. При настройке телеметрии в Intellect в настройках объекта \"Контроллер телеметрии\" протокол следует выбирать \"в явном виде\" (напр. Peclo-D, Panasonic-850), а не \"IPCamera\" как на большинстве других ip-устройств\n ","1. If only one channel is enabled, its max. frame rate is 25 fps. If multiplex is enabled (that is, two channels or more), you have 16 fps for all the channels - this mean: if you have two channels, each gets 16/2=8 fps, if you have four channels, each gets 16/4=4 fps\n2. The AxxonSoft software does not implement telemetry. For correct works between the device and ITV | AxxonSoft software is recommended to leave fiend decompressor blank in camera settings, or specify the decompressor \"Wavelet\". When choosing other decompressors correct work of Software is not guaranteed.\n "]
["Stream Labs","WaveServer 1554H encoder","Encoder ","Ubicom 2.4.0.0; PNX Bios 2.5.0.0; PNX Main 2.9.0.0","4","1",{"$nulls":3},"+",null,"768x576(PAL) / 640x480(NTSC)","+",null,"+",null,null,"-","+.",null,"ограничение 50 fps в сумме на 4 канала. Для корректной работы устройства в ПО ITV рекомендуется в настройках камеры поле декомпрессор оставлять пустым, либо указывать декомпрессор Wavelet 2. При выборе других декомпрессоров корректная работа ПО не гарантируется. ","It is limitation in the amount of 50 fps for 4 channels.For correct works between the device and ITV | AxxonSoft software is recommended to leave fiend decompressor blank in camera settings, or specify the decompressor \"Wavelet\". When choosing other decompressors correct work of Software is not guaranteed."]
["Stream Labs","WaveServer 1554H encoder (ONVIF)","Encoder ","0.10.2.0","4","1","+",null,"+",null,null,"768x576","+",null,"+","-","-","+.","+.","-","1. Устройство выдает 50 fps, эта частота кадров будет \"делиться\" между задействованными каналами\n2. Лучи необходимо замыкать под напряжением\n3. в Intellect настройки \"Кодек\" и \"fps\" применяются одновременно для всех каналов, Axxon Next такого ограничения лишен.\n4. Для получения звука необходимо использовать активный микрофон\n5. Телеметрия реализована через serial port, а serial port в свою очередь не поддерживается ONVIF'ом в нашем ПО. Т.о. телеметрия не работает ни в Axxon Next ни в Intellect\n6. Через ONVIF реализованы только два Луча и два Реле из 4-х и 3-х соответственно имеющихся на самом устройстве","1) If the device is running at 50 fps, then the total fps is distributed between the streams. Close the sensors when they are energized\n3. The Codec and Fps settings are applied simultaneously for all channels in Intellect. Axxon Next let you configure them individually.\n4) Use only active mics to get sound. 5. Telemetry is implemented via serial port. Serial ports are not not ONVIF ready in the AxxonSoft software. So telemetry doesn't work neither in Axxon Next nor in Intellect. 6. Only 2 sensors and 2 relays out of 4 and 3 correspondingly are supported via ONVIF"]
["Stream Labs","WaveServer 1554S encoder","Encoder ","Ubicom 2.1.0.0; PNX Bios 2.4.0.0; PNX Main 2.6.1.0","4","1",{"$nulls":3},"+",null,"768х576(PAL)/640х480(NTSC)",null,null,"+","+.","-","+","+",null,"1. Лучи следует замыкать под напряжением.\n2. Звук только с активными микрофоном и динамиком\n3. ограничение 25 fps суммарно на 4 канала","1. Close the sensors when they are energized\n2. Use only active mic and speakers to get sound. 3. The max fps is 25 for 4 streams combined."]
["Stream Labs","WaveServer 2554H encoder (Onvif)","Encoder ","PNX BIOS: 2.5.0.0 PNX MAIN: 0.16.1.0 UBICOM: 0.21.0.0","4","1","+.",null,"+.",null,null,"768x576","+",null,"+",null,null,"-","+.",null,"Устройство работает только по протоколу ONVIF.","We checked this device only via Onvif."]
["Stretch","Stretch VRC6004 card","Video Capture Board ","SDK 7.4.1","4","1","+","+","+",null,null,"PAL 720x576; NTSC 720x480","+",{"$nulls":3},"-","+","+","motion detection.","На одной платформе работает только одна плата Stretch.Для переключения стандартов PAL/NTSC требуется перезапуск ПО ITV.В intellect для корректной работы лучей/реле необходимо подключенное видео.PTZ-устройство подключается через RS485-разъем на дополнительной IO-плате.","Only 1 Stretch card works on the same platform To switch between PAL and NTSC, apply the changes and restart the AxxonSoft software. In Intellect, connect a video channel for sensors and relays to operate properly. Connect PTZ devices via RS485 in the additional IO card."]
["Stretch","Stretch VRC6008 card","Video Capture Board ","SDK 7.4.1","8","1","+","+","+",null,null,"PAL 720х576; NTSC 720x480","+",null,"+",null,"-","+","+","+","На одной платформе работает только одна плата Stretch.Для переключения стандартов PAL/NTSC требуется перезапуск ПО ITV.В intellect для корректной работы лучей/реле необходимо подключенное видео.PTZ-устройство подключается через RS485-разъем на дополнительной IO-плате.","Only 1 Stretch card works on the same platform To switch between PAL and NTSC, apply the changes and restart the AxxonSoft software. In Intellect, connect a video channel for sensors and relays to operate properly. Connect PTZ devices via RS485 in the additional IO card."]
["Stretch","Stretch VRC6404HD card","Video Capture Board ","SDK 7.4.1","4","1","+","+","+.",null,null,"1920x1072","+",{"$nulls":4},"+","+","-","На одной платформе работает только одна плата Stretch. Настройка изображения недоступна из ПО ITV. При изменении разрешения на камере (например, с 1080p на 720p) необходимо перезапустить ПО ITV. ","Only 1 Stretch card works on the same platform. You can't configure video in the AxxonSoft software. After you change the resolution e.g. from 1080 to 720, restart the AxxonSoft software to apply the changes. "]
["Stretch","Stretch VRC6416 card","Video Capture Board ","SDK 7.4.1","16","1","+","+","+",null,null,"PAL 720х576; NTSC 720x480","+",null,"+",null,"-","+","+","motion detection.","На одной платформе работает только одна плата Stretch.Для переключения стандартов PAL/NTSC требуется перезапуск ПО ITV.В intellect для корректной работы лучей/реле необходимо подключенное видео.PTZ-устройство подключается через RS485-разъем на дополнительной IO-плате.","Only 1 Stretch card works on the same platform To switch between PAL and NTSC, apply the changes and restart the AxxonSoft software. In Intellect, connect a video channel for sensors and relays to operate properly. Connect PTZ devices via RS485 in the additional IO card."]
["Stretch","Stretch VRC7008L card","Video Capture Board ","SDK 7.4.1","8","1","+","+","+",null,null,"PAL 720х576; NTSC 720x480","+",null,"+",null,null,"+","+","motion detection.","На одной платформе работает только одна плата Stretch.Для переключения стандартов PAL/NTSC требуется перезапуск ПО ITV.В intellect для корректной работы лучей/реле необходимо подключенное видео.","Only 1 Stretch card works on the same platform To switch between PAL and NTSC, apply the changes and restart the AxxonSoft software. In Intellect, connect a video channel for sensors and relays to operate properly. "]
["Stretch","Stretch VRC7016LX card","Video Capture Board ","SDK 7.4.1","16","1","+","+","+",null,null,"PAL 720х576; NTSC 720x480","+",null,"+",null,null,"+","+","+","На одной платформе работает только одна плата Stretch. Для переключения стандартов PAL/NTSC требуется перезапуск ПО ITV. В intellect для корректной работы лучей/реле необходимо подключенное видео.","Only 1 Stretch card works on the same platform. After you change the resolution e.g. from 1080 to 720, restart the AxxonSoft software to apply the changes. In Intellect, connect a video channel for sensors and relays to operate properly. "]
["Sunell","Sunell SN-IPR54/14ALDN","Camera","v1.6_build044014_216","1","3","+",null,"+",null,null,"1920x1080","+",null,"-","-",{"$nulls":3},"-","Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.При смене разрешений для кодека H.264 меняется диапазон значений битрейта. Если при переходе на новое разрешение текущий битрейт не попадает в новый диапазон, то настройка не применяется.Частота опорных кадров задается в секундах и может принимать значения от 1 до 3.","To connect to camera in Axxonsoft, please specify 30001 port. If you change the resolution for the H.264 codec, value of bit rate will be changed. If you select a new resolution, a new bit rate misses the new range, the setting will not be applied. Key frame rate is set in seconds and can have value from 1 to 3.","new"]
["Sunell","Sunell SN-IPV54/14UDR","Camera","v1.6_build044014_145","1","3","+","-","+","-","-","1920x1080","+","-","-","-","-","-","-",null,"Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.При смене разрешений для кодека H.264 меняется диапазон значений битрейта. Если при переходе на новое разрешение текущий битрейт не попадает в новый диапазон, то настройка не применяется.Частота опорных кадров задается в секундах и может принимать значения от 1 до 3.","To connect to camera in Axxonsoft, please specify 30001 port. If you change the resolution for the H.264 codec, value of bit rate will be changed. If you select a new resolution, a new bit rate misses the new range, the setting will not be applied. Key frame rate is set in seconds and can have value from 1 to 3."]
["Sunell","Sunell SN-IPR54/31AKDN","Camera ","v1.6_build044014_148","1","3","+",null,"+",null,null,"2048x1536","+",{"$nulls":7},"Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\nНабор разрешений в ПО ITV/Axxon зависит от значения настройки Source Resolution в веб-интерфейсе.\nПри смене разрешений для кодека H.264 меняется диапазон значений битрейта. Если при переходе на новое разрешение текущий битрейт не попадает в новый диапазон, то настройка не применяется.\nДля корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz.","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. The list of resolution in Axxonsoft SW depends on value of Source Resolution in web interface.\n3. When resolution for H.264 is changed, range of bitrate value is also changed. If there's no current bitrate value for new resolution, in this case setting is not applied.\n4. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["Sunell","Sunell SN-IPV54/31UDR","Camera ","v1.6_build044014_148","1","2","+",null,"+",null,null,"2048x1536","+",{"$nulls":7},"Для подключения к устройству необходимо в настройках подключения в ПО ITV/Axxon указывать порт 30001.\nНабор разрешений и значение максимального fps в ПО ITV/Axxon зависит от значения настройки Source Resolution в веб-интерфейсе.\nПри смене разрешений для кодека H.264 меняется диапазон значений битрейта. Если при переходе на новое разрешение текущий битрейт не попадает в новый диапазон, то настройка не применяется.\nДля корректной работы настройки FPS в ПО ITV/Axxon рекомендуется через веб-интерфейс установить на камере режим 60Hz.","1. To connect to camera in Axxonsoft SW, please specify 30001 port.\n2. The list of resolution and maximum fps value in Axxonsoft SW depends on value of Source Resolution in web interface.\n3. When resolution for H.264 is changed, range of bitrate value is also changed. If there's no current bitrate value for new resolution, in this case setting is not applied.\n4. Please set on 60Hz mode in camera web interface to work with FPS setting in Axxonsoft SW correctly."]
["Tamron","Tamron 300QV-P-CM","Fisheye Camera","20131118.172655","1","9","+","+","+",null,null,"640x480 (H.264) / 1280x960 (mjpeg) / 1280x960 (mpeg4)","+",null,"+","-","-","-","-","-","В ПО ITV при переходе на полное разрешение, на камере происходит переключение профиля камеры с compensated на originalВ ПО Axxon для того чтобы получать видео с 3, 4 и 6 потоков, необходимо в веб-интерфейсе камеры для настройки split выбрать соответствующий режим","In Axxon software when you change resolution to full value, the camera switches profile from compensated to original. In Axxon software to receive video from 3, 4 and 6 streams, you should select the appropriate mode for Split setting in web-interface of the camera.","improved"]
["Tantos","Tantos TSi-C211F","Camera"," v3.3.2.1","1","3","+","+","+",null,"-","1920x1080","+",null,"+",null,"-",null,"-"]
["Tantos","Tantos TSi-SDW211Z22","Camera","v1.6_build044014_213","1","3","+","-","+",null,"-","1920x1080","+",null,null,"-","+",null,"-",null,"Настройка \"Частота опорных\" в Интеллекте задается в секундах и может принимать значения от 1 до 3.","In Axxon Intellect \"Reference rate\" setting is expressed in seconds and can take values ​​from 1 to 3."]
["TBK","TBK DVR PLUS 4","DVR","V2.2.4 build 130702","4","2",null,null,"+",null,null,"704x576","+"]
["Tiandy","Tiandy TC-NC9000S3-2MP-E","Camera","NVSSv5.2.0_20121109","1","2","+","-","+",null,"-","1920x1080","+",null,"-","-","-","-","-"]
["Tiandy","Tiandy TC-NC9100S3-2MP-E-IR30","Camera","5.2.0_20121109","1","2","+","-","+","-","-","1920x1080","+",null,"-","-","-","-","-","-"]
["Tiandy","Tiandy TC-NC9200S3-2MP-E-IR30","Camera","5.2.0_20121109","1","2","+","-","+","-","-","1920x1080","+",null,"-","-","-","-","-","-"]
["Tiandy","Tiandy TC-NC9400S3E-MP-IR30","Camera","NVSS_V6.0.0_20130115","1","2","+","-","+",null,"-","1280x960","+",null,"-","-","-","-","-"]
["Tiandy","Tiandy TC-NC9500S3E-MP-IR30","Camera","V6.0.0_20130115","1","2","+","-","+","-","-","1280x960","+",null,"-","-","-","-","-","-"]
["TRENDnet","TRENDNet TV-IP100W","Camera ","3.12 (2005-08-18)","1",null,"+",{"$nulls":4},"640x480",{"$nulls":7},"-","1. При разрешении 640х480на скорость видео накладывется ограничение в 10 fps. Ограничение самой камеры, а не нашего ПО","1) With the 640x480 resolution, the frame rate is limited to 10 fps. This is a limitation of the camera itself, not of our software. "]
["TRENDnet","TRENDnet TV-IP110","Camera ","1.0.0.57","1",null,"+",{"$nulls":4},"640x480",{"$nulls":8},"1.Настройки fps, качество и разрешение принимаются после 30 сек ребута.\n","1. After you change the settings (resolution, quality, frame rate), the camera may take up to 30 seconds to restart.\n"]
["TRENDnet","TRENDNet TV-IP201","Camera ","2.00 build: 110","1",null,"+",{"$nulls":4},"640x480",null,null,"+",null,null,"-","+",null,"1. Интегрирован только PCM аудиокодек. ADPCM пока не интегрирован\n ","1) The PCM audio codec is integrated. ADPCM is not integrated yet.\n "]
["TRENDnet","TRENDNet TV-IP212W","Camera ","1.0.0 build: 18","1",null,"+","+",{"$nulls":3},"640x480",null,null,"+","-",{"$nulls":3},"-","1.Настройки fps, качество и разрешение принимаются после 30 сек ребута. Особенность камеры2. Настройка цветности не работает на самой камере. Т.е. даже в родном вебе значение цветности меняется, но картинка не меняется\n","1. After you change the settings (resolution, quality, frame rate), the camera may take up to 30 seconds to restart. This is a limitation of the camera itself.2 The Color setting on the camera does not work . i.e. it is applied in the web interface, but the video image doesn't change.\n"]
["TRENDnet","TRENDNet TV-IP312W","Camera ","1.0.0 build: 56","1",null,"+","+.",{"$nulls":3},"640x480",null,null,"+","-",{"$nulls":3},"-","1.Настройки fps, качество и разрешение принимаются после 30 сек ребута. Особенность камеры\n","1. After you change the settings (resolution, quality, frame rate), the camera may take up to 30 seconds to restart. This is a limitation of the camera itself.\n"]
["TRENDnet","TRENDNet TV-IP400","Camera ","3.36","1",null,"+",{"$nulls":4},"640x480",{"$nulls":4},"+",null,null,"-","1. При разрешении 640х480 накладывается ограничение на скорость видео в 10 fps. Ограничение самой камеры, а не нашего ПО\n2. У камеры нет оптических зума и фокуса, поэтому кнопки управления \"Масштаб\" и \"Фокус\" на Панели Телеметрии работать не будут.\n3. У камеры нет настройки скорости поворота в чистом виде, поэтому настройка \"Скорость\" на Панели Телеметрии изменяет не скорость, а угол поворота.","1) With the 640x480 resolution, the frame rate is limited to 10 fps. This is a limitation of the camera itself, not of our software. \n2. Since the camera doesn't have optical zoom and focus controls, the Zoom and Focus control buttons do not work in the PTZ Control Panel.\n3) Since the camera doesn't have the Pan Speed control as such, you can use the Speed setting in he PTZ Control Panel to change its pan angle."]
["TRENDnet","TRENDnet TV-IP410","Camera ","1.1.0 build: 53","1","1","+",{"$nulls":4},"640x480",{"$nulls":4},"+.","-","+","-","Изменение настроек видео приводит к перезагрузке устройства.","If you change video settings, the camera restarts."]
["TRENDnet","TRENDnet TV-IP422","Camera ","1.1.0 build: 68","1","1","+","-",{"$nulls":3},"640x480",null,null,"+","-","+","-","+","-","Изменение настроек видео приводит к перезагрузке устройства.","If you change video settings, the camera restarts."]
["TVT","TVT TD2304SS-B","DVR","3.2.0.P-3520A-00","4","1","-","-","+","-","-","704x480","-",null,"-","-","-","-","-","-","При настройке параметров подключения в ПО Axxon / ITV необходимо указывать порт, соответствующий аналогичной настройке в веб-интерфейсе устройства (CONFIG → Network → Server Port). По умолчанию значение порта - 6036.","When setting the connection parameters in Axxonsoft, specify the port corresponding to the similar setting in the camera web interface (CONFIG → Network → Server Port). Default value of the port is 6036."]
["UDP","UDP IPE5500","Encoder","1.06.05 ","1","2","+","+","+",null,"-","720x576 (PAL) / 720x480 (NTSC)","+",null,"+.","+.","+","+","+",null,"В MJPEG максимальная частота кадров - 5 fps.Настройки для аудиовыхода и аудиовхода должны быть одинаковыми.Луч приходит в положение готовности спустя 10-50 секунд после включения в нашем ПО. В дальнейшем замыкание/размыкание луча отрабатывается без задержек.Аудио-выход камеры воспроизводит звук с задержкой в 5 секунд - проблема камеры.Чтобы заработал звук, нужно выставить максимальный уровень громкости на динамике.","With MJPEG, maximum frame rate is 5fps. The audio input and output settings must be identical. It takes a sensor 10 to 50 seconds to activate after it has been enabled in the AxxonSoft software. After that, the sensor opens and closes with no delay. The problem is that audio output on the camera is delayed by 5 seconds. To get audio, you need to tune max volume value at audio out."]
["UDP","UDP NVC1000","Encoder ","1.06.05","1","2","+","+","+",null,null,"720x576 (PAL) / 720x480 (NTSC)","+",null,"+.","+","+","+","+","-","В кодеке MJPEG возможны задержки видео и падение частоты кадров, чем выше качество видео, тем они сильнее. В веб-интерфейсе поведение такое же.Настройки для аудиовыхода и аудиовхода должны быть одинаковыми.Луч приходит в положение готовности спустя 10-50 секунд после включения в нашем ПО. В дальнейшем замыкание/размыкание луча отрабатывается без задержек.Аудио-выход камеры воспроизводит звук с задержкой в 5 секунд - проблема камеры.","With MJPEG, video is delayed the frame rate drops, this all the more frequent and steep when you want better quality video. Same in the web interface. The audio input and output settings must be identical. It takes a sensor 10 to 50 seconds to activate after it has been enabled in the AxxonSoft software. After that, the sensor opens and closes with no delay. The problem is that audio output on the camera is delayed by 5 seconds."]
["UDP","UDP NVC4000L","Encoder ","1.2.0","4","1",null,null,"+",null,null,"720x480","+"]
["Veilux","Veilux VVIP-2L2812","Camera","v1.6_build044014_117","1","3","+",null,"+",null,null,"1920x1080 / 1280x720","+",null,"-","-",null,"-","-",null,"Максимальное разрешение (1920х1080 или 1280х720) зависит от настройки Source Resolution в веб-интерфейсеВ настройках подключения в ПО ITV/Axxon нужно указывать порт, соответствующий значению поля Control Port в веб-интерфейсе камерыИзменение ТВ-стандарта нужно делать через веб-интерфейс","The max. resolution (1920х1080 or 1280х720) depends on the Source Resolution setting in the camera web interface. Specify  Control Port in the VMS settings. You can configure TV standard via web interface.","improved"]
["Videosec","Videosec ICS-20F","Camera ","vt20120525NSA","1","2","+",null,"+",null,null,"1920x1080","+"]
["Videosec","Videosec ICS-20W","Camera ","vt20120525NSA","1","2","+",null,"+",null,null,"1920x1080","+"]
["Videosec","Videosec ICS-50W","Camera ","vt20120525NSA","1","2","+",null,"+",null,null,"2592x1944(H264)/1920x1080(MJPEG)","+"]
["Videosec","Videosec ID-20","Camera ","vt20120525NSA","1","2","+",null,"+",null,null,"1920x1080","+"]
["Videosec","Videosec IPTZ-20","Camera ","vt20120525NSA","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":3},"+"]
["Videosec","Videosec IRD-20W","Camera ","vt20120525NSA","1","2","+",null,"+",null,null,"1920x1080","+"]
["Videosec","Videosec IRW-20W","Camera ","vt20120525NSA","1","2","+",null,"+",null,null,"1920x1080","+"]
["ViDigi","ViDigi S-2101 / S-2103f / S-2104v / S-2105v / S-2106v","Camera","1.0.5.1.019","1","2","+",null,"+",null,null,"1920x1080","+",null,"+","+","-","+","+","motion detection",null,null,"improved"]
["VIDO","VIDO G70HD820","Camera ","2.7.5 May 28 2012","1","2","+",null,"+",null,null,"1920x1072","+",null,"-","-","+.","-","-",null,"1. Для работы фокуса необходимо для настройки Focus установить значение Manual.\n2. Для работы с нашим ПО нужно указывать Dev Port из вкладки Settings -> ServerParam\n3. В ПО ITV/Axxon устройство определяется как EH4300.","1. To make Focus work, set its settings to Manual.\n2. To make it work with AxxonSoft software, you have to select Dev Port in the Settings -> ServerParam\n3. In the AxxonSoft products, this camera is identified as EH4300."]
["VIDO","VIDO HX600HD / IRC600HD / IRC650HD","Camera ","2.7.5","1",null,"+",null,"+",null,null,"1920х1072","+",null,"-","-","+","-","-",null,"1. В ПО ITV/Axxon модели определяются как VIDO SE600.","1. In the AxxonSoft products, the cameras are identified as VIDO SE600."]
["Visiocom","Visiocom VR-9632NI-ST","NVR","V2.1.0 build 111017","32","2",null,null,"+",null,null,"2048x1536",{"$nulls":8}," Для подключения к устройству используется порт 8000 "," Please use port 8000 to connect to device."]
["Vision","VISIONxIP PM2Ti","Camera","1.1.3.3 20130620","1","3","+","-","+",null,"-","1920x1080","+",null,"-","-","+","-","-",null,"В ПО ITV со стандартным разрешением камера не показывает видео, особенность работы камеры.","In AxxonSoft products, standard camera resolution doesn't show video (camera's feature)."]
["Vision","Vision VC58SM3i","Camera ","1.1.0.16 20120316","1","2","+",null,"+",null,null,"H264: 1920x1080 MJPEG: 1280x720","+",null,"-","-",null,"-","-","-","1. Разрешение на втором потоке не может быть больше, чем на первом. Например, если на первом стоит 320x240, то на втором не применяется 640x480 .Если на первом потоке выбрано разрешение 640x480, то на втором автоматически тоже устанавливается 640x480 и никакие другие не применяются.\n2. На камере не работает настройка яркости.","1. Resolution on the second stream can not be higher than on the first. For example, if there is 320x240 on the first stream, then 640x480 is not applied on the second. If on the first stream there is 640x480, then 640x480 is automatically set on the second stream.\n2. Brightness control is disabled on the camera.\n"]
["Vision","Vision VDA110SM3i-IR","Camera ","1.1.0.16 20120316","1","2","+",null,"+",null,null,"H264: 1920x1080 MJPEG: 1280x720","+",null,"-","-",null,"-",null,"-","1. Разрешение на втором потоке не может быть больше, чем на первом. Например, если на первом стоит 320x240, то на втором не применяется 640x480 .Если на первом потоке выбрано разрешение 640x480, то на втором автоматически тоже устанавливается 640x480 и никакие другие не применяются.","1. Resolution on the second stream can not be higher than on the first. For example, if there is 320x240 on the first stream, then 640x480 is not applied on the second. If on the first stream there is 640x480, then 640x480 is automatically set on the second stream and any others aren't applied."]
["Vision","Vision VDA50SMi","Camera ","1.1.0.16 20120316 ","1","2","+",null,"+",null,null,"1280x720","+",{"$nulls":6},"-","1. Разрешение на втором потоке не может быть больше, чем на первом. Например, если на первом стоит 320x240, то на втором не применяется 640x480 .Если на первом потоке выбрано разрешение 640x480, то на втором автоматически тоже устанавливается 640x480 и никакие другие не применяются.","1. Resolution on the second stream can't be more than on the first. For example, if on the first costs 320x240, on the second it is not applied 640x480. If on the first stream resolution 640x480 is chosen, on the second automatically too is established 640x480 and any others aren't applied."]
["Vitek","Vitek VT-PTZ220NP","Camera ","4.16-B0-ds-VI","1","2","+",null,"+",null,null,"1920x1080","+",{"$nulls":3},"+","-","-","-"]
["Vitek","Vitek VTC-IR402","Camera ","4.16-B2-ds-VI","1","2","+",null,"+",null,null,"1280x720 ","+"]
["Vitek","Vitek VTD-MV20VRN","Camera ","4.18-B1-ds","1","2","+",null,"+",null,null,"1920x1080","+"]
["Vivotek","Vivotek CC8130","Camera ","CC8130-VVTK-0200c","1","2","+",null,"+",null,null,"1280x800","+",null,"+",{"$nulls":4},"motion detection; tampering detection","Цифровая телеметрия работает только на первом потоке.","Digital PTZ works only on first stream."]
["Vivotek","Vivotek FD7131","Camera ","0201c","1",null,"+",{"$nulls":4},"640x480"]
["Vivotek","Vivotek FD7141","Camera ","0101b","1",null,"+",{"$nulls":4},"720x480",{"$nulls":7},"-"]
["Vivotek","Vivotek FD8131/V","Camera ","0100e","1","4","+","+","+",null,null,"1280x800","+",{"$nulls":3},"+"]
["Vivotek","Vivotek FD8133(V) / FD8134(V)","Camera","FD8134-VVTK-0109a","1","4","+","+","+","-","-","1280x800","+","-","-","-","-","+","-","motion detection; tampering detection","Частота опорных в Интеллекте указывается в миллисекундах.","In Intellect, you can set up the key frame rate in milliseconds."]
["Vivotek","Vivotek FD8135H","Camera ","FD8135_VVTK_0201a","1","2","+","+","+",null,null,"1280x800","+",null,"+","+","+","+","+","motion detection; tampering detection"]
["Vivotek","Vivotek FD8136","Camera ","FD8136-VVTK-0101a","1","2","+","+","+",null,null,"1280x800","+",null,"+",null,"+",null,null,"motion detection; tampering detection"]
["Vivotek","Vivotek FD8137H / FD8137HV","Camera","FD8137-VVTK-0101a","1","2","+","-","+","-","-","1280x800","+","-","-","-","+","-","-","motion detection"]
["Vivotek","Vivotek FD8151V","Camera ","FD8151V-VVTK-0103a","1","2","+",null,"+",null,null,"1280x1024","+",null,"+",null,"+","+",null,"motion detection; tampering detection"," Цифровая телеметрия работает только на первом потоке.","Digital PTZ works only on first stream."]
["Vivotek","Vivotek FD8161","Camera ","0105b ","1","4","+","+","+",null,null,"1600x1200","+",{"$nulls":3},"+.",null,null,"-","1. Особенность данной камеры: потоки (streams) управления телеметрией. Для каждого из них свой набор пресетов. ","1) This is a peculiarity of the camera itself. PTZ control panel settings. Each stream has a range of presets of its own. "]
["Vivotek","Vivotek FD8162","Camera ","0103a","1","4","+","+","+",null,null,"1920x1080","+",null,"+",null,"+",null,null,"+"]
["Vivotek","Vivotek FD8335H","Camera","FD8335-VVTK-0202c","1","2","+","+","+",null,"-","1280x800","+",null,"+",null,"+","+","+","motion detection; hacking detection"]
["Vivotek","Vivotek FD8362(E)","Camera","FD8362E-VVTK-0103f","1","4","+","+","+",null,null,"1920x1080","+",null,"+",null,"+","+","+","motion detection; tampering detection",null,null,"improved"]
["Vivotek","Vivotek FE8171V","Fisheye Camera","0100d","1","4","+","+","+",null,null,"1536x1536","+",null,"+",null,null,"+","+","-","Через Onvif работает видео и звук.","Video and audio streams works via ONVIF."]
["Vivotek ","Vivotek FE8172 / FE8172V","Fisheye Camera","FE8172-VVTK-0100g","1","3","+","+","+",null,null,"1920 x 1080 (FullHD) / 1920 x 1920 (Fisheye)","+",null,"+",null,null,"+","+","motion detection; tampering detection","В Интеллекте интервал включения опорных кадров задается в миллисекундах и может принимать следующие значения: 250, 500, 1000, 2000, 3000, 4000.","In Intellect, you can set up the keyframe rate in milliseconds at: 250, 500, 1000, 2000, 3000, 4000."]
["Vivotek","Vivotek IP6112/6122","Camera ","0105b","1",null,"+","+",{"$nulls":3},"704x576",null,null,"-","-",null,"-","+","-","1) для камеры с прошивкой 0101e следует использовать граббер Vivotek, для камеры с прошивкой 0105b - Vivotek(mjpeg) и Vivotek(mpeg4)","1) For cameras with the 0101e firmware use the Vivotek, grabber, for version 0105b - Vivotek(mjpeg) and Vivotek(mpeg4)"]
["Vivotek","Vivotek IP7130","Camera ","0101b","1","2","+",{"$nulls":4},"640x480"]
["Vivotek","Vivotek IP7133","Camera ","0200b","1",null,"+",{"$nulls":4},"640x480",{"$nulls":4},"-",{"$nulls":3},"у камеры Digital PTZ","The camera has Digital PTZ (digital telemetry)."]
["Vivotek","Vivotek IP7138","Camera ","0300a","1",null,"+","+",{"$nulls":3},"1280x1024(MJPEG) / 800x600(MPEG-4)",null,null,"+.","-",null,"+","+","-","1. У самой камеры в Полном разрешении есть ограничение на частоту кадров, равное 8 fps","1. With the Full resolution, the camera itself allows 8 fps max. "]
["Vivotek","Vivotek IP7139","Camera ","0201b","1",null,"+","+",{"$nulls":3},"1280x1024(MJPEG) / 800x600(MPEG-4)",null,null,"+.","-",null,"+","+","-","1. У самой камеры в Полном разрешении есть ограничение на частоту кадров, равное 8 fps","1. With the Full resolution, the camera itself allows 8 fps max."]
["Vivotek","Vivotek IP7154","Camera ","0200a","1",null,"+",{"$nulls":4},"640x480",{"$nulls":3},"-"]
["Vivotek","Vivotek IP7160","Camera ","0103c","1",null,"+","+",{"$nulls":3},"1280x720",null,null,"+.","-","+",null,null,"-","1. Камера не поворотная, но есть Digital Telemetry","1. This is not a PTZ camera, but it has Digital Telemetry. "]
["Vivotek","Vivotek IP7161","Camera ","0103b","1","4","+",{"$nulls":4},"1600x1200",{"$nulls":4},"+",null,null,"-"]
["Vivotek","Vivotek IP7330","Camera ","0200b","1",null,"+","+",{"$nulls":3},"640x480",{"$nulls":5},"+",null,"-"]
["Vivotek","Vivotek IP7361","Camera ","0200b","1",null,"+",{"$nulls":4},"1280x720",null,null,"+",null,"+",{"$nulls":3},"камера поддерживает только Digital PTZ","The camera supports only Digital PTZ. "]
["Vivotek","Vivotek IP8133/W","Camera ","0102a","1","3","+","+","+",null,null,"1280x800","+",{"$nulls":6},"+"]
["Vivotek","Vivotek IP8151","Camera ","0301e","1","4","+","+","+",null,null,"1280x1024","+",null,"+","+","+","+","+","+","В мануале написано, что камера поддерживает аналоговую телеметрию (внешнее поворотное устройство). Заставить ее работать не удалось.","According to the guide, the camera supports analog telemetry (a pan/tilt drive). We did not manage to make it work. "]
["Vivotek","Vivotek IP8151P","Camera ","0300f","1","4","+","+","+",null,null,"1280x1024","+",{"$nulls":3},"+",null,null,"+","Камера отличается от IP8151 списком настроек, т.к. тестирование производилось на разных версиях прошивки. Физически камеры различаются только параметрами оптики (судя по спецификации).","The list of settings for that camera is different from the one of IP8151 as we tested the cameras with different firmware versions. According the specs, the cameras differ in the optics."]
["Vivotek","Vivotek IP8152","Camera ","IP8152-VVTK-0101b","1","2","+",null,"+",null,null,"1280x1024","+",null,"+","+","+","+",null,"motion detection; tampering detection"," Цифровая телеметрия работает только на первом потоке.","Digital PTZ works only on first stream."]
["Vivotek","Vivotek IP8161","Camera ","0103a","1","4","+","+","+",null,null,"1600x1200",{"$nulls":4},"+",null,null,"-"]
["Vivotek","Vivotek IP8162/-P","Camera ","0100f","1","4","+","+","+",null,null,"1920x1080","+",null,"+",null,"+",null,null,"+"]
["Vivotek","Vivotek IP8172(P)","Camera","IP8172-VVTK-0102b","1","3","+","+","+","-","-","2560x1920","+","-","+","-","+","+","+","motion detection; tampering detection","Доступный набор разрешений в Интеллекте зависит от настройки в веб интерфейсе камеры ( Configuration > Media  > Video > FOV).","The list of available resolutions in Intellect depends on the settings of camera web interface (Configuration > Media  > Video > FOV)."]
["Vivotek","Vivotek IP8330","Camera ","0100g","1",null,"+",{"$nulls":4},"640x480"]
["Vivotek","Vivotek IP8332 / IP8332-C","Camera","IP8332-VVTK-0200d","1","4","+","+","+","-","-","1280x800","+","-","-","-","-","-","-","motion detection; tampering detection","\nЧастота опорных кадров в Интеллекте указывается в миллисекундах. ","In Intellect, you can set up the key frame rate in milliseconds."]
["Vivotek","Vivotek IP8335H","Camera ","0100h","1","2","+","+","+",null,null,"1280x800","+",null,"+","+","+","+","+","+"]
["Vivotek","Vivotek IP8352","Camera ","0102a","1","4","+","+","+",null,null,"1280x1024","+",null,"+","+.","+","+","+","+","Аудио-выход не работает, если выбран кодек MJPEG.","If you select the MJPEG codec, the audio output does not work."]
["Vivotek","Vivotek IP8362","Camera ","0101b","1","4","+","+","+",null,null,"1920x1080","+",null,"+","-","+","+","+","-","Через Onvif не работают лучи.","Via the ONVIF protocol, the sensors do not work. "]
["Vivotek","Vivotek IP8371E","Camera","IP8371E-VVTK-0100j","1","4","+","+","+",null,null,"2048x1536(3mp)/1920x1080(Full HD)","+",null,"-","-","+","-","-","-",null,null,"improved"]
["Vivotek","Vivotek MD7560D","Camera ","MD7560-VVTK-0100e","1","4","+","+",{"$nulls":3},"1600x1200","+",null,null,"-","+",null,null,"-"]
["Vivotek","Vivotek MD8562","Camera ","0102a","1","4","+","+","+",null,null,"1920x1080","+",{"$nulls":3},"+",null,null,"+"]
["Vivotek","Vivotek PT8133/W","Camera ","0100e","1","3","+","+","+",null,null,"1280x800","+",{"$nulls":3},"+",null,null,"+"]
["Vivotek","Vivotek PZ7111","Camera ","0200a","1",null,"+",{"$nulls":4},"704x480",{"$nulls":4},"+."]
["Vivotek","Vivotek PZ7131","Camera ","0200a","1",null,"+",{"$nulls":4},"640x480",{"$nulls":3},"-","+",null,null,"-"]
["Vivotek","Vivotek PZ81x1/W","Camera ","0100e","1","4","+","+","+",null,null,"720x480","+",{"$nulls":3},"+.",null,null,"+"]
["Vivotek","Vivotek SD73x3 series","Camera ","0103c","1",null,"+",{"$nulls":4},"704x480",{"$nulls":4},"+."]
["Vivotek","Vivotek SD81x1","Camera ","0103c","1","3","+","+","+",null,null,"720x480(NTSC)/720x576(PAL)","+",{"$nulls":3},"+"]
["Vivotek","Vivotek SD8362E","Camera ","SD8362-VVTK-0203d","1","4","+","+","+",null,null,"1920x1080","+",null,"+","+","+","+","+","motion detection."]
["Vivotek","Vivotek SD8363E","Camera","SD8363-VVTK-0200d","1","4","+","+","+",null,"-","1920x1080","+",null,"+","+","+","+","+","motion detection; audio detection","Кодек SVC не интегрированМаксимальное разрешение и FPS, в ПО ITV, зависит от выбранного значения(Full HD (MAX1080P 30fps) или Exceptional frame rate ( 720P 60fps) ) в разделе FOV веб-интерфейса камеры. При смене этих режимов в веб-интерфесе камеры, для первого потока автоматически применяется кодек SVC","SVC codec is not integrated. In AxxonSoft products, maximum resolution and FPS products depends on value (Full HD (MAX1080P 30fps) or Exceptional frame rate (720P 60fps)) in FOV section of web-interface. When you change the modes in camera web interface, SVC codec will be automatically applied on first stream."]
["Vivotek","Vivotek SD83X2","Camera ","SD83X3-VVTK-0202b","1","4","+","+","+",null,null,"720x576","+",{"$nulls":3},"+",{"$nulls":3},"ТВ-стандарт нужно выбирать в соответствии с модификацией камеры:\nSD8322 - PAL\nSD8312 - NTSC","TV-standart should be selected in accordance with camera's modification: SD8322- PAL, SD8312- NTSC."]
["Vivotek","Vivotek SD83X3","Camera ","0100g","1","4","+","+","+",null,null,"720x576","+",{"$nulls":3},"+",null,null,"motion detection","ТВ-стандарт нужно выбирать в соответствии с модификацией камеры:SD8323 - PALSD8313 - NTSC","Select the TV standard as follows: SD8323 - PAL, SD8313 - NTSC"]
["Vivotek","Vivotek SF8172 / SF8172V","Fisheye Camera","SF8172-VVTK-0100d","1","3","+","+","+",null,null,"1920x1920 / 1920x1080","+",null,"+","-","+","+","+","motion detection; tampering detection","В Интеллекте частота опорных кадров задается в миллисекундах и может принимать следующие значения: 250, 500, 1000, 2000, 3000, 4000.Для данной камеры реализована функция Panoramic PTZ. Для ее работы требуется поворотная камера Vivotek SD8362E. Более подробную информацию можно найти на сайте Vivotek.","In Intellect, you can set up the keyframe rate in milliseconds at: 250, 500, 1000, 2000, 3000 and 4000. Panoramic PTZ feature is enabled for this camera. Vivotek ","new"]
["Vivotek","Vivotek VS2403 coder","Encoder ","VS2403-VVTK-0103e","4","1","+",{"$nulls":4},"704x576","+",null,"-","-","+","+","+",null,"Видеосервер физически имеет 4 канала. Но интегрирован в наше ПО как 5-канальный. Через 5-й канал идет видео со всех камер сразу в режиме 4-кратора.Настройки изображения работают только при выключенном веб-интерфейсе.Удалять предустановки телеметрии через ПО ITV нельзя.","Physically, the video encoder has 4 channels. But our software integrates it as a 5-channel device. Channel 5 feeds video from all cameras simultaneously in the Quad mode. Video settings are available only if the web interface is disabled. You can not delete presets via the AxxonSoft software."]
["Vivotek","Vivotek VS8102 encoder","Encoder ","0200c5","1",null,"+",{"$nulls":4},"720x480"]
["Vivotek","Vivotek VS8401","Encoder ","0200a","4","2","+","+","+",null,null,"720x480/640х480","+",null,"-","-","-","-","-","-","1. Частота опорных кадров в Интеллекте задается в миллисекундах.","1. In Intellect, you set the keyframe rate in milliseconds."]
["Vivotek","Vivotek VS8801","Encoder ","0200a","8","1","+","+","+",null,null,"720x480","+",null,"-","-","-","-","-","-"]
["WuT","WuT WEB-IO","I/O Module","3.40","0",{"$nulls":6},"from WEB",{"$nulls":5},"+","+",null,"1. 12 Input x 12 Output Нумерация в Интеллекте начинается с 1 (единицы), а на устройстве - с 0 (нуля).\n2. При включении/выключении всех реле одновременно (макрокомандой, например) некоторые могут не сработать и остаться в предыдущем состоянии.","1. 12 Input x 12 Output. Intellect's numbering tart with 1, whereas the device's range starts with 0.\n2. If you enable/disable all relays at a time e.g. with a macro, some will fail to switch to the new status."]
["Y-cam ","Y-cam Bullet HD 1080","Camera ","1.3057","1","3","+",null,"+",null,null,"1920x1080","+"]
["Y-cam","Y-cam Cube HD 1080","Camera","5.46","1","3","+","+","+",null,"-","1920x1080","+",null,null,"-","-","-","-"]
["Y-cam","Y-cam Cube HD 720","Camera","5.46","1","3","+","+","+",null,"-","1280x720","+",null,"+","-","-","-","-"]
["Yudor Technologies","Yudor CO-i03MY1 (YUC-HS94)","Camera ","V1.0.32_Y ","1","2","+","-","+",null,null,"640x480","+",null,"+","+",{"$nulls":3},"+"]
["Yudor Technologies","Yudor CO-i04DY2(3.7-12) (YUC-HM93-312)","Camera ","V1.0.32_Y","1","2","+","-","+",null,null,"720x576","+",null,"+","+",null,"+","+","+","Между переходами луча в состояние \"замкнуто\" должен соблюдаться временной интервал, настраиваемый через веб-интерфейс. Минимальное значение - 10 секунд.Через Onvif камера работает только в режиме совместимости. Видео и звук идут, но никакие настройки не применяются.В Интеллекте поиск находит камеру как FineCCTV.","You can configure the delay before a sensor closes. Min 10 seconds. The camera works via the ONVIF protocol, but only in compatibility mode Video and audio streams are there but changes can't be applied. Intellect identifies the camera as FineCCTV."]
["Yudor Technologies","Yudor CO-i13MY1 (CO-YUC-HS95)","Camera ","V1.0.32_Y","1","2","+","-","+",null,null,"1280x1024","+",null,"+","+",{"$nulls":3},"+","На камере есть ограничение FPS в зависимости от разрешения:\n Для разрешений не больше 640x480 ограничение составляет 30 fps, для больших разрешений - 15. Ограничение включается для всех потоков, если разрешение >640x480 установлено хотя бы на одном из двух потоков.","The camera has frame rate limits (depending on the resolution):\n For resolutions lower than 640x480 the max fps is 30, fro greater resolutions it is 15. This limitation applies to all streams if a resolution greater than 640x480 is set for any of the 2 streams."]
["Yudor Technologies","Yudor CO-i20DY2(2,7-9) (CO-YUC-HM96-279)","Camera ","V1.0.32_Y","1","2","+","-","+",null,null,"1600x1200","+",null,"+","+",null,"+","+","+","Поиск в Axxon Next не определяет прошивку: ее нужно выбрать самостоятельно.Между переходами луча в состояние \"замкнуто\" должен соблюдаться временной интервал, настраиваемый через веб-интерфейс. Минимальное значение - 10 секунд.Прошивка V1.0.32_Y: через Onvif камера работает только в режиме совместимости. Видео и звук идут, но никакие настройки не применяются. Поиском не находится.В Интеллекте поиск находит камеру как FineCCTV.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В Axxon Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.","In Axxon Next, the search does not find the device's firmware. You must select the right firmware yourself. You can configure the delay before a sensor closes. Min 10 seconds. With firmware V1.0.32_Y and via the ONVIF protocol, the camera works only in the compatibility mode. Video and audio streams are there but changes can't be applied. The camera can't be located by search. Intellect device discovery identifies it as Fine CCTV. The camera offers the Video Parameters option (the max. resolution and max. frame rate). In Axxon Next, you must make sure that there is not conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value."]
["Yudor Technologies","Yudor CO-i20DY2IRPV (CO-YUC-Hi96RP)","Camera ","V1.0.32_Y","1","2","+","-","+",null,null,"1600x1200","+",null,"+","+",null,"+","+","+","Настройка \"Параметры видео\" определяет ограничение FPS в зависимости от разрешения. Для получения максимального FPS необходимо следить за тем, чтобы разрешение настройки \"Параметры видео\" было не больше, чем выбренное разрешение получаемого видео.После размыкания датчика реакция на следующее замыкание может произойти не раньше, чем через 10 секунд.","The Video Parameters setting is used to limit fps depending on the resolution: To get the maximum frame rate, make sure that the Video Parameters setting has the the same or lower resolution than you selected for your video. After opening, the sensor can close in not earlier than 10 seconds."]
["Yudor Technologies","Yudor CO-YUC-H696","Camera ","V1.0.26_Y","1","2",null,null,"+",null,null,"1600x1200",null,null,"+","-","+","+","+","+","Поиск в Axxon Next не определяет прошивку: ее нужно выбрать самостоятельно.Прошивка V1.0.26_Y: камера работает по Onvif только в режиме совместимости, поиском как Onvif не находится.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В Axxon Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.","In Axxon Next, the search does not find the device's firmware. you must select the right firmware yourself. The V1.0.26_Y firmware: Via the ONVIF protocol, the camera works only in compatibility mode; the search does not find the camera as a device that supports ONVIF. The camera has the ***Video Parameters *** option (the max. resolution and max. frame rate). In Axxon Next, you must make sure that there is not conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value."]
["Yudor Technologies","Yudor CO-YUC-H696P","Camera ","V1.0.26._Y","1","2",null,null,"+",null,null,"1600x1200",null,null,"+","-","+","+","+","+","Поиск в Axxon Next не определяет прошивку: ее нужно выбрать самостоятельно.Прошивка V1.0.26_Y: камера работает по Onvif только в режиме совместимости, поиском как Onvif не находится.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В Axxon Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.","In Axxon Next, the search does not find the device's firmware. you must select the right firmware yourself. The V1.0.26_Y firmware: Via the ONVIF protocol, the camera works only in compatibility mode; the search does not find the camera as a device that supports ONVIF. The camera has the ***Video Parameters *** option (the max. resolution and max. frame rate). In Axxon Next, you must make sure that there is not conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value."]
["Yudor Technologies","Yudor CO-YUC-H696RP","Camera ","V1.0.26_Y","1","2",null,null,"+",null,null,"1600x1200",null,null,"+","-","+","+","+","+","Поиск в Axxon Next не определяет прошивку: ее нужно выбрать самостоятельно.Прошивка V1.0.26_Y: камера работает по Onvif только в режиме совместимости, поиском как Onvif не находится.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В Axxon Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.","In Axxon Next, the search does not find the device's firmware. you must select the right firmware yourself. The V1.0.26_Y firmware: Via the ONVIF protocol, the camera works only in compatibility mode; the search does not find the camera as a device that supports ONVIF. The camera has the ***Video Parameters *** option (the max. resolution and max. frame rate). In Axxon Next, you must make sure that there is not conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value."]
["Yudor Technologies","Yudor CO-YUC-H696RW","Camera ","V1.0.20_Y","1","2",null,null,"+",null,null,"1600x1200",null,null,"+","-","+","+","+","+","Поиск в Axxon Next не определяет прошивку: ее нужно выбрать самостоятельно.На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В Axxon Next необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект перед работой с камерой необходимо выбрать нужное значение в веб-интерфейсе.","In Axxon Next, the search does not find the device's firmware. you must select the right firmware yourself. The camera has the ***Video Parameters *** option (the max. resolution and max. frame rate). In Axxon Next, you must make sure that there is not conflict between the current settings and the selected value of this option. In Intellect, before using the camera, go to the web interface and select the required value."]
["Yudor Technologies","Yudor YUC-H686 / YUC-H626 / YUC-Hi26 / YUC-HL26 / YUC-7A26 / YUC-H7926 ","Camera ","VC1.0.10","1","2","+",null,"+",null,null,"1920х1080","+",null,"+.","+.",null,"+","+.","motion detection."]
["Yudor Technologies","Yudor YUC-H796R","Camera ","1.0.38_Y","1","2","+",null,"+",null,null,"1600x1200","+",null,"-","-",null,"+","+","motion detection.","1. На камере есть опция \"Параметры видео\" (максимальные разрешение и частота кадров). В AN необходимо контролировать конфликт текущих настроек с выбранным значением данной опции. В Интеллект после добавления камеры необходимо выбрать нужное значение в веб-интерфейсе.\n2. Протокол ONVIF: при переключение кодека с MJPEG на H.264 - нет видео. Проблема устройства. Чтобы получить видео необходимо выставить кодек в веб-интерфейсе и перезапустить продукт\n","1. The camera has the Video Parameters option (the max. resolution and max. frame rate). In the AxxonSoft products, you must make sure that this setting doesn't conflict with settings on the VMS. In AxxonSoft Intellect, after adding the camera, go to the web interface and select the required value.\n2. ONVIF: when you switch from MJPEG to H.264, video stream is lost. This is a problem of the camera itself. To get video, go to the camera's web interface, select a codec and restart the VMS.\n"]
["ZAVIO ","ZAVIO F3115","Camera ","M2.1.6.02 ","1","4","+","+","+",null,null,"1280x800 ","+"]
["ZAVIO ","ZAVIO B5111 ","Camera ","M2.1.6.03C019","1","4","+","+","+",null,null,"from WEB ","+",{"$nulls":7}," Разрешение в ПО ITV/Axxon меняется только после смены кодека. Это особенность текущей прошивки. \n\n","Resolution in Axxon SW changes only after codec changing. This is a limitation of the current firmware."]
["ZAVIO ","ZAVIO F531E ","Camera ","LM.1.6.18P10","1","1",null,"+",{"$nulls":3},"640x480 ","+"]
["ZAVIO ","ZAVIO F7210 ","Camera ","M2.1.6.01C2 ","1","5","+","+","+",null,null,"1920x1080","+"]

{"sheet":"AxxonNext (ONVIF)","index":5,"n_rows":249,"n_cols":5,"rows_kept":249,"flags":["formulas_cached_only"]}
["Vendor","Model","Firmware","Notes","Notes in English"]
["3S Vision","3S Vision N1011","V1.03_STD-1"]
["3S Vision","3S Vision N1031","V1.02_STD-1"]
["3S Vision","3S Vision N1072","V1.09_STD-1"]
["3S Vision","3S Vision N3011","V1.03_STD-1"]
["3S Vision","3S Vision N3031","V1.02_STD-1"]
["3S Vision","3S Vision N3072","V1.07_STD-1"]
["3S Vision","3S Vision N5011","V1.05_STD-1"]
["3S Vision","3S Vision N5012","V1.05_STD-1"]
["3S Vision","3S Vision N5013","V1.01_STD-1"]
["3S Vision","3S Vision N6013","V1.03_STD-1"]
["3S Vision","3S Vision N6033","V1.02_STD-1"]
["3S Vision","3S Vision N6076","V1.07_STD-1"]
["3S Vision","3S Vision N8012","V1.03_STD-1"]
["3S Vision","3S Vision N8032","V1.02_STD-1"]
["3S Vision","3S Vision N8072","V1.07_STD-1"]
["3S Vision","3S Vision N9071","V1.10_STD-1"]
["3S Vision","3S Vision S2071","V1.06_STD-1"]
["3S Vision","3S Vision S4071","V1.06_STD-1"]
["Acumen","Acumen AiP-B34","1.0.496(Ai)"]
["Acumen","Acumen AiP-M53","1.1.004(Ai)"]
["Avigilon","Avigilon xx-H3PTZ-xx","2.4.4.26(7969) "]
["Avigilon","Avigilon xx-H3-xx","2.4.2.16(7966)"]
["Canon","Canon VB-H41","1.0.0"]
["Canon","Canon VB-H410","1.0.0"]
["Canon","Canon VB-H6100D","1.0.0"]
["Canon","Canon VB-H6100VE","1.0.0"]
["Canon","Canon VB-H610D","1.0.0"]
["Canon","Canon VB-H610VE","1.0.0"]
["Canon","Canon VB-H7100F","1.0.0"]
["Canon","Canon VB-H710F","1.0.0"]
["Canon","Canon VB-S300D","1.0.0"]
["Canon","Canon VB-S30D","1.0.0"]
["Canon","Canon VB-S310D","1.0.0"]
["Canon","Canon VB-S31D","1.0.0"]
["Canon","Canon VB-S8000D","1.0.0"]
["Canon","Canon VB-S800D","1.0.0"]
["Canon","Canon VB-S9000F","1.0.0"]
["Canon","Canon VB-S900F","1.0.0"]
["Dahua","Dahua DH-IPC-HD2100","V4.1.1"]
["Dahua","Dahua DH-IPC-HD3100","V4.1.1"]
["Dahua","Dahua DH-IPC-HD3200","V4.1.1"]
["Dahua","Dahua DH-IPC-HDB3100","V4.1.1"]
["Dahua","Dahua DH-IPC-HDB3101","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDB3110","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDB3200","V4.1.1"]
["Dahua","Dahua DH-IPC-HDB3200C","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDB3202","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDB3300","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDBW3100","V4.1.1"]
["Dahua","Dahua DH-IPC-HDBW3101","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDBW3110","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDBW3200","V4.1.1"]
["Dahua","Dahua DH-IPC-HDBW3300","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HDW2100","V4.1.1"]
["Dahua","Dahua DH-IPC-HDW3100","V4.1.1"]
["Dahua","Dahua DH-IPC-HDW3200S","V4.1.1"]
["Dahua","Dahua DH-IPC-HF3100","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HF3101","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HF3110","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HF3200","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HF3211","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HF3300","V2.103.02"]
["Dahua","Dahua DH-IPC-HF3500","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HFW2100","V4.1.1"]
["Dahua","Dahua DH-IPC-HFW3110","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HFW3200C","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HFW3200S","V4.1.1"]
["Dahua","Dahua DH-IPC-HFW3202C","V4.1.1"]
["Dahua","Dahua DH-IPC-HFW3300","V2.2.6.1"]
["Dahua","Dahua DH-IPC-HFW3300C","V2.2.6.1"]
["Dahua","Dahua DH-IPC-K100A","V4.1.1"]
["Dahua","Dahua DH-SD6580C-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6580-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6581-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6582A-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6582-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6582-HNI","V2.2.6.1"]
["Dahua","Dahua DH-SD65XX-HN","V2.103.02"]
["Dahua","Dahua DH-SD6980C-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6980-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6981-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6982A-HN","V2.2.6.1"]
["Dahua","Dahua DH-SD6982-HN","V2.2.6.1"]
["Dahua","Dahua DH-SDZ1018","V4.1.1"]
["Dahua","Dahua DH-SDZ2020","V4.1.1"]
["Dahua","Dahua HD-IPC-HDW3200","V4.1.1"]
["Dahua","Dahua IPC-HDBW3202","V2.2.6.1"]
["Dahua","Dahua IPC-HFW3101C","V2.2.6.1"]
["Digimerge ","Digimerge DNB14TL2","v1.6_build044014_104 "]
["Digimerge ","Digimerge SyncroIP (DNB14TL2, DNB13TL2, DND13TL2, DNE14TL2, DNV14TL2 )","v1.6_build044014_148"]
["FLIR","FLIR A310PT","Nexus v2.5.16.0"]
["FLIR","FLIR D-Series","Nexus v2.5.16.0 "]
["FLIR","FLIR F-Series","Nexus v2.5.16.0  "]
["FLIR","FLIR FC-Series","Nexus v2.5.15.0"]
["FLIR","FLIR F-Series","Nexus v2.5.16.0"]
["FLIR","FLIR PT-Series","Nexus v2.5.16.0"]
["FLIR","FLIR SyncroIP (DNB14TL2, DNB13TL2, DND13TL2, DNE14TL2, DNV14TL2 )","v1.6_build044014_148"]
["FLIR","FLIR TrafiBot","4.13.0"]
["FLIR","FLIR Traficon VIP-TX","4.13.0"]
["GeoVision ","GeoVision GV-BL1200","v2.059"]
["GeoVision ","GeoVision GV-BL120D","v2.059"]
["GeoVision ","GeoVision GV-BL1210","v2.059"]
["GeoVision ","GeoVision GV-BL1300","v2.059"]
["GeoVision ","GeoVision GV-BL130D","v2.059"]
["GeoVision ","GeoVision GV-BL1500","v2.059"]
["GeoVision ","GeoVision GV-BL220D","v2.059"]
["GeoVision ","GeoVision GV-BL2400","v2.059"]
["GeoVision ","GeoVision GV-BL2410","v2.059"]
["GeoVision ","GeoVision GV-BL2500","v2.09"]
["GeoVision ","GeoVision GV-BL320D","v2.059"]
["GeoVision ","GeoVision GV-BL3400","v2.059"]
["GeoVision ","GeoVision GV-BL3410 ","v2.059"]
["GeoVision ","GeoVision GV-BL5310","v2.059"]
["GeoVision ","GeoVision GV-BX120D","v2.059"]
["GeoVision ","GeoVision GV-BX1300","v2.059"]
["GeoVision ","GeoVision GV-BX130D","v2.059"]
["GeoVision ","GeoVision GV-BX140DW","v2.059"]
["GeoVision ","GeoVision GV-BX1500 ","v2.059"]
["GeoVision ","GeoVision GV-BX1500-E","v2.059"]
["GeoVision ","GeoVision GV-BX220D","v2.059"]
["GeoVision ","GeoVision GV-BX2400","v2.059"]
["GeoVision ","GeoVision GV-BX2500","v2.09"]
["GeoVision ","GeoVision GV-BX320D","v2.059"]
["GeoVision ","GeoVision GV-BX3400","v2.059"]
["GeoVision ","GeoVision GV-BX520D","v2.059"]
["GeoVision ","GeoVision GV-BX5300","v2.059"]
["GeoVision ","GeoVision GV-CA120","v2.059"]
["GeoVision ","GeoVision GV-CA220","v2.059"]
["GeoVision ","GeoVision GV-CAW120","v2.059"]
["GeoVision ","GeoVision GV-CAW220","v2.059"]
["GeoVision ","GeoVision GV-CB120","v2.059"]
["GeoVision ","GeoVision GV-CB220","v2.059"]
["GeoVision ","GeoVision GV-CBW120","v2.059"]
["GeoVision ","GeoVision GV-CBW220 ","v2.059"]
["GeoVision ","GeoVision GV-CR420","v1.019"]
["GeoVision ","GeoVision GV-EBL1100","v1.00"]
["GeoVision ","GeoVision GV-EBX1100","v1.00"]
["GeoVision ","GeoVision GV-EFD1100","v1.00"]
["GeoVision ","GeoVision GV-FD1200","v2.059"]
["GeoVision ","GeoVision GV-FD120D","v2.059"]
["GeoVision ","GeoVision GV-FD1500","v2.059"]
["GeoVision ","GeoVision GV-FD1510","v2.09"]
["GeoVision ","GeoVision GV-FD220D","v2.059"]
["GeoVision ","GeoVision GV-FD2400","v2.059"]
["GeoVision ","GeoVision GV-FD2500","v2.09"]
["GeoVision ","GeoVision GV-FD2510","v2.09"]
["GeoVision ","GeoVision GV-FD3400","v2.059"]
["GeoVision ","GeoVision GV-FD5300 ","v2.059"]
["GeoVision ","GeoVision GV-FE2301","v2.059"]
["GeoVision ","GeoVision GV-FE420 ","v2.059"]
["GeoVision ","GeoVision GV-FE4301","v2.059"]
["GeoVision ","GeoVision GV-FE520 ","v2.059"]
["GeoVision ","GeoVision GV-FER521 ","v2.059"]
["GeoVision ","GeoVision GV-Hybrid","v1.019"]
["GeoVision ","GeoVision GV-MDR120","v2.059"]
["GeoVision ","GeoVision GV-MDR220","v2.059"]
["GeoVision ","GeoVision GV-MDR2400 ","v2.059"]
["GeoVision ","GeoVision GV-MDR320 ","v2.059"]
["GeoVision ","GeoVision GV-MDR3400","v2.059"]
["GeoVision ","GeoVision GV-MDR520 ","v2.059"]
["GeoVision ","GeoVision GV-MFD120","v2.059"]
["GeoVision ","GeoVision GV-MFD130","v2.059"]
["GeoVision ","GeoVision GV-MFD1501","v2.059"]
["GeoVision ","GeoVision GV-MFD220 ","v2.059"]
["GeoVision ","GeoVision GV-MFD2501","v2.09"]
["GeoVision ","GeoVision GV-MFD320","v2.059"]
["GeoVision ","GeoVision GV-MFD520","v2.059"]
["GeoVision ","GeoVision GV-PT130D","v2.099"]
["GeoVision ","GeoVision GV-PT220D","v2.099"]
["GeoVision ","GeoVision GV-PT320D","v2.099"]
["GeoVision ","GeoVision GV-SD200 ","V103"]
["GeoVision ","GeoVision GV-SD200-S","V103"]
["GeoVision ","GeoVision GV-SD220","v1.009"]
["GeoVision ","GeoVision GV-SD220-S ","v1.009"]
["GeoVision ","GeoVision GV-UBL3401","v2.059"]
["GeoVision ","GeoVision GV-UBX1301","v2.059"]
["GeoVision ","GeoVision GV-UBX2301 ","v2.059"]
["GeoVision ","GeoVision GV-UBX3301 ","v2.059"]
["GeoVision ","GeoVision GV-UFD1501","v2.09"]
["GeoVision ","GeoVision GV-UFD2501","v2.09"]
["GeoVision ","GeoVision GV-VD1200 ","v2.059"]
["GeoVision ","GeoVision GV-VD120D","v2.059"]
["GeoVision ","GeoVision GV-VD1500","v2.059"]
["GeoVision ","GeoVision GV-VD1540","v2.09"]
["GeoVision ","GeoVision GV-VD1540-E","v2.09"]
["GeoVision ","GeoVision GV-VD220D","v2.059"]
["GeoVision ","GeoVision GV-VD2400","v2.059"]
["GeoVision ","GeoVision GV-VD2430","v2.09"]
["GeoVision ","GeoVision GV-VD2500","v2.09"]
["GeoVision ","GeoVision GV-VD320D","v2.059"]
["GeoVision ","GeoVision GV-VD3400","v2.059"]
["GeoVision ","GeoVision GV-VD3440","v2.09"]
["GeoVision ","GeoVision GV-VD3440-E","v2.09"]
["GeoVision ","GeoVision GV-VD5300","v2.059"]
["GeoVision ","GeoVision V-FD320D ","v2.059"]
["Honeywell","Honeywell HDZ20HDEX","HS20131118NSA"]
["iCanTek","iCanView326MP","1.0.6"]
["iCanTek","iCanView346MP","1.0.6"]
["iCanTek","iCanView390MP ","2.0.34"]
["iCanTek","iCanView392MP","2.0.34"]
["Legrand","Legrand Seried3:IP Speed Domes","2.103.General 00.0.R, build: 2013-07-17(V4.1.1)"]
["Legrand","Legrand Series 1: IP Cameras","2.103.General 00.0.R, build: 2013-07-27(V4.1.1)"]
["Legrand","Legrand Series 2: IP Cameras","2.103.General 00.0.R, build: 2013-07-27(V4.1.1) "]
["Legrand","Legrand Series 4: IP Cameras","2.103.General 00.0.R, build: 2013-07-27(V4.1.1)"]
["Legrand","Legrand Series 5 : IP Speed Domes","2.211.General 00.0.R, build: 2013-10-08(V4.1.1) "]
["NEXCOM ","NEXCOM NCb-301","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCb-311","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCi-301-V","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCi-311","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCi-311-R","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCi-312","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCm-301-2V","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCM-301-V","NexWare_01.00.0009"]
["NEXCOM ","NEXCOM NCo-301-VHR","NexWare_01.00.0010"]
["NEXCOM ","NEXCOM NCr-301-VHR","NexWare_01.00.0010"]
["Qihan","Qihan IPCamera","v2.3.4"]
["RVi","RVi RVi-IPC12","6.C.2.11896"]
["RVi","RVi RVi-IPC12W","6.C.2.11896"]
["RVi","RVi RVi-IPC20DN","V045_1"]
["RVi","RVi RVi-IPC21","V017_1"]
["RVi","RVi RVi-IPC21DN","V047_1"]
["RVi","RVi RVi-IPC21DNL","V082_1"]
["RVi","RVi RVi-IPC22DN","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)"]
["RVi","RVi RVi-IPC23DN","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)"]
["RVi","RVi RVi-IPC23DN","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)  "]
["RVi","RVi RVi-IPC31DN","V053_1"]
["RVi","RVi RVi-IPC31DNL","V110_1"]
["RVi","RVi RVi-IPC32DNS","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)  "]
["RVi","RVi RVi-IPC32M","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)"]
["RVi","RVi RVi-IPC41DNL","V0114_1"]
["RVi","RVi RVi-IPC41DNS","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)  "]
["RVi","RVi RVi-IPC42DN","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1) "]
["RVi","RVi RVi-IPC42DNS","2.211.Group 00.0.R, build: 2013-09-02(V4.1.1)  "]
["RVi","RVi RVi-IPC50DN36","V035_1"]
["RVi","RVi RVi-IPC51DN18","V069_1"]
["RVi","RVi RVI-IPC52DN20","2.103.Group 00.0.R, build: 2013-08-22(V4.1.1)  "]
["RVi","RVi RVi-IPS125","V029_1"]
["RVi","RVi RVi-IPS125A","2.608.GP00.0.T,Build:2013-11-4(V2.2.5.1)  "]
["RVi","RVi RVi-IPS4100A","2.608.GP00.0.T,Build:2013-11-4(V2.2.5.1)  "]
["Stream Labs","Stream Labs WaveCam S1","0.2.0.0"]
["Stream Labs","Stream Labs WaveCam S1V","2.13.7.10"]
["Stream Labs","Stream Labs WaveServer 3554","2.13.7.10"]
["Stream Labs","Stream Labs WaveServer R3554","2.13.7.10"]
["Surveon","Surveon 2301A","V2.1.E04"]
["Surveon","Surveon 4321","V2.1.E04"]
["Surveon","Surveon 4361","V2.1.E04"]
["Surveon","Surveon CAM6181","fr20130223NSA"]
["Surveon","Surveon CAM6351","fr20130223NSA"]

{"sheet":"Special Notes","index":6,"n_rows":14,"n_cols":3,"rows_kept":14,"flags":["formulas_cached_only"]}
["Brand","Особые заметки ","Special comments "]
["!ONVIF","Работа устройства за NAT не поддерживается. Устройство должно быть с отдельным внешним IP адресом."," It's not supported if device is connected via NAT. It must have separate external IP address."]
["!PSIA","Работа устройства за NAT не поддерживается. Устройство должно быть с отдельным внешним IP адресом."," It's not supported if device is connected via NAT. It must have separate external IP address."]
["ACTi","В случае проблем с видеопотоком (рывки, артефакты изображения) рекомендуется отключить в веб-интерфейсе RTP B2 заголовки (запрос http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&RTP_B2=1) или обновить устройство на последнюю версию прошивки.","If you have problems with video such as artifacting etc., you should disable the RTP B2 headings in the web interface (go to http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&RTP_B2=1) or update the firmware."]
["Arecont Vision","В случае, если устройство имеет логин и пароль не по умолчанию, поиск будет работать некорректно - камеру нужно добавлять вручную.","If there's a non-default login and password setting on the device, it will be identified incorrectly and you will have to add it manually."]
["AXIS","Для получения видео с кодеком H264 в ПО ITV/Axxon в настройках RTSP на камере должен быть указан 554 порт. Поддержка протокола Multicast реализована только для кодеков H264 и MPEG4.","To receive video using codec H264 in ITV | AxxonSoft products in device settings RTSP port must be set as 554 port. To use multicast protocol support need to select H264 and MPEG4 codecs."]
["Bosch","Информация по h263:\n1. Для того, чтобы получить видео в ПО ITV в веб-интерфейсе камеры необходимо выбрать кодек MPEG4-SH++, а в Интеллекте выбрать граббер \"Bosch\".\n2. Для корректного воспроизведения видео необходимо в веб-интерфейсе камеры менять значение параметра \"I-frame distance\" c 0 на любое другое. \n\nДругие примечания:\nВ случае, если для камеры Jassun установлена надстройка ActiveX, при работе с камерой Bosch могут возникать ошибки. Данная надстройка предлагается к установке при входе в веб интерфейс камеры.","Comments on H263:\n1. To get video in Intellect, choose Bosch grabber in the VMS and select MPEG4-SH++ in the camera's web interface.\n2. To get video playback right, the \"I-frame distance\" value in the camera's web interface must be other than 0. \nOther notes:\nIn case if for Jassun device installed ActiveX superstructure, while working with Bosch devices may be issues. This superstructure is proposed to be installed with entrance to camera's web interface."]
["EverFocus","Чтобы в Интеллекте работал аудио-выход в настройках динамика необходимо выбрать кодек \"VNDR.0.9\".","To make audio output in Intellect work, select VNDR.0.9 codec in the speaker settings."]
["Grandstream","В Интеллект вендору \"Grandstream\" соответствуют платы видеоввода \"GS\".","In Intellect, Grandstream products correspond to the GS video capture cards."]
["Jassun","В случае, если для камеры Jassun установлена надстройка ActiveX, при работе с камерой Bosch могут возникать ошибки. Данная надстройка предлагается к установке при входе в веб интерфейс камеры.","In case if for Jassun device installed ActiveX superstructure, while working with Bosch devices may be issues. This superstructure is proposed to be installed with entrance to camera's web interface."]
["Panasonic i-Pro","Поддержка протокола Multicast реализована только для кодеков H264 и MPEG4.","To use multicast protocol support need to select H264 and MPEG4 codecs."]
["Sony","Поддержка протокола Multicast реализована только для кодеков H264 и MPEG4.","To use multicast protocol support need to select H264 and MPEG4 codecs."]
["Stretch","В ПО VideoIQ7 не работает кодек SVC.","In VideoIQ7, the SVC codec doesn't work."]
["Vivotek","Частота опорных кадров для кодеков H264 и MPEG4 в Интеллекте настраивается в миллисекундах и может принимать следующие значения: 250, 500, 1000, 2000, 3000, 4000.","In Intellect, you can set up the keyframe rate of H264 and MPEG4 in milliseconds at: 250, 500, 1000, 2000, 3000, 4000."]

{"sheet":"AS IS","index":7,"n_rows":3,"n_cols":2,"rows_kept":3,"flags":["formulas_cached_only"]}
["Vendor","Model "]
["RTSP-protocol","RTSP-client"]
[null,"web-cam / usb-cam"]

{"sheet":"Out of Support","index":8,"n_rows":2,"n_cols":2,"rows_kept":2,"flags":["formulas_cached_only"]}
["Vendor","Model "]
["StreamLabs","WaveHub"]